{"text_format":"1","workbook":"xlsx","n_sheets":8,"sheets":["EI Calculation","HEL determination ","Area 1","Area 2","Area 3","Area 4","Area 5","R_Values"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":1,"defined_names":180,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"EI Calculation","index":0,"n_rows":31,"n_cols":16,"rows_kept":31,"cut":false,"hidden":false,"merged":[[4,13,7,14],[0,6,3,14],[4,1,4,5],[5,1,5,2],[6,1,6,2],[4,10,4,12],[5,10,5,12],[7,1,7,2],[0,0,3,5]]}
[null,null,null,null,null,null,"Soil Erodibility Index for HEL Determinations"]
[]
[]
[]
["Producer:",null,null,null,null,null,null,null,null,"By:",null,null,null,null,null,"EI = erodibility index"]
["Farm:",null,null,null,null,null,null,null,null,"Date:",{"$f":"TODAY()","v":"2012-05-23"},null,null,null,null,"R = rainfall and runoff"]
["Tract:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"K = susceptibility of the soil to water erosion"]
["County:","Select",null,null,null,null,null,null,null,null,null,null,null,null,null,"LS = the combined effects of slope length and steepness"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T = soil loss tolerance"]
["Field Number","Soil Musym","Soil Name","Slope %","Slope Length (FT)","R","x","K","x","LS","/","T","=","EI","HEL if EI =>8"]
[null,"Select",{"$f":"VLOOKUP(B11,INDIRECT($B$8&\"_data\"),3,FALSE)","v":"none"},null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,{"$f":"VLOOKUP(B11,INDIRECT($B$8&\"_data\"),5,FALSE)","v":0},null,{"$f":"SUM((0.065+(0.0456*(D11)))+(0.006541*(D11^2)))*((E11/72.5)^IF(D11<1,0.2,IF(AND(1<=D11,D11<3),0.3,IF(AND(3<=D11,D11<5),0.4,0.5))))","v":0},null,{"$f":"VLOOKUP(B11,INDIRECT($B$8&\"_data\"),4,FALSE)","v":0},null,{"$f":"IF(J11>0,((F11*H11*J11)/L11),0)","v":0},{"$f":"(IF(N11>8,\"HEL\",\"NHEL\"))","v":"NHEL"}]
[null,"Select",{"$f":"VLOOKUP(B12,INDIRECT($B$8&\"_data\"),3,FALSE)","v":"none"},null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,{"$f":"VLOOKUP(B12,INDIRECT($B$8&\"_data\"),5,FALSE)","v":0},null,{"$f":"SUM((0.065+(0.0456*(D12)))+(0.006541*(D12^2)))*((E12/72.5)^IF(D12<1,0.2,IF(AND(1<=D12,D12<3),0.3,IF(AND(3<=D12,D12<5),0.4,0.5))))","v":0},null,{"$f":"VLOOKUP(B12,INDIRECT($B$8&\"_data\"),4,FALSE)","v":0},null,{"$f":"IF(J12>0,((F12*H12*J12)/L12),0)","v":0},{"$f":"(IF(N12>8,\"HEL\",\"NHEL\"))","v":"NHEL"}]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,{"$f":"SUM((0.065+(0.0456*(D13)))+(0.006541*(D13^2)))*((E13/72.5)^IF(D13<1,0.2,IF(AND(1<=D13,D13<3),0.3,IF(AND(3<=D13,D13<5),0.4,0.5))))","v":0},null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]
[null,"Select","none",null,null,{"$f":"VLOOKUP($B$8,R_Values!$A$3:$B$91,2,FALSE)","v":0},null,0,null,0,null,0,null,0,"NHEL"]

{"sheet":"HEL determination ","index":1,"n_rows":53,"n_cols":13,"rows_kept":53,"cut":false,"hidden":false,"merged":[[0,0,3,3],[51,0,51,2],[52,0,52,2],[0,4,3,8],[50,0,50,2],[4,1,4,4],[5,1,5,4],[6,1,6,4],[4,7,4,8],[5,7,5,8],[6,7,6,8],[44,6,45,6],[44,7,45,7],[46,0,46,7],[47,0,48,7],[16,6,17,6],[49,0,49,3],[16,7,17,7],[30,6,31,6],[30,7,31,7],[32,0,32,7],[33,0,34,7],[19,0,20,7],[18,0,18,7]]}
[null,null,null,null,"HEL Determination Sheet"]
[]
[]
[]
["Producer:",null,null,null,null,null,"By:",null,null,null,null,null,"This field is HEL based on the determination.  Soil map units with HEL Class 1 (HEL) constitute 33.33 percent or more of the acreage in the field."]
["Farm:",null,null,null,null,null,null,{"$f":"TODAY()","v":"2012-05-23"},null,null,"HEL",null,"This field is HEL based on the determination.  This field contains 50 or more acres of soil map units with HEL Class 1 (HEL)"]
["Tract:",null,null,null,null,null,"County:","Select",null,null,"NHEL",null,"This field is NHEL based on the determination.  Soil map units with HEL Class 3 (NHEL) constitute 66.67 percent or more of the acreage in the field, and soil map units with HEL Class 1 (HEL) do not equal 50 acres or more."]
[null,null,null,null,null,null,null,null,null,null,null,null,"This determination was completed in the field by NRCS."]
["Field Number:",null,"Soil MUSYM","Soil Acres","% of Field","HEL Class"]
["Field Acres:",null,"Select",null,{"$f":"IF(D10>0,D10/$B$10,\"\")","v":""},null,null,null,null,null,{"$f":"IF(F10=\"HEL\",E10,0)","v":0}]
[null,null,"Select",null,{"$f":"IF(D11>0,D11/$B$10,\"\")","v":""},null,null,null,null,null,{"$f":"IF(F11=\"HEL\",E11,0)","v":0}]
[null,null,"Select",null,"",null,null,null,null,null,{"$f":"IF(F12=\"HEL\",E12,0)","v":0}]
[null,null,"Select",null,{"$f":"IF(D13>0,D13/$B$10,\"\")","v":""},null,null,null,null,null,{"$f":"IF(F13=\"HEL\",E13,0)","v":0}]
[null,null,"Select",null,"",null,null,null,null,null,0]
[null,null,"Select",null,"",null,null,null,null,null,0]
[null,null,"Select",null,"",null,null,null,null,null,0]
[null,null,"Select",null,"",null,"HEL Determination:",{"$f":"IF(K19>33.32,\"HEL\",IF((K19/100)*B10>49.99,\"HEL\",\"NHEL\"))","v":"NHEL"},null,null,0]
[null,null,"Select",null,"",null,null,null,null,null,0]
["Determination Notes or Comments",null,null,null,null,null,null,null,null,null,{"$f":"SUM(K10:K18)*100","v":0}]
[]
[]
[]
["Field Number:",null,"Soil MUSYM","Soil Acres","% of Field","HEL Class"]
["Field Acres:",null,"Select",null,{"$f":"IF(D24>0,D24/$B$24,\"\")","v":""},null,null,null,null,null,{"$f":"IF(F24=\"HEL\",E24,0)","v":0}]
[null,null,"Select",null,{"$f":"IF(D25>0,D25/$B$24,\"\")","v":""},null,null,null,null,null,{"$f":"IF(F25=\"HEL\",E25,0)","v":0}]
[null,null,"Select",null,{"$f":"IF(D26>0,D26/$B$24,\"\")","v":""},null,null,null,null,null,{"$f":"IF(F26=\"HEL\",E26,0)","v":0}]
[null,null,"Select",null,"",null,null,null,null,null,0]
[null,null,"Select",null,"",null,null,null,null,null,0]
[null,null,"Select",null,"",null,null,null,null,null,0]
[null,null,"Select",null,"",null,null,null,null,null,0]
[null,null,"Select",null,"",null,"HEL Determination:",{"$f":"IF(K33>33.32,\"HEL\",IF((K33/100)*B24>49.99,\"HEL\",\"NHEL\"))","v":"NHEL"},null,null,0]
[null,null,"Select",null,"",null,null,null,null,null,0]
["Determination Notes or Comments",null,null,null,null,null,null,null,null,null,{"$f":"SUM(K24:K32)*100","v":0}]
[]
[]
[]
["Field Number:",null,"Soil MUSYM","Soil Acres","% of Field","HEL Class"]
["Field Acres:",null,"Select",null,{"$f":"IF(D38>0,D38/$B$38,\"\")","v":""},null,null,null,null,null,{"$f":"IF(F38=\"HEL\",E38,0)","v":0}]
[null,null,"Select",null,{"$f":"IF(D39>0,D39/$B$38,\"\")","v":""},null,null,null,null,null,{"$f":"IF(F39=\"HEL\",E39,0)","v":0}]
[null,null,"Select",null,"",null,null,null,null,null,0]
[null,null,"Select",null,"",null,null,null,null,null,0]
[null,null,"Select",null,"",null,null,null,null,null,{"$f":"IF(F42=\"HEL\",E42,0)","v":0}]
[null,null,"Select",null,"",null,null,null,null,null,{"$f":"IF(F43=\"HEL\",E43,0)","v":0}]
[null,null,"Select",null,"",null,null,null,null,null,0]
[null,null,"Select",null,"",null,"HEL Determination:",{"$f":"IF(K47>33.32,\"HEL\",IF((K47/100)*B38>49.99,\"HEL\",\"NHEL\"))","v":"NHEL"},null,null,0]
[null,null,"Select",null,"",null,null,null,null,null,0]
["Determination Notes or Comments",null,null,null,null,null,null,null,null,null,{"$f":"SUM(K38:K46)*100","v":0}]
[]
[]
["IF the highly erodible soil map units in a field. . .",null,null,null,"THEN the field is…",null,"Designation Definitions:"]
["Constitute 33.33 percent or more of the acreage in the field,",null,null,">>>","HEL",null,"HEL = Highly Erodible Land"]
["Equal 50 or more acres,",null,null,">>>","HEL",null,"NHEL = Not Highly Erodible Land"]
["Do not constitute 33.33 percent nor equal 50 or more acres",null,null,">>>","NHEL",null,"PHEL = Potentially Highly Erodible Land"]

{"sheet":"Area 1","index":2,"n_rows":1387,"n_cols":7,"rows_kept":1387,"cut":false,"hidden":false,"merged":[]}
["County","symbol","map unit name","Component","T","Kw","HEL"]
[null,"Select","none","none"]
["Allen","Bm","Belmore loam, 0 to 2 percent slopes","Belmore",4,0.32,"NHEL"]
["Allen","BmB","Belmore loam, 2 to 6 percent slopes","Belmore",4,0.32,"PHEL"]
["Allen","BmC2","Belmore loam, 6 to 12 percent slopes, moderately eroded","Belmore",4,0.32,"PHEL"]
["Allen","BmD2","Belmore loam, 12 to 18 percent slopes, moderately eroded","Belmore",4,0.32,"HEL"]
["Allen","Bn","Blount loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Allen","BnB","Blount loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Allen","Bo","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Allen","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Allen","BoB2","Blount silt loam, 2 to 6 percent slopes, moderately eroded","Blount",3,0.43,"PHEL"]
["Allen","Bp","Borrow pits","Borrow"]
["Allen","CaB","Casco silt loam, 0 to 6 percent slopes","Casco",3,0.24,"PHEL"]
["Allen","CfC2","Casco and Fox soils, 6 to 12 percent slopes, moderately eroded","Casco",3,0.24,"PHEL"]
["Allen","Co","Colwood loam","Colwood",5,0.28000000000000003,"NHEL"]
["Allen","Cw","Colwood silt loam","Colwood",5,0.28000000000000003,"NHEL"]
["Allen","Db","Digby fine sandy loam, 0 to 2 percent slopes","Digby",4,0.24,"NHEL"]
["Allen","DbB","Digby fine sandy loam, 2 to 6 percent slopes","Digby",4,0.24,"PHEL"]
["Allen","Dm","Digby loam, 0 to 2 percent slopes","Digby",4,0.32,"NHEL"]
["Allen","DmB","Digby loam, 2 to 6 percent slopes","Digby",4,0.32,"PHEL"]
["Allen","Ds","Digby silt loam, 0 to 2 percent slopes","Digby",4,0.32,"NHEL"]
["Allen","DsB","Digby silt loam, 2 to 6 percent slopes","Digby",4,0.32,"PHEL"]
["Allen","Em","Eel silt loam","Eel",5,0.37,"NHEL"]
["Allen","FoB","Fox loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Allen","Gn","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Allen","Gp","Gravel pit","Gravel"]
["Allen","Ha","Haney fine sandy loam, 0 to 2 percent slopes","Haney",4,0.28000000000000003,"NHEL"]
["Allen","HaB","Haney fine sandy loam, 2 to 6 percent slopes","Haney",4,0.28000000000000003,"PHEL"]
["Allen","Hd","Haney loam, 0 to 2 percent slopes","Haney",4,0.32,"NHEL"]
["Allen","HdB","Haney loam, 2 to 6 percent slopes","Haney",4,0.32,"PHEL"]
["Allen","HdC2","Haney loam, 6 to 12 percent slopes, moderately eroded","Haney",4,0.32,"PHEL"]
["Allen","Hf","Haney silt loam, 0 to 2 percent slopes","Haney",4,0.32,"NHEL"]
["Allen","HfB","Haney silt loam, 2 to 6 percent slopes","Haney",4,0.32,"PHEL"]
["Allen","Hh","Haskins and Digby fine sandy loams, over clay, 0 to 2 percent slopes","Haskins",4,0.24,"NHEL"]
["Allen","HhB","Haskins and Digby fine sandy loams, over clay, 2 to 6 percent slopes","Haskins",4,0.24,"PHEL"]
["Allen","Hk","Haskins and Digby loams, over clay, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Allen","HkB","Haskins and Digby loams, over clay, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Allen","Hm","Haskins and Digby silt loams, over clay, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Allen","HmB","Haskins and Digby silt loams, over clay, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Allen","Hs","Hoytville silt loam","Hoytville",5,0.28000000000000003,"NHEL"]
["Allen","Ht","Hoytville silty clay","Hoytville",5,0.28000000000000003,"NHEL"]
["Allen","Hv","Hoytville silty clay loam","Hoytville",5,0.28000000000000003,"NHEL"]
["Allen","Kb","Kibbie loam, 0 to 2 percent slopes","Kibbie",5,0.28000000000000003,"NHEL"]
["Allen","Ks","Kibbie silt loam, 0 to 2 percent slopes","Kibbie",5,0.28000000000000003,"NHEL"]
["Allen","Ln","Lenawee silt loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Allen","Lw","Linwood muck","Linwood",2,null,"NHEL"]
["Allen","Ma","Made land","Made"]
["Allen","Mb","Millgrove loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Allen","Mc","Millgrove loam, over clay","Millgrove",5,0.28000000000000003,"NHEL"]
["Allen","Md","Millgrove silt loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Allen","Mf","Millgrove silt loam, over clay","Millgrove",5,0.28000000000000003,"NHEL"]
["Allen","Mg","Millgrove silty clay loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Allen","Mh","Millgrove silty clay loam, over clay","Millgrove",5,0.28000000000000003,"NHEL"]
["Allen","Mk","Millgrove silty clay","Millgrove",5,0.28000000000000003,"NHEL"]
["Allen","Ml","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Allen","Mm","Montgomery silty clay","Montgomery",5,0.37,"NHEL"]
["Allen","Mn","Montgomery silty clay loam","Montgomery",5,0.37,"NHEL"]
["Allen","MoB","Morley loam, 2 to 6 percent slopes","Morley",3,0.43,"PHEL"]
["Allen","MrB","Morley silt loam, 2 to 6 percent slopes","Morley",3,0.43,"PHEL"]
["Allen","MrB2","Morley silt loam, 2 to 6 percent slopes, moderately eroded","Morley",3,0.43,"PHEL"]
["Allen","MrC","Morley silt loam, 6 to 12 percent slopes","Morley",3,0.43,"PHEL"]
["Allen","MrC2","Morley silt loam, 6 to 12 percent slopes, moderately eroded","Morley",3,0.43,"PHEL"]
["Allen","MrD2","Morley silt loam, 12 to 18 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Allen","MrE2","Morley silt loam, 18 to 25 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Allen","MrF2","Morley silt loam, 25 to 35 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Allen","MsC3","Morley soils, 6 to 12 percent slopes, severely eroded","Morley",2,0.43,"HEL"]
["Allen","Na","Nappanee loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Allen","Np","Nappanee silt loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Allen","NpB","Nappanee silt loam, 2 to 6 percent slopes","Nappanee",3,0.43,"NHEL"]
["Allen","Pa","Pewamo silt loam","Pewamo",5,0.24,"NHEL"]
["Allen","Pc","Pewamo silty clay","Pewamo",5,0.24,"NHEL"]
["Allen","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Allen","Qu","Quarry","Quarry"]
["Allen","Ra","Randolph silt loam, 0 to 2 percent slopes","Randolph",3,0.37,"NHEL"]
["Allen","RmB","Rawson loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Allen","RmC2","Rawson loam, 6 to 12 percent slopes, moderately eroded","Rawson",4,0.32,"PHEL"]
["Allen","RsB","Rawson silt loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Allen","Rt","Rimer and Tedrow loamy fine sands, over clay, 0 to 2 percent slopes","Rimer",4,0.17,"NHEL"]
["Allen","RtB","Rimer and Tedrow loamy fine sands, over clay, 2 to 6 percent slopes","Rimer",4,0.17,"PHEL"]
["Allen","ScB","St. Clair silt loam, 2 to 6 percent slopes","St. Clair",3,0.37,"PHEL"]
["Allen","ScC2","St. Clair silt loam, 6 to 12 percent slopes, moderately eroded","St. Clair",3,0.37,"PHEL"]
["Allen","ScD2","St. Clair silt loam, 12 to 25 percent slopes, moderately eroded","St. Clair",3,0.37,"HEL"]
["Allen","SdB","Seward fine sandy loam, 2 to 6 percent slopes","Seward",4,0.17,"NHEL"]
["Allen","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Allen","Sm","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Allen","Sn","Sloan silty clay loam, over limestone","Sloan",5,0.37,"NHEL"]
["Allen","SpB","Spinks loamy fine sand, 2 to 6 percent slopes","Spnks",5,0.17,"NHEL"]
["Allen","To","Toledo silty clay loam","Toledo",5,0.28000000000000003,"NHEL"]
["Allen","TsB","Tuscola loam, 2 to 6 percent slopes","Tuscola",5,0.32,"PHEL"]
["Allen","TtB","Tuscola silt loam, 2 to 6 percent slopes","Tuscola",5,0.32,"PHEL"]
["Allen","Ur","Urban land","Urban"]
["Allen","Wa","Wabash silty clay","Wabash",5,0.28000000000000003,"NHEL"]
[null,"Select","none","none"]
["Auglaize","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Auglaize","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Auglaize","Ca","Carlisle silty clay loam","Carlisle",2,0.37,"NHEL"]
["Auglaize","Dc","Defiance silty clay, frequently flooded","Defiance",5,0.37,"NHEL"]
["Auglaize","DeA","Del Rey silt loam, till substratum, 0 to 3 percent slopes","Del Rey",3,0.43,"PHEL"]
["Auglaize","DmA","Digby loam, 0 to 2 percent slopes","Digby",4,0.32,"NHEL"]
["Auglaize","DmB","Digby loam, 2 to 6 percent slopes","Digby",4,0.32,"PHEL"]
["Auglaize","DoA","Digby variant silt loam, 0 to 2 percent slopes","Digby",4,0.37,"NHEL"]
["Auglaize","EmB","Eldean loam, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Auglaize","EmC","Eldean loam, 6 to 12 percent slopes","Eldean",4,0.37,"PHEL"]
["Auglaize","EnA","Eldean silt loam, 0 to 3 percent slopes","Eldean",4,0.37,"NHEL"]
["Auglaize","GaB","Gallman loam, 2 to 6 percent slopes","Gallman",5,0.32,"PHEL"]
["Auglaize","Gn","Genesee silt loam, occasionally flooded","Genesee",5,0.37,"NHEL"]
["Auglaize","GwB","Glynwood silt loam, 2 to 6 percent slopes","Glynwood",3,0.43,"PHEL"]
["Auglaize","HkA","Haskins loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Auglaize","HkB","Haskins loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Auglaize","La","Latty silty clay","Latty",5,0.28000000000000003,"NHEL"]
["Auglaize","McA","McGary silt loam, 0 to 4 percent slopes","McGary",3,0.43,"PHEL"]
["Auglaize","Mf","Milford silty clay","Milford",5,0.28000000000000003,"NHEL"]
["Auglaize","Mk","Millgrove clay loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Auglaize","Mp","Montgomery silty clay","Montgomery",5,0.37,"NHEL"]
["Auglaize","MrC2","Morley clay loam, 6 to 12 percent slopes, eroded","Morley",3,0.43,"HEL"]
["Auglaize","MrD2","Morley clay loam, 12 to 18 percent slopes, eroded","Morley",3,0.43,"HEL"]
["Auglaize","Mu","Muskego muck","Muskego",2,null,"NHEL"]
["Auglaize","Po","Pewamo silt loam, overwash","Pewamo",5,0.24,"NHEL"]
["Auglaize","Pw","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Auglaize","Px","Pits, gravel","Pits"]
["Auglaize","Sh","Shoals silt loam, occasionally flooded","Shoals",5,0.37,"NHEL"]
["Auglaize","So","Sloan silty clay loam, frequently flooded","Sloan",5,0.37,"NHEL"]
["Auglaize","Ud","Udorthents, loamy, rolling","Udorthents"]
["Auglaize","W","Water","Water"]
[null,"Select","none","none"]
["Crawford","AdB","Alexandria silt loam, 2 to 6 percent slopes","Alexandria",4,0.37,"PHEL"]
["Crawford","AdC2","Alexandria silt loam, 6 to 12 percent slopes, moderately eroded","Alexandria",4,0.37,"PHEL"]
["Crawford","AdD2","Alexandria silt loam, 12 to 18 percent slopes, moderately eroded","Alexandria",4,0.37,"HEL"]
["Crawford","BgA","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Crawford","BgB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Crawford","BhB","Bennington-Urban land complex, undulating","Bennington",3,0.43,"PHEL"]
["Crawford","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Crawford","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Crawford","BtA","Bogart loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Crawford","BtB","Bogart loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Crawford","Bw","Bono silty clay loam","Bono",5,0.28000000000000003,"NHEL"]
["Crawford","CdB","Cardington silt loam, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Crawford","CdB2","Cardington silt loam, 2 to 6 percent slopes, moderately eroded","Cardington",4,0.37,"PHEL"]
["Crawford","CdC2","Cardington silt loam, 6 to 12 percent slopes, moderately eroded","Cardington",4,0.37,"PHEL"]
["Crawford","CdD2","Cardington silt loam, 12 to 18 percent slopes, moderately eroded","Cardington",4,0.37,"HEL"]
["Crawford","CeC","Cardington-Urban land complex, rolling","Cardington",4,0.37,"PHEL"]
["Crawford","Ck","Carlisle muck","Carlisle",2,null,"NHEL"]
["Crawford","CnA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Crawford","CnB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Crawford","CnC2","Chili loam, 6 to 12 percent slopes, moderately eroded","Chili",4,0.32,"PHEL"]
["Crawford","CnD2","Chili loam, 12 to 18 percent slopes, moderately eroded","Chili",4,0.32,"HEL"]
["Crawford","Co","Colwood silt loam","Colwood",5,0.28000000000000003,"NHEL"]
["Crawford","Cr","Condit-Bennington silt loams","Condit",5,0.37,"NHEL"]
["Crawford","DeA","Del Rey silt loam, 0 to 2 percent slopes","Del Rey",3,0.43,"NHEL"]
["Crawford","Du","Dumps","Dumps"]
["Crawford","EtA","Elliott silt loam, 0 to 3 percent slopes","Elliot",4,0.28000000000000003,"NHEL"]
["Crawford","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Crawford","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Crawford","GaA","Gallman silt loam, 0 to 2 percent slopes","Gallman",5,0.32,"NHEL"]
["Crawford","GaB","Gallman silt loam, 2 to 6 percent slopes","Gallman",5,0.32,"PHEL"]
["Crawford","GwB","Glynwood silt loam, 2 to 6 percent slopes","Glynwood",3,0.43,"PHEL"]
["Crawford","GwB2","Glynwood silt loam, 2 to 6 percent slopes, moderately eroded","Glynwood",3,0.43,"PHEL"]
["Crawford","GwC2","Glynwood silt loam, 6 to 12 percent slopes, moderately eroded","Glynwood",3,0.43,"PHEL"]
["Crawford","GwD2","Glynwood silt loam, 12 to 18 percent slopes, moderately eroded","Glynwood",3,0.43,"HEL"]
["Crawford","HpE","Hennepin-Alexandria silt loams, 18 to 50 percent slopes","Hennepin",4,0.32,"HEL"]
["Crawford","JtA","Jimtown loam, 0 to 2 percent slopes","Jimtown",4,0.32,"NHEL"]
["Crawford","JtB","Jimtown loam, 2 to 6 percent slopes","Jimtown",4,0.32,"PHEL"]
["Crawford","KbA","Kibbie fine sandy loam, 0 to 2 percent slopes","Kibbie",5,0.2,"NHEL"]
["Crawford","KcB","Kibbie-Bennington complex, 2 to 6 percent slopes","Kibbie",5,0.2,"PHEL"]
["Crawford","Le","Lenawee silty clay loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Crawford","Lg","Lenawee silt loam, overwash","Lenawee",4,0.28000000000000003,"NHEL"]
["Crawford","Lh","Lenawee Variant silty clay loam","Lenawee",5,0.37,"NHEL"]
["Crawford","Lo","Lobdell silt loam","Lobdell",5,0.37,"NHEL"]
["Crawford","Lu","Luray silty clay loam","Luray",5,0.32,"NHEL"]
["Crawford","Lw","Luray-Urban land complex","Luray",5,0.32,"NHEL"]
["Crawford","LzB","Lykens silt loam, 2 to 6 percent slopes","Luray",4,0.37,"PHEL"]
["Crawford","Mb","Marengo silty clay loam","Marengo",5,0.28000000000000003,"NHEL"]
["Crawford","Md","Medway silt loam","Medway",5,0.32,"NHEL"]
["Crawford","MkA","Mitiwanga silt loam, 0 to 3 percent slopes","Mitiwanga",4,0.32,"NHEL"]
["Crawford","Mu","Muskego muck","Muskego",2,null,"NHEL"]
["Crawford","On","Olentangy mucky silt loam","Olentangy",5,0.28000000000000003,"NHEL"]
["Crawford","Os","Olmsted silty clay loam","Olentangy",5,0.24,"NHEL"]
["Crawford","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Crawford","Po","Pits, gravel","Pits"]
["Crawford","Pp","Pits, quarry","Pits"]
["Crawford","Sb","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Crawford","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Crawford","So","Sloan silt loam","Sloan",5,0.37,"NHEL"]
["Crawford","TrA","Tiro silt loam, 0 to 2 percent slopes","Tiro",4,0.37,"NHEL"]
["Crawford","TrB","Tiro silt loam, 2 to 6 percent slopes","Tiro",4,0.37,"PHEL"]
["Crawford","TsB","Tuscola fine sandy loam, 2 to 6 percent slopes","Tuscola",5,0.24,"PHEL"]
["Crawford","TuB","Tuscola-Bennington complex, 2 to 6 percent slopes","Tuscola",5,0.24,"PHEL"]
["Crawford","Ud","Udorthents, loamy","Udorthents"]
["Crawford","Ur","Urban land","Urban"]
["Crawford","W","Water","Water"]
["Crawford","WaA","Wadsworth silt loam, 0 to 2 percent slopes","Wadsworth",4,0.43,"NHEL"]
["Crawford","WaB","Wadsworth silt loam, 2 to 6 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Crawford","Wb","Wallkill silt loam","Wallkill",5,0.32,"NHEL"]
["Crawford","WlA","Wilmer Variant silt loam, 0 to 2 percent slopes","Wilmer",5,0.32,"NHEL"]
["Crawford","WlB","Wilmer Variant silt loam, 2 to 6 percent slopes","Wilmer",5,0.32,"PHEL"]
[null,"Select","none","none"]
["Defiance","BmB","Belmore loam, 2 to 6 percent slopes","Belmore",4,0.32,"PHEL"]
["Defiance","BnA","Blount loam, 0 to 3 percent slopes","Belmore",3,0.43,"NHEL"]
["Defiance","Bp","Bono silty clay loam","Bono",5,0.28000000000000003,"NHEL"]
["Defiance","BrB","Bronson sandy loam, 1 to 6 percent slopes","Bronson",4,0.24,"PHEL"]
["Defiance","BsB","Boyer loamy sand, 1 to 6 percent slopes","Boyer",4,0.17,"NHEL"]
["Defiance","BvE","Broughton silt loam, 12 to 35 percent slopes","Broughton",3,0.43,"HEL"]
["Defiance","BwC3","Broughton clay, 6 to 12 percent slopes, severely eroded","Broughton",2,0.32,"PHEL"]
["Defiance","Ca","Carlisle muck","Carlisle",2,null,"NHEL"]
["Defiance","Cm","Colwood loam","Colwood",5,0.28000000000000003,"NHEL"]
["Defiance","Db","Defiance silty clay loam, frequently flooded","Defiance",5,0.37,"NHEL"]
["Defiance","DfA","Del Rey silt loam, 0 to 3 percent slopes","Del Rey",3,0.43,"NHEL"]
["Defiance","DgA","Del Rey Variant silt loam, 0 to 3 percent slopes","Del Rey",4,0.43,"NHEL"]
["Defiance","DmA","Digby loam, 0 to 3 percent slopes","Digby",4,0.32,"NHEL"]
["Defiance","FsA","Fulton loam, 0 to 3 percent slopes","Fulton",3,0.43,"NHEL"]
["Defiance","FtA","Fulton silty clay loam, 0 to 3 percent slopes","Fulton",3,0.43,"NHEL"]
["Defiance","Ge","Genesee loam, occasionally flooded","Genesee",5,0.37,"NHEL"]
["Defiance","Gf","Gilford fine sandy loam","Gilford",4,0.2,"NHEL"]
["Defiance","GwB","Glynwood loam, 2 to 6 percent slopes","Glynwood",3,0.43,"PHEL"]
["Defiance","GwB2","Glynwood loam, 2 to 6 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Defiance","GwC2","Glynwood loam, 6 to 12 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Defiance","HnA","Haskins loam, 0 to 3 percent slopes","Haskins",4,0.37,"NHEL"]
["Defiance","Ho","Hoytville clay loam","Hoytville",5,0.28000000000000003,"NHEL"]
["Defiance","Hv","Hoytville clay","Hoytville",5,0.28000000000000003,"NHEL"]
["Defiance","KfA","Kibbie loam, 0 to 3 percent slopes","Kibbie",5,0.28000000000000003,"NHEL"]
["Defiance","Lb","Landes fine sandy loam, occasionally flooded","Landes",5,0.2,"NHEL"]
["Defiance","Lc","Latty silty clay","Latty",5,0.28000000000000003,"NHEL"]
["Defiance","Lf","Lenawee silty clay loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Defiance","Md","Mermill loam","Mermill",5,0.28000000000000003,"NHEL"]
["Defiance","Mh","Millgrove loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Defiance","MrD2","Morley clay loam, 12 to 18 percent slopes, eroded","Morley",3,0.43,"HEL"]
["Defiance","NnA","Nappanee loam, 0 to 3 percent slopes","Nappanee",3,0.43,"NHEL"]
["Defiance","NpA","Nappanee silty clay loam, 0 to 3 percent slopes","Nappanee",3,0.43,"NHEL"]
["Defiance","OsB","Oshtemo sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"NHEL"]
["Defiance","OtB","Ottokee loamy fine sand, 1 to 6 percent slopes","Ottokee",5,0.17,"NHEL"]
["Defiance","Pa","Paulding clay","Paulding",5,0.28000000000000003,"NHEL"]
["Defiance","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Defiance","Pt","Pits, gravel","Pits"]
["Defiance","RmB","Rawson sandy loam, 2 to 6 percent slopes","Rawson",4,0.24,"PHEL"]
["Defiance","RnA","Rimer loamy fine sand, 0 to 3 percent slopes","Rimer",4,0.17,"NHEL"]
["Defiance","RrA","Roselms loam, 0 to 3 percent slopes","Roselms",3,0.32,"NHEL"]
["Defiance","RsA","Roselms silty clay, 0 to 3 percent slopes","Roselms",3,0.32,"NHEL"]
["Defiance","Ru","Ross silt loam, occasionally flooded","Ross",5,0.32,"NHEL"]
["Defiance","SaB","St. Clair loam, 2 to 6 percent slopes","St. Clair",3,0.37,"PHEL"]
["Defiance","SbC2","St. Clair silty clay loam, 6 to 12 percent slopes, eroded","St. Clair",3,0.37,"PHEL"]
["Defiance","SbE","St. Clair silty clay loam, 18 to 35 percent slopes","St. Clair",3,0.37,"HEL"]
["Defiance","ScD3","St. Clair clay, 12 to 18 percent slopes, severely eroded","St. Clair",2,0.37,"HEL"]
["Defiance","ScE3","St. Clair clay, 18 to 35 percent slopes, severely eroded","St. Clair",2,0.37,"HEL"]
["Defiance","SdB","Seward loamy fine sand, 1 to 6 percent slopes","Seward",4,0.17,"NHEL"]
["Defiance","Sh","Shoals silt loam, frequently flooded","Shoals",5,0.37,"NHEL"]
["Defiance","So","Sloan silty clay loam, frequently flooded","Sloan",5,0.37,"NHEL"]
["Defiance","TdA","Tedrow loamy fine sand, 0 to 3 percent slopes","Tedrow",5,0.17,"NHEL"]
["Defiance","Tn","Toledo silty clay loam","Toledo",5,0.28000000000000003,"NHEL"]
["Defiance","TsB","Tuscola very fine sandy loam, 2 to 6 percent slopes","Tuscola",5,0.24,"NHEL"]
["Defiance","Ud","Udorthents, rolling","Udorthents"]
["Defiance","Ur","Urban land","Urban"]
["Defiance","W","Water","Water"]
["Defiance","Wa","Wabasha silty clay loam, frequently flooded","Wabasha",5,0.32,"NHEL"]
["Defiance","Wd","Wallkill Variant silty clay","Wallkill",5,0.28000000000000003,"NHEL"]
["Defiance","Wf","Wauseon fine sandy loam","Wauseon",4,0.17,"NHEL"]
[null,"Select","none","none"]
["Fulton","Ad","Adrian muck","Adrian",2,null,"NHEL"]
["Fulton","BcA","Bixler loamy fine sand, 0 to 3 percent slopes","Bixler",5,0.15,"NHEL"]
["Fulton","BnA","Blount loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Fulton","BnB","Blount loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Fulton","BoB","Blount-Rimer complex, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Fulton","BrB","Boyer loamy sand, 1 to 6 percent slopes","Boyer",4,0.17,"NHEL"]
["Fulton","ByA","Brady sandy loam, 0 to 3 percent slopes","Boyer",5,0.2,"NHEL"]
["Fulton","Ch","Cohoctah fine sandy loam, frequently flooded","Cohoctah",5,0.28000000000000003,"NHEL"]
["Fulton","Cn","Colwood loam","Colwood",5,0.28000000000000003,"NHEL"]
["Fulton","DfA","Del Rey silt loam, 0 to 3 percent slopes","Del Rey",3,0.43,"PHEL"]
["Fulton","DmA","Digby loam, 0 to 3 percent slopes","Digby",4,0.32,"NHEL"]
["Fulton","DtA","Dixboro fine sandy loam, 0 to 3 percent slopes","Dixboro",5,0.2,"NHEL"]
["Fulton","Ee","Eel silt loam, frequently flooded","Eel",5,0.37,"NHEL"]
["Fulton","FtA","Fulton silty clay loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Fulton","FtB","Fulton silty clay loam, 2 to 6 percent slopes","Fulton",3,0.43,"PHEL"]
["Fulton","GaB","Galen loamy fine sand, 1 to 6 percent slopes","Galen",3,0.17,"PHEL"]
["Fulton","Gf","Gilford fine sandy loam","Gilford",4,0.2,"NHEL"]
["Fulton","GnB2","Glynwood loam, 2 to 6 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Fulton","GnC2","Glynwood loam, 6 to 12 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Fulton","GnD2","Glynwood loam, 12 to 18 percent slopes, eroded","Glynwood",3,0.43,"HEL"]
["Fulton","GoC3","Glynwood clay loam, 6 to 12 percent slopes, severely eroded","Glynwood",2,0.43,"HEL"]
["Fulton","Gr","Granby loamy fine sand","Granby",5,0.17,"NHEL"]
["Fulton","HkA","Haskins loam, 0 to 3 percent slopes","Haskins",4,0.37,"NHEL"]
["Fulton","Ho","Hoytville clay loam","Hoytville",5,0.28000000000000003,"NHEL"]
["Fulton","KfA","Kibbie loam, 0 to 3 percent slopes","Kibbie",5,0.28000000000000003,"NHEL"]
["Fulton","La","Lamson fine sandy loam","Lamson",5,0.28000000000000003,"NHEL"]
["Fulton","Lc","Latty silty clay","Latty",5,0.28000000000000003,"NHEL"]
["Fulton","Lf","Lenawee silty clay loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Fulton","Mf","Mermill loam","Mermill",5,0.28000000000000003,"NHEL"]
["Fulton","Mo","Millgrove loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Fulton","NnA","Nappanee loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Fulton","NnB","Nappanee loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Fulton","OaB","Oakville fine sand, 0 to 6 percent slopes","Oakville",5,0.15,"NHEL"]
["Fulton","OaC","Oakville fine sand, 6 to 12 percent slopes","Oakville",5,0.15,"PHEL"]
["Fulton","OrB","Oshtemo loamy sand, 0 to 6 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Fulton","OtB","Ottokee fine sand, 0 to 6 percent slopes","Ottokee",5,0.17,"NHEL"]
["Fulton","OuB","Ottokee-Glynwood complex, 3 to 8 percent slopes","Ottokee",5,0.17,"PHEL"]
["Fulton","PeB","Perrin sandy loam, 2 to 6 percent slopes","Perrin",4,0.17,"NHEL"]
["Fulton","Pm","Pewamo clay loam","Pewamo",5,0.24,"NHEL"]
["Fulton","Ps","Psammaquents, nearly level","Psammaquents"]
["Fulton","RbB","Rawson sandy loam, 2 to 6 percent slopes","Rawson",4,0.24,"PHEL"]
["Fulton","RnA","Rimer loamy fine sand, 0 to 3 percent slopes","Rimer",4,0.17,"NHEL"]
["Fulton","SdB","Seward loamy fine sand, 2 to 6 percent slopes","Seward",4,0.17,"NHEL"]
["Fulton","SdC","Seward loamy fine sand, 6 to 12 percent slopes","Seward",4,0.17,"PHEL"]
["Fulton","SfB2","Shinrock silty clay loam, 2 to 6 percent slopes, eroded","Shinrock",3,0.37,"PHEL"]
["Fulton","SfC2","Shinrock silty clay loam, 6 to 12 percent slopes, eroded","Shinrock",3,0.37,"HEL"]
["Fulton","SgB2","Shinrock-Tuscola complex, 3 to 8 percent slopes, eroded","Shinrock",3,0.37,"PHEL"]
["Fulton","Sh","Shoals silt loam, frequently flooded","Shoals",5,0.37,"NHEL"]
["Fulton","So","Sloan silty clay loam, frequently flooded","Sloan",5,0.37,"NHEL"]
["Fulton","SpB","Spinks fine sand, 1 to 6 percent slopes","Spinks",5,0.17,"NHEL"]
["Fulton","SpC","Spinks fine sand, 6 to 12 percent slopes","Spinks",5,0.17,"PHEL"]
["Fulton","SpD","Spinks fine sand, 12 to 18 percent slopes","Spinks",5,0.17,"PHEL"]
["Fulton","TdA","Tedrow loamy fine sand, 0 to 3 percent slopes","Tedrow",5,0.17,"NHEL"]
["Fulton","TuB","Tuscola fine sandy loam, 3 to 8 percent slopes","Tuscola",5,0.24,"PHEL"]
["Fulton","Uo","Udorthents, loamy","Udorthents"]
["Fulton","W","Water","Water"]
["Fulton","Wf","Wauseon fine sandy loam","Wauseon",4,0.17,"NHEL"]
[null,"Select","none","none"]
["Hancock","Ad","Adrian muck","Adrian",2,null,"NHEL"]
["Hancock","BlA","Belmore sandy loam, 0 to 2 percent slopes","Belmore",4,0.24,"NHEL"]
["Hancock","BlB","Belmore sandy loam, 2 to 6 percent slopes","Belmore",4,0.24,"PHEL"]
["Hancock","BmA","Belmore loam, 0 to 2 percent slopes","Belmore",4,0.32,"NHEL"]
["Hancock","BmB","Belmore loam, 2 to 6 percent slopes","Belmore",4,0.32,"PHEL"]
["Hancock","BmC","Belmore loam, 6 to 12 percent slopes","Belmore",4,0.32,"PHEL"]
["Hancock","BnA","Blount loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Hancock","BnB","Blount loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Hancock","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Hancock","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Hancock","BoB2","Blount silt loam, 2 to 6 percent slopes, moderately eroded","Blount",3,0.43,"PHEL"]
["Hancock","CeA","Celina silt loam, limestone substratum, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Hancock","Cl","Clay pits","Clay"]
["Hancock","Co","Colwood loam","Colwood",5,0.28000000000000003,"NHEL"]
["Hancock","CrA","Crosby silt loam, limestone substratum, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Hancock","Cu","Cut and fill land","Cut"]
["Hancock","DgA","Digby sandy loam, 0 to 2 percent slopes","Digby",4,0.24,"NHEL"]
["Hancock","DmA","Digby loam, 0 to 2 percent slopes","Digby",4,0.32,"NHEL"]
["Hancock","DmB","Digby loam, 2 to 6 percent slopes","Digby",4,0.32,"PHEL"]
["Hancock","DuB","Dunbridge loamy fine sand, 2 to 6 percent slopes","Dunbridge",2,0.17,"PHEL"]
["Hancock","Ea","Eel loam","Eel",5,0.37,"NHEL"]
["Hancock","Em","Eel silt loam","Eel",5,0.37,"NHEL"]
["Hancock","FtA","Fulton silt loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Hancock","FtB","Fulton silt loam, 2 to 6 percent slopes","Fulton",3,0.43,"PHEL"]
["Hancock","Gn","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Hancock","Go","Granby loamy fine sand","Granby",5,0.17,"NHEL"]
["Hancock","Gp","Gravel pits","Gravel"]
["Hancock","HaA","Haney sandy loam, 0 to 2 percent slopes","Haney",4,0.28000000000000003,"NHEL"]
["Hancock","HaB","Haney sandy loam, 2 to 6 percent slopes","Haney",4,0.28000000000000003,"PHEL"]
["Hancock","HdA","Haney loam, 0 to 2 percent slopes","Haney",4,0.32,"NHEL"]
["Hancock","HdB","Haney loam, 2 to 6 percent slopes","Haney",4,0.32,"PHEL"]
["Hancock","HkA","Haskins fine sandy loam, 0 to 2 percent slopes","Haskins",4,0.24,"NHEL"]
["Hancock","HkB","Haskins fine sandy loam, 2 to 6 percent slopes","Haskins",4,0.24,"PHEL"]
["Hancock","HnA","Haskins loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Hancock","HnB","Haskins loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Hancock","Ho","Hoytville clay loam","Hoytville",5,0.28000000000000003,"NHEL"]
["Hancock","Hv","Hoytville clay","Hoytville",5,0.28000000000000003,"NHEL"]
["Hancock","Jo","Joliet silty clay loam","Joilet",2,0.28000000000000003,"NHEL"]
["Hancock","KfA","Kibbie fine sandy loam, 0 to 2 percent slopes","Kibbie",5,0.2,"NHEL"]
["Hancock","KfB","Kibbie fine sandy loam, 2 to 6 percent slopes","Kibbie",5,0.2,"PHEL"]
["Hancock","KlA","Kibbie loam, 0 to 2 percent slopes","Kibbie",5,0.28000000000000003,"NHEL"]
["Hancock","KlB","Kibbie loam, 2 to 6 percent slopes","Kibbie",5,0.28000000000000003,"PHEL"]
["Hancock","KsA","Kibbie silt loam, 0 to 2 percent slopes","Kibbie",5,0.28000000000000003,"NHEL"]
["Hancock","KsB","Kibbie silt loam, 2 to 6 percent slopes","Kibbie",5,0.28000000000000003,"PHEL"]
["Hancock","Le","Lenawee loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Hancock","Ln","Lenawee silty clay loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Hancock","Lw","Linwood muck","Linwood",2,null,"NHEL"]
["Hancock","Me","Mermill loam","Mermill",5,0.28000000000000003,"NHEL"]
["Hancock","Mf","Mermill clay loam","Mermill",5,0.28000000000000003,"NHEL"]
["Hancock","Mg","Millgrove fine sandy loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Hancock","Mh","Millgrove loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Hancock","Mk","Millgrove clay loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Hancock","Mm","Millsdale loam","Millsdale",4,0.32,"NHEL"]
["Hancock","Mn","Millsdale silt loam","Millsdale",4,0.32,"NHEL"]
["Hancock","Mo","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Hancock","MrA","Milton silt loam, 0 to 2 percent slopes","Milton",4,0.37,"NHEL"]
["Hancock","MrB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Hancock","MsB","Morley loam, 2 to 6 percent slopes","Morley",3,0.43,"PHEL"]
["Hancock","MyB","Morley silt loam, 2 to 6 percent slopes","Morley",3,0.43,"PHEL"]
["Hancock","MyB2","Morley silt loam, 2 to 6 percent slopes, moderately eroded","Morley",3,0.43,"PHEL"]
["Hancock","MyC","Morley silt loam, 6 to 12 percent slopes","Morley",3,0.43,"PHEL"]
["Hancock","MyC2","Morley silt loam, 6 to 12 percent slopes, moderately eroded","Morley",3,0.43,"PHEL"]
["Hancock","MyD2","Morley silt loam, 12 to 18 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Hancock","NaA","Nappanee loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Hancock","NaB","Nappanee loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Hancock","NpA","Nappanee silt loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Hancock","NpB","Nappanee silt loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Hancock","NpC2","Nappanee silt loam, 4 to 10 percent slopes, moderately eroded","Nappanee",3,0.43,"PHEL"]
["Hancock","OtB","Ottokee loamy fine sand, 0 to 4 percent slopes","Ottokee",5,0.17,"NHEL"]
["Hancock","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Hancock","Po","Pewamo clay","Pewamo",5,0.24,"NHEL"]
["Hancock","Qu","Quarry","Quarry"]
["Hancock","RbA","Randolph loam, 0 to 2 percent slopes","Randolph",3,0.37,"NHEL"]
["Hancock","RlA","Randolph silt loam, 0 to 2 percent slopes","Randolph",3,0.37,"NHEL"]
["Hancock","RlB","Randolph silt loam, 2 to 6 percent slopes","Randolph",3,0.37,"PHEL"]
["Hancock","RmA","Rawson loam, 0 to 2 percent slopes","Rawson",4,0.32,"NHEL"]
["Hancock","RmB","Rawson loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Hancock","RnA","Rimer loamy fine sand, 0 to 2 percent slopes","Rimer",4,0.17,"NHEL"]
["Hancock","RnB","Rimer loamy fine sand, 2 to 6 percent slopes","Rimer",4,0.17,"NHEL"]
["Hancock","RrB","Ritchey silt loam, 1 to 5 percent slopes","Ritchey",2,0.37,"PHEL"]
["Hancock","RsC","Romeo silt loam, 0 to 10 percent slopes","Romeo",1,0.37,"PHEL"]
["Hancock","SdA","Seward loamy fine sand, 0 to 2 percent slopes","Seward",4,0.17,"NHEL"]
["Hancock","SdB","Seward loamy fine sand, 2 to 6 percent slopes","Seward",4,0.17,"NHEL"]
["Hancock","SeB","Shinrock silt loam, 2 to 6 percent slopes","Shinrock",3,0.37,"PHEL"]
["Hancock","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Hancock","Sn","Sloan loam","Sloan",5,0.37,"NHEL"]
["Hancock","So","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Hancock","To","Toledo silty clay loam","Toledo",5,0.28000000000000003,"NHEL"]
["Hancock","TpA","Tuscola fine sandy loam, 0 to 2 percent slopes","Tuscola",5,0.24,"NHEL"]
["Hancock","TpB","Tuscola fine sandy loam, 2 to 6 percent slopes","Tuscola",5,0.24,"NHEL"]
["Hancock","TsB","Tuscola loam, 2 to 6 percent slopes","Tuscola",5,0.32,"PHEL"]
["Hancock","VaB","Vaughnsville loam, 1 to 4 percent slopes","Vaughnsville",4,0.32,"NHEL"]
[null,"Select","none","none"]
["Hardin","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Hardin","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Hardin","BpA","Blount silt loam, limestone substratum, 0 to 3 percent slopes","Blount",3,0.43,"NHEL"]
["Hardin","Ca","Carlisle muck","Carlisle",2,null,"NHEL"]
["Hardin","Co","Colwood loam","Colwood",5,0.28000000000000003,"NHEL"]
["Hardin","DeA","Del Rey silt loam, 0 to 3 percent slopes","Del Rey",3,0.43,"NHEL"]
["Hardin","Ee","Eel silt loam, occasionally flooded","Eel",5,0.37,"NHEL"]
["Hardin","FoA","Fox silt loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Hardin","FoB","Fox silt loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Hardin","FpC2","Fox clay loam, 6 to 12 percent slopes, eroded","Fox",4,0.37,"PHEL"]
["Hardin","FuA","Fulton silt loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Hardin","FuB","Fulton silt loam, 2 to 6 percent slopes","Fulton",3,0.43,"PHEL"]
["Hardin","GwB","Glynwood silt loam, 2 to 6 percent slopes","Glynwood",3,0.43,"PHEL"]
["Hardin","GyB2","Glynwood clay loam, 2 to 6 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Hardin","GyC2","Glynwood clay loam, 6 to 12 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Hardin","HkA","Haskins silt loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Hardin","HkB","Haskins silt loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Hardin","KaB","Kendallville silt loam, 2 to 6 percent slopes","Kendallville",3,0.37,"PHEL"]
["Hardin","KbA","Kibbie loam, 0 to 3 percent slopes","Kibbie",5,0.28000000000000003,"NHEL"]
["Hardin","La","Latty silty clay loam","Latty",5,0.28000000000000003,"NHEL"]
["Hardin","Le","Latty silty clay","Latty",5,0.28000000000000003,"NHEL"]
["Hardin","Ln","Linwood muck","Linwood",2,null,"NHEL"]
["Hardin","MaB","Martinsville loam, 1 to 4 percent slopes","Martinsville",5,0.37,"NHEL"]
["Hardin","Mc","McGuffey muck","McGuffey",3,null,"NHEL"]
["Hardin","Mf","Milford silty clay loam","Milford",5,0.28000000000000003,"NHEL"]
["Hardin","Mk","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Hardin","Mo","Montgomery silty clay loam","Montgomery",5,0.37,"NHEL"]
["Hardin","Mp","Montgomery silty clay loam, gravelly substratum","Montgomery",5,0.37,"NHEL"]
["Hardin","MrD2","Morley clay loam, 12 to 18 percent slopes, eroded","Morley",3,0.43,"HEL"]
["Hardin","MsC2","Morley-Belmore complex, 6 to 15 percent slopes, eroded","Morley",3,0.43,"PHEL"]
["Hardin","MtB","Morley-Milton silt loams, 2 to 6 percent slopes","Morley",3,0.43,"PHEL"]
["Hardin","Ne","Newark silt loam, occasionally flooded","Newark",5,0.32,"NHEL"]
["Hardin","No","Nolin silt loam, occasionally flooded","Nolin",5,0.43,"NHEL"]
["Hardin","OcA","Ockley loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Hardin","OcB","Ockley loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Hardin","Ot","Olentangy silt loam","Olentangy",5,0.28000000000000003,"NHEL"]
["Hardin","Pa","Patton silty clay loam","Patton",5,0.28000000000000003,"NHEL"]
["Hardin","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Hardin","Po","Pewamo variant muck","Pewamo",2,null,"NHEL"]
["Hardin","Ps","Pits, gravel","Pits"]
["Hardin","Pt","Pits, quarry","Pits"]
["Hardin","Ro","Roundhead muck","Roundhead",5,null,"NHEL"]
["Hardin","Sa","Saranac silty clay loam, occasionally flooded","Saranac",5,0.24,"NHEL"]
["Hardin","ShB","Shinrock silt loam, 2 to 6 percent slopes","Shinrock",3,0.37,"PHEL"]
["Hardin","SkA","Sleeth silt loam, 0 to 3 percent slopes","Sleeth",5,0.32,"NHEL"]
["Hardin","So","Sloan silt loam, frequently flooded","Sloan",5,0.37,"NHEL"]
["Hardin","W","Water","Water"]
["Hardin","Wa","Wallkill silt loam, frequently flooded","Wallkill",5,0.32,"NHEL"]
["Hardin","We","Westland clay loam","Westland",5,0.28000000000000003,"NHEL"]
[null,"Select","none","none"]
["Henry","Ad","Adrian muck","Adrian",2,null,"NHEL"]
["Henry","ArB","Arkport fine sand, 2 to 6 percent slopes","Arkport",3,0.17,"PHEL"]
["Henry","ArC","Arkport fine sand, 6 to 12 percent slopes","Arkport",3,0.17,"PHEL"]
["Henry","Ca","Clay pits","Clay"]
["Henry","Ch","Cohoctah fine sandy loam","Cohoctah",5,0.28000000000000003,"NHEL"]
["Henry","Cn","Colwood loam","Colwood",5,0.28000000000000003,"NHEL"]
["Henry","Co","Colwood silt loam","Colwood",5,0.28000000000000003,"NHEL"]
["Henry","Cu","Cut and fill land","Cut"]
["Henry","DeA","Del Rey loam, 0 to 2 percent slopes","Del Rey",3,0.43,"NHEL"]
["Henry","DfA","Del Rey silt loam, 0 to 2 percent slopes","Del Rey",3,0.43,"NHEL"]
["Henry","DuA","Digby fine sandy loam, 0 to 2 percent slopes","Digby",4,0.24,"NHEL"]
["Henry","DyA","Digby loam, 0 to 2 percent slopes","Digby",4,0.32,"NHEL"]
["Henry","FsA","Fulton loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Henry","FsB","Fulton loam, 2 to 6 percent slopes","Fulton",3,0.43,"PHEL"]
["Henry","FuA","Fulton silty clay loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Henry","FuB","Fulton silty clay loam, 2 to 6 percent slopes","Fulton",3,0.43,"PHEL"]
["Henry","FvA","Fulton loam, sandy subsoil variant, 0 to 2 percent slopes","Fulton",3,0.32,"NHEL"]
["Henry","GaA","Galen fine sand, 0 to 2 percent slopes","Galen",3,0.15,"NHEL"]
["Henry","GaB","Galen fine sand, 2 to 6 percent slopes","Galen",3,0.15,"PHEL"]
["Henry","Gm","Genesee loam","Genesee",5,0.37,"NHEL"]
["Henry","Go","Gilford fine sandy loam","Gilford",4,0.2,"NHEL"]
["Henry","Gr","Granby loamy fine sand","Granby",5,0.17,"NHEL"]
["Henry","Gv","Gravel pits","Gravel"]
["Henry","HaA","Haney fine sandy loam, 0 to 2 percent slopes","Haney",4,0.28000000000000003,"NHEL"]
["Henry","HaB","Haney fine sandy loam, 2 to 6 percent slopes","Haney",4,0.28000000000000003,"PHEL"]
["Henry","HdA","Haney loam, 0 to 2 percent slopes","Haney",4,0.32,"NHEL"]
["Henry","HdB","Haney loam, 2 to 6 percent slopes","Haney",4,0.32,"PHEL"]
["Henry","HeC","Haney and Rawson loams, 6 to 12 percent slopes","Haney",4,0.32,"PHEL"]
["Henry","HkA","Haskins fine sandy loam, 0 to 2 percent slopes","Haskins",4,0.24,"NHEL"]
["Henry","HlA","Haskins loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Henry","HnA","Haskins fine sandy loam, stratified substratum, 0 to 2 percent slopes","Haskins",4,0.24,"NHEL"]
["Henry","Ho","Hoytville clay loam","Hoytville",5,0.28000000000000003,"NHEL"]
["Henry","Hv","Hoytville clay","Hoytville",5,0.28000000000000003,"NHEL"]
["Henry","Hw","Hoytville clay, thin solum variant","Hoytville",5,0.28000000000000003,"NHEL"]
["Henry","KfA","Kibbie fine sandy loam, 0 to 2 percent slopes","Kibbie",5,0.2,"NHEL"]
["Henry","KlA","Kibbie loam, 0 to 2 percent slopes","Kibbie",5,0.28000000000000003,"NHEL"]
["Henry","La","Latty clay","Latty",5,0.28000000000000003,"NHEL"]
["Henry","Le","Lenawee loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Henry","Lf","Lenawee silty clay loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Henry","LwB2","Lucas silty clay loam, 2 to 6 percent slopes, moderately eroded","Lucas",3,0.43,"PHEL"]
["Henry","LwC2","Lucas silty clay loam, 6 to 12 percent slopes, moderately eroded","Lucas",3,0.43,"PHEL"]
["Henry","LxC3","Lucas silty clay, 6 to 12 percent slopes, severely eroded","Lucas",2,0.43,"HEL"]
["Henry","LxE3","Lucas silty clay, 12 to 45 percent slopes, severely eroded","Lucas",2,0.43,"HEL"]
["Henry","Md","Medway silt loam","Medway",5,0.32,"NHEL"]
["Henry","Me","Mermill loam","Mermill",5,0.28000000000000003,"NHEL"]
["Henry","Mf","Mermill clay loam","Mermill",5,0.28000000000000003,"NHEL"]
["Henry","Mg","Mermill loam, stratified substratum","Mermill",5,0.28000000000000003,"NHEL"]
["Henry","Mh","Millgrove loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Henry","Mk","Millgrove clay loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Henry","NaA","Nappanee loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Henry","NaB","Nappanee loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Henry","NtA","Nappanee silty clay loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Henry","NtB","Nappanee silty clay loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Henry","NtB2","Nappanee silty clay loam, 2 to 6 percent slopes, moderately eroded","Nappanee",3,0.43,"PHEL"]
["Henry","OaC","Oakville fine sand, 2 to 12 percent slopes","Oakville",5,0.15,"PHEL"]
["Henry","OsB","Oshtemo sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Henry","OtB","Ottokee fine sand, 1 to 5 percent slopes","Ottokee",5,0.17,"NHEL"]
["Henry","Pa","Paulding clay","Paulding",5,0.28000000000000003,"NHEL"]
["Henry","RaB","Rawson sandy loam, 2 to 6 percent slopes","Rawson",4,0.24,"PHEL"]
["Henry","RdB","Rawson loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Henry","ReB","Rawson fine sandy loam, stratified substratum, 2 to 6 percent slopes","Rawson",4,0.24,"PHEL"]
["Henry","RfA","Rimer loamy fine sand, 0 to 2 percent slopes","Rimer",4,0.17,"NHEL"]
["Henry","RmA","Rimer loamy fine sand, stratified substratum, 0 to 2 percent slopes","Rimer",4,0.17,"NHEL"]
["Henry","RoA","Roselms silty clay loam, 0 to 2 percent slopes","Roselms",3,0.32,"NHEL"]
["Henry","Rs","Ross loam","Ross",5,0.32,"NHEL"]
["Henry","SbB2","St. Clair silty clay loam, 2 to 6 percent slopes, moderately eroded","St. Clair",3,0.37,"PHEL"]
["Henry","SbC2","St. Clair silty clay loam, 6 to 12 percent slopes, moderately eroded","St. Clair",3,0.37,"PHEL"]
["Henry","ScC3","St. Clair silty clay, 6 to 12 percent slopes, severely eroded","St. Clair",2,0.37,"HEL"]
["Henry","ScD3","St. Clair silty clay, 12 to 18 percent slopes, severely eroded","St. Clair",2,0.37,"HEL"]
["Henry","ScE3","St. Clair silty clay, 18 to 25 percent slopes, severely eroded","St. Clair",2,0.37,"HEL"]
["Henry","ScF3","St. Clair silty clay, 25 to 45 percent slopes, severely eroded","St. Clair",2,0.37,"HEL"]
["Henry","SdB","Seward loamy fine sand, 2 to 6 percent slopes","Seward",4,0.17,"NHEL"]
["Henry","SdC","Seward loamy fine sand, 6 to 12 percent slopes","Seward",4,0.17,"PHEL"]
["Henry","SdD","Seward loamy fine sand, 12 to 18 percent slopes","Seward",4,0.17,"PHEL"]
["Henry","SeB","Seward loamy fine sand, stratified substratum, 2 to 6 percent slopes","Seward",4,0.17,"NHEL"]
["Henry","SeC","Seward loamy fine sand, stratified substratum, 6 to 12 percent slopes","Seward",4,0.17,"PHEL"]
["Henry","SfA","Shinrock silt loam, sandy subsoil variant, 0 to 2 percent slopes","Shinrock",3,0.37,"NHEL"]
["Henry","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Henry","So","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Henry","SpB","Spinks fine sand, 2 to 6 percent slopes","Spinks",5,0.17,"NHEL"]
["Henry","SpC","Spinks fine sand, 6 to 12 percent slopes","Spinks",5,0.17,"PHEL"]
["Henry","SpD","Spinks fine sand, 12 to 18 percent slopes","Spinks",5,0.17,"PHEL"]
["Henry","TdA","Tedrow loamy fine sand, 0 to 2 percent slopes","Tedrow",5,0.17,"NHEL"]
["Henry","TeA","Tedrow loamy fine sand, silty subsoil variant, 0 to 2 percent slopes","Tedrow",5,0.17,"NHEL"]
["Henry","To","Toledo silty clay loam","Toledo",5,0.28000000000000003,"NHEL"]
["Henry","Tt","Toledo silty clay","Toledo",5,0.28000000000000003,"NHEL"]
["Henry","TuB2","Tuscola loam, 2 to 6 percent slopes, moderately eroded","Tuscola",5,0.32,"PHEL"]
["Henry","TuC2","Tuscola loam, 6 to 12 percent slopes, moderately eroded","Tuscola",5,0.32,"PHEL"]
["Henry","Ur","Urban land","Urban"]
["Henry","VaA","Vaughnsville loam, 0 to 2 percent slopes","Vaughnsville",4,0.32,"NHEL"]
["Henry","W","Water","Water"]
["Henry","Wa","Wabasha silty clay","Wabasha",5,0.32,"NHEL"]
["Henry","Wc","Warners muck","Warners",5,null,"NHEL"]
["Henry","Wf","Wauseon fine sandy loam","Wauseon",4,0.17,"NHEL"]
["Henry","Wg","Wauseon loamy fine sand, stratified substratum","Wauseon",4,0.17,"NHEL"]
[null,"Select","none","none"]
["Lucas","BxA","Bixler loamy fine sand, 0 to 2 percent slopes","Bixler",5,0.15,"NHEL"]
["Lucas","BxB","Bixler loamy fine sand, 2 to 6 percent slopes","Bixler",5,0.15,"NHEL"]
["Lucas","ByA","Bixler-Urban land complex, 0 to 3 percent slopes","Bixler",5,0.15,"NHEL"]
["Lucas","Ce","Ceresco sandy loam, occasionally flooded","Ceresco",5,0.2,"NHEL"]
["Lucas","Co","Colwood loam","Colwood",5,0.28000000000000003,"NHEL"]
["Lucas","Cp","Colwood-Urban land complex","Colwood",5,0.28000000000000003,"NHEL"]
["Lucas","DcA","Del Rey-Urban land complex, 0 to 3 percent slopes","Del Rey",3,0.43,"PHEL"]
["Lucas","DdA","Del Rey loam, 0 to 3 percent slopes","Del Rey",3,0.43,"PHEL"]
["Lucas","DeA","Del Rey loam, sandy substratum, 0 to 2 percent slopes","Del Rey",3,0.43,"NHEL"]
["Lucas","DgA","Digby sandy loam, 0 to 2 percent slopes","Digby",4,0.24,"NHEL"]
["Lucas","DgB","Digby sandy loam, 2 to 6 percent slopes","Digby",4,0.24,"PHEL"]
["Lucas","DoA","Digby-Urban land complex, 0 to 3 percent slopes","Digby",4,0.24,"NHEL"]
["Lucas","DsA","Dixboro fine sandy loam, 0 to 2 percent slopes","Dixboro",5,0.2,"NHEL"]
["Lucas","DtA","Dixboro-Urban land complex, 0 to 2 percent slopes","Dixboro",5,0.2,"NHEL"]
["Lucas","DuB","Dunbridge sandy loam, 0 to 4 percent slopes","Dunbridge",2,0.17,"NHEL"]
["Lucas","Ee","Eel loam, occasionally flooded","Eel",5,0.37,"NHEL"]
["Lucas","FuA","Fulton silty clay loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Lucas","FuB","Fulton silty clay loam, 2 to 6 percent slopes","Fulton",3,0.43,"PHEL"]
["Lucas","FwA","Fulton-Urban land complex, 0 to 3 percent slopes","Fulton",3,0.43,"PHEL"]
["Lucas","Gf","Gilford fine sandy loam","Gilford",4,0.2,"NHEL"]
["Lucas","Gr","Granby loamy fine sand","Granby",5,0.17,"NHEL"]
["Lucas","Gs","Granby-Urban land complex","Granby",5,0.17,"NHEL"]
["Lucas","HnA","Haskins loam, 0 to 3 percent slopes","Haskins",4,0.37,"NHEL"]
["Lucas","Ho","Hoytville clay loam","Hoytville",5,0.28000000000000003,"NHEL"]
["Lucas","La","Lamson fine sandy loam","Lamson",5,0.28000000000000003,"NHEL"]
["Lucas","Lc","Latty silty clay","Latty",5,0.28000000000000003,"NHEL"]
["Lucas","Lf","Lenawee silty clay loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Lucas","Lg","Lenawee-Urban land complex","Lenawee",4,0.28000000000000003,"NHEL"]
["Lucas","Mf","Mermill loam","Mermill",5,0.28000000000000003,"NHEL"]
["Lucas","Mh","Mermill-Urban land complex","Mermill",5,0.28000000000000003,"NHEL"]
["Lucas","MmA","Metamora sandy loam, 0 to 3 percent slopes","Metamora",5,0.2,"NHEL"]
["Lucas","Mu","Muskego muck","Muskego",2,null,"NHEL"]
["Lucas","NnA","Nappanee loam, 0 to 3 percent slopes","Nappanee",3,0.43,"PHEL"]
["Lucas","OaB","Oakville fine sand, 2 to 6 percent slopes","Oakville",5,0.15,"NHEL"]
["Lucas","OaC","Oakville fine sand, 6 to 18 percent slopes","Oakville",5,0.15,"PHEL"]
["Lucas","OcB","Oakville-Urban land complex, 2 to 12 percent slopes","Oakville",5,0.15,"PHEL"]
["Lucas","OtB","Ottokee fine sand, 0 to 6 percent slopes","Ottokee",5,0.17,"NHEL"]
["Lucas","OuB","Ottokee-Urban land complex, 0 to 6 percent slopes","Ottokee",5,0.17,"NHEL"]
["Lucas","Pq","Pits, quarry","Pits"]
["Lucas","Ps","Pits, sand","Pits"]
["Lucas","RnA","Rimer loamy fine sand, 0 to 3 percent slopes","Rimer",4,0.17,"NHEL"]
["Lucas","Rs","Ross loam, occasionally flooded","Ross",5,0.32,"NHEL"]
["Lucas","SdB","Seward loamy fine sand, 2 to 6 percent slopes","Seward",4,0.17,"NHEL"]
["Lucas","Sh","Shoals loam, occasionally flooded","Shoals",5,0.37,"NHEL"]
["Lucas","SmB","Sisson loam, 2 to 6 percent slopes","Sisson",5,0.32,"PHEL"]
["Lucas","SmC","Sisson loam, 6 to 12 percent slopes","Sisson",5,0.32,"PHEL"]
["Lucas","SmD","Sisson loam, 12 to 18 percent slopes","Sisson",5,0.32,"PHEL"]
["Lucas","SnB","Sisson-Urban land complex, 2 to 12 percent slopes","Sisson",5,0.32,"PHEL"]
["Lucas","So","Sloan loam, occasionally flooded","Sloan",5,0.37,"NHEL"]
["Lucas","StB","Spinks fine sand, 2 to 6 percent slopes","Spinks",5,0.17,"NHEL"]
["Lucas","SuC2","St. Clair silty clay loam, 4 to 12 percent slopes, eroded","St. Clair",3,0.37,"PHEL"]
["Lucas","SuE3","St. Clair silty clay loam, 12 to 25 percent slopes, severely eroded","St. Clair",2,0.37,"HEL"]
["Lucas","TdA","Tedrow fine sand, 0 to 3 percent slopes","Tedrow",5,0.17,"NHEL"]
["Lucas","TeA","Tedrow-Urban land complex, 0 to 3 percent slopes","Tedrow",5,0.17,"NHEL"]
["Lucas","To","Toledo silty clay","Toledo",5,0.28000000000000003,"NHEL"]
["Lucas","Tp","Toledo silty clay, ponded","Toledo",5,0.28000000000000003,"NHEL"]
["Lucas","Ts","Toledo-Urban land complex","Toledo",5,0.28000000000000003,"NHEL"]
["Lucas","Un","Udorthents, sandy","Udorthents"]
["Lucas","Uo","Udorthents, loamy","Udorthents"]
["Lucas","Up","Udorthents, clayey","Udorthents"]
["Lucas","Ur","Urban land","Urban"]
["Lucas","W","Water","Water"]
["Lucas","Wt","Wauseon fine sandy loam","Wauseon",4,0.17,"NHEL"]
[null,"Select","none","none"]
["Marion","BgA","Bennington silt loam, 0 to 3 percent slopes","Bennington",3,0.43,"PHEL"]
["Marion","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Marion","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Marion","BuB","Blount-Urban land complex, undulating","Blount",3,0.43,"PHEL"]
["Marion","CdB","Cardington silt loam, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Marion","CdC2","Cardington silt loam, 6 to 12 percent slopes, eroded","Cardington",4,0.37,"PHEL"]
["Marion","CeB","Centerburg silt loam, 1 to 4 percent slopes","Centerburg",4,0.37,"PHEL"]
["Marion","DeA","Del Rey silt loam, 0 to 3 percent slopes","Del Rey",3,0.43,"PHEL"]
["Marion","EtA","Elliott silty clay loam, 0 to 3 percent slopes","Elliott",4,0.28000000000000003,"NHEL"]
["Marion","FcA","Fitchville silt loam, 0 to 3 percent slopes","Fitchville",5,0.37,"NHEL"]
["Marion","FoA","Fox loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Marion","FoB","Fox loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Marion","FtA","Fulton silty clay loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Marion","FtB","Fulton silty clay loam, 2 to 6 percent slopes","Fulton",3,0.43,"PHEL"]
["Marion","GwA","Glynwood silt loam, 0 to 2 percent slopes","Glynwood",3,0.43,"NHEL"]
["Marion","GwB","Glynwood silt loam, 2 to 6 percent slopes","Glynwood",3,0.43,"PHEL"]
["Marion","GwC2","Glynwood silt loam, 6 to 12 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Marion","GwD2","Glynwood silt loam, 12 to 18 percent slopes, eroded","Glynwood",3,0.43,"HEL"]
["Marion","GzB","Glynwood-Urban land complex, undulating","Glynwood",3,0.43,"PHEL"]
["Marion","KeB","Kendallville loam, 2 to 6 percent slopes","Kendallville",3,0.37,"PHEL"]
["Marion","KeD2","Kendallville loam, 12 to 18 percent slopes, eroded","Kendallville",3,0.37,"HEL"]
["Marion","La","Latty silty clay","Latty",5,0.28000000000000003,"NHEL"]
["Marion","MaA","Martinsville loam, 0 to 2 percent slopes","Martinsville",5,0.37,"NHEL"]
["Marion","MaB","Martinsville loam, 2 to 6 percent slopes","Martinsville",5,0.37,"PHEL"]
["Marion","Me","Medway clay loam, rarely flooded","Medway",5,0.32,"NHEL"]
["Marion","Mf","Milford silty clay loam","Milford",5,0.28000000000000003,"NHEL"]
["Marion","MnB","Milton silt loam, 1 to 4 percent slopes","Milton",4,0.37,"PHEL"]
["Marion","Mu","Muskego muck","Muskego",2,null,"NHEL"]
["Marion","Ne","Newark silt loam, occasionally flooded","Newark",5,0.32,"NHEL"]
["Marion","No","Nolin silt loam, occasionally flooded","Nolin",5,0.43,"NHEL"]
["Marion","OcA","Ockley loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Marion","OcB","Ockley loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Marion","Pa","Paulding clay","Paulding",5,0.28000000000000003,"NHEL"]
["Marion","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Marion","Po","Pewamo-Urban land complex","Pewamo",5,0.24,"NHEL"]
["Marion","Ps","Pits, gravel","Pits"]
["Marion","Pt","Pits, quarry","Pits"]
["Marion","Sa","Saranac silty clay loam, occasionally flooded","Saranac",5,0.24,"NHEL"]
["Marion","Sc","Saranac silty clay loam, frequently flooded","Saranac",5,0.24,"NHEL"]
["Marion","ShB","Shinrock silt loam, 2 to 6 percent slopes","Shinrock",3,0.37,"PHEL"]
["Marion","ShC2","Shinrock silt loam, 6 to 12 percent slopes, eroded","Shinrock",3,0.37,"PHEL"]
["Marion","SkA","Sleeth loam, 0 to 3 percent slopes","Sleeth",5,0.32,"NHEL"]
["Marion","So","Sloan silty clay loam, occasionally flooded","Sloan",5,0.37,"NHEL"]
["Marion","Ud","Udorthents, loamy","Udorthents"]
["Marion","W","Water","Water"]
["Marion","We","Westland clay loam","Westland",5,0.28000000000000003,"NHEL"]
["Marion","WhA","Whitaker loam, 0 to 3 percent slopes","Whitaker",5,0.37,"NHEL"]
[null,"Select","none","none"]
["Morrow","AdB","Amanda silt loam, 2 to 6 percent slopes","Amanda",4,0.37,"PHEL"]
["Morrow","AdC2","Amanda silt loam, 6 to 12 percent slopes, eroded","Amanda",4,0.37,"PHEL"]
["Morrow","AdD2","Amanda silt loam, 12 to 18 percent slopes, eroded","Amanda",4,0.37,"HEL"]
["Morrow","AdE2","Amanda silt loam, 18 to 25 percent slopes, eroded","Amanda",4,0.37,"HEL"]
["Morrow","BeA","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Morrow","BeB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Morrow","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Morrow","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Morrow","CaB","Canfield silt loam, 2 to 6 percent slopes","Canfield",4,0.37,"PHEL"]
["Morrow","CaC","Canfield silt loam, 6 to 12 percent slopes","Canfield",4,0.37,"PHEL"]
["Morrow","CaC2","Canfield silt loam, 6 to 12 percent slopes, eroded","Canfield",4,0.37,"PHEL"]
["Morrow","Cb","Carlisle muck","Carlisle",2,null,"NHEL"]
["Morrow","CdB","Centerburg silt loam, 2 to 6 percent slopes","Centerburg",4,0.37,"PHEL"]
["Morrow","CdC","Centerburg silt loam, 6 to 12 percent slopes","Centerburg",4,0.37,"PHEL"]
["Morrow","CdC2","Centerburg silt loam, 6 to 12 percent slopes, eroded","Centerburg",4,0.37,"PHEL"]
["Morrow","ChB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Morrow","ChC","Chili loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Morrow","CkF","Colyer Variant silt loam, 25 to 70 percent slopes","Colyer",4,0.37,"HEL"]
["Morrow","Co","Condit silt loam","Condit",5,0.37,"NHEL"]
["Morrow","GaB","Gallman silt loam, loamy substratum, 2 to 6 percent slopes","Gallman",5,0.32,"PHEL"]
["Morrow","GaC","Gallman silt loam, loamy substratum, 6 to 12 percent slopes","Gallman",5,0.32,"PHEL"]
["Morrow","GnB2","Glynwood clay loam, 2 to 6 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Morrow","GnC2","Glynwood clay loam, 6 to 12 percent slopes, eroded","Glynwood",3,0.43,"HEL"]
["Morrow","Lo","Lobdell silt loam, occasionally flooded","Lobdell",5,0.37,"NHEL"]
["Morrow","Mf","Milford silty clay loam","Milford",5,0.28000000000000003,"NHEL"]
["Morrow","Mg","Millgrove silt loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Morrow","MoC","Morley silt loam, 6 to 12 percent slopes","Morley",3,0.43,"PHEL"]
["Morrow","MoC2","Morley silt loam, 6 to 12 percent slopes, eroded","Morley",3,0.43,"PHEL"]
["Morrow","MoD2","Morley silt loam, 12 to 18 percent slopes, eroded","Morley",3,0.43,"HEL"]
["Morrow","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Morrow","OcC","Ockley silt loam, 6 to 12 percent slopes","Ockley",5,0.37,"PHEL"]
["Morrow","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Morrow","Ps","Pits, gravel","Pits"]
["Morrow","RsB","Rittman silt loam, 2 to 6 percent slopes","Rittman",4,0.43,"PHEL"]
["Morrow","RsC","Rittman silt loam, 6 to 12 percent slopes","Rittman",4,0.43,"PHEL"]
["Morrow","RsC2","Rittman silt loam, 6 to 12 percent slopes, eroded","Rittman",4,0.43,"PHEL"]
["Morrow","Sh","Shoals silt loam, occasionally flooded","Shoals",5,0.37,"NHEL"]
["Morrow","SkA","Sleeth silt loam, loamy substratum, 0 to 3 percent slopes","Sleeth",5,0.32,"NHEL"]
["Morrow","So","Sloan silty clay loam, sandy substratum, occasionally flooded","Sloan",5,0.37,"NHEL"]
["Morrow","Tg","Tioga loam, occasionally flooded","Tioga",5,0.37,"NHEL"]
["Morrow","Ud","Udorthents, loamy","Udorthents"]
["Morrow","W","Water","Water"]
["Morrow","WaA","Wadsworth silt loam, 0 to 2 percent slopes","Wadsworth",4,0.43,"NHEL"]
["Morrow","WaB","Wadsworth silt loam, 2 to 6 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Morrow","WsB","Wooster silt loam, 2 to 6 percent slopes","Wooster",4,0.37,"PHEL"]
["Morrow","WsC","Wooster silt loam, 6 to 12 percent slopes","Wooster",4,0.37,"PHEL"]
["Morrow","WsC2","Wooster silt loam, 6 to 12 percent slopes, eroded","Wooster",4,0.37,"PHEL"]
["Morrow","WsD2","Wooster silt loam, 12 to 18 percent slopes, eroded","Wooster",4,0.37,"HEL"]
["Morrow","WsE2","Wooster silt loam, 18 to 25 percent slopes, eroded","Wooster",4,0.37,"HEL"]
[null,"Select","none","none"]
["Ottawa","Ag","Algansee fine sand, occasionally flooded","Algansee",5,0.17,"NHEL"]
["Ottawa","Bo","Bono silty clay","Bono",5,0.28000000000000003,"NHEL"]
["Ottawa","ChB","Castalia very stony fine sandy loam, 1 to 6 percent slopes","Castalia",2,0.2,"PHEL"]
["Ottawa","Co","Colwood loam","Colwood",5,0.28000000000000003,"NHEL"]
["Ottawa","DeA","Del Rey silt loam, 1 to 3 percent slopes","Del Rey",3,0.43,"NHEL"]
["Ottawa","DuB","Dunbridge fine sandy loam, 2 to 6 percent slopes","Dunbridge",2,0.17,"PHEL"]
["Ottawa","Gn","Genesee silt loam, frequently flooded","Genesee",5,0.37,"NHEL"]
["Ottawa","Go","Genesee variant loam, frequently flooded","Genesee",4,0.37,"NHEL"]
["Ottawa","Gr","Glendora loamy fine sand, frequently flooded","Glendora",5,0.17,"NHEL"]
["Ottawa","HaA","Haskins loam, 0 to 3 percent slopes","Haskins",4,0.37,"NHEL"]
["Ottawa","Hy","Hoytville silty clay loam","Hoytville",5,0.28000000000000003,"NHEL"]
["Ottawa","KfA","Kibbie fine sandy loam, 0 to 2 percent slopes","Kibbie",5,0.2,"NHEL"]
["Ottawa","Lc","Latty silty clay","Latty",5,0.28000000000000003,"NHEL"]
["Ottawa","Lf","Lenawee silty clay loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Ottawa","Mh","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Ottawa","MtB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Ottawa","NpA","Nappanee silty clay loam, 0 to 3 percent slopes","Nappanee",3,0.43,"NHEL"]
["Ottawa","OaB","Oakville fine sand, 2 to 8 percent slopes","Oakville",5,0.15,"PHEL"]
["Ottawa","Pt","Pits, quarry","Pits"]
["Ottawa","RaB","Rawson loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Ottawa","RmA","Rimer loamy fine sand, stratified substratum, 0 to 2 percent slopes","Rimer",4,0.17,"NHEL"]
["Ottawa","SbC2","St. Clair silty clay loam, 4 to 12 percent slopes, eroded","St. Clair",3,0.37,"PHEL"]
["Ottawa","Sh","Shoals silt loam, frequently flooded","Shoals",5,0.37,"NHEL"]
["Ottawa","To","Toledo silty clay","Toledo",5,0.28000000000000003,"NHEL"]
["Ottawa","Tp","Toledo silty clay, ponded","Toledo",5,0.28000000000000003,"NHEL"]
["Ottawa","Ud","Udorthents, gently sloping","Udorthents"]
["Ottawa","W","Water","Water"]
["Ottawa","Wa","Wabasha silty clay, frequently flooded","Wabasha",5,0.32,"NHEL"]
[null,"Select","none","none"]
["Paulding","BaB1","Belmore loam, 2 to 6 percent slopes, slightly eroded","Belmore",4,0.32,"PHEL"]
["Paulding","BbC3","Broughton clay, 6 to 12 percent slopes, severely eroded","Broughton",2,0.32,"HEL"]
["Paulding","BbD3","Broughton clay, 12 to 18 percent slopes, severely eroded","Broughton",2,0.32,"HEL"]
["Paulding","BcB1","Broughton silty clay loam, 2 to 6 percent slopes, slightly eroded","Broughton",3,0.43,"PHEL"]
["Paulding","BcB2","Broughton silty clay loam, 2 to 6 percent slopes, moderately eroded","Broughton",3,0.43,"PHEL"]
["Paulding","BcC2","Broughton silty clay loam, 6 to 12 percent slopes, moderately eroded","Broughton",3,0.43,"HEL"]
["Paulding","BcD2","Broughton silty clay loam, 12 to 18 percent slopes, moderately eroded","Broughton",3,0.43,"HEL"]
["Paulding","BcE2","Broughton silty clay loam, 18 to 35 percent slopes, moderately or severely eroded","Broughton",3,0.43,"HEL"]
["Paulding","Da","Defiance silty clay loam","Defiance",5,0.37,"NHEL"]
["Paulding","DbA","Digby fine sandy loam, 0 to 2 percent slopes","Digby",4,0.24,"NHEL"]
["Paulding","DcA","Digby loam, 0 to 2 percent slopes","Digby",4,0.32,"NHEL"]
["Paulding","DcB1","Digby loam, 2 to 6 percent slopes, slightly or moderately eroded","Digby",4,0.32,"PHEL"]
["Paulding","DdA","Digby silt loam, 0 to 2 percent slopes","Digby",4,0.32,"NHEL"]
["Paulding","DdB1","Digby silt loam, 2 to 6 percent slopes, slightly or moderately eroded","Digby",4,0.32,"PHEL"]
["Paulding","Ea","Eel loam","Eel",5,0.37,"NHEL"]
["Paulding","Eb","Eel silt loam","Eel",5,0.37,"NHEL"]
["Paulding","Ec","Eel silty clay loam","Eel",5,0.37,"NHEL"]
["Paulding","FaA","Fulton fine sandy loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Paulding","FbB","Fulton loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Paulding","FcA","Fulton silt loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Paulding","FcB1","Fulton silt loam, 2 to 6 percent slopes, slightly eroded","Fulton",3,0.43,"PHEL"]
["Paulding","FcB2","Fulton silt loam, 2 to 6 percent slopes, moderately eroded","Fulton",3,0.43,"PHEL"]
["Paulding","FdA","Fulton silt loam, sandy substratum, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Paulding","FdB1","Fulton silt loam, sandy substratum, 2 to 6 percent slopes, slightly eroded","Fulton",3,0.43,"PHEL"]
["Paulding","FdB2","Fulton silt loam, sandy substratum, 2 to 6 percent slopes, moderately eroded","Fulton",3,0.43,"PHEL"]
["Paulding","FeA","Fulton silty clay loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Paulding","FfA","Fulton silty clay loam, sandy substratum, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Paulding","Ga","Genesee fine sandy loam","Genesee",5,0.37,"NHEL"]
["Paulding","Gb","Genesee loam","Genesee",5,0.37,"NHEL"]
["Paulding","Gc","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Paulding","Gd","Granby fine sandy loam","Granby",5,0.17,"NHEL"]
["Paulding","HaA","Haney silt loam and loam, 0 to 2 percent slopes","Haney",4,0.32,"NHEL"]
["Paulding","HaB1","Haney silt loam and loam, 2 to 6 percent slopes, slightly or moderately eroded","Haney",4,0.32,"PHEL"]
["Paulding","HaC2","Haney silt loam and loam, 6 to 15 percent slopes, moderately eroded","Haney",4,0.32,"PHEL"]
["Paulding","Hb","Haskins loam","Haskins",4,0.37,"NHEL"]
["Paulding","Hc","Haskins silt loam","Haskins",4,0.37,"NHEL"]
["Paulding","Hd","Hoytville clay","Hoytville",5,0.28000000000000003,"NHEL"]
["Paulding","He","Hoytville silt loam","Hoytville",5,0.28000000000000003,"NHEL"]
["Paulding","Hf","Hoytville silty clay loam","Hoytville",5,0.28000000000000003,"NHEL"]
["Paulding","La","Latty clay","Latty",5,0.28000000000000003,"NHEL"]
["Paulding","Lb","Latty silty clay loam","Latty",5,0.28000000000000003,"NHEL"]
["Paulding","LcB1","Lucas silt loam, 2 to 6 percent slopes, slightly or moderately eroded","Lucas",3,0.43,"PHEL"]
["Paulding","LcC2","Lucas silt loam, 6 to 12 percent slopes, moderately eroded","Lucas",3,0.43,"PHEL"]
["Paulding","LcD2","Lucas silt loam, 12 to 25 percent slopes, moderately eroded","Lucas",3,0.43,"HEL"]
["Paulding","LdA","Lucas silt loam, sandy substratum, 0 to 2 percent slopes","Lucas",3,0.43,"NHEL"]
["Paulding","LdB1","Lucas silt loam, sandy substratum, 2 to 6 percent slopes, slightly eroded","Lucas",3,0.43,"PHEL"]
["Paulding","LdB2","Lucas silt loam, sandy substratum, 2 to 6 percent slopes, moderately eroded","Lucas",3,0.43,"PHEL"]
["Paulding","LdC2","Lucas silt loam, sandy substratum, 6 to 12 percent slopes, moderately eroded","Lucas",3,0.43,"PHEL"]
["Paulding","LdD2","Lucas silt loam, sandy substratum, 12 to 25 percent slopes, moderately or severely eroded","Lucas",3,0.43,"HEL"]
["Paulding","Ma","Mermill loam","Mermill",5,0.28000000000000003,"NHEL"]
["Paulding","Mb","Mermill silt loam","Mermill",5,0.28000000000000003,"NHEL"]
["Paulding","Mc","Mermill silty clay loam","Mermill",5,0.28000000000000003,"NHEL"]
["Paulding","Md","Millgrove loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Paulding","Me","Millgrove silt loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Paulding","Mf","Millgrove silty clay loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Paulding","NaA","Nappanee fine sandy loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Paulding","NbA","Nappanee loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Paulding","NcA","Nappanee silt loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Paulding","NcB1","Nappanee silt loam, 2 to 6 percent slopes, slightly eroded","Nappanee",3,0.43,"PHEL"]
["Paulding","NcB2","Nappanee silt loam, 2 to 6 percent slopes, moderately eroded","Nappanee",3,0.43,"PHEL"]
["Paulding","NdA","Nappanee silty clay loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Paulding","NdB1","Nappanee silty clay loam, 2 to 6 percent slopes, slightly eroded","Nappanee",3,0.43,"PHEL"]
["Paulding","NdB2","Nappanee silty clay loam, 2 to 6 percent slopes, moderately eroded","Nappanee",3,0.43,"PHEL"]
["Paulding","OaA","Ottokee loamy sand, 0 to 2 percent slopes","Ottokee",5,0.17,"NHEL"]
["Paulding","OaB1","Ottokee loamy sand, 2 to 6 percent slopes, slightly eroded","Ottokee",5,0.17,"NHEL"]
["Paulding","Pa","Paulding clay","Paulding",5,0.28000000000000003,"NHEL"]
["Paulding","Pb","Paulding loam","Paulding",5,0.28000000000000003,"NHEL"]
["Paulding","Pc","Paulding silty clay loam","Paulding",5,0.28000000000000003,"NHEL"]
["Paulding","RaA","Rimer fine sandy loam, 0 to 2 percent slopes","Rimer",4,0.17,"NHEL"]
["Paulding","RaB1","Rimer fine sandy loam, 2 to 6 percent slopes, slightly eroded","Rimer",4,0.17,"NHEL"]
["Paulding","RbA","Rimer sandy loam, 0 to 2 percent slopes","Rimer",4,0.17,"NHEL"]
["Paulding","RbB1","Rimer sandy loam, 2 to 6 percent slopes, slightly eroded","Rimer",4,0.17,"NHEL"]
["Paulding","RcA","Roselms clay, 0 to 2 percent slopes","Roselms",3,0.32,"NHEL"]
["Paulding","RdA","Roselms fine sandy loam, 0 to 2 percent slopes","Roselms",3,0.32,"NHEL"]
["Paulding","ReA","Roselms loam, 0 to 2 percent slopes","Roselms",3,0.32,"NHEL"]
["Paulding","ReB1","Roselms loam, 2 to 6 percent slopes, slightly eroded","Roselms",3,0.32,"PHEL"]
["Paulding","RfA","Roselms silt loam, 0 to 2 percent slopes","Roselms",3,0.32,"NHEL"]
["Paulding","RfB1","Roselms silt loam, 2 to 6 percent slopes, slightly eroded","Roselms",3,0.32,"PHEL"]
["Paulding","RfB2","Roselms silt loam, 2 to 6 percent slopes, moderately eroded","Roselms",3,0.32,"PHEL"]
["Paulding","RgA","Roselms silty clay loam, 0 to 2 percent slopes","Roselms",3,0.32,"NHEL"]
["Paulding","RgB1","Roselms silty clay loam, 2 to 6 percent slopes, slightly eroded","Roselms",3,0.32,"PHEL"]
["Paulding","RgB2","Roselms silty clay loam, 2 to 6 percent slopes, moderately eroded","Roselms",3,0.32,"PHEL"]
["Paulding","Rh","Ross silt loam","Ross",5,0.32,"NHEL"]
["Paulding","SaA","Seward fine sandy loam, 0 to 2 percent slopes","Seward",4,0.17,"NHEL"]
["Paulding","SaB1","Seward fine sandy loam, 2 to 6 percent slopes, slightly eroded","Seward",4,0.17,"NHEL"]
["Paulding","SaC1","Seward fine sandy loam, 6 to 15 percent slopes, slightly eroded","Seward",4,0.17,"PHEL"]
["Paulding","SbB1","Seward sandy loam, 2 to 6 percent slopes, slightly eroded","Seward",4,0.17,"NHEL"]
["Paulding","Sc","Shoals silt loam","shoals",5,0.37,"NHEL"]
["Paulding","Sd","Sloan silt loam","Sloan",5,0.37,"NHEL"]
["Paulding","Se","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Paulding","SfC3","St. Clair clay, 6 to 12 percent slopes, severely eroded","St. Clair",2,0.37,"HEL"]
["Paulding","SfD3","St. Clair clay, 12 to 18 percent slopes, severely eroded","St. Clair",2,0.37,"HEL"]
["Paulding","SfF3","St. Clair clay, 25 to 35 percent slopes, severely eroded","St. Clair",2,0.37,"HEL"]
["Paulding","SgB1","St. Clair silt loam, 2 to 6 percent slopes, slightly eroded","St. Clair",3,0.37,"PHEL"]
["Paulding","SgB2","St. Clair silt loam, 2 to 6 percent slopes, moderately eroded","St. Clair",3,0.37,"PHEL"]
["Paulding","SgC2","St. Clair silt loam, 6 to 12 percent slopes, moderately eroded","St. Clair",3,0.37,"PHEL"]
["Paulding","SgD2","St. Clair silt loam, 12 to 18 percent slopes, moderately eroded","St. Clair",3,0.37,"HEL"]
["Paulding","SgE2","St. Clair silt loam, 18 to 25 percent slopes, moderately eroded","St. Clair",3,0.37,"HEL"]
["Paulding","Ta","Tedrow loamy fine sand","Tedrow",5,0.17,"NHEL"]
["Paulding","Tb","Toledo loam","Toledo",5,0.28000000000000003,"NHEL"]
["Paulding","Tc","Toledo silt loam","Toledo",5,0.28000000000000003,"NHEL"]
["Paulding","Td","Toledo silty clay","Toledo",5,0.28000000000000003,"NHEL"]
["Paulding","Te","Toledo silty clay loam","Toledo",5,0.28000000000000003,"NHEL"]
["Paulding","Wa","Wabash silty clay","Wabash",5,0.28000000000000003,"NHEL"]
["Paulding","Wb","Wauseon fine sandy loam","Wauseon",4,0.17,"NHEL"]
["Paulding","Wc","Wauseon loam","Wauseon",4,0.17,"NHEL"]
["Paulding","Wd","Wetzel clay","Wetzel",5,0.37,"NHEL"]
["Paulding","We","Wetzel silty clay loam","Wetzel",5,0.37,"NHEL"]
[null,"Select","none","none"]
["Putnam","ArB","Arkport loamy fine sand, 2 to 6 percent slopes","Arkport",3,0.17,"PHEL"]
["Putnam","BlB","Belmore sandy loam, 2 to 6 percent slopes","Belmore",4,0.24,"PHEL"]
["Putnam","BmA","Belmore loam, 0 to 2 percent slopes","Belmore",4,0.32,"NHEL"]
["Putnam","BmB","Belmore loam, 2 to 6 percent slopes","Belmore",4,0.32,"PHEL"]
["Putnam","BmC","Belmore loam, 6 to 12 percent slopes","Belmore",4,0.32,"PHEL"]
["Putnam","BnA","Blount loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Putnam","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Putnam","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Putnam","BrB","Blount-Del Rey silt loams, 1 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Putnam","Bs","Bono silty clay loam","Bono",5,0.28000000000000003,"NHEL"]
["Putnam","BtB","Broughton silty clay loam, 2 to 6 percent slopes","Broughton",3,0.43,"PHEL"]
["Putnam","BuB2","Broughton clay, 2 to 6 percent slopes, moderately eroded","Broughton",2,0.32,"PHEL"]
["Putnam","BuC2","Broughton clay, 6 to 12 percent slopes, moderately eroded","Broughton",2,0.32,"PHEL"]
["Putnam","BuD2","Broughton clay, 12 to 18 percent slopes, moderately eroded","Broughton",2,0.32,"HEL"]
["Putnam","BuE3","Broughton clay, 18 to 25 percent slopes, severely eroded","Broughton",2,0.32,"HEL"]
["Putnam","Cp","Clay pits","Clay"]
["Putnam","Cw","Colwood loam","Colwood",5,0.28000000000000003,"NHEL"]
["Putnam","Cx","Cut and fill land","Cut"]
["Putnam","Df","Defiance silty clay loam","Defiance",5,0.37,"NHEL"]
["Putnam","DgA","Del Rey loam, 0 to 2 percent slopes","Del Rey",3,0.43,"NHEL"]
["Putnam","DlA","Del Rey silt loam, 0 to 2 percent slopes","Del Rey",3,0.43,"NHEL"]
["Putnam","DlB","Del Rey silt loam, 2 to 6 percent slopes","Del Rey",3,0.43,"PHEL"]
["Putnam","DmB","Del Rey-Fulton silt loams, 1 to 6 percent slopes","Del Rey",3,0.43,"PHEL"]
["Putnam","DnA","Digby loam, 0 to 2 percent slopes","Digby",4,0.32,"NHEL"]
["Putnam","DnB","Digby loam, 2 to 6 percent slopes","Digby",4,0.32,"PHEL"]
["Putnam","DoA","Digby loam, moderately shallow variant, 0 to 2 percent slopes","Digby",4,0.32,"NHEL"]
["Putnam","FtA","Fulton loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Putnam","FuA","Fulton silty clay loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Putnam","FuB","Fulton silty clay loam, 2 to 6 percent slopes","Fulton",3,0.43,"PHEL"]
["Putnam","FvA","Fulton silty clay loam, gravelly substratum, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Putnam","Gn","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Putnam","Gp","Gravel pits","Gravel"]
["Putnam","HaB","Haney sandy loam, 2 to 6 percent slopes","Haney",4,0.28000000000000003,"PHEL"]
["Putnam","HdA","Haney loam, 0 to 2 percent slopes","Haney",4,0.32,"NHEL"]
["Putnam","HdB","Haney loam, 2 to 6 percent slopes","Haney",4,0.32,"PHEL"]
["Putnam","HkA","Haskins fine sandy loam, 0 to 2 percent slopes","Haskins",4,0.24,"NHEL"]
["Putnam","HkB","Haskins fine sandy loam, 2 to 6 percent slopes","Haskins",4,0.24,"PHEL"]
["Putnam","HnA","Haskins loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Putnam","HnB","Haskins loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Putnam","Ho","Hoytville silty clay loam","Hoytville",5,0.28000000000000003,"NHEL"]
["Putnam","Hv","Hoytville clay","Hoytville",5,0.28000000000000003,"NHEL"]
["Putnam","KbA","Kibbie loam, 0 to 2 percent slopes","Kibbie",5,0.28000000000000003,"NHEL"]
["Putnam","KsA","Kibbie silt loam, 0 to 2 percent slopes","Kibbie",5,0.28000000000000003,"NHEL"]
["Putnam","KtB","Kibbie-Del Rey silt loams, 1 to 6 percent slopes","Kibbie",5,0.28000000000000003,"PHEL"]
["Putnam","La","Latty silty clay loam","Latty",5,0.28000000000000003,"NHEL"]
["Putnam","Lc","Latty clay","Latty",5,0.28000000000000003,"NHEL"]
["Putnam","Ln","Lenawee silt loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Putnam","Ls","Lenawee silty clay loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Putnam","LwB","Lucas silty clay loam, 2 to 6 percent slopes","Lucas",3,0.43,"PHEL"]
["Putnam","LwC2","Lucas silty clay loam, 6 to 12 percent slopes, moderately eroded","Lucas",3,0.43,"PHEL"]
["Putnam","LwD2","Lucas silty clay loam, 12 to 18 percent slopes, moderately eroded","Lucas",3,0.43,"HEL"]
["Putnam","Md","Mermill loam","Mermill",5,0.28000000000000003,"NHEL"]
["Putnam","Me","Mermill silty clay loam","Mermill",5,0.28000000000000003,"NHEL"]
["Putnam","Mf","Millgrove loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Putnam","Mg","Millgrove silty clay loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Putnam","MrB","Morley silt loam, 2 to 6 percent slopes","Morley",3,0.43,"PHEL"]
["Putnam","NaA","Nappanee loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Putnam","NaB","Nappanee loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Putnam","NpA","Nappanee silt loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Putnam","NpB","Nappanee silt loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Putnam","NtA","Nappanee silty clay loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Putnam","OkB","Ottokee loamy fine sand, 1 to 6 percent slopes","Ottokee",5,0.17,"NHEL"]
["Putnam","OtB","Ottokee-Tuscola complex, 2 to 6 percent slopes","Ottokee",5,0.17,"NHEL"]
["Putnam","Pa","Paulding silty clay loam","Paulding",5,0.28000000000000003,"NHEL"]
["Putnam","Pd","Paulding clay","Paulding",5,0.28000000000000003,"NHEL"]
["Putnam","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Putnam","Qu","Quarries","Quarries"]
["Putnam","RmA","Rawson loam, 0 to 2 percent slopes","Rawson",4,0.32,"NHEL"]
["Putnam","RmB","Rawson loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Putnam","RmC2","Rawson loam, 6 to 12 percent slopes, moderately eroded","Rawson",4,0.32,"PHEL"]
["Putnam","RnA","Rimer loamy fine sand, 0 to 2 percent slopes","Rimer",4,0.17,"NHEL"]
["Putnam","RnB","Rimer loamy fine sand, 2 to 6 percent slopes","Rimer",4,0.17,"NHEL"]
["Putnam","RoA","Roselms silt loam, 0 to 2 percent slopes","Roselms",3,0.32,"NHEL"]
["Putnam","RoB","Roselms silt loam, 2 to 6 percent slopes","Roselms",3,0.32,"PHEL"]
["Putnam","RsA","Roselms silty clay loam, 0 to 2 percent slopes","Roselms",3,0.32,"NHEL"]
["Putnam","RsB","Roselms silty clay loam, 2 to 6 percent slopes","Roselms",3,0.32,"PHEL"]
["Putnam","SaB","St. Clair loam, 2 to 6 percent slopes","St. Clair",3,0.37,"PHEL"]
["Putnam","ScB","St. Clair silt loam, 2 to 6 percent slopes","St. Clair",3,0.37,"PHEL"]
["Putnam","ScC2","St. Clair silt loam, 6 to 12 percent slopes, moderately eroded","St. Clair",3,0.37,"PHEL"]
["Putnam","ScD2","St. Clair silt loam, 12 to 18 percent slopes, moderately eroded","St. Clair",3,0.37,"HEL"]
["Putnam","SdA","Seward loamy fine sand, 0 to 2 percent slopes","seward",4,0.17,"NHEL"]
["Putnam","SdB","Seward loamy fine sand, 2 to 6 percent slopes","seward",4,0.17,"NHEL"]
["Putnam","SfB","Shinrock silt loam, 2 to 6 percent slopes","Shinrock",3,0.37,"PHEL"]
["Putnam","SfC2","Shinrock silt loam, 6 to 12 percent slopes, moderately eroded","Shinrock",3,0.37,"PHEL"]
["Putnam","Sh","Shoals silt loam","shoals",5,0.37,"NHEL"]
["Putnam","Sk","Shoals silt loam, moderately shallow variant","shoals",4,0.37,"NHEL"]
["Putnam","So","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Putnam","TdA","Tedrow loamy fine sand, 0 to 3 percent slopes","Tedrow",5,0.17,"NHEL"]
["Putnam","To","Toledo silty clay loam","Toledo",5,0.28000000000000003,"NHEL"]
["Putnam","Tt","Toledo silty clay","Toledo",5,0.28000000000000003,"NHEL"]
["Putnam","TuB","Tuscola loam, 2 to 6 percent slopes","Tuscola",5,0.32,"PHEL"]
["Putnam","TwB","Tuscola-Shinrock complex, 2 to 6 percent slopes","Tuscola",5,0.32,"PHEL"]
["Putnam","Ur","Urban land","Urban"]
["Putnam","VaB","Vaughnsville loam, 2 to 6 percent slopes","Vaughnsville",4,0.32,"PHEL"]
["Putnam","W","Water","Water"]
["Putnam","Wa","Wabasha silty clay","Wabasha",5,0.32,"NHEL"]
["Putnam","Wb","Wabasha silty clay loam, moderately shallow variant","Wabasha",5,0.28000000000000003,"NHEL"]
["Putnam","Wf","Wauseon fine sandy loam","Wauseon",4,0.17,"NHEL"]
["Putnam","Wm","Willette muck","Willette",2,null,"NHEL"]
[null,"Select","none","none"]
["Sandusky","An","Aquents, nearly level","Aquents",null,null,"NHEL"]
["Sandusky","BaB","Belmore loam, 2 to 6 percent slopes","Belmore",4,0.32,"PHEL"]
["Sandusky","BeA","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Sandusky","BkB","Bixler loamy fine sand, 2 to 6 percent slopes","Bixler",5,0.15,"NHEL"]
["Sandusky","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Sandusky","Bt","Bono silty clay","Bono",5,0.28000000000000003,"NHEL"]
["Sandusky","ChB","Castalia very stony loam, 1 to 6 percent slopes","Castalia",2,0.2,"PHEL"]
["Sandusky","Co","Colwood fine sandy loam","Colwood",5,0.28000000000000003,"NHEL"]
["Sandusky","DeA","Del Rey silt loam, 0 to 2 percent slopes","Del Rey",3,0.43,"NHEL"]
["Sandusky","DkA","Dixboro-Kibbie complex, 0 to 2 percent slopes","Dixboro",5,0.2,"NHEL"]
["Sandusky","Do","Dumps","Dumps"]
["Sandusky","DuB","Dunbridge sandy loam, 1 to 4 percent slopes","Dunbridge",2,0.17,"NHEL"]
["Sandusky","FuA","Fulton silty clay loam, 0 to 3 percent slopes","Fulton",3,0.43,"NHEL"]
["Sandusky","Ge","Gilford fine sandy loam","Gilford",4,0.2,"NHEL"]
["Sandusky","GtB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Sandusky","GwB","Glynwood silt loam, 2 to 6 percent slopes","Glynwood",3,0.43,"PHEL"]
["Sandusky","Gx","Granby loamy sand","Granby",5,0.17,"NHEL"]
["Sandusky","HaB","Haskins sandy loam, 1 to 4 percent slopes","Haskins",4,0.24,"NHEL"]
["Sandusky","Ht","Hoytville silty clay loam","Hoytville",5,0.28000000000000003,"NHEL"]
["Sandusky","KbA","Kibbie fine sandy loam, 0 to 2 percent slopes","Kibbie",5,0.2,"NHEL"]
["Sandusky","Le","Lenawee silty clay loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Sandusky","LuB","Lucas silty clay, 2 to 6 percent slopes","Lucas",3,0.43,"PHEL"]
["Sandusky","MeB","Mentor silt loam, 1 to 4 percent slopes","Mentor",5,0.37,"NHEL"]
["Sandusky","MeF","Mentor silt loam, 25 to 50 percent slopes","Mentor",5,0.37,"HEL"]
["Sandusky","Mo","Mermill loam","Mermill",5,0.28000000000000003,"NHEL"]
["Sandusky","Mp","Mermill Variant sandy loam","Mermill",4,0.24,"NHEL"]
["Sandusky","Ms","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Sandusky","NpA","Nappanee silt loam, 0 to 3 percent slopes","Nappanee",3,0.43,"NHEL"]
["Sandusky","Pe","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Sandusky","Pq","Pits, quarry","Pits"]
["Sandusky","RoB","Rimer loamy fine sand, 1 to 4 percent slopes","Rimer",4,0.17,"NHEL"]
["Sandusky","Rs","Rossburg silt loam, occasionally flooded","Rossburg",5,0.37,"NHEL"]
["Sandusky","Sa","Sandusky gravelly coarse sandy loam","Sandusky",4,0.15,"NHEL"]
["Sandusky","SbC2","Saylesville silty clay loam, 6 to 12 percent slopes, eroded","Saylesville",5,0.37,"PHEL"]
["Sandusky","SeB","Seward loamy fine sand, 2 to 6 percent slopes","Seward",4,0.17,"NHEL"]
["Sandusky","Sh","Shoals silt loam, frequently flooded","shoals",5,0.37,"NHEL"]
["Sandusky","SoB","Spinks fine sand, 2 to 6 percent slopes","Spinks",5,0.17,"NHEL"]
["Sandusky","TeA","Tedrow loamy fine sand, 0 to 2 percent slopes","Tedrow",5,0.17,"NHEL"]
["Sandusky","TfA","Tedrow-Dixboro complex, 0 to 2 percent slopes","Tedrow",5,0.17,"NHEL"]
["Sandusky","To","Toledo silty clay","Toledo",5,0.28000000000000003,"NHEL"]
["Sandusky","Tp","Toledo silty clay loam, ponded","Toledo",5,0.28000000000000003,"NHEL"]
["Sandusky","Un","Udorthents, strongly sloping","Udorthents"]
["Sandusky","W","Water","Water"]
["Sandusky","Wa","Weyers coarse sandy loam","Weyers",5,0.2,"NHEL"]
[null,"Select","none","none"]
["Seneca","BdB","Belmore loam, 2 to 6 percent slopes","Belmore",4,0.32,"PHEL"]
["Seneca","BfF2","Belmore-Morley complex, 18 to 50 percent slopes, eroded","Belmore",4,0.32,"HEL"]
["Seneca","BgB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Seneca","BgB2","Bennington silt loam, 2 to 6 percent slopes, eroded","Bennington",3,0.43,"PHEL"]
["Seneca","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Seneca","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Seneca","Bp","Bono silty clay, loamy substratum","Bono",5,0.28000000000000003,"NHEL"]
["Seneca","Ca","Carlisle muck","Carlisle",2,null,"NHEL"]
["Seneca","Ch","Chagrin silt loam, occasionally flooded","Chagrin",5,0.32,"NHEL"]
["Seneca","CnA","Channahon silt loam, 0 to 2 percent slopes","Channahon",2,0.37,"NHEL"]
["Seneca","CnB","Channahon silt loam, 2 to 6 percent slopes","Channahon",2,0.37,"PHEL"]
["Seneca","Co","Colwood silt loam","Colwood",5,0.28000000000000003,"NHEL"]
["Seneca","DmA","Digby loam, 1 to 4 percent slopes","Digby",4,0.32,"NHEL"]
["Seneca","FcA","Fitchville silt loam, 1 to 4 percent slopes","Fitchville",5,0.37,"NHEL"]
["Seneca","GaA","Gallman loam, 0 to 2 percent slopes","Gallman",5,0.32,"NHEL"]
["Seneca","GaB","Gallman loam, 2 to 6 percent slopes","Gallman",5,0.32,"PHEL"]
["Seneca","GwA","Glynwood silt loam, 0 to 2 percent slopes","Glynwood",3,0.43,"NHEL"]
["Seneca","GwB","Glynwood silt loam, 2 to 6 percent slopes","Glynwood",3,0.43,"PHEL"]
["Seneca","GxB2","Glynwood silty clay loam, 2 to 6 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Seneca","GxC2","Glynwood silty clay loam, 6 to 12 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Seneca","HaA","Haney loam, 0 to 2 percent slopes","Haney",4,0.32,"NHEL"]
["Seneca","HaB","Haney loam, 2 to 6 percent slopes","Haney",4,0.32,"PHEL"]
["Seneca","HaC2","Haney loam, 6 to 12 percent slopes, eroded","Haney",4,0.32,"PHEL"]
["Seneca","HkA","Haskins loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Seneca","HkB","Haskins loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Seneca","HmB","Haskins-Seward complex, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Seneca","Ht","Hoytville silty clay loam","Hoytville",5,0.28000000000000003,"NHEL"]
["Seneca","KbA","Kibbie fine sandy loam, 0 to 2 percent slopes","Kibbie",5,0.2,"NHEL"]
["Seneca","Le","Lenawee silty clay loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Seneca","Lw","Linwood muck","Linwood",2,null,"NHEL"]
["Seneca","Me","Mermill loam","Mermill",5,0.28000000000000003,"NHEL"]
["Seneca","Mf","Millgrove loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Seneca","Mm","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Seneca","MnA","Milton silt loam, 0 to 2 percent slopes","Milton",4,0.37,"NHEL"]
["Seneca","MnB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Seneca","MoA","Milton variant loam, 0 to 2 percent slopes","Milton",4,0.32,"NHEL"]
["Seneca","MoB","Milton variant loam, 2 to 6 percent slopes","Milton",4,0.32,"PHEL"]
["Seneca","MrD2","Morley silt loam, 12 to 18 percent slopes, eroded","Morley",3,0.43,"HEL"]
["Seneca","MrF2","Morley silt loam, 18 to 50 percent slopes, eroded","Morley",3,0.43,"HEL"]
["Seneca","NpA","Nappanee silt loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Seneca","NpB","Nappanee silt loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Seneca","OpB","Oshtemo sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Seneca","Pa","Pandora silt loam","Pandora",5,0.37,"NHEL"]
["Seneca","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Seneca","Pt","Pits, quarries","Pits"]
["Seneca","RbA","Randolph silt loam, 0 to 2 percent slopes","Randolph",3,0.37,"NHEL"]
["Seneca","RmB","Rawson loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Seneca","RoA","Rimer loamy sand, 0 to 2 percent slopes","Rimer",4,0.17,"NHEL"]
["Seneca","Ru","Ross silt loam, occasionally flooded","Ross",5,0.32,"NHEL"]
["Seneca","Sb","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Seneca","SdA","Seward loamy fine sand, 0 to 2 percent slopes","Seward",4,0.17,"NHEL"]
["Seneca","SdB","Seward loamy fine sand, 2 to 6 percent slopes","Seward",4,0.17,"PHEL"]
["Seneca","Sh","Shoals silt loam, frequently flooded","shoals",5,0.37,"NHEL"]
["Seneca","SpB","Spinks loamy sand, 2 to 6 percent slopes","Spinks",5,0.17,"NHEL"]
["Seneca","TrA","Tiro silt loam, 0 to 2 percent slopes","Tiro",4,0.37,"NHEL"]
["Seneca","TrB","Tiro silt loam, 2 to 6 percent slopes","Tiro",4,0.37,"PHEL"]
["Seneca","Ua","Udorthents, loamy","Udorthents"]
["Seneca","Ur","Urban land","Urban"]
["Seneca","W","Water","Water"]
[null,"Select","none","none"]
["Van Wert","BlB","Belmore sandy loam, 2 to 6 percent slopes","Belmore",4,0.24,"PHEL"]
["Van Wert","BmA","Belmore loam, 0 to 2 percent slopes","Belmore",4,0.32,"NHEL"]
["Van Wert","BmB","Belmore loam, 2 to 6 percent slopes","Belmore",4,0.32,"PHEL"]
["Van Wert","BmC","Belmore loam, 6 to 12 percent slopes","Belmore",4,0.32,"PHEL"]
["Van Wert","BnA","Blount loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Van Wert","BnB","Blount loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Van Wert","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Van Wert","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Van Wert","BoB2","Blount silt loam, 2 to 6 percent slopes, moderately eroded","Blount",3,0.43,"PHEL"]
["Van Wert","Cp","Clay pits","Clay"]
["Van Wert","Cw","Colwood silt loam","Colwood",5,0.28000000000000003,"NHEL"]
["Van Wert","Cx","Cut and fill land","Cut"]
["Van Wert","De","Defiance silt loam","Defiance",5,0.37,"NHEL"]
["Van Wert","Df","Defiance silty clay loam","Defiance",5,0.37,"NHEL"]
["Van Wert","DgA","Digby sandy loam, 0 to 2 percent slopes","Digby",4,0.24,"NHEL"]
["Van Wert","DgB","Digby sandy loam, 2 to 6 percent slopes","Digby",4,0.24,"PHEL"]
["Van Wert","DmA","Digby loam, 0 to 2 percent slopes","Digby",4,0.32,"NHEL"]
["Van Wert","DmB","Digby loam, 2 to 6 percent slopes","Digby",4,0.32,"PHEL"]
["Van Wert","Em","Eel silt loam","Eel",5,0.37,"NHEL"]
["Van Wert","EoB","Elliott silt loam, 0 to 4 percent slopes","Elliott",4,0.28000000000000003,"NHEL"]
["Van Wert","HaB","Haney sandy loam, 2 to 6 percent slopes","Haney",4,0.28000000000000003,"PHEL"]
["Van Wert","HdA","Haney loam, 0 to 2 percent slopes","Haney",4,0.32,"NHEL"]
["Van Wert","HdB","Haney loam, 2 to 6 percent slopes","Haney",4,0.32,"PHEL"]
["Van Wert","HkA","Haskins fine sandy loam, 0 to 2 percent slopes","Haskins",4,0.24,"NHEL"]
["Van Wert","HkB","Haskins fine sandy loam, 2 to 6 percent slopes","Haskins",4,0.24,"PHEL"]
["Van Wert","HnA","Haskins loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Van Wert","HnB","Haskins loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Van Wert","Ho","Hoytville silty clay loam","Hoytville",5,0.28000000000000003,"NHEL"]
["Van Wert","Hs","Hoytville silty clay loam, moderately shallow variant","Hoytville",5,0.28000000000000003,"NHEL"]
["Van Wert","Hv","Hoytville clay","Hoytville",5,0.28000000000000003,"NHEL"]
["Van Wert","Ks","Kibbie silt loam","Kibbie",5,0.28000000000000003,"NHEL"]
["Van Wert","La","Latty silty clay loam","Latty",5,0.28000000000000003,"NHEL"]
["Van Wert","Lc","Latty clay","Latty",5,0.28000000000000003,"NHEL"]
["Van Wert","Mc","McGary silt loam","McGary",3,0.43,"NHEL"]
["Van Wert","Md","Mermill silt loam","Mermill",5,0.28000000000000003,"NHEL"]
["Van Wert","Me","Millgrove silt loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Van Wert","Mg","Millgrove silty clay loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Van Wert","Mm","Montgomery silty clay loam","Montgomery",5,0.37,"NHEL"]
["Van Wert","Mn","Montgomery silty clay","Montgomery",5,0.37,"NHEL"]
["Van Wert","MoB","Morley loam, 2 to 6 percent slopes","Morley",3,0.43,"PHEL"]
["Van Wert","MrB","Morley silt loam, 2 to 6 percent slopes","Morley",3,0.43,"PHEL"]
["Van Wert","MrB2","Morley silt loam, 2 to 6 percent slopes, moderately eroded","Morley",3,0.43,"PHEL"]
["Van Wert","MrC2","Morley silt loam, 6 to 12 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Van Wert","MrD2","Morley silt loam, 12 to 18 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Van Wert","NaA","Nappanee loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Van Wert","NpA","Nappanee silt loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Van Wert","NpB","Nappanee silt loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Van Wert","NtA","Nappanee silty clay loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Van Wert","NtB","Nappanee silty clay loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Van Wert","NtB2","Nappanee silty clay loam, 2 to 6 percent slopes, moderately eroded","Nappanee",3,0.43,"PHEL"]
["Van Wert","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Van Wert","Po","Pewamo silty clay","Pewamo",5,0.24,"NHEL"]
["Van Wert","Qu","Quarry","Quarry"]
["Van Wert","RmB","Rawson loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Van Wert","ScB","St. Clair silt loam, 2 to 6 percent slopes","St. Clair",3,0.37,"PHEL"]
["Van Wert","ScC2","St. Clair silt loam, 6 to 12 percent slopes, moderately eroded","St. Clair",3,0.37,"PHEL"]
["Van Wert","Sh","Shoals silt loam","shoals",5,0.37,"NHEL"]
["Van Wert","So","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Van Wert","To","Toledo silty clay","Toledo",5,0.28000000000000003,"NHEL"]
["Van Wert","W","Water","Water"]
["Van Wert","Wa","Wabasha silty clay loam","Wabasha",5,0.32,"NHEL"]
["Van Wert","Wb","Wabasha silty clay loam, moderately shallow variant","Wabasha",5,0.28000000000000003,"NHEL"]
["Van Wert","Wh","Wabasha silty clay","Wabasha",5,0.32,"NHEL"]
[null,"Select","none","none"]
["Williams","ApB","Arkport loamy fine sand, 2 to 6 percent slopes","Arkport",3,0.17,"PHEL"]
["Williams","BlB","Belmore sandy loam, 1 to 6 percent slopes","Belmore",4,0.24,"PHEL"]
["Williams","BnA","Blount loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Williams","BnB","Blount loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Williams","BnB2","Blount loam, 2 to 6 percent slopes, moderately eroded","Blount",3,0.43,"PHEL"]
["Williams","BoA","Blount loam, loamy substratum, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Williams","BoB","Blount loam, loamy substratum, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Williams","Bp","Bono silty clay loam","Bono",5,0.28000000000000003,"NHEL"]
["Williams","BrB","Boyer loamy sand, 1 to 6 percent slopes","Boyer",4,0.17,"NHEL"]
["Williams","BrC","Boyer loamy sand, 6 to 12 percent slopes","Boyer",4,0.17,"PHEL"]
["Williams","BsD","Boyer gravelly loamy sand, 12 to 18 percent slopes","Boyer",4,0.17,"PHEL"]
["Williams","Ca","Carlisle muck","Carlisle",2,null,"NHEL"]
["Williams","Ce","Ceresco sandy loam","Ceresco",5,0.2,"NHEL"]
["Williams","Ch","Cohoctah loam","Cohoctah",5,0.28000000000000003,"NHEL"]
["Williams","Cp","Colwood silt loam","Colwood",5,0.28000000000000003,"NHEL"]
["Williams","DeA","Del Rey loam, 0 to 2 percent slopes","Del Rey",3,0.43,"NHEL"]
["Williams","DeB","Del Rey loam, 2 to 6 percent slopes","Del Rey",3,0.43,"PHEL"]
["Williams","DfA","Del Rey silty clay loam, 0 to 2 percent slopes","Del Rey",3,0.43,"NHEL"]
["Williams","DfB","Del Rey silty clay loam, 2 to 6 percent slopes","Del Rey",3,0.43,"PHEL"]
["Williams","DgA","Digby sandy loam, 0 to 3 percent slopes","Digby",4,0.24,"NHEL"]
["Williams","DmA","Digby loam, 0 to 3 percent slopes","Digby",4,0.32,"NHEL"]
["Williams","Ed","Edwards muck","Edwards",2,null,"NHEL"]
["Williams","Ee","Eel loam","Eel",5,0.37,"NHEL"]
["Williams","FsA","Fulton loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Williams","FsB","Fulton loam, 2 to 6 percent slopes","Fulton",3,0.43,"PHEL"]
["Williams","FuA","Fulton silty clay loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Williams","FuB","Fulton silty clay loam, 2 to 6 percent slopes","Fulton",3,0.43,"PHEL"]
["Williams","Ge","Genesee loam","Genesee",5,0.37,"NHEL"]
["Williams","Gf","Gilford fine sandy loam","Gilford",4,0.2,"NHEL"]
["Williams","GlB","Glynwood loam, 2 to 6 percent slopes","Glynwood",3,0.43,"PHEL"]
["Williams","GlB2","Glynwood loam, 2 to 6 percent slopes, moderately eroded","Glynwood",3,0.43,"PHEL"]
["Williams","GlC","Glynwood loam, 6 to 12 percent slopes","Glynwood",3,0.43,"PHEL"]
["Williams","GlC2","Glynwood loam, 6 to 12 percent slopes, moderately eroded","Glynwood",3,0.43,"PHEL"]
["Williams","GlD2","Glynwood loam, 12 to 18 percent slopes, moderately eroded","Glynwood",3,0.43,"HEL"]
["Williams","GlE2","Glynwood loam, 18 to 40 percent slopes, moderately eroded","Glynwood",3,0.43,"HEL"]
["Williams","HaB","Haney loam, 1 to 6 percent slopes","Haney",4,0.32,"PHEL"]
["Williams","HeB","Haney-Rawson sandy loams, 1 to 6 percent slopes","Haney",4,0.28000000000000003,"PHEL"]
["Williams","HeC","Haney-Rawson sandy loams, 6 to 12 percent slopes","Haney",4,0.28000000000000003,"PHEL"]
["Williams","HkA","Haskins sandy loam, 0 to 3 percent slopes","Haskins",4,0.24,"NHEL"]
["Williams","HnA","Haskins loam, 0 to 3 percent slopes","Haskins",4,0.37,"NHEL"]
["Williams","Hv","Hoytville clay","Hoytville",5,0.28000000000000003,"NHEL"]
["Williams","KlA","Kibbie very fine sandy loam, 0 to 2 percent slopes","Kibbie",5,0.2,"NHEL"]
["Williams","KlB","Kibbie very fine sandy loam, 2 to 6 percent slopes","Kibbie",5,0.2,"PHEL"]
["Williams","La","Lamson very fine sandy loam","Lamson",5,0.28000000000000003,"NHEL"]
["Williams","Lb","Landes sandy loam","Landes",5,0.2,"NHEL"]
["Williams","Lc","Latty silty clay","Latty",5,0.28000000000000003,"NHEL"]
["Williams","Lf","Lenawee silty clay loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Williams","LuB2","Lucas silty clay loam, 2 to 6 percent slopes, moderately eroded","Lucas",3,0.43,"PHEL"]
["Williams","LuC2","Lucas silty clay loam, 6 to 12 percent slopes, moderately eroded","Lucas",3,0.43,"PHEL"]
["Williams","LuD2","Lucas silty clay loam, 12 to 25 percent slopes, moderately eroded","Lucas",3,0.43,"HEL"]
["Williams","Ma","Martisco muck","Martisco",3,null,"NHEL"]
["Williams","Md","Mermill loam","Mermill",5,0.28000000000000003,"NHEL"]
["Williams","Mh","Millgrove loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Williams","Mk","Millgrove clay loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Williams","NnA","Nappanee loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Williams","NnB","Nappanee loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Williams","NpA","Nappanee silty clay loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Williams","OrB","Oshtemo loamy sand, 2 to 6 percent slopes","Oshtemo",5,0.24,"NHEL"]
["Williams","OrC","Oshtemo loamy sand, 6 to 12 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Williams","OsB","Oshtemo sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"NHEL"]
["Williams","OtB","Ottokee fine sand, 0 to 6 percent slopes","Ottokee",5,0.17,"NHEL"]
["Williams","Pa","Paulding clay","Paulding",5,0.28000000000000003,"NHEL"]
["Williams","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Williams","RlB","Rawson sandy loam, 2 to 6 percent slopes","Rawson",4,0.24,"PHEL"]
["Williams","RlC","Rawson sandy loam, 6 to 12 percent slopes","Rawson",4,0.24,"PHEL"]
["Williams","RmB","Rawson loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Williams","RmC","Rawson loam, 6 to 12 percent slopes","Rawson",4,0.32,"PHEL"]
["Williams","RnA","Rimer loamy fine sand, 0 to 3 percent slopes","Rimer",4,0.17,"NHEL"]
["Williams","RsA","Roselms silty clay, 0 to 2 percent slopes","Roselms",3,0.32,"NHEL"]
["Williams","RsB","Roselms silty clay, 2 to 6 percent slopes","Roselms",3,0.32,"PHEL"]
["Williams","SbB2","St. Clair silty clay loam, 2 to 6 percent slopes, moderately eroded","St. Clair",3,0.37,"PHEL"]
["Williams","SbC2","St. Clair silty clay loam, 6 to 12 percent slopes, moderately eroded","St. Clair",3,0.37,"PHEL"]
["Williams","SbD2","St. Clair silty clay loam, 12 to 25 percent slopes, moderately eroded","St. Clair",3,0.37,"HEL"]
["Williams","SdB","Seward loamy fine sand, 2 to 6 percent slopes","Seward",4,0.17,"NHEL"]
["Williams","SgB","Shinrock silt loam, 2 to 6 percent slopes","Shinrock",3,0.37,"PHEL"]
["Williams","SgC","Shinrock silt loam, 6 to 12 percent slopes","Shinrock",3,0.37,"PHEL"]
["Williams","Sh","Shoals loam","Shoals",5,0.37,"NHEL"]
["Williams","Sn","Sloan loam","Sloan",5,0.37,"NHEL"]
["Williams","So","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Williams","SpB","Spinks fine sand, 2 to 6 percent slopes","Spinks",5,0.17,"NHEL"]
["Williams","SpC","Spinks fine sand, 6 to 18 percent slopes","Spinks",5,0.17,"PHEL"]
["Williams","To","Toledo silty clay","Toledo",5,0.28000000000000003,"NHEL"]
["Williams","TuB","Tuscola Variant fine sandy loam, 1 to 6 percent slopes","Tuscola",5,0.37,"PHEL"]
["Williams","TuC","Tuscola Variant fine sandy loam, 6 to 12 percent slopes","Tuscola",5,0.37,"PHEL"]
["Williams","Ud","Udorthents","Udorthents"]
["Williams","Uf","Udorthents, sandy","Udorthents"]
["Williams","Ur","Urban land","Urban"]
["Williams","W","Water","Water"]
["Williams","Wc","Wallkill silt loam","Wallkill",5,0.32,"NHEL"]
["Williams","Wk","Wallkill Variant silty clay loam","Wallkill",3,0.32,"NHEL"]
[null,"Select","none","none"]
["Wood","Al","Alluvial land","Alluvial"]
["Wood","BmB","Belmore loam, 1 to 4 percent slopes","Belmore",4,0.32,"NHEL"]
["Wood","BnB","Belmore sandy loam, 1 to 4 percent slopes","Belmore",4,0.24,"NHEL"]
["Wood","Co","Colwood loam","Colwood",5,0.28000000000000003,"NHEL"]
["Wood","Cs","Colwood fine sandy loam","Colwood",5,0.28000000000000003,"NHEL"]
["Wood","Dm","Digby loam, 0 to 2 percent slopes","Digby",4,0.32,"NHEL"]
["Wood","Dn","Digby sandy loam, 0 to 2 percent slopes","Digby",4,0.24,"NHEL"]
["Wood","Dr","Dunbridge sandy loam, 0 to 2 percent slopes","Dunbridge",2,0.17,"NHEL"]
["Wood","Ds","Dunbridge and Spinks loamy fine sands, over limestone, 0 to 2 percent slopes","Dunbridge",2,0.17,"NHEL"]
["Wood","DsB","Dunbridge and Spinks loamy fine sands, over limestone, 2 to 6 percent slopes","Dunbridge",2,0.17,"PHEL"]
["Wood","Dx","Dunbridge and Spinks stony loamy fine sands, over limestone, 0 to 2 percent slopes","Dunbridge",2,0.17,"NHEL"]
["Wood","Ea","Eel loam","Eel",5,0.37,"NHEL"]
["Wood","Em","Eel silt loam","Eel",5,0.37,"NHEL"]
["Wood","Er","Eel silt loam, over limestone","Eel",5,0.37,"NHEL"]
["Wood","Fu","Fulton silty clay loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Wood","FuB","Fulton silty clay loam, 2 to 6 percent slopes","Fulton",3,0.43,"PHEL"]
["Wood","Gm","Genesee loam","Genesee",5,0.37,"NHEL"]
["Wood","Gn","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Wood","Hd","Haney loam, 0 to 2 percent slopes","Haney",4,0.32,"NHEL"]
["Wood","HdB","Haney loam, 2 to 6 percent slopes","Haney",4,0.32,"PHEL"]
["Wood","Hn","Haney sandy loam, 0 to 2 percent slopes","Haney",4,0.28000000000000003,"NHEL"]
["Wood","HnB","Haney sandy loam, 2 to 6 percent slopes","Haney",4,0.28000000000000003,"PHEL"]
["Wood","Hs","Haskins and Digby loams, over clay, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Wood","HsB","Haskins and Digby loams, over clay, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Wood","Ht","Haskins and Digby fine sandy loams, over clay, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Wood","HtB","Haskins and Digby fine sandy loams, over clay, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Wood","Hv","Hoytville clay","Hoytville",5,0.28000000000000003,"NHEL"]
["Wood","Hw","Hoytville clay, thin solum variant","Hoytville",5,0.28000000000000003,"NHEL"]
["Wood","Hy","Hoytville clay loam","Hoytville",5,0.28000000000000003,"NHEL"]
["Wood","Jo","Joliet silty clay loam","Joliet",2,0.28000000000000003,"NHEL"]
["Wood","Kf","Kibbie fine sandy loam, 0 to 2 percent slopes","Kibbie",5,0.2,"NHEL"]
["Wood","KfB","Kibbie fine sandy loam, 2 to 6 percent slopes","Kibbie",5,0.2,"PHEL"]
["Wood","Ks","Kibbie loamy fine sand, 0 to 2 percent slopes","Kibbie",5,0.2,"NHEL"]
["Wood","Ma","Made land and borrow pits","Made"]
["Wood","Mb","Millgrove loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Wood","Mf","Mermill fine sandy loam","Mermill",5,0.28000000000000003,"NHEL"]
["Wood","Mg","Mermill sandy clay loam","Mermill",5,0.28000000000000003,"NHEL"]
["Wood","Mh","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Wood","Mm","Millsdale stony silty clay loam","Millsdale",4,0.32,"NHEL"]
["Wood","Mn","Milton loam, 0 to 2 percent slopes","Milton",4,0.37,"NHEL"]
["Wood","MnB","Milton loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Wood","Mu","Muck","Muck",2,null,"NHEL"]
["Wood","Na","Nappanee loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Wood","NaB","Nappanee loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Wood","NaB2","Nappanee loam, 2 to 6 percent slopes, moderately eroded","Nappanee",3,0.43,"PHEL"]
["Wood","Ns","Nappanee sandy loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Wood","NsB","Nappanee sandy loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Wood","Nt","Nappanee silty clay loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Wood","NtB","Nappanee silty clay loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Wood","NtB2","Nappanee silty clay loam, 2 to 6 percent slopes, moderately eroded","Nappanee",3,0.43,"PHEL"]
["Wood","Os","Ottokee and Spinks loamy fine sands, 0 to 2 percent slopes","Ottokee",5,0.17,"NHEL"]
["Wood","OsB","Ottokee and Spinks loamy fine sands, 2 to 6 percent slopes","Ottokee",5,0.17,"NHEL"]
["Wood","Qu","Quarries","Quarries"]
["Wood","Rb","Randolph loam, 0 to 2 percent slopes","Randolph",3,0.37,"NHEL"]
["Wood","RbB","Randolph loam, 2 to 6 percent slopes","Randolph",3,0.37,"PHEL"]
["Wood","Rd","Randolph stony loam, 0 to 2 percent slopes","Randolph",3,0.37,"NHEL"]
["Wood","Rf","Rimer and Tedrow loamy fine sands, over clay, 0 to 2 percent slopes","Rimer",4,0.17,"NHEL"]
["Wood","RfB","Rimer and Tedrow loamy fine sands, over clay, 2 to 6 percent slopes","Rimer",4,0.17,"NHEL"]
["Wood","Rh","Ritchey loam, 0 to 2 percent slopes","Ritchey",2,0.37,"NHEL"]
["Wood","RhB","Ritchey loam, 2 to 6 percent slopes","Ritchey",2,0.37,"PHEL"]
["Wood","Rk","Ritchey stony loam, 0 to 2 percent slopes","Ritchey",2,0.37,"NHEL"]
["Wood","Rs","Romeo soils, 0 to 2 percent slopes","Romeo",1,0.37,"PHEL"]
["Wood","RsB","Romeo soils, 2 to 4 percent slopes","Romeo",1,0.37,"PHEL"]
["Wood","SaB","St. Clair loam, 2 to 6 percent slopes","St. Clair",3,0.37,"PHEL"]
["Wood","SaC2","St. Clair loam, 6 to 12 percent slopes, moderately eroded","St. Clair",3,0.37,"PHEL"]
["Wood","SbB2","St. Clair silty clay loam, 2 to 6 percent slopes, moderately eroded","St. Clair",3,0.37,"PHEL"]
["Wood","SbC2","St. Clair silty clay loam, 6 to 12 percent slopes, moderately eroded","St. Clair",3,0.37,"PHEL"]
["Wood","SbD2","St. Clair silty clay loam, 12 to 18 percent slopes, moderately eroded","St. Clair",3,0.37,"HEL"]
["Wood","SbE2","St. Clair silty clay loam, 18 to 25 percent slopes, moderately eroded","St. Clair",3,0.37,"HEL"]
["Wood","Sf","Seward and Ottokee loamy fine sands, over clay, 0 to 2 percent slopes","Seward",4,0.17,"NHEL"]
["Wood","SfB","Seward and Ottokee loamy fine sands, over clay, 2 to 6 percent slopes","Seward",4,0.17,"NHEL"]
["Wood","Sg","Shoals loam","Shoals",5,0.37,"NHEL"]
["Wood","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Wood","Sk","Shoals silty clay loam","Shoals",5,0.37,"NHEL"]
["Wood","Sm","Shoals and Sloan soils, over limestone","Shoals",5,0.37,"NHEL"]
["Wood","Sn","Sloan silt loam","Sloan",5,0.37,"NHEL"]
["Wood","So","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Wood","SpB","Spinks fine sand, 2 to 6 percent slopes","Spinks",5,0.17,"NHEL"]
["Wood","SpC","Spinks fine sand, 6 to 12 percent slopes","Spinks",5,0.17,"PHEL"]
["Wood","SpD","Spinks fine sand, 12 to 18 percent slopes","Spinks",5,0.17,"PHEL"]
["Wood","SsB","Spinks loamy fine sand, 2 to 6 percent slopes","Spinks",5,0.17,"NHEL"]
["Wood","SsC","Spinks loamy fine sand, 6 to 12 percent slopes","Spinks",5,0.17,"PHEL"]
["Wood","Td","Tedrow loamy fine sand, 0 to 2 percent slopes","Tedrow",5,0.17,"NHEL"]
["Wood","TdB","Tedrow loamy fine sand, 2 to 6 percent slopes","Tedrow",5,0.17,"NHEL"]
["Wood","To","Toledo silty clay","Toledo",5,0.28000000000000003,"NHEL"]
["Wood","Tt","Toledo silty clay loam","Toledo",5,0.28000000000000003,"NHEL"]
["Wood","Ur","Urban land","Urban"]
["Wood","Wc","Warners soils, over clay","Warners",5,0.43,"NHEL"]
["Wood","Wf","Wauseon fine sandy loam","Wauseon",4,0.17,"NHEL"]
["Wood","Wm","Wauseon fine sandy loam, over clay","Wauseon",4,0.17,"NHEL"]
["Wood","Wn","Wauseon loamy fine sand","Wauseon",4,0.17,"NHEL"]
["Wood","Ws","Wauseon loamy fine sand, over clay","Wauseon",4,0.17,"NHEL"]
[null,"Select","none","none"]
["Wyandot","BeA","Belmore loam, 0 to 2 percent slopes","Belmore",4,0.32,"NHEL"]
["Wyandot","BeB","Belmore loam, 2 to 6 percent slopes","Belmore",4,0.32,"PHEL"]
["Wyandot","BgA","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Wyandot","BgB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Wyandot","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Wyandot","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Wyandot","Br","Bono silty clay","Bono",5,0.28000000000000003,"NHEL"]
["Wyandot","CdB2","Cardington silt loam, 2 to 6 percent slopes, eroded","Cardington",4,0.37,"PHEL"]
["Wyandot","CdC2","Cardington silt loam, 6 to 12 percent slopes, eroded","Cardington",4,0.37,"PHEL"]
["Wyandot","CdD2","Cardington silt loam, 12 to 18 percent slopes, eroded","Cardington",4,0.37,"HEL"]
["Wyandot","Ck","Carlisle muck","Carlisle",2,null,"NHEL"]
["Wyandot","Cm","Chagrin silt loam, rarely flooded","Chagrin",5,0.32,"PHEL"]
["Wyandot","Co","Colwood silt loam","Colwood",5,0.28000000000000003,"PHEL"]
["Wyandot","DeA","Del Rey silt loam, 0 to 2 percent slopes","Del Rey",3,0.43,"NHEL"]
["Wyandot","DeB","Del Rey silt loam, 2 to 6 percent slopes","Del Rey",3,0.43,"PHEL"]
["Wyandot","DgA","Digby loam, 0 to 3 percent slopes","Digby",4,0.32,"NHEL"]
["Wyandot","EtA","Elliott silt loam, 0 to 3 percent slopes","Elliott",4,0.28000000000000003,"NHEL"]
["Wyandot","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Wyandot","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Wyandot","FuA","Fulton silty clay loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Wyandot","Ge","Genesee silt loam, occasionally flooded","Genesee",5,0.37,"NHEL"]
["Wyandot","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Wyandot","GwB","Glynwood silt loam, 2 to 6 percent slopes","Glynwood",3,0.43,"PHEL"]
["Wyandot","GwB2","Glynwood silt loam, 2 to 6 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Wyandot","GwC2","Glynwood silt loam, 6 to 12 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Wyandot","HaA","Haney loam, 0 to 2 percent slopes","Haney",4,0.32,"NHEL"]
["Wyandot","HaB","Haney loam, 2 to 6 percent slopes","Haney",4,0.32,"PHEL"]
["Wyandot","HkA","Haskins loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Wyandot","HkB","Haskins loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Wyandot","KbA","Kibbie fine sandy loam, till substratum, 0 to 2 percent slopes","Kibbie",5,0.2,"NHEL"]
["Wyandot","KbB","Kibbie fine sandy loam, till substratum, 2 to 6 percent slopes","Kibbie",5,0.2,"PHEL"]
["Wyandot","KcA","Kibbie-Blount complex, 0 to 2 percent slopes","Kibbie",5,0.2,"NHEL"]
["Wyandot","KcB","Kibbie-Blount complex, 2 to 6 percent slopes","Kibbie",5,0.2,"PHEL"]
["Wyandot","Lb","Latty silty clay loam","Latty",5,0.28000000000000003,"NHEL"]
["Wyandot","Lc","Latty silty clay","Latty",5,0.28000000000000003,"NHEL"]
["Wyandot","Lk","Lindside silt loam, occasionally flooded","Lindside",5,0.28000000000000003,"NHEL"]
["Wyandot","Lu","Luray silty clay loam","Luray",5,0.32,"NHEL"]
["Wyandot","LyA","Lykens silt loam, 0 to 2 percent slopes","Lykens",4,0.37,"NHEL"]
["Wyandot","LyB","Lykens silt loam, 2 to 6 percent slopes","Lykens",4,0.37,"PHEL"]
["Wyandot","LzB","Lykens-Milton silt loams, 2 to 6 percent slopes","Lykens",4,0.37,"PHEL"]
["Wyandot","MaB","Martinsville fine sandy loam, 2 to 6 percent slopes","Martinsville",5,0.37,"PHEL"]
["Wyandot","Md","Medway silt loam, rarely flooded","Medway",5,0.32,"NHEL"]
["Wyandot","Mf","Mermill loam","Mermill",5,0.28000000000000003,"NHEL"]
["Wyandot","Mg","Mermill silty clay loam","Mermill",5,0.28000000000000003,"NHEL"]
["Wyandot","Mh","Milford silty clay loam","Milford",5,0.28000000000000003,"NHEL"]
["Wyandot","Mk","Millgrove silt loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Wyandot","Mm","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Wyandot","MoA","Milton silt loam, 0 to 2 percent slopes","Milton",4,0.37,"NHEL"]
["Wyandot","MoB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Wyandot","MrC2","Morley silt loam, 6 to 12 percent slopes, eroded","Morley",3,0.43,"PHEL"]
["Wyandot","MrD2","Morley silt loam, 12 to 18 percent slopes, eroded","Morley",3,0.43,"HEL"]
["Wyandot","MrF2","Morley silt loam, 18 to 50 percent slopes, eroded","Morley",3,0.43,"HEL"]
["Wyandot","NpB","Nappanee silt loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Wyandot","NtA","Nappanee silty clay loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Wyandot","NtB2","Nappanee silty clay loam, 2 to 6 percent slopes, eroded","Nappanee",3,0.43,"PHEL"]
["Wyandot","NtC2","Nappanee silty clay loam, 6 to 12 percent slopes, eroded","Nappanee",3,0.43,"PHEL"]
["Wyandot","On","Olentangy mucky silt loam","Olentangy",5,0.28000000000000003,"NHEL"]
["Wyandot","OsB","Oshtemo fine sandy loam, 1 to 6 percent slopes","Oshtemo",5,0.24,"NHEL"]
["Wyandot","OsC2","Oshtemo fine sandy loam, 6 to 18 percent slopes, eroded","Oshtemo",5,0.24,"PHEL"]
["Wyandot","OsE","Oshtemo fine sandy loam, 18 to 35 percent slopes","Oshtemo",5,0.24,"HEL"]
["Wyandot","Pa","Pandora silty clay loam","Pandora",5,0.37,"NHEL"]
["Wyandot","Pd","Paulding clay","Pauldig",5,0.28000000000000003,"NHEL"]
["Wyandot","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Wyandot","Ps","Pits, gravel","Pits"]
["Wyandot","Pu","Pits, quarry","Pits"]
["Wyandot","RaA","Randolph silt loam, 0 to 3 percent slopes","Randolph",3,0.37,"NHEL"]
["Wyandot","RhB","Ritchey silt loam, 1 to 6 percent slopes","Ritchey",2,0.37,"PHEL"]
["Wyandot","RhC","Ritchey silt loam, 6 to 12 percent slopes","Ritchey",2,0.37,"HEL"]
["Wyandot","SeB2","Shinrock silt loam, 2 to 6 percent slopes, eroded","Shinrock",3,0.37,"PHEL"]
["Wyandot","SeC2","Shinrock silt loam, 6 to 12 percent slopes, eroded","Shinrock",3,0.37,"PHEL"]
["Wyandot","SfC2","Shinrock-Martinsville complex, 6 to 12 percent slopes, eroded","Shinrock",3,0.37,"PHEL"]
["Wyandot","SfD2","Shinrock-Martinsville complex, 12 to 18 percent slopes, eroded","Shinrock",3,0.37,"HEL"]
["Wyandot","Sg","Shoals silt loam, rarely flooded","Shoals",5,0.37,"NHEL"]
["Wyandot","Sh","Shoals silt loam, occasionally flooded","Shoals",5,0.37,"NHEL"]
["Wyandot","So","Sloan silt loam, occasionally flooded","Sloan",5,0.37,"NHEL"]
["Wyandot","TrA","Tiro silt loam, 0 to 2 percent slopes","Tiro",4,0.37,"NHEL"]
["Wyandot","TrB","Tiro silt loam, 2 to 6 percent slopes","Tiro",4,0.37,"PHEL"]
["Wyandot","TuB","Tuscola fine sandy loam, 2 to 6 percent slopes","Tuscola",5,0.24,"NHEL"]
["Wyandot","Ud","Udorthents, loamy","Udorthents"]
["Wyandot","Ur","Urban land-Udorthents complex","Urban"]
["Wyandot","W","Water","Water"]

{"sheet":"Area 2","index":3,"n_rows":1896,"n_cols":7,"rows_kept":1896,"cut":false,"hidden":false,"merged":[]}
["County","symbol","map unit name","Component","T","Kw","HEL"]
[null,"Select","none","none"]
["Ashland","AdD2","Alexandria silt loam, 12 to 18 percent slopes, eroded","Alexandria",4,0.37,"HEL"]
["Ashland","AdE","Alexandria silt loam, 18 to 25 percent slopes","Alexandria",4,0.37,"HEL"]
["Ashland","AdF","Alexandria silt loam, 25 to 50 percent slopes","Alexandria",4,0.37,"HEL"]
["Ashland","Ag","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Ashland","BnA","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Ashland","BnB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Ashland","BrD","Berks channery silt loam, 12 to 18 percent slopes","Berks",3,0.24,"PHEL"]
["Ashland","BsG","Berks-Rock outcrop complex, 30 to 60 percent slopes","Berks",3,0.24,"HEL"]
["Ashland","BtA","Bogart gravelly loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Ashland","BtB","Bogart gravelly loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Ashland","BvA","Bogart silt loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Ashland","BvB","Bogart silt loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Ashland","CaB","Canfield silt loam, 2 to 6 percent slopes","Canfield",4,0.37,"PHEL"]
["Ashland","CaC","Canfield silt loam, 6 to 12 percent slopes","Canfield",4,0.37,"PHEL"]
["Ashland","CaC2","Canfield silt loam, 6 to 12 percent slopes, eroded","Canfield",4,0.37,"PHEL"]
["Ashland","CdB","Cardington silt loam, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Ashland","CdB2","Cardington silt loam, 2 to 6 percent slopes, eroded","Cardington",4,0.37,"PHEL"]
["Ashland","CdC","Cardington silt loam, 6 to 12 percent slopes","Cardington",4,0.37,"PHEL"]
["Ashland","CdC2","Cardington silt loam, 6 to 12 percent slopes, eroded","Cardington",4,0.37,"PHEL"]
["Ashland","CeC3","Cardington silty clay loam, 6 to 12 percent slopes, severely eroded","Cardington",4,0.37,"PHEL"]
["Ashland","Cf","Carlisle muck","Carlisle",2,null,"NHEL"]
["Ashland","CgB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Ashland","CgC","Chili loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Ashland","ChC","Chili-Wooster complex, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Ashland","ChD","Chili-Wooster complex, 12 to 18 percent slopes","Chili",4,0.32,"HEL"]
["Ashland","ChE","Chili-Wooster complex, 18 to 25 percent slopes","Chili",4,0.32,"HEL"]
["Ashland","CkD","Chili and Conotton gravelly loams, 12 to 18 percent slopes","Chili",4,0.24,"HEL"]
["Ashland","CkE","Chili and Conotton gravelly loams, 18 to 35 percent slopes","Chili",4,0.24,"HEL"]
["Ashland","Cr","Condit silt loam","Condit",5,0.37,"NHEL"]
["Ashland","CtD","Conotton Variant gravelly loam, 10 to 20 percent slopes","Conotton",3,0.28000000000000003,"HEL"]
["Ashland","CvB","Coshocton loam, 2 to 6 percent slopes","Coshocton",4,0.37,"PHEL"]
["Ashland","CvC","Coshocton loam, 6 to 15 percent slopes","Coshocton",4,0.37,"PHEL"]
["Ashland","ElB2","Ellsworth silt loam, 2 to 6 percent slopes, eroded","Ellsworth",3,0.43,"PHEL"]
["Ashland","ElC2","Ellsworth silt loam, 6 to 12 percent slopes, eroded","Ellsworth",3,0.43,"PHEL"]
["Ashland","ElE2","Ellsworth silt loam, 12 to 25 percent slopes, eroded","Ellsworth",3,0.43,"HEL"]
["Ashland","FcA","Fitchville silt loam, 1 to 4 percent slopes","Fitchville",5,0.37,"NHEL"]
["Ashland","GfA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Ashland","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Ashland","GfC","Glenford silt loam, 6 to 12 percent slopes","Glenford",5,0.37,"PHEL"]
["Ashland","Ho","Holly silt loam","Holly",5,0.28000000000000003,"NHEL"]
["Ashland","JwA","Jimtown silt loam, 0 to 2 percent slopes","Jimtown",4,0.32,"NHEL"]
["Ashland","JwB","Jimtown silt loam, 2 to 6 percent slopes","Jimtown",4,0.32,"PHEL"]
["Ashland","Kb","Killbuck silt loam","Killbuck",5,0.37,"NHEL"]
["Ashland","Ln","Linwood muck","Linwood",2,null,"NHEL"]
["Ashland","Lo","Lobdell silt loam","Lobdell",5,0.37,"NHEL"]
["Ashland","LtB","Lordstown silt loam, 2 to 6 percent slopes","Lordstown",3,0.28000000000000003,"PHEL"]
["Ashland","LtC","Lordstown silt loam, 6 to 12 percent slopes","Lordstown",3,0.28000000000000003,"PHEL"]
["Ashland","LtD","Lordstown silt loam, 12 to 18 percent slopes","Lordstown",3,0.28000000000000003,"HEL"]
["Ashland","LtE","Lordstown silt loam, 18 to 25 percent slopes","Lordstown",3,0.28000000000000003,"HEL"]
["Ashland","LtF","Lordstown silt loam, 25 to 40 percent slopes","Lordstown",3,0.28000000000000003,"HEL"]
["Ashland","LvB","Loudonville silt loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Ashland","LvC","Loudonville silt loam, 6 to 12 percent slopes","Loudonville",4,0.32,"PHEL"]
["Ashland","LvD","Loudonville silt loam, 12 to 18 percent slopes","Loudonville",4,0.32,"HEL"]
["Ashland","LvE","Loudonville silt loam, 18 to 25 percent slopes","Loudonville",4,0.32,"HEL"]
["Ashland","Ly","Luray silty clay loam","Luray",5,0.32,"NHEL"]
["Ashland","LzB","Lykens silt loam, 2 to 6 percent slopes","Lykens",4,0.37,"PHEL"]
["Ashland","MaA","Mahoning silt loam, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Ashland","MaB","Mahoning silt loam, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Ashland","MaB2","Mahoning silt loam, 2 to 6 percent slopes, eroded","Mahoning",3,0.43,"PHEL"]
["Ashland","Os","Orrville Variant silt loam","Orrville",4,0.32,"NHEL"]
["Ashland","OtB","Oshtemo sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Ashland","OtC","Oshtemo sandy loam, 6 to 12 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Ashland","Pc","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Ashland","Pg","Pits, gravel","Pits"]
["Ashland","RnA","Ravenna silt loam, 0 to 2 percent slopes","Ravenna",3,0.37,"NHEL"]
["Ashland","RnB","Ravenna silt loam, 2 to 6 percent slopes","Ravenna",3,0.37,"PHEL"]
["Ashland","RrC","Rigley sandy loam, 6 to 12 percent slopes","Rigley",4,0.24,"PHEL"]
["Ashland","RsB","Rittman silt loam, 2 to 6 percent slopes","Rittman",4,0.43,"PHEL"]
["Ashland","RsB2","Rittman silt loam, 2 to 6 percent slopes, eroded","Rittman",4,0.43,"PHEL"]
["Ashland","RsC","Rittman silt loam, 6 to 12 percent slopes","Rittman",4,0.43,"PHEL"]
["Ashland","RsC2","Rittman silt loam, 6 to 12 percent slopes, eroded","Rittman",4,0.43,"PHEL"]
["Ashland","RsD2","Rittman silt loam, 12 to 18 percent slopes, eroded","Rittman",4,0.43,"HEL"]
["Ashland","ScE","Schaffenaker loamy sand, 10 to 40 percent slopes","Schaffenaker",3,0.17,"PHEL"]
["Ashland","Sg","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Ashland","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Ashland","Sn","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Ashland","ToA","Tiro silt loam, 1 to 4 percent slopes","Tiro",4,0.37,"PHEL"]
["Ashland","Ud","Udorthents","Udorthents"]
["Ashland","Ur","Urban land","Urban"]
["Ashland","W","Water","Water"]
["Ashland","WaA","Wadsworth silt loam, 0 to 2 percent slopes","Wadsworth",4,0.43,"NHEL"]
["Ashland","WaB","Wadsworth silt loam, 2 to 6 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Ashland","Wb","Wallkill silt loam","Wallkill",5,0.32,"NHEL"]
["Ashland","WhA","Wheeling silt loam, 0 to 2 percent slopes","Wheeling",4,0.37,"NHEL"]
["Ashland","WhB","Wheeling silt loam, 2 to 6 percent slopes","Wheeling",4,0.37,"PHEL"]
["Ashland","WhC","Wheeling silt loam, 6 to 12 percent slopes","Wheeling",4,0.37,"PHEL"]
["Ashland","WsB","Wooster silt loam, 2 to 6 percent slopes","Wooster",4,0.37,"PHEL"]
["Ashland","WsC","Wooster silt loam, 6 to 12 percent slopes","Wooster",4,0.37,"PHEL"]
["Ashland","WsD2","Wooster silt loam, 12 to 18 percent slopes, eroded","Wooster",4,0.37,"HEL"]
["Ashland","WsE","Wooster silt loam, 18 to 35 percent slopes","Wooster",4,0.37,"HEL"]
[null,"Select","none","none"]
["Ashtabula","As","Allis silt loam","Allis",3,0.43,"NHEL"]
["Ashtabula","At","Atherton silt loam","Atherton",5,0.37,"NHEL"]
["Ashtabula","Be","Beaches","Beaches"]
["Ashtabula","BrA","Braceville loam, 0 to 2 percent slopes","Braceville",3,0.24,"NHEL"]
["Ashtabula","BrB","Braceville loam, 2 to 6 percent slopes","Braceville",3,0.24,"PHEL"]
["Ashtabula","BrC2","Braceville loam, 6 to 12 percent slopes, moderately eroded","Braceville",3,0.24,"PHEL"]
["Ashtabula","CaB","Cambridge silt loam, 2 to 6 percent slopes","Cambridge",4,0.43,"PHEL"]
["Ashtabula","CaB2","Cambridge silt loam, 2 to 6 percent slopes, moderately eroded","Cambridge",4,0.43,"PHEL"]
["Ashtabula","CaC","Cambridge silt loam, 6 to 12 percent slopes","Cambridge",4,0.43,"PHEL"]
["Ashtabula","CaC2","Cambridge silt loam, 6 to 12 percent slopes, moderately eroded","Cambridge",4,0.43,"PHEL"]
["Ashtabula","CaD2","Cambridge silt loam, 12 to 18 percent slopes, moderately eroded","Cambridge",4,0.43,"HEL"]
["Ashtabula","CbB","Cambridge silt loam, sandstone substratum, 2 to 6 percent slopes","Cambridge",4,0.43,"PHEL"]
["Ashtabula","CbC2","Cambridge silt loam, sandstone substratum, 6 to 12 percent slopes, moderately eroded","Cambridge",4,0.43,"PHEL"]
["Ashtabula","Cc","Canadice silt loam","Canadice",5,0.49,"NHEL"]
["Ashtabula","Cd","Canadice soils, mucky variant","Canadice",5,null,"NHEL"]
["Ashtabula","CeA","Canadice-Caneadea silt loams, 0 to 2 percent slopes","Canadice",5,0.49,"NHEL"]
["Ashtabula","CfA","Caneadea silt loam, 0 to 2 percent slopes","Caneadea",3,0.43,"NHEL"]
["Ashtabula","CfB","Caneadea silt loam, 2 to 6 percent slopes","Caneadea",3,0.43,"PHEL"]
["Ashtabula","CfC2","Caneadea silt loam, 6 to 12 percent slopes, moderately eroded","Caneadea",3,0.43,"PHEL"]
["Ashtabula","CfD2","Caneadea silt loam, 12 to 18 percent slopes, moderately eroded","Caneadea",3,0.43,"HEL"]
["Ashtabula","Cg","Carlisle muck","Carlisle",2,null,"NHEL"]
["Ashtabula","Ch","Chagrin silt loam","Chagrin",5,0.32,"NHEL"]
["Ashtabula","CkA","Chenango silt loam, 0 to 2 percent slopes","Chenago",3,0.32,"NHEL"]
["Ashtabula","CkB","Chenango silt loam, 2 to 6 percent slopes","Chenago",3,0.32,"PHEL"]
["Ashtabula","CkC2","Chenango silt loam, 6 to 12 percent slopes, moderately eroded","Chenago",3,0.32,"PHEL"]
["Ashtabula","CkD2","Chenango silt loam, 12 to 18 percent slopes, moderately eroded","Chenago",3,0.32,"HEL"]
["Ashtabula","ClA","Chenango gravelly loam, 0 to 2 percent slopes","Chenago",3,0.24,"NHEL"]
["Ashtabula","ClB","Chenango gravelly loam, 2 to 6 percent slopes","Chenago",3,0.24,"PHEL"]
["Ashtabula","ClC2","Chenango gravelly loam, 6 to 12 percent slopes, moderately eroded","Chenago",3,0.24,"PHEL"]
["Ashtabula","CmA","Claverack loamy fine sand, silty subsoil variant, 0 to 2 percent slopes","Claverack",5,0.28000000000000003,"NHEL"]
["Ashtabula","CmB","Claverack loamy fine sand, silty subsoil variant, 2 to 6 percent slopes","Claverack",5,0.28000000000000003,"PHEL"]
["Ashtabula","CmC","Claverack loamy fine sand, silty subsoil variant, 6 to 12 percent slopes","Claverack",5,0.28000000000000003,"PHEL"]
["Ashtabula","CnB","Claverack loamy fine sand, moderately shallow variant, 2 to 6 percent slopes","Claverack",5,0.28000000000000003,"NHEL"]
["Ashtabula","CoB","Colonie loamy fine sand, 2 to 6 percent slopes","Colonie",4,0.17,"NHEL"]
["Ashtabula","CoD","Colonie loamy fine sand, 6 to 18 percent slopes","Colonie",4,0.17,"PHEL"]
["Ashtabula","Ct","Conneaut silt loam","Conneaut",4,0.37,"NHEL"]
["Ashtabula","ElB","Elnora loamy fine sand, 1 to 5 percent slopes","Elnora",4,0.17,"NHEL"]
["Ashtabula","Fr","Frenchtown silt loam","Frenchtown",3,0.37,"NHEL"]
["Ashtabula","Fs","Frenchtown silt loam, sandstone substratum","Frenchtown",3,0.37,"NHEL"]
["Ashtabula","Gp","Gravel and sand pits","Gravel"]
["Ashtabula","Hm","Holly silt loam","Holly",5,0.28000000000000003,"NHEL"]
["Ashtabula","HoB","Hornell silt loam, 2 to 6 percent slopes","Hornell",3,0.43,"PHEL"]
["Ashtabula","HoC2","Hornell silt loam, 6 to 12 percent slopes, moderately eroded","Hornell",3,0.43,"PHEL"]
["Ashtabula","HoD2","Hornell silt loam, 12 to 18 percent slopes, moderately eroded","Hornell",3,0.43,"HEL"]
["Ashtabula","Io","Ilion silt loam","Ilion",3,0.37,"NHEL"]
["Ashtabula","Kf","Kingsville fine sandy loam","Kingsville",5,0.24,"NHEL"]
["Ashtabula","Kg","Kingsville silty clay","Kingsville",5,0.28000000000000003,"NHEL"]
["Ashtabula","Lb","Lobdell silt loam","Lobdell",5,0.37,"NHEL"]
["Ashtabula","Ma","Made land","Made"]
["Ashtabula","MsB","Mahoning silt loam, shale substratum, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Ashtabula","MsB2","Mahoning silt loam, shale substratum, 2 to 6 percent slopes, moderately eroded","Mahoning",3,0.43,"PHEL"]
["Ashtabula","Or","Orrville fine sandy loam","Orrville",5,0.37,"NHEL"]
["Ashtabula","Os","Orrville silt loam","Orrville",5,0.37,"NHEL"]
["Ashtabula","OtB","Otisville sandy loam, 1 to 6 percent slopes","Otisville",3,0.17,"PHEL"]
["Ashtabula","OuB","Otisville gravelly sandy loam, 1 to 6 percent slopes","Otisville",3,0.17,"PHEL"]
["Ashtabula","OuC","Otisville gravelly sandy loam, 6 to 12 percent slopes","Otisville",3,0.17,"PHEL"]
["Ashtabula","OvE","Otisville and Chenango soils, 12 to 25 percent slopes","Otisville",3,0.17,"PHEL"]
["Ashtabula","OvE","Otisville and Chenango soils, 12 to 25 percent slopes","Otisville",3,0.24,"PHEL"]
["Ashtabula","PeB","Pierpont silt loam, 2 to 6 percent slopes","Pierpont",4,0.43,"PHEL"]
["Ashtabula","PeB2","Pierpont silt loam, 2 to 6 percent slopes, moderately eroded","Pierpont",4,0.43,"PHEL"]
["Ashtabula","PeC2","Pierpont silt loam, 6 to 12 percent slopes, moderately eroded","Pierpont",4,0.43,"PHEL"]
["Ashtabula","PoD2","Pierpont and Platea soils, 12 to 18 percent slopes, moderately eroded","Pierpont",4,0.43,"HEL"]
["Ashtabula","PsA","Platea silt loam, 0 to 2 percent slopes","Platea",3,0.43,"NHEL"]
["Ashtabula","PsB","Platea silt loam, 2 to 6 percent slopes","Platea",3,0.43,"PHEL"]
["Ashtabula","PsB2","Platea silt loam, 2 to 6 percent slopes, moderately eroded","Platea",3,0.43,"PHEL"]
["Ashtabula","PsC","Platea silt loam, 6 to 12 percent slopes","Platea",3,0.43,"PHEL"]
["Ashtabula","PsC2","Platea silt loam, 6 to 12 percent slopes, moderately eroded","Platea",3,0.43,"PHEL"]
["Ashtabula","PsC3","Platea silt loam, 6 to 12 percent slopes, severely eroded","Platea",2,0.43,"HEL"]
["Ashtabula","Qu","Quarries","Quarries"]
["Ashtabula","RhB","Red Hook silt loam, 0 to 4 percent slopes","Red Hook",3,0.32,"PHEL"]
["Ashtabula","Rw","Riverwash","Riverwash"]
["Ashtabula","Sf","Sheffield silt loam","Sheffield",4,0.37,"NHEL"]
["Ashtabula","Sh","Sheffield silt loam, stratified substratum","Sheffield",4,0.37,"NHEL"]
["Ashtabula","Sm","Steep land, loamy","Steep"]
["Ashtabula","Sn","Steep land, silty and clayey","Steep"]
["Ashtabula","Sw","Swanton fine sandy loam, silty subsoil variant","Swanton",4,0.28000000000000003,"NHEL"]
["Ashtabula","VeA","Venango silt loam, 0 to 2 percent slopes","Venango",4,0.37,"NHEL"]
["Ashtabula","VeB","Venango silt loam, 2 to 6 percent slopes","Venango",4,0.37,"PHEL"]
["Ashtabula","VeB2","Venango silt loam, 2 to 6 percent slopes, moderately eroded","Venango",4,0.37,"PHEL"]
["Ashtabula","VeC","Venango silt loam, 6 to 12 percent slopes","Venango",4,0.37,"PHEL"]
["Ashtabula","VeC2","Venango silt loam, 6 to 12 percent slopes, moderately eroded","Venango",4,0.37,"PHEL"]
["Ashtabula","VgA","Venango silt loam, sandstone substratum, 0 to 2 percent slopes","Venango",4,0.37,"NHEL"]
["Ashtabula","VgB","Venango silt loam, sandstone substratum, 2 to 6 percent slopes","Venango",4,0.37,"PHEL"]
["Ashtabula","WaA","Wallington silt loam, 0 to 2 percent slopes","Wallington",3,0.49,"NHEL"]
["Ashtabula","WaB","Wallington silt loam, 2 to 6 percent slopes","Wallington",3,0.49,"PHEL"]
["Ashtabula","We","Willette muck","Willette",2,null,"NHEL"]
["Ashtabula","WlA","Williamson silt loam, 0 to 2 percent slopes","Williamson",3,0.49,"NHEL"]
["Ashtabula","WlB","Williamson silt loam, 2 to 6 percent slopes","Williamson",3,0.49,"PHEL"]
["Ashtabula","WlC2","Williamson silt loam, 6 to 12 percent slopes, moderately eroded","Williamson",3,0.49,"PHEL"]
["Ashtabula","WlD2","Williamson silt loam, 12 to 18 percent slopes, moderately eroded","Williamson",3,0.49,"HEL"]
[null,"Select","none","none"]
["Columbiana","AhC","Allegheny silt loam, 5 to 10 percent slopes","Allegheny",4,0.32,"PHEL"]
["Columbiana","AhC2","Allegheny silt loam, 5 to 10 percent slopes, moderately eroded","Allegheny",4,0.32,"PHEL"]
["Columbiana","AhD","Allegheny silt loam, 10 to 15 percent slopes","Allegheny",4,0.32,"HEL"]
["Columbiana","AhD2","Allegheny silt loam, 10 to 15 percent slopes, moderately eroded","Allegheny",4,0.32,"HEL"]
["Columbiana","AlC","Allegheny silt loam, sandstone substratum, 5 to 10 percent slopes","Allegheny",4,0.32,"PHEL"]
["Columbiana","AmB","Allegheny and Monongahela silt loams, 2 to 5 percent slopes","Allegheny",4,0.32,"PHEL"]
["Columbiana","AmB2","Allegheny and Monongahela silt loams, 2 to 5 percent slopes, moderately eroded","Allegheny",4,0.32,"PHEL"]
["Columbiana","BgA","Bogart loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Columbiana","BgB","Bogart loam, 2 to 5 percent slopes","Bogart",5,0.32,"PHEL"]
["Columbiana","BoA","Bogart silt loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Columbiana","BoB","Bogart silt loam, 2 to 5 percent slopes","Bogart",5,0.32,"PHEL"]
["Columbiana","BsC","Bogart soils, 5 to 10 percent slopes","Bogart",5,0.32,"PHEL"]
["Columbiana","BsC2","Bogart soils, 5 to 10 percent slopes, moderately eroded","Bogart",5,0.32,"PHEL"]
["Columbiana","CaB","Canfield silt loam, 2 to 5 percent slopes","Canfield",4,0.37,"PHEL"]
["Columbiana","CaB2","Canfield silt loam, 2 to 5 percent slopes, moderately eroded","Canfield",4,0.37,"PHEL"]
["Columbiana","CaC","Canfield silt loam, 5 to 10 percent slopes","Canfield",4,0.37,"PHEL"]
["Columbiana","CaC2","Canfield silt loam, 5 to 10 percent slopes, moderately eroded","Canfield",4,0.37,"PHEL"]
["Columbiana","Cc","Carlisle muck","Carlisle",2,null,"NHEL"]
["Columbiana","CdB","Cavode silt loam, 2 to 5 percent slopes","Cavode",3,0.37,"PHEL"]
["Columbiana","CdC","Cavode silt loam, 5 to 10 percent slopes","Cavode",3,0.37,"PHEL"]
["Columbiana","CdC2","Cavode silt loam, 5 to 10 percent slopes, moderately eroded","Cavode",3,0.37,"PHEL"]
["Columbiana","Ce","Chagrin loam","Chagrin",5,0.32,"NHEL"]
["Columbiana","Cg","Chagrin silt loam","Chagrin",5,0.32,"NHEL"]
["Columbiana","ChB","Chili gravelly loam, 2 to 5 percent slopes","Chili",4,0.24,"PHEL"]
["Columbiana","ChC2","Chili gravelly loam, 5 to 10 percent slopes, moderately eroded","Chili",4,0.24,"PHEL"]
["Columbiana","ChD2","Chili gravelly loam, 10 to 15 percent slopes, moderately eroded","Chili",4,0.24,"PHEL"]
["Columbiana","ClA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Columbiana","ClB","Chili loam, 2 to 5 percent slopes","Chili",4,0.32,"PHEL"]
["Columbiana","ClB2","Chili loam, 2 to 5 percent slopes, moderately eroded","Chili",4,0.32,"PHEL"]
["Columbiana","ClC","Chili loam, 5 to 10 percent slopes","Chili",4,0.32,"PHEL"]
["Columbiana","ClC2","Chili loam, 5 to 10 percent slopes, moderately eroded","Chili",4,0.32,"PHEL"]
["Columbiana","ClD","Chili loam, 10 to 15 percent slopes","Chili",4,0.32,"HEL"]
["Columbiana","ClD2","Chili loam, 10 to 15 percent slopes, moderately eroded","Chili",4,0.32,"HEL"]
["Columbiana","ClE2","Chili loam, 15 to 20 percent slopes, moderately eroded","Chili",4,0.32,"HEL"]
["Columbiana","CmC3","Chili soils, 5 to 10 percent slopes, severely eroded","Chili",3,0.32,"PHEL"]
["Columbiana","CmD3","Chili soils, 10 to 15 percent slopes, severely eroded","Chili",3,0.32,"HEL"]
["Columbiana","CmE3","Chili soils, 15 to 20 percent slopes, severely eroded","Chili",3,0.32,"HEL"]
["Columbiana","CnF","Chili, Conotton, and Negley soils, 20 to 50 percent slopes","Chili",4,0.32,"HEL"]
["Columbiana","CnF3","Chili, Conotton, and Negley soils, 20 to 50 percent slopes, severely eroded","Chili",3,0.32,"HEL"]
["Columbiana","Co","Chilo silty clay loam","Chilo",5,0.28000000000000003,"NHEL"]
["Columbiana","Da","Damascus silt loam","Damascus",5,0.32,"NHEL"]
["Columbiana","DeB","Dekalb loam, 2 to 5 percent slopes","Dekalb",2,0.24,"PHEL"]
["Columbiana","DeC","Dekalb loam, 5 to 10 percent slopes","Dekalb",2,0.24,"PHEL"]
["Columbiana","DeC2","Dekalb loam, 5 to 10 percent slopes, moderately eroded","Dekalb",2,0.24,"PHEL"]
["Columbiana","DeD2","Dekalb loam, 10 to 15 percent slopes, moderately eroded","Dekalb",2,0.24,"HEL"]
["Columbiana","DeE2","Dekalb loam, 15 to 20 percent slopes, moderately eroded","Dekalb",2,0.24,"HEL"]
["Columbiana","DeF","Dekalb loam, 20 to 35 percent slopes","Dekalb",2,0.24,"HEL"]
["Columbiana","DeF2","Dekalb loam, 20 to 35 percent slopes, moderately eroded","Dekalb",2,0.24,"HEL"]
["Columbiana","DkF3","Dekalb soils, 20 to 35 percent slopes, severely eroded","Dekalb",2,0.24,"HEL"]
["Columbiana","DsD","Dekalb stony loam, 5 to 20 percent slopes","Dekalb",2,0.24,"PHEL"]
["Columbiana","DsF","Dekalb stony loam, 20 to 50 percent slopes","Dekalb",2,0.24,"HEL"]
["Columbiana","ErC","Ernest silt loam, 5 to 10 percent slopes","Ernest",3,0.43,"PHEL"]
["Columbiana","ErD2","Ernest silt loam, 10 to 15 percent slopes, moderately eroded","Ernest",3,0.43,"HEL"]
["Columbiana","ErE2","Ernest silt loam, 15 to 20 percent slopes, moderately eroded","Ernest",3,0.43,"HEL"]
["Columbiana","ErF2","Ernest silt loam, 20 to 35 percent slopes, moderately eroded","Ernest",3,0.43,"HEL"]
["Columbiana","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Columbiana","FcB","Fitchville silt loam, 2 to 5 percent slopes","Fitchville",5,0.37,"PHEL"]
["Columbiana","Fr","Frenchtown silt loam","Frenchtown",3,0.37,"NHEL"]
["Columbiana","GfB","Glenford silt loam, 2 to 5 percent slopes","Glenford",5,0.37,"PHEL"]
["Columbiana","GfC","Glenford silt loam, 5 to 10 percent slopes","Glenford",5,0.37,"PHEL"]
["Columbiana","GfC2","Glenford silt loam, 5 to 10 percent slopes, moderately eroded","Glenford",5,0.37,"PHEL"]
["Columbiana","Gp","Gravel pits","Gravel"]
["Columbiana","GrB","Gresham silt loam, 2 to 5 percent slopes","Gresham",4,0.37,"PHEL"]
["Columbiana","GrC","Gresham silt loam, 5 to 10 percent slopes","Gresham",4,0.37,"PHEL"]
["Columbiana","GuB","Guernsey silt loam, 2 to 5 percent slopes","Guernsey",3,0.43,"PHEL"]
["Columbiana","GuC","Guernsey silt loam, 5 to 10 percent slopes","Guernsey",3,0.43,"PHEL"]
["Columbiana","GuC2","Guernsey silt loam, 5 to 10 percent slopes, moderately eroded","Guernsey",3,0.43,"PHEL"]
["Columbiana","GuD2","Guernsey silt loam, 10 to 15 percent slopes, moderately eroded","Guernsey",3,0.43,"HEL"]
["Columbiana","GvD2","Guernsey silty clay loam, thin solum variant, 10 to 15 percent slopes, moderately eroded","Guernsey",3,0.43,"HEL"]
["Columbiana","GvE2","Guernsey silty clay loam, thin solum variant, 15 to 20 percent slopes, moderately eroded","Guernsey",3,0.43,"HEL"]
["Columbiana","HaB","Hanover silt loam, 2 to 5 percent slopes","Hanover",5,0.37,"PHEL"]
["Columbiana","HaB2","Hanover silt loam, 2 to 5 percent slopes, moderately eroded","Hanover",5,0.37,"PHEL"]
["Columbiana","HaC","Hanover silt loam, 5 to 10 percent slopes","Hanover",5,0.37,"PHEL"]
["Columbiana","HaC2","Hanover silt loam, 5 to 10 percent slopes, moderately eroded","Hanover",5,0.37,"PHEL"]
["Columbiana","HaD2","Hanover silt loam, 10 to 15 percent slopes, moderately eroded","Hanover",5,0.37,"PHEL"]
["Columbiana","HaE2","Hanover silt loam, 15 to 20 percent slopes, moderately eroded","Hanover",5,0.37,"HEL"]
["Columbiana","JtA","Jimtown loam, 0 to 2 percent slopes","Jimtown",4,0.32,"NHEL"]
["Columbiana","JtB","Jimtown loam, 2 to 5 percent slopes","Jimtown",4,0.32,"PHEL"]
["Columbiana","JwA","Jimtown silt loam, 0 to 2 percent slopes","Jimtown",4,0.32,"NHEL"]
["Columbiana","JwB","Jimtown silt loam, 2 to 5 percent slopes","Jimtown",4,0.32,"PHEL"]
["Columbiana","Km","Kerston muck","Kerston",2,null,"NHEL"]
["Columbiana","LaC","Laidig stony loam, 5 to 10 percent slopes","Laidig",4,0.28000000000000003,"PHEL"]
["Columbiana","LaD","Laidig stony loam, 10 to 15 percent slopes","Laidig",4,0.28000000000000003,"PHEL"]
["Columbiana","LaE","Laidig stony loam, 15 to 20 percent slopes","Laidig",4,0.28000000000000003,"HEL"]
["Columbiana","LaF","Laidig stony loam, 20 to 35 percent slopes","Laidig",4,0.28000000000000003,"HEL"]
["Columbiana","Lb","Lobdell loam","Lobdell",5,0.37,"NHEL"]
["Columbiana","Ld","Lobdell silt loam","Lobdell",5,0.37,"NHEL"]
["Columbiana","Ln","Lorain clay","Lorain",5,0.32,"NHEL"]
["Columbiana","LoB","Loudonville silt loam, 2 to 5 percent slopes","Loudonville",4,0.32,"PHEL"]
["Columbiana","LoB2","Loudonville silt loam, 2 to 5 percent slopes, moderately eroded","Loudonville",4,0.32,"PHEL"]
["Columbiana","LoC","Loudonville silt loam, 5 to 10 percent slopes","Loudonville",4,0.32,"PHEL"]
["Columbiana","LoC2","Loudonville silt loam, 5 to 10 percent slopes, moderately eroded","Loudonville",4,0.32,"PHEL"]
["Columbiana","LoD2","Loudonville silt loam, 10 to 15 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Columbiana","LoE2","Loudonville silt loam, 15 to 20 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Columbiana","LuB","Loudonville and Muskingum soils, 2 to 5 percent slopes","Loudonville",4,0.32,"PHEL"]
["Columbiana","LuB2","Loudonville and Muskingum soils, 2 to 5 percent slopes, moderately eroded","Loudonville",4,0.32,"PHEL"]
["Columbiana","LuC2","Loudonville and Muskingum soils, 5 to 10 percent slopes, moderately eroded","Loudonville",4,0.32,"PHEL"]
["Columbiana","LuC3","Loudonville and Muskingum soils, 5 to 15 percent slopes, severely eroded","Loudonville",4,0.32,"PHEL"]
["Columbiana","LuD2","Loudonville and Muskingum soils, 10 to 15 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Columbiana","LuE","Loudonville and Muskingum soils, 15 to 20 percent slopes","Loudonville",4,0.32,"HEL"]
["Columbiana","LuE3","Loudonville and Muskingum soils, 15 to 20 percent slopes, severely eroded","Loudonville",4,0.32,"HEL"]
["Columbiana","Lv","Luray and Marengo silty clay loams","Luray",5,0.32,"NHEL"]
["Columbiana","Lw","Luray and Marengo silt loams","Luray",5,0.32,"NHEL"]
["Columbiana","Ma","Made land","Made"]
["Columbiana","MoB","Monongahela silt loam, 2 to 5 percent slopes","Monongahela",3,0.43,"PHEL"]
["Columbiana","MoC","Monongahela silt loam, 5 to 10 percent slopes","Monongahela",3,0.43,"PHEL"]
["Columbiana","MoC2","Monongahela silt loam, 5 to 10 percent slopes, moderately eroded","Monongahela",3,0.43,"PHEL"]
["Columbiana","MoD","Monongahela silt loam, 10 to 15 percent slopes","Monongahela",3,0.43,"HEL"]
["Columbiana","MoD2","Monongahela silt loam, 10 to 15 percent slopes, moderately eroded","Monongahela",3,0.43,"HEL"]
["Columbiana","NeB","Negley gravelly loam, 2 to 5 percent slopes","Negley",3,0.32,"PHEL"]
["Columbiana","NeC2","Negley gravelly loam, 5 to 10 percent slopes, moderately eroded","Negley",3,0.32,"PHEL"]
["Columbiana","NeD2","Negley gravelly loam, 10 to 15 percent slopes, moderately eroded","Negley",3,0.32,"HEL"]
["Columbiana","NgB","Negley loam, 2 to 5 percent slopes","Negley",3,0.32,"PHEL"]
["Columbiana","NgC","Negley loam, 5 to 10 percent slopes","Negley",3,0.32,"PHEL"]
["Columbiana","NgC2","Negley loam, 5 to 10 percent slopes, moderately eroded","Negley",3,0.32,"PHEL"]
["Columbiana","NgD2","Negley loam, 10 to 15 percent slopes, moderately eroded","Negley",3,0.32,"HEL"]
["Columbiana","NlB","Negley silt loam, 2 to 5 percent slopes","Negley",3,0.32,"PHEL"]
["Columbiana","NlC2","Negley silt loam, 5 to 10 percent slopes, moderately eroded","Negley",3,0.32,"PHEL"]
["Columbiana","NlD2","Negley silt loam, 10 to 15 percent slopes, moderately eroded","Negley",3,0.32,"HEL"]
["Columbiana","NsE2","Negley soils, 15 to 20 percent slopes, moderately eroded","Negley",3,0.32,"HEL"]
["Columbiana","NsE3","Negley soils, 10 to 20 percent slopes, severely eroded","Negley",2,0.32,"HEL"]
["Columbiana","Od","Olmsted silt loam","Olmstead",5,0.24,"NHEL"]
["Columbiana","Om","Olmsted silty clay loam","Olmstead",5,0.24,"NHEL"]
["Columbiana","Or","Orrville loam","Orrville",5,0.37,"NHEL"]
["Columbiana","Ov","Orrville silt loam","Orrville",5,0.37,"NHEL"]
["Columbiana","Pa","Papakating silt loam","Papakating",5,0.28000000000000003,"NHEL"]
["Columbiana","Pc","Papakating silty clay loam","Papakating",5,0.28000000000000003,"NHEL"]
["Columbiana","PkB","Parke silt loam, 2 to 5 percent slopes","Parke",5,0.37,"PHEL"]
["Columbiana","PkC","Parke silt loam, 5 to 10 percent slopes","Parke",5,0.37,"PHEL"]
["Columbiana","PkC2","Parke silt loam, 5 to 10 percent slopes, moderately eroded","Parke",5,0.37,"PHEL"]
["Columbiana","Pu","Purdy silt loam","Purdy",3,0.43,"NHEL"]
["Columbiana","RaB","Rainsboro silt loam, 2 to 5 percent slopes","Rainsboro",4,0.43,"PHEL"]
["Columbiana","RaC","Rainsboro silt loam, 5 to 10 percent slopes","Rainsboro",4,0.43,"PHEL"]
["Columbiana","RaC2","Rainsboro silt loam, 5 to 10 percent slopes, moderately eroded","Rainsboro",4,0.43,"PHEL"]
["Columbiana","RnA","Ravenna silt loam, 0 to 2 percent slopes","Ravenna",3,0.37,"NHEL"]
["Columbiana","RnB","Ravenna silt loam, 2 to 5 percent slopes","Ravenna",3,0.37,"PHEL"]
["Columbiana","RsB","Rittman silt loam, 2 to 5 percent slopes","Rittman",4,0.43,"PHEL"]
["Columbiana","RsC2","Rittman silt loam, 5 to 10 percent slopes, moderately eroded","Rittman",4,0.43,"PHEL"]
["Columbiana","RsD2","Rittman silt loam, 10 to 15 percent slopes, moderately eroded","Rittman",4,0.43,"HEL"]
["Columbiana","RsE2","Rittman silt loam, 15 to 20 percent slopes, moderately eroded","Rittman",4,0.43,"HEL"]
["Columbiana","RtD3","Rittman soils, 10 to 15 percent slopes, severely eroded","Rittman",3,0.43,"HEL"]
["Columbiana","RtE3","Rittman soils, 15 to 20 percent slopes, severely eroded","Rittman",3,0.43,"HEL"]
["Columbiana","Sb","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Columbiana","Sc","Sebring silty clay loam","Sebring",5,0.37,"NHEL"]
["Columbiana","SgD","Strip mine spoil, glacial materials, rolling","Strip Mine"]
["Columbiana","SmD","Strip mine spoil, sandstone and shale materials, rolling","Strip Mine"]
["Columbiana","SpF","Strip mine spoil, steep","Strip Mine"]
["Columbiana","Ss","Strip mine spoil, very acid","Strip Mine"]
["Columbiana","SuB","Summitville silt loam, 2 to 5 percent slopes","Summitville",3,0.37,"PHEL"]
["Columbiana","SuC","Summitville silt loam, 5 to 10 percent slopes","Summitville",3,0.37,"PHEL"]
["Columbiana","SuC2","Summitville silt loam, 5 to 10 percent slopes, moderately eroded","Summitville",3,0.37,"PHEL"]
["Columbiana","SuD2","Summitville silt loam, 10 to 15 percent slopes, moderately eroded","Summitville",3,0.37,"HEL"]
["Columbiana","TuB","Titusville silt loam, 2 to 5 percent slopes","Titusville",4,0.37,"PHEL"]
["Columbiana","TuC","Titusville silt loam, 5 to 10 percent slopes","Titusville",4,0.37,"PHEL"]
["Columbiana","TuC2","Titusville silt loam, 5 to 10 percent slopes, moderately eroded","Titusville",4,0.37,"PHEL"]
["Columbiana","TuD","Titusville silt loam, 10 to 15 percent slopes","Titusville",4,0.37,"HEL"]
["Columbiana","TuD2","Titusville silt loam, 10 to 15 percent slopes, moderately eroded","Titusville",4,0.37,"HEL"]
["Columbiana","TyA","Tyler silt loam, 0 to 2 percent slopes","Tyler",3,0.43,"NHEL"]
["Columbiana","TyB","Tyler silt loam, 2 to 5 percent slopes","Tyler",3,0.43,"PHEL"]
["Columbiana","UmB2","Upshur-Muskingum complex, 2 to 5 percent slopes, moderately eroded","Upshur",3,0.43,"PHEL"]
["Columbiana","UmC2","Upshur-Muskingum complex, 5 to 10 percent slopes, moderately eroded","Upshur",3,0.43,"PHEL"]
["Columbiana","UmD2","Upshur-Muskingum complex, 10 to 15 percent slopes, moderately eroded","Upshur",3,0.43,"HEL"]
["Columbiana","UmE2","Upshur-Muskingum complex, 15 to 20 percent slopes, moderately eroded","Upshur",3,0.43,"HEL"]
["Columbiana","UmF2","Upshur-Muskingum complex, 20 to 50 percent slopes, moderately eroded","Upshur",3,0.43,"HEL"]
["Columbiana","UmF3","Upshur-Muskingum complex, 20 to 35 percent slopes, severely eroded","Upshur",2,0.43,"HEL"]
["Columbiana","WaA","Wadsworth silt loam, 0 to 2 percent slopes","Wadsworth",4,0.43,"NHEL"]
["Columbiana","WaB","Wadsworth silt loam, 2 to 5 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Columbiana","Wc","Wayland silt loam","Wayland",5,0.43,"NHEL"]
["Columbiana","Wd","Wayland silty clay loam","Wayland",5,0.43,"NHEL"]
["Columbiana","WmB","Weikert and Muskingum soils, 2 to 5 percent slopes","Weikert",2,0.28000000000000003,"PHEL"]
["Columbiana","WmB2","Weikert and Muskingum soils, 2 to 5 percent slopes, moderately eroded","Weikert",2,0.28000000000000003,"PHEL"]
["Columbiana","WmC","Weikert and Muskingum soils, 5 to 10 percent slopes","Weikert",2,0.28000000000000003,"PHEL"]
["Columbiana","WmC2","Weikert and Muskingum soils, 5 to 10 percent slopes, moderately eroded","Weikert",2,0.28000000000000003,"PHEL"]
["Columbiana","WmC3","Weikert and Muskingum soils, 5 to 10 percent slopes, severely eroded","Weikert",2,0.28000000000000003,"PHEL"]
["Columbiana","WmD","Weikert and Muskingum soils, 10 to 15 percent slopes","Weikert",2,0.28000000000000003,"HEL"]
["Columbiana","WmD2","Weikert and Muskingum soils, 10 to 15 percent slopes, moderately eroded","Weikert",2,0.28000000000000003,"HEL"]
["Columbiana","WmD3","Weikert and Muskingum soils, 10 to 15 percent slopes, severely eroded","Weikert",2,0.28000000000000003,"HEL"]
["Columbiana","WmE2","Weikert and Muskingum soils, 15 to 20 percent slopes, moderately eroded","Weikert",2,0.28000000000000003,"HEL"]
["Columbiana","WmE3","Weikert and Muskingum soils, 15 to 20 percent slopes, severely eroded","Weikert",2,0.28000000000000003,"HEL"]
["Columbiana","WmF","Weikert and Muskingum soils, 20 to 35 percent slopes","Weikert",2,0.28000000000000003,"HEL"]
["Columbiana","WmF3","Weikert and Muskingum soils, 20 to 35 percent slopes, severely eroded","Weikert",2,0.28000000000000003,"HEL"]
["Columbiana","WmG","Weikert and Muskingum soils, 35 to 50 percent slopes","Weikert",2,0.28000000000000003,"HEL"]
["Columbiana","WmG3","Weikert and Muskingum soils, 35 to 50 percent slopes, severely eroded","Weikert",2,0.28000000000000003,"HEL"]
["Columbiana","WnB","Wellston silt loam, 2 to 5 percent slopes","Wellston",4,0.37,"PHEL"]
["Columbiana","WnC","Wellston silt loam, 5 to 10 percent slopes","Wellston",4,0.37,"PHEL"]
["Columbiana","WnC2","Wellston silt loam, 5 to 10 percent slopes, moderately eroded","Wellston",4,0.37,"PHEL"]
["Columbiana","WnD2","Wellston silt loam, 10 to 15 percent slopes, moderately eroded","Wellston",4,0.37,"HEL"]
["Columbiana","WnE2","Wellston silt loam, 15 to 20 percent slopes, moderately eroded","Wellston",4,0.37,"HEL"]
["Columbiana","WoB","Wharton silt loam, 2 to 5 percent slopes","Wharton",3,0.37,"PHEL"]
["Columbiana","WoC","Wharton silt loam, 5 to 10 percent slopes","Wharton",3,0.37,"PHEL"]
["Columbiana","WoC2","Wharton silt loam, 5 to 10 percent slopes, moderately eroded","Wharton",3,0.37,"PHEL"]
["Columbiana","WoD2","Wharton silt loam, 10 to 15 percent slopes, moderately eroded","Wharton",3,0.37,"HEL"]
["Columbiana","Wp","Willette muck","Willette",2,null,"NHEL"]
["Columbiana","WrC2","Wooster loam, 5 to 10 percent slopes, moderately eroded","Wooster",4,0.37,"PHEL"]
["Columbiana","WsB","Wooster silt loam, 2 to 5 percent slopes","Wooster",4,0.37,"PHEL"]
["Columbiana","WsB2","Wooster silt loam, 2 to 5 percent slopes, moderately eroded","Wooster",4,0.37,"PHEL"]
["Columbiana","WsC","Wooster silt loam, 5 to 10 percent slopes","Wooster",4,0.37,"PHEL"]
["Columbiana","WsC2","Wooster silt loam, 5 to 10 percent slopes, moderately eroded","Wooster",4,0.37,"PHEL"]
["Columbiana","WtD","Wooster soils, 10 to 15 percent slopes","Wooster",4,0.37,"HEL"]
["Columbiana","WtD2","Wooster soils, 10 to 15 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
["Columbiana","WtD3","Wooster soils, 10 to 15 percent slopes, severely eroded","Wooster",4,0.37,"HEL"]
["Columbiana","WtE2","Wooster soils, 15 to 20 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
["Columbiana","WtE3","Wooster soils, 15 to 20 percent slopes, severely eroded","Wooster",4,0.37,"HEL"]
["Columbiana","WtF2","Wooster soils, 20 to 35 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
["Columbiana","WtF3","Wooster soils, 20 to 35 percent slopes, severely eroded","Wooster",4,0.37,"HEL"]
["Columbiana","WtG2","Wooster soils, 35 to 50 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
[null,"Select","none","none"]
["Cuyahoga","As","Allis silt loam","Allis",3,0.43,"NHEL"]
["Cuyahoga","At","Allis-Urban land complex","Allis",3,0.43,"NHEL"]
["Cuyahoga","BgB","Bogart loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Cuyahoga","BhB","Bogart-Urban land complex, undulating","Bogart",5,0.32,"PHEL"]
["Cuyahoga","BrF","Brecksville silt loam, 25 to 70 percent slopes","Brecksville",4,0.43,"HEL"]
["Cuyahoga","Ca","Canadice silty clay loam","Canadice",5,0.49,"NHEL"]
["Cuyahoga","CcA","Caneadea silt loam, 0 to 2 percent slopes","Caneadea",3,0.43,"NHEL"]
["Cuyahoga","Cg","Carlisle silty clay loam","Carlisle",2,0.37,"NHEL"]
["Cuyahoga","Ch","Chagrin silt loam, occasionally flooded","Chagrin",5,0.32,"NHEL"]
["Cuyahoga","CnA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Cuyahoga","CnB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Cuyahoga","CnC","Chili loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Cuyahoga","CoD","Chili gravelly loam, 12 to 18 percent slopes","Chili",4,0.24,"PHEL"]
["Cuyahoga","Ct","Condit silty clay loam","Condit",5,0.37,"NHEL"]
["Cuyahoga","Cu","Condit-Urban land complex","Condit",5,0.37,"NHEL"]
["Cuyahoga","DaA","Darien silt loam, 0 to 2 percent slopes","Darien",3,0.37,"NHEL"]
["Cuyahoga","DkF","Dekalb-Loudonville complex, 25 to 70 percent slopes","Dekalb",2,0.24,"HEL"]
["Cuyahoga","Du","Dumps","Dumps"]
["Cuyahoga","ElB","Ellsworth silt loam, 2 to 6 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Cuyahoga","ElC","Ellsworth silt loam, 6 to 12 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Cuyahoga","ElD","Ellsworth silt loam, 12 to 18 percent slopes","Ellsworth",3,0.43,"HEL"]
["Cuyahoga","ElF","Ellsworth silt loam, 25 to 70 percent slopes","Ellsworth",3,0.43,"HEL"]
["Cuyahoga","EsC","Ellsworth-Urban land complex, rolling","Ellsworth",3,0.43,"HEL"]
["Cuyahoga","EuA","Euclid silt loam","Euclid",5,0.37,"NHEL"]
["Cuyahoga","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Cuyahoga","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Cuyahoga","GeF","Geeburg-Mentor silt loams, 25 to 70 percent slopes","Geeburg",3,0.43,"HEL"]
["Cuyahoga","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Cuyahoga","GfC","Glenford silt loam, 6 to 12 percent slopes","Glenford",5,0.37,"PHEL"]
["Cuyahoga","HaA","Haskins loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Cuyahoga","HaB","Haskins loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Cuyahoga","HbA","Haskins-Urban land complex, nearly level","Haskins",4,0.37,"NHEL"]
["Cuyahoga","Ho","Holly silt loam, frequently flooded","Holly",5,0.28000000000000003,"NHEL"]
["Cuyahoga","HrB","Hornell silt loam, 2 to 6 percent slopes","Hornell",3,0.43,"PHEL"]
["Cuyahoga","HrC","Hornell silt loam, 6 to 12 percent slopes","Hornell",3,0.43,"PHEL"]
["Cuyahoga","HrD","Hornell silt loam, 12 to 18 percent slopes","Hornell",3,0.43,"HEL"]
["Cuyahoga","HsC","Hornell-Urban land complex, rolling","Hornell",3,0.43,"HEL"]
["Cuyahoga","JtA","Jimtown loam, 0 to 3 percent slopes","Jimtown",4,0.32,"NHEL"]
["Cuyahoga","JuA","Jimtown-Urban land complex, nearly level","Jimtown",4,0.32,"NHEL"]
["Cuyahoga","LoB","Loudonville silt loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Cuyahoga","LoC","Loudonville silt loam, 6 to 12 percent slopes","Loudonville",4,0.32,"PHEL"]
["Cuyahoga","LoD","Loudonville silt loam, 12 to 18 percent slopes","Loudonville",4,0.32,"HEL"]
["Cuyahoga","LuC","Loudonville-Urban land complex, rolling","Loudonville",4,0.32,"PHEL"]
["Cuyahoga","MgA","Mahoning silt loam, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Cuyahoga","MgB","Mahoning silt loam, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Cuyahoga","MmB","Mahoning-Urban land complex, undulating","Mahoning",3,0.43,"PHEL"]
["Cuyahoga","Mo","Mermill loam","Mermill",5,0.28000000000000003,"NHEL"]
["Cuyahoga","Mr","Miner silty clay loam","Miner",5,0.32,"NHEL"]
["Cuyahoga","MtA","Mitiwanga silt loam, 0 to 2 percent slopes","Mitiwanga",4,0.32,"NHEL"]
["Cuyahoga","MtB","Mitiwanga silt loam, 2 to 6 percent slopes","Mitiwanga",4,0.32,"PHEL"]
["Cuyahoga","MxB","Mitiwanga-Urban land compex, undulating","Mitiwanga",4,0.32,"NHEL"]
["Cuyahoga","Or","Orrville silt loam, frequently flooded","Orrville",5,0.37,"NHEL"]
["Cuyahoga","OsA","Oshtemo sandy loam, 0 to 2 percent slopes","Oshtemo",5,0.24,"NHEL"]
["Cuyahoga","OsB","Oshtemo sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Cuyahoga","OsF","Oshtemo sandy loam, 25 to 55 percent slopes","Oshtemo",5,0.24,"HEL"]
["Cuyahoga","OtB","Oshtemo-Urban land complex, undulating","Oshtemo",5,0.24,"NHEL"]
["Cuyahoga","Pg","Pits, gravel","Pits"]
["Cuyahoga","Pt","Pits, quarry","Pits"]
["Cuyahoga","RsB","Rittman silt loam, 2 to 6 percent slopes","Rittman",4,0.43,"PHEL"]
["Cuyahoga","RsC","Rittman silt loam, 6 to 12 percent slopes","Rittman",4,0.43,"PHEL"]
["Cuyahoga","Sb","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Cuyahoga","St","Stafford variant sandy loam","Stafford",4,0.24,"NHEL"]
["Cuyahoga","Tg","Tioga loam, frequently flooded","Tioga",5,0.37,"NHEL"]
["Cuyahoga","Th","Tioga variant loam","Tioga",4,0.32,"NHEL"]
["Cuyahoga","Ua","Udorthents, loamy","Udorthents"]
["Cuyahoga","Ub","Urban land","Urban"]
["Cuyahoga","Uc","Urban land-Allis complex","Urban"]
["Cuyahoga","UeA","Urban land-Elnora complex, nearly level","Urban"]
["Cuyahoga","UmB","Urban land-Mahoning complex, undulating","Urban"]
["Cuyahoga","UnB","Urban land-Mitiwanga complex, undulating","Urban"]
["Cuyahoga","UoB","Urban land-Oshtemo complex, undulating","Urban"]
["Cuyahoga","W","Water","Water"]
["Cuyahoga","WaA","Wadsworth silt loam, 0 to 2 percent slopes","Wadsworth",4,0.43,"NHEL"]
["Cuyahoga","WaB","Wadsworth silt loam, 2 to 6 percent slopes","Wadsworth",4,0.43,"PHEL"]
[null,"Select","none","none"]
["Erie","AdD","Alexandria silt loam, 6 to 18 percent slopes","Alexandria",4,0.37,"PHEL"]
["Erie","AdF2","Alexandria silt loam, 18 to 40 percent slopes, moderately eroded","Alexandria",4,0.37,"HEL"]
["Erie","AlA","Allis silty clay loam, 0 to 2 percent slopes","Allis",3,0.43,"NHEL"]
["Erie","AlB","Allis silty clay loam, 2 to 6 percent slopes","Allis",3,0.43,"PHEL"]
["Erie","AoA","Allis stony silt loam, 0 to 2 percent slopes","Allis",3,0.43,"NHEL"]
["Erie","ArA","Arkport loamy fine sand, 0 to 2 percent slopes","Arkport",3,0.17,"NHEL"]
["Erie","ArB","Arkport loamy fine sand, 2 to 6 percent slopes","Arkport",3,0.17,"PHEL"]
["Erie","ArC","Arkport loamy fine sand, 6 to 12 percent slopes","Arkport",3,0.17,"PHEL"]
["Erie","ArD","Arkport loamy fine sand, 12 to 18 percent slopes","Arkport",3,0.17,"HEL"]
["Erie","AtA","Arkport loamy fine sand, moderately shallow variant, 0 to 2 percent slopes","Arkport",3,0.17,"NHEL"]
["Erie","AtB","Arkport loamy fine sand, moderately shallow variant, 2 to 6 percent slopes","Arkport",3,0.17,"PHEL"]
["Erie","Bc","Beaches","Beaches"]
["Erie","Be","Beaches, wet","Beaches"]
["Erie","BlB","Belmore sandy loam, 2 to 6 percent slopes","Belmore",4,0.24,"PHEL"]
["Erie","BlC","Belmore sandy loam, 6 to 12 percent slopes","Belmore",4,0.24,"PHEL"]
["Erie","BmA","Belmore loam, 0 to 2 percent slopes","Belmore",4,0.32,"NHEL"]
["Erie","BmB","Belmore loam, 2 to 6 percent slopes","Belmore",4,0.32,"PHEL"]
["Erie","BnA","Bennington loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Erie","BoA","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Erie","BoB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Erie","BpA","Bennington-Pyrmont silt loams, limestone substratum, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Erie","BrB","Berks channery silt loam, 0 to 6 percent slopes","Berks",3,0.24,"PHEL"]
["Erie","BrD","Berks channery silt loam, 6 to 18 percent slopes","Berks",3,0.24,"PHEL"]
["Erie","BsF","Berks channery soils, 18 to 60 percent slopes","Berks",3,0.24,"HEL"]
["Erie","BtA","Bogart loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Erie","BtB","Bogart loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Erie","Bw","Borrow pits","Borrow"]
["Erie","CaA","Cardington silt loam, 0 to 2 percent slopes","Cardington",4,0.37,"NHEL"]
["Erie","CaB","Cardington silt loam, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Erie","CfA","Casco loam, very flaggy subsoil variant, 0 to 2 percent slopes","Casco",3,0.24,"NHEL"]
["Erie","CfB","Casco loam, very flaggy subsoil variant, 2 to 6 percent slopes","Casco",3,0.24,"PHEL"]
["Erie","CfD","Casco loam, very flaggy subsoil variant, 6 to 18 percent slopes","Casco",3,0.24,"PHEL"]
["Erie","ChA","Castalia very channery silt loam, 0 to 2 percent slopes","Castalia",2,0.2,"NHEL"]
["Erie","ChB","Castalia very channery silt loam, 2 to 6 percent slopes","Castalia",2,0.2,"PHEL"]
["Erie","ClA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Erie","ClB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Erie","ClC","Chili loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Erie","ClD","Chili loam, 12 to 18 percent slopes","Chili",4,0.32,"HEL"]
["Erie","Cm","Colwood fine sandy loam","Coolwood",5,0.28000000000000003,"NHEL"]
["Erie","Co","Colwood silt loam","Coolwood",5,0.28000000000000003,"NHEL"]
["Erie","Cp","Colwood silt loam, limestone substratum","Coolwood",5,0.28000000000000003,"NHEL"]
["Erie","Cr","Colwood silt loam, acid variant","Coolwood",5,0.28000000000000003,"NHEL"]
["Erie","Cs","Colwood silty clay loam, acid variant","Coolwood",5,0.28000000000000003,"NHEL"]
["Erie","CtA","Colyer shaly loam, 0 to 2 percent slopes","Colyer",2,0.28000000000000003,"NHEL"]
["Erie","CtC","Colyer shaly loam, 2 to 12 percent slopes","Colyer",2,0.28000000000000003,"PHEL"]
["Erie","CyE","Colyer soils, 12 to 50 percent slopes","Colyer",2,0.28000000000000003,"HEL"]
["Erie","Da","Darroch silt loam","Darroch",5,0.32,"NHEL"]
["Erie","Dc","Darroch fine sandy loam, coarse subsoil variant","Darroch",5,0.24,"NHEL"]
["Erie","DkA","Dekalb fine sandy loam, 0 to 2 percent slopes","Dekalb",2,0.24,"NHEL"]
["Erie","DkB","Dekalb fine sandy loam, 2 to 6 percent slopes","Dekalb",2,0.24,"PHEL"]
["Erie","DrA","Del Rey loam, 0 to 2 percent slopes","Del Rey",3,0.43,"NHEL"]
["Erie","DsA","Del Rey silt loam, 0 to 2 percent slopes","Del Rey",3,0.43,"NHEL"]
["Erie","DsB","Del Rey silt loam, 2 to 6 percent slopes","Del Rey",3,0.43,"PHEL"]
["Erie","DtA","Digby sandy loam, 0 to 2 percent slopes","Digby",4,0.24,"NHEL"]
["Erie","DyA","Digby loam, 0 to 2 percent slopes","Digby",4,0.32,"NHEL"]
["Erie","Ee","Eel silt loam","Eel",5,0.37,"NHEL"]
["Erie","EhA","Elliott silt loam, 0 to 2 percent slopes","Elliott",4,0.28000000000000003,"NHEL"]
["Erie","EkA","Elliott silty clay loam, 0 to 2 percent slopes","Elliott",4,0.28000000000000003,"NHEL"]
["Erie","ElA","Ellsworth silt loam, 0 to 2 percent slopes","Ellsworth",3,0.43,"NHEL"]
["Erie","ElB","Ellsworth silt loam, 2 to 6 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Erie","ElC2","Ellsworth silt loam, 6 to 12 percent slopes, moderately eroded","Ellsworth",3,0.43,"PHEL"]
["Erie","ElD2","Ellsworth silt loam, 12 to 18 percent slopes, moderately eroded","Ellsworth",3,0.43,"HEL"]
["Erie","EwF","Ellsworth and Chili soils, 18 to 50 percent slopes","Ellsworth",3,0.43,"HEL"]
["Erie","Fr","Fries silt loam","Fries",4,0.28000000000000003,"NHEL"]
["Erie","Fs","Fries silty clay loam","Fries",4,0.28000000000000003,"NHEL"]
["Erie","FuA","Fulton silty clay loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Erie","FuB","Fulton silty clay loam, 2 to 6 percent slopes","Fulton",3,0.43,"PHEL"]
["Erie","GaA","Galen loamy fine sand, 0 to 2 percent slopes","Galen",3,0.17,"NHEL"]
["Erie","GaB","Galen loamy fine sand, 2 to 6 percent slopes","Galen",3,0.17,"PHEL"]
["Erie","GfB","Galen loamy fine sand, limestone substratum, 0 to 6 percent slopes","Galen",3,0.17,"PHEL"]
["Erie","GlB","Galen loamy fine sand, shale substratum, 0 to 6 percent slopes","Galen",3,0.17,"PHEL"]
["Erie","Go","Gilford fine sandy loam","Gilford",4,0.2,"NHEL"]
["Erie","Gp","Gravel pits","Gravel"]
["Erie","HsA","Haskins loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Erie","HsB","Haskins loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Erie","HtA","Haskins loam, dark surface variant, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Erie","JtA","Jimtown loam, 0 to 2 percent slopes","Jimtown",4,0.32,"NHEL"]
["Erie","Ju","Joliet silt loam","Joliet",2,0.28000000000000003,"NHEL"]
["Erie","KbA","Kibbie fine sandy loam, 0 to 2 percent slopes","Kibbie",5,0.2,"NHEL"]
["Erie","KbB","Kibbie fine sandy loam, 2 to 6 percent slopes","Kibbie",5,0.2,"PHEL"]
["Erie","KeA","Kibbie silt loam, 0 to 2 percent slopes","Kibbie",5,0.28000000000000003,"NHEL"]
["Erie","KfA","Kibbie fine sandy loam, moderately shallow variant, 0 to 2 percent slopes","Kibbie",4,0.24,"NHEL"]
["Erie","KhA","Kibbie silt loam, acid variant, 0 to 2 percent slopes","Kibbie",5,0.2,"NHEL"]
["Erie","La","Lenawee silt loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Erie","Lc","Lenawee silty clay loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Erie","LeA","Lewisburg silt loam, 0 to 2 percent slopes","Lewisburg",3,0.43,"NHEL"]
["Erie","LeB","Lewisburg silt loam, 2 to 6 percent slopes","Lewisburg",3,0.43,"PHEL"]
["Erie","LgA","Lewisburg silt loam, moderately shallow variant, 0 to 2 percent slopes","Lewisburg",3,0.43,"NHEL"]
["Erie","LgB","Lewisburg silt loam, moderately shallow variant, 2 to 6 percent slopes","Lewisburg",3,0.43,"PHEL"]
["Erie","LgC","Lewisburg silt loam, moderately shallow variant, 6 to 12 percent slopes","Lewisburg",3,0.43,"PHEL"]
["Erie","Lm","Lobdell silt loam","Lobdell",5,0.37,"NHEL"]
["Erie","LoA","Loudonville loam, 0 to 2 percent slopes","Loudonville",4,0.32,"NHEL"]
["Erie","LoB","Loudonville loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Erie","LoC","Loudonville loam, 6 to 12 percent slopes","Loudonville",4,0.32,"PHEL"]
["Erie","Ma","Made land","Made"]
["Erie","MfA","Mahoning loam, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Erie","MgA","Mahoning silt loam, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Erie","MgB","Mahoning silt loam, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Erie","MhA","Mahoning stony silt loam, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Erie","MkA","Mahoning loam, sandstone substratum, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Erie","MlA","Mahoning silt loam, shale substratum, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Erie","Mm","Marsh","Marsh",null,null,"NHEL"]
["Erie","Mn","Mermill silt loam","Mermill",5,0.28000000000000003,"NHEL"]
["Erie","Mo","Mermill silty clay loam","Mermill",5,0.28000000000000003,"NHEL"]
["Erie","MrA","Metea loamy fine sand, 0 to 2 percent slopes","Metea",5,0.17,"NHEL"]
["Erie","MrB","Metea loamy fine sand, 2 to 6 percent slopes","Metea",5,0.17,"NHEL"]
["Erie","MrC","Metea loamy fine sand, 6 to 12 percent slopes","Metea",5,0.17,"PHEL"]
["Erie","Ms","Millgrove loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Erie","Mt","Millgrove silty clay loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Erie","Mu","Millsdale silt loam","Millsdale",4,0.32,"NHEL"]
["Erie","Mv","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Erie","Mw","Miner silty clay loam","Miner",5,0.32,"NHEL"]
["Erie","MxA","Mitiwanga loam, 0 to 2 percent slopes","Mitiwanga",4,0.32,"NHEL"]
["Erie","OaB","Oakville loamy fine sand, 2 to 6 percent slopes","Oakville",5,0.15,"NHEL"]
["Erie","OaC","Oakville loamy fine sand, 6 to 12 percent slopes","Oakville",5,0.15,"PHEL"]
["Erie","OaE","Oakville loamy fine sand, 12 to 25 percent slopes","Oakville",5,0.15,"PHEL"]
["Erie","Or","Orrville silt loam","Orrville",5,0.37,"NHEL"]
["Erie","OsA","Oshtemo loamy sand, 0 to 2 percent slopes","Oshtemo",5,0.24,"NHEL"]
["Erie","OsB","Oshtemo loamy sand, 2 to 6 percent slopes","Oshtemo",5,0.24,"NHEL"]
["Erie","OtA","Oshtemo sandy loam, 0 to 2 percent slopes","Oshtemo",5,0.24,"NHEL"]
["Erie","OtB","Oshtemo sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"NHEL"]
["Erie","Pc","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Erie","Pe","Pewamo silty clay","Pewamo",5,0.24,"NHEL"]
["Erie","Ph","Pewamo silty clay loam, limestone substratum","Pewamo",5,0.24,"NHEL"]
["Erie","PmA","Prout loam, 0 to 2 percent slopes","Prout",4,0.37,"NHEL"]
["Erie","PrA","Prout channery loam, 0 to 2 percent slopes","Prout",4,0.37,"NHEL"]
["Erie","PsA","Prout loam, brown subsoil variant, 0 to 2 percent slopes","Prout",4,0.37,"NHEL"]
["Erie","PsB","Prout loam, brown subsoil variant, 2 to 6 percent slopes","Prout",4,0.37,"PHEL"]
["Erie","PuA","Prout silt loam, deep variant, 0 to 2 percent slopes","Prout",5,0.37,"NHEL"]
["Erie","PyA","Pyrmont silt loam, 0 to 2 percent slopes","Prymont",3,0.43,"NHEL"]
["Erie","PzA","Pyrmont silt loam, moderately shallow variant, 0 to 2 percent slopes","Prymont",3,0.43,"NHEL"]
["Erie","Qu","Quarries","Quarries"]
["Erie","RcB","Rawson fine sandy loam, 2 to 6 percent slopes","Rawson",4,0.24,"PHEL"]
["Erie","RdA","Rawson loam, 0 to 2 percent slopes","Rawson",4,0.32,"NHEL"]
["Erie","Rf","Rimer loamy fine sand","Rimer",4,0.17,"NHEL"]
["Erie","Rg","Rimer fine sandy loam","Rimer",4,0.17,"NHEL"]
["Erie","RhB","Ritchey loam, 0 to 6 percent slopes","Ritchey",2,0.37,"PHEL"]
["Erie","RsB","Romeo silt loam, 0 to 6 percent slopes","Romeo",1,0.37,"PHEL"]
["Erie","RsD","Romeo silt loam, 6 to 18 percent slopes","Romeo",1,0.37,"HEL"]
["Erie","RsF","Romeo silt loam, 18 to 50 percent slopes","Romeo",1,0.37,"HEL"]
["Erie","Sa","Sand pits","Sand"]
["Erie","ShA","Shinrock loam, 0 to 2 percent slopes","Shinrock",3,0.37,"NHEL"]
["Erie","SkA","Shinrock silt loam, 0 to 2 percent slopes","Shinrock",3,0.37,"PHEL"]
["Erie","SkB","Shinrock silt loam, 2 to 6 percent slopes","Shinrock",3,0.37,"PHEL"]
["Erie","SkC2","Shinrock silt loam, 6 to 12 percent slopes, moderately eroded","Shinrock",3,0.37,"PHEL"]
["Erie","SkD2","Shinrock silt loam, 12 to 18 percent slopes, moderately eroded","Shinrock",3,0.37,"HEL"]
["Erie","SlE","Shinrock soils, 18 to 25 percent slopes","Shinrock",3,0.37,"HEL"]
["Erie","SlF","Shinrock soils, 25 to 40 percent slopes","Shinrock",3,0.37,"HEL"]
["Erie","Sm","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Erie","SnB","Sisson loamy fine sand, 2 to 6 percent slopes","Sisson",5,0.24,"NHEL"]
["Erie","SoB","Sisson fine sandy loam, 2 to 6 percent slopes","Sisson",5,0.24,"NHEL"]
["Erie","SoC2","Sisson fine sandy loam, 6 to 12 percent slopes, moderately eroded","Sisson",5,0.24,"PHEL"]
["Erie","SsB","Sisson silt loam, 2 to 6 percent slopes","Sisson",5,0.32,"PHEL"]
["Erie","SsC2","Sisson silt loam, 6 to 12 percent slopes, moderately eroded","Sisson",5,0.32,"PHEL"]
["Erie","SsD2","Sisson silt loam, 12 to 18 percent slopes, moderately eroded","Sisson",5,0.32,"PHEL"]
["Erie","SsD3","Sisson silt loam, 12 to 18 percent slopes, severely eroded","Sisson",5,0.32,"PHEL"]
["Erie","SsE2","Sisson silt loam, 18 to 25 percent slopes, moderately eroded","Sisson",5,0.32,"HEL"]
["Erie","StF","Sisson soils, 25 to 50 percent slopes","Sisson",5,0.32,"HEL"]
["Erie","Sv","Sloan silt loam","Sloan",5,0.37,"NHEL"]
["Erie","Ta","Tawas muck","Tawas",2,null,"NHEL"]
["Erie","Tc","Toledo silty clay loam","Toledo",5,0.28000000000000003,"NHEL"]
["Erie","To","Toledo silty clay","Toledo",5,0.28000000000000003,"NHEL"]
["Erie","Tp","Toledo silty clay, calcareous variant","Toledo",5,0.28000000000000003,"NHEL"]
["Erie","Tr","Trumbull silt loam","Trumbull",3,0.37,"NHEL"]
["Erie","TsA","Tuscola loamy fine sand, 0 to 2 percent slopes","Tuscola",5,0.17,"NHEL"]
["Erie","TuA","Tuscola fine sandy loam, 0 to 2 percent slopes","Tuscola",5,0.24,"NHEL"]
["Erie","TuB","Tuscola fine sandy loam, 2 to 6 percent slopes","Tuscola",5,0.24,"NHEL"]
["Erie","TwA","Tuscola silt loam, 0 to 2 percent slopes","Tuscola",5,0.32,"NHEL"]
["Erie","TwB","Tuscola silt loam, 2 to 6 percent slopes","Tuscola",5,0.32,"PHEL"]
["Erie","Va","Vaughnsville loam","Vaughnsville",4,0.32,"NHEL"]
["Erie","W","Water","Water"]
["Erie","Wa","Warners soils","Warners",5,null,"NHEL"]
["Erie","Wc","Warners soils, clayey subsoil variant","Warners",2,0.32,"NHEL"]
["Erie","Wh","Washtenaw soils","Washtenaw",5,0.37,"NHEL"]
["Erie","Wn","Wayland silt loam","Wayland",5,0.43,"NHEL"]
["Erie","Wo","Wilmer loam","Wilmer",5,0.28000000000000003,"NHEL"]
[null,"Select","none","none"]
["Geauga","BgB","Bogart loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Geauga","BrF","Brecksville silt loam, 25 to 70 percent slopes","Brecksville",4,0.43,"HEL"]
["Geauga","Ca","Canadice silt loam","Canadice",5,0.49,"NHEL"]
["Geauga","CcA","Caneadea silt loam, 0 to 2 percent slopes","Caneadea",3,0.43,"NHEL"]
["Geauga","CcB","Caneadea silt loam, 2 to 6 percent slopes","Caneadea",3,0.43,"PHEL"]
["Geauga","CdB","Canfield silt loam, 2 to 6 percent slopes","Canfield",4,0.37,"PHEL"]
["Geauga","CdC","Canfield silt loam, 6 to 12 percent slopes","Canfield",4,0.37,"PHEL"]
["Geauga","Cf","Carlisle muck, ponded","Carlisle",2,null,"NHEL"]
["Geauga","CnA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Geauga","CnB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Geauga","CnC","Chili loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Geauga","CoD2","Chili gravelly loam, 12 to 18 percent slopes, eroded","Chili",4,0.24,"PHEL"]
["Geauga","CyD","Chili-Oshtemo complex, 6 to 18 percent slopes","Chili",4,0.24,"PHEL"]
["Geauga","CyF","Chili-Oshtemo complex, 25 to 50 percent slopes","Chili",4,0.24,"HEL"]
["Geauga","Da","Damascus silt loam","Damascus",5,0.32,"NHEL"]
["Geauga","DrA","Darien silt loam, bedrock substratum, 0 to 2 percent slopes","Darien",3,0.37,"NHEL"]
["Geauga","DrB","Darien silt loam, bedrock substratum, 2 to 6 percent slopes","Darien",3,0.37,"PHEL"]
["Geauga","EhB","Ellsworth silt loam, 2 to 6 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Geauga","EhB2","Ellsworth silt loam, 2 to 6 percent slopes, eroded","Ellsworth",3,0.43,"PHEL"]
["Geauga","EhC","Ellsworth silt loam, 6 to 12 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Geauga","EhC2","Ellsworth silt loam, 6 to 12 percent slopes, eroded","Ellsworth",3,0.43,"PHEL"]
["Geauga","EhD","Ellsworth silt loam, 12 to 18 percent slopes","Ellsworth",3,0.43,"HEL"]
["Geauga","EhD2","Ellsworth silt loam, 12 to 18 percent slopes, eroded","Ellsworth",3,0.43,"HEL"]
["Geauga","EhE","Ellsworth silt loam, 18 to 25 percent slopes","Ellsworth",3,0.43,"HEL"]
["Geauga","EhF","Ellsworth silt loam, 25 to 50 percent slopes","Ellsworth",3,0.43,"HEL"]
["Geauga","EmC","Ellsworth silt loam, shale substratum, 6 to 12 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Geauga","EmD","Ellsworth silt loam, shale substratum, 12 to 18 percent slopes","Ellsworth",3,0.43,"HEL"]
["Geauga","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Geauga","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Geauga","GbB","Geeburg silt loam, 2 to 6 percent slopes","Geeburg",3,0.43,"PHEL"]
["Geauga","GbC","Geeburg silt loam, 6 to 12 percent slopes","Geeburg",3,0.43,"PHEL"]
["Geauga","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Geauga","GfC","Glenford silt loam, 6 to 12 percent slopes","Glenford",5,0.37,"PHEL"]
["Geauga","Ho","Holly silt loam, frequently flooded","Holly",5,0.28000000000000003,"NHEL"]
["Geauga","HsA","Haskins loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Geauga","HsB","Haskins loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Geauga","JtA","Jimtown silt loam, 0 to 3 percent slopes","Jimtown",4,0.32,"NHEL"]
["Geauga","LrB","Lordstown loam, 2 to 6 percent slopes","Lordstown",3,0.28000000000000003,"PHEL"]
["Geauga","LrC","Lordstown loam, 6 to 12 percent slopes","Lordstown",3,0.28000000000000003,"PHEL"]
["Geauga","LxD","Lordstown-Rock outcrop complex, 12 to 18 percent slopes","Lordstown",3,0.28000000000000003,"HEL"]
["Geauga","LxF","Lordstown-Rock outcrop complex, 18 to 70 percent slopes","Lordstown",3,0.28000000000000003,"HEL"]
["Geauga","LyB","Loudonville silt loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Geauga","LyC","Loudonville silt loam, 6 to 12 percent slopes","Loudonville",4,0.32,"PHEL"]
["Geauga","MgA","Mahoning silt loam, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Geauga","MgB","Mahoning silt loam, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Geauga","MgC","Mahoning silt loam, 6 to 12 percent slopes","Mahoning",3,0.43,"PHEL"]
["Geauga","MsA","Mahoning silt loam, shale substratum, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Geauga","MsB","Mahoning silt loam, shale substratum, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Geauga","MtA","Mitiwanga silt loam, 0 to 3 percent slopes","Mitiwanga",4,0.32,"NHEL"]
["Geauga","Or","Orrville silt loam, frequently flooded","Orrville",5,0.37,"NHEL"]
["Geauga","OsB","Oshtemo sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"NHEL"]
["Geauga","OsC","Oshtemo sandy loam, 6 to 12 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Geauga","Pg","Pits, gravel","Pits"]
["Geauga","Pq","Pits, quarry","Pits"]
["Geauga","PsA","Platea silt loam, 0 to 2 percent slopes","Platea",3,0.43,"NHEL"]
["Geauga","PsB","Platea silt loam, 2 to 6 percent slopes","Platea",3,0.43,"PHEL"]
["Geauga","ReA","Ravenna silt loam, 0 to 2 percent slopes","Ravenna",3,0.37,"NHEL"]
["Geauga","ReB","Ravenna silt loam, 2 to 6 percent slopes","Ravenna",3,0.37,"PHEL"]
["Geauga","RmB","Rawson silt loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Geauga","RsB","Rittman silt loam, 2 to 6 percent slopes","Rittman",4,0.43,"PHEL"]
["Geauga","RsC","Rittman silt loam, 6 to 12 percent slopes","Rittman",4,0.43,"PHEL"]
["Geauga","RsC2","Rittman silt loam, 6 to 12 percent slopes, eroded","Rittman",4,0.43,"PHEL"]
["Geauga","RsD","Rittman silt loam, 12 to 18 percent slopes","Rittman",4,0.43,"HEL"]
["Geauga","RsE","Rittman silt loam, 18 to 25 percent slopes","Rittman",4,0.43,"HEL"]
["Geauga","RsF","Rittman silt loam, 25 to 50 percent slopes","Rittman",4,0.43,"HEL"]
["Geauga","Sb","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Geauga","Sf","Sheffield silt loam","Sheffield",4,0.37,"NHEL"]
["Geauga","Tg","Tioga loam, frequently flooded","Tioga",5,0.37,"NHEL"]
["Geauga","Ud","Udorthents, loamy","Udorthents"]
["Geauga","Ur","Urban land","Urban"]
["Geauga","W","Water","Water"]
["Geauga","Wa","Wabasha silty clay loam, ponded","Wabasha",5,0.32,"NHEL"]
["Geauga","WbA","Wadsworth silt loam, 0 to 2 percent slopes","Wadsworth",4,0.43,"NHEL"]
["Geauga","WbB","Wadsworth silt loam, 2 to 6 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Geauga","Wc","Wallkill silt loam, ponded","Wallkill",5,0.32,"NHEL"]
["Geauga","Wt","Willette muck, ponded","Willette",2,null,"NHEL"]
["Geauga","WuD","Wooster silt loam, 12 to 18 percent slopes","Wooster",4,0.37,"HEL"]
[null,"Select","none","none"]
["Huron","AcF","Alexandria silt loam, 25 to 50 percent slopes","Alexandria",4,0.37,"HEL"]
["Huron","AdD2","Alexandria silty clay loam, 12 to 18 percent slopes, eroded","Alexandria",4,0.37,"HEL"]
["Huron","BgA","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Huron","BgB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Huron","BkA","Bixler loamy fine sand, 0 to 2 percent slopes","Bixler",5,0.15,"NHEL"]
["Huron","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Huron","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Huron","BrF","Brecksville silt loam, 40 to 70 percent slopes","Brecksville",4,0.43,"HEL"]
["Huron","CdB","Cardington silt loam, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Huron","CdC2","Cardington silt loam, 6 to 12 percent slopes, eroded","Cardington",4,0.37,"PHEL"]
["Huron","Ce","Carlisle muck","Carlisle",2,null,"NHEL"]
["Huron","Cf","Carlisle muck, ponded","Carlisle",2,null,"NHEL"]
["Huron","CgB","Castalia channery silt loam, 2 to 6 percent slopes","Castalia",2,0.2,"PHEL"]
["Huron","ChB","Chili loam, loamy substratum, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Huron","ChC","Chili loam, loamy substratum, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Huron","CkE","Chili-Udorthents complex, 18 to 30 percent slopes","Chili",4,0.32,"HEL"]
["Huron","Cm","Colwood silt loam","Colwood",5,0.28000000000000003,"NHEL"]
["Huron","Co","Condit silty clay loam","Condit",5,0.37,"NHEL"]
["Huron","EnA","Elnora loamy fine sand, 1 to 3 percent slopes","Elnora",4,0.17,"NHEL"]
["Huron","Fr","Fries silty clay loam","Fries",4,0.28000000000000003,"NHEL"]
["Huron","GwB2","Glynwood silty clay loam, 2 to 6 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Huron","HkA","Haskins loam, 0 to 3 percent slopes","Haskins",4,0.37,"NHEL"]
["Huron","Ho","Holly silt loam, frequently flooded","Holly",5,0.28000000000000003,"NHEL"]
["Huron","JtA","Jimtown loam, 0 to 3 percent slopes","Jimtown",4,0.32,"NHEL"]
["Huron","KbA","Kibbie loam, 0 to 2 percent slopes","Kibbie",5,0.28000000000000003,"NHEL"]
["Huron","Le","Lenawee silty clay loam","Lenawee",4,0.28000000000000003,"NHEL"]
["Huron","Lf","Lenawee variant silty clay loam","Lenawee",5,0.37,"NHEL"]
["Huron","Lm","Linwood muck","Linwood",2,null,"NHEL"]
["Huron","Ln","Lobdell silt loam, rarely flooded","Lobdell",5,0.37,"NHEL"]
["Huron","Lo","Lobdell silt loam, frequently flooded","Lobdell",5,0.37,"NHEL"]
["Huron","LrB","Lordstown loam, 2 to 6 percent slopes","Lordstown",3,0.28000000000000003,"PHEL"]
["Huron","Mm","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Huron","MnB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Huron","Mr","Miner silty clay loam","Miner",5,0.32,"NHEL"]
["Huron","MwB","Mitiwanga silt loam, 1 to 4 percent slopes","Mitiwanga",4,0.32,"NHEL"]
["Huron","Or","Orrville silt loam, frequently flooded","Orrville",5,0.37,"NHEL"]
["Huron","OsB","Oshtemo fine sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"NHEL"]
["Huron","OtB","Otisville gravelly sandy loam, 2 to 6 percent slopes","Otisville",3,0.17,"PHEL"]
["Huron","Pa","Pandora silty clay loam","Pandora",5,0.37,"NHEL"]
["Huron","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Huron","Pn","Pinnebog muck","Pinnebog",5,null,"NHEL"]
["Huron","Ps","Pits","Pits"]
["Huron","PuA","Prout silt loam, 0 to 2 percent slopes","Prout",4,0.37,"NHEL"]
["Huron","SaF","Saylesville silt loam, 25 to 40 percent slopes","Saylesville",5,0.37,"HEL"]
["Huron","ScB","Shinrock silt loam, 2 to 6 percent slopes","Shinrock",3,0.37,"PHEL"]
["Huron","SpB","Spinks loamy fine sand, 2 to 6 percent slopes","Spinks",5,0.17,"NHEL"]
["Huron","Tg","Tioga loam, occasionally flooded","Tioga",5,0.37,"NHEL"]
["Huron","TrA","Tiro silt loam, 0 to 2 percent slopes","Tiro",4,0.37,"NHEL"]
["Huron","TrB","Tiro silt loam, 2 to 6 percent slopes","Tiro",4,0.37,"PHEL"]
["Huron","TuA","Tuscola fine sandy loam, 0 to 2 percent slopes","Tuscola",5,0.24,"NHEL"]
["Huron","TuB","Tuscola fine sandy loam, 2 to 6 percent slopes","Tuscola",5,0.24,"NHEL"]
["Huron","Ud","Udorthents, loamy","Udorthents"]
["Huron","W","Water","Water"]
["Huron","Wa","Wallkill silt loam, lacustrine substratum, occasionally flooded","Wallkill",5,0.32,"NHEL"]
[null,"Select","none","none"]
["Lake","Ad","Adrian muck","Adrian",2,null,"NHEL"]
["Lake","As","Allis silt loam","Allis",3,0.43,"NHEL"]
["Lake","Bs","Beaches","Beaches"]
["Lake","Cg","Carlisle muck","Carlisle",2,null,"NHEL"]
["Lake","CoB","Colonie loamy fine sand, 2 to 6 percent slopes","Colonie",4,0.17,"PHEL"]
["Lake","CoD","Colonie loamy fine sand, 6 to 18 percent slopes","Colonie",4,0.17,"PHEL"]
["Lake","CoF","Colonie loamy fine sand, 25 to 50 percent slopes","Colonie",4,0.17,"HEL"]
["Lake","CtA","Conneaut silt loam, 0 to 1 percent slopes","Conneaut",4,0.37,"NHEL"]
["Lake","CtB","Conneaut silt loam, 1 to 4 percent slopes","Conneaut",4,0.37,"PHEL"]
["Lake","CwA","Conneaut silt loam, shale substratum, 0 to 2 percent slopes","Conneaut",4,0.37,"NHEL"]
["Lake","CxA","Conotton loam, 0 to 2 percent slopes","Conotton",3,0.24,"NHEL"]
["Lake","CyB","Conotton gravelly loam, 2 to 6 percent slopes","Conotton",3,0.24,"PHEL"]
["Lake","CyC","Conotton gravelly loam, 6 to 15 percent slopes","Conotton",3,0.24,"PHEL"]
["Lake","DaA","Darien silt loam, 0 to 1 percent slopes","Darien",3,0.37,"NHEL"]
["Lake","DaB","Darien silt loam, 1 to 4 percent slopes","Darien",3,0.37,"PHEL"]
["Lake","DaC","Darien silt loam, 6 to 12 percent slopes","Darien",3,0.37,"PHEL"]
["Lake","Dc","Dumps, covered","Dumps"]
["Lake","Du","Dumps, chemical waste","Dumps"]
["Lake","ElB","Ellsworth silt loam, 2 to 6 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Lake","ElC","Ellsworth silt loam, 6 to 12 percent slopes","Ellsworth",3,0.43,"HEL"]
["Lake","ElD","Ellsworth silt loam, 12 to 18 percent slopes","Ellsworth",3,0.43,"HEL"]
["Lake","ElF","Ellsworth silt loam, 25 to 70 percent slopes","Ellsworth",3,0.43,"HEL"]
["Lake","EmC","Ellsworth silt loam, shale substratum, 6 to 12 percent slopes","Ellsworth",3,0.43,"HEL"]
["Lake","EmD","Ellsworth silt loam, shale substratum, 12 to 18 percent slopes","Ellsworth",3,0.43,"HEL"]
["Lake","EnB","Elnora loamy fine sand, 1 to 5 percent slopes","Elnora",4,0.17,"NHEL"]
["Lake","EuA","Euclid silt loam, 0 to 2 percent slopes","Euclid",5,0.37,"NHEL"]
["Lake","FcA","Fitchville silt loam, 1 to 4 percent slopes","Fitchville",5,0.37,"NHEL"]
["Lake","GfA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Lake","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Lake","GoF","Gosport silty clay loam, 25 to 70 percent slopes","Gosport",3,0.43,"HEL"]
["Lake","Gr","Granby sandy loam","Granby",5,0.17,"NHEL"]
["Lake","Kf","Kingsville fine sand","Kingsville",5,0.24,"NHEL"]
["Lake","Lb","Lobdell silt loam","Lobdell",5,0.37,"NHEL"]
["Lake","LrB","Lordstown channery silt loam, 2 to 6 percent slopes","Lordstown",3,0.28000000000000003,"PHEL"]
["Lake","LrC","Lordstown channery silt loam, 6 to 12 percent slopes","Lordstown",3,0.28000000000000003,"PHEL"]
["Lake","LxF","Lordstown-Rock outcrop complex, 25 to 70 percent slopes","Lordstown",3,0.28000000000000003,"HEL"]
["Lake","MgA","Mahoning silt loam, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Lake","MgB","Mahoning silt loam, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Lake","MhB","Mahoning silt loam, shale substratum, 1 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Lake","Mo","Minoa fine sandy loam","Minoa",4,0.28000000000000003,"NHEL"]
["Lake","MtA","Mitiwanga silt loam, 0 to 2 percent slopes","Mitiwanga",4,0.32,"NHEL"]
["Lake","Or","Orrville silt loam","Orrville",5,0.37,"NHEL"]
["Lake","OsA","Oshtemo sandy loam, 0 to 2 percent slopes","Oshtemo",5,0.24,"NHEL"]
["Lake","OsB","Oshtemo sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Lake","OtB","Otisville gravelly loamy sand, 1 to 6 percent slopes","Otisville",3,0.17,"PHEL"]
["Lake","Pa","Painesville fine sandy loam","Painesville",4,0.24,"NHEL"]
["Lake","PeB","Pierpont silt loam, 2 to 6 percent slopes","Pierpont",4,0.43,"PHEL"]
["Lake","PeB2","Pierpont silt loam, 2 to 6 percent slopes, moderately eroded","Pierpont",4,0.43,"PHEL"]
["Lake","PeC2","Pierpont silt loam, 6 to 12 percent slopes, moderately eroded","Pierpont",4,0.43,"PHEL"]
["Lake","PeD2","Pierpont silt loam, 12 to 18 percent slopes, moderately eroded","Pierpont",4,0.43,"HEL"]
["Lake","Po","Pits, gravel","Pits"]
["Lake","PsA","Platea silt loam, 0 to 2 percent slopes","Platea",3,0.43,"NHEL"]
["Lake","PsB","Platea silt loam, 2 to 6 percent slopes","Platea",3,0.43,"PHEL"]
["Lake","RhA","Red Hook sandy loam, 0 to 2 percent slopes","Red Hook",3,0.32,"NHEL"]
["Lake","Rv","Riverwash","Riverwash"]
["Lake","St","Stafford loamy fine sand","Stafford",4,0.17,"NHEL"]
["Lake","Sw","Swanton fine sandy loam","Swanton",3,0.28000000000000003,"NHEL"]
["Lake","Tg","Tioga loam","Tioga",5,0.37,"NHEL"]
["Lake","Th","Tioga Variant silt loam","Tioga",4,0.32,"NHEL"]
["Lake","TyB","Tyner loamy sand, 1 to 6 percent slopes","Tyner",5,0.17,"NHEL"]
["Lake","TyC","Tyner loamy sand, 6 to 12 percent slopes","Tyner",5,0.17,"PHEL"]
["Lake","TzA","Tyner Variant sandy loam","Tyner",5,0.17,"NHEL"]
["Lake","UdB","Udorthents, gently sloping","Udorthents"]
["Lake","UdD","Udorthents, moderately steep","Udorthents"]
["Lake","Ur","Urban land","Urban"]
["Lake","W","Water","Water"]
[null,"Select","none","none"]
["Lorain","AkA","Allis loam, 0 to 2 percent slopes","Allis",3,0.43,"NHEL"]
["Lorain","AlA","Allis silty clay loam, 0 to 2 percent slopes","Allis",3,0.43,"NHEL"]
["Lorain","AmA","Allis-Urban land complex, nearly level","Allis",3,0.43,"NHEL"]
["Lorain","BsA","Bogart sandy loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Lorain","BtA","Bogart loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Lorain","BtB","Bogart loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Lorain","Cg","Carlisle mucky silt loam","Carlisle",2,0.37,"NHEL"]
["Lorain","Ch","Chagrin silt loam","Chagrin",5,0.32,"NHEL"]
["Lorain","ClA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Lorain","ClB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Lorain","ClD2","Chili loam, 6 to 18 percent slopes, moderately eroded","Chili",4,0.32,"PHEL"]
["Lorain","CnB","Chili-Urban land complex, gently sloping","Chili",4,0.32,"PHEL"]
["Lorain","CoB","Conotton gravelly loam, 2 to 6 percent slopes","Conotton",3,0.24,"PHEL"]
["Lorain","CoC","Conotton gravelly loam, 6 to 12 percent slopes","Conotton",3,0.24,"PHEL"]
["Lorain","Cz","Udorthents","Udorthents"]
["Lorain","DkB","Dekalb very channery loam, 1 to 6 percent slopes","Dekalb",2,0.24,"PHEL"]
["Lorain","DsB","Del Rey silt loam, 1 to 4 percent slopes","Del Rey",3,0.43,"PHEL"]
["Lorain","ElB","Ellsworth silt loam, 2 to 6 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Lorain","ElB2","Ellsworth silt loam, 2 to 6 percent slopes, moderately eroded","Ellsworth",3,0.43,"PHEL"]
["Lorain","ElC2","Ellsworth silt loam, 6 to 12 percent slopes, moderately eroded","Ellsworth",3,0.43,"PHEL"]
["Lorain","ElD2","Ellsworth silt loam, 12 to 18 percent slopes, moderately eroded","Ellsworth",3,0.43,"HEL"]
["Lorain","ElF2","Ellsworth silt loam, 18 to 50 percent slopes, moderately eroded","Ellsworth",3,0.43,"HEL"]
["Lorain","EnA","Elnora loamy fine sand, 1 to 3 percent slopes","Elnora",4,0.17,"NHEL"]
["Lorain","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Lorain","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Lorain","FdA","Fitchville silt loam, low terrace, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Lorain","FeA","Fitchville-Urban land complex, nearly level","Fitchville",5,0.37,"NHEL"]
["Lorain","FuA","Fulton silt loam, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Lorain","FuB","Fulton silt loam, 2 to 6 percent slopes","Fulton",3,0.43,"PHEL"]
["Lorain","FvA","Fulton silt loam, sandy substratum, 0 to 2 percent slopes","Fulton",3,0.43,"NHEL"]
["Lorain","HsA","Haskins loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Lorain","HsB","Haskins loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Lorain","HtA","Haskins-Urban land complex, nearly level","Haskins",4,0.37,"NHEL"]
["Lorain","Hy","Holly silt loam","Holly",5,0.28000000000000003,"NHEL"]
["Lorain","HzA","Hornell silt loam, 0 to 2 percent slopes","Hornell",3,0.43,"NHEL"]
["Lorain","HzB","Hornell silt loam, 2 to 6 percent slopes","Hornell",3,0.43,"PHEL"]
["Lorain","JsA","Jimtown sandy loam, 0 to 2 percent slopes","Jimtown",4,0.32,"NHEL"]
["Lorain","JtA","Jimtown loam, 0 to 2 percent slopes","Jimtown",4,0.32,"NHEL"]
["Lorain","JtB","Jimtown loam, 2 to 6 percent slopes","Jimtown",4,0.32,"PHEL"]
["Lorain","JuA","Jimtown-Urban land complex, nearly level","Jimtown",4,0.32,"NHEL"]
["Lorain","Lb","Lobdell silt loam","Lobdell",5,0.37,"NHEL"]
["Lorain","LcB","Lockport silty clay loam, 1 to 4 percent slopes","Lockport",3,0.43,"PHEL"]
["Lorain","Ln","Lorain silty clay loam","Lorain",5,0.32,"NHEL"]
["Lorain","Ls","Lorain silty clay loam, sandy substratum","Lorain",5,0.32,"NHEL"]
["Lorain","Ly","Luray silty clay loam","Luray",5,0.32,"NHEL"]
["Lorain","MgA","Mahoning silt loam, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Lorain","MgB","Mahoning silt loam, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Lorain","MgB2","Mahoning silt loam, 2 to 6 percent slopes, moderately eroded","Mahoning",3,0.43,"PHEL"]
["Lorain","MhA","Mahoning silt loam, sandstone substratum, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Lorain","MkA","Mahoning-Tiro silt loams, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Lorain","MkB","Mahoning-Tiro silt loams, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Lorain","MmA","Mahoning-Urban land complex, nearly level","Mahoning",3,0.43,"NHEL"]
["Lorain","MnB","Mentor silt loam, 2 to 6 percent slopes","Mentor",5,0.37,"PHEL"]
["Lorain","MnC","Mentor silt loam, 6 to 12 percent slopes","Mentor",5,0.37,"PHEL"]
["Lorain","MnE","Mentor silt loam, 12 to 25 percent slopes","Mentor",5,0.37,"HEL"]
["Lorain","Mo","Mermill loam","Mermill",5,0.28000000000000003,"NHEL"]
["Lorain","Mr","Miner silty clay loam","Miner",5,0.32,"NHEL"]
["Lorain","Ms","Miner silty clay loam, shale substratum","Miner",5,0.32,"NHEL"]
["Lorain","MtA","Mitiwanga silt loam, 0 to 2 percent slopes","Mitiwanga",4,0.32,"NHEL"]
["Lorain","MtB","Mitiwanga silt loam, 2 to 6 percent slopes","Mitiwanga",4,0.32,"PHEL"]
["Lorain","MvB","Mitiwanga channery loam, 1 to 4 percent slopes","Mitiwanga",4,0.32,"NHEL"]
["Lorain","MxB","Mitiwanga-Urban land complex, gently sloping","Mitiwanga",4,0.32,"PHEL"]
["Lorain","Om","Olmsted fine sandy loam","Olmstead",5,0.24,"NHEL"]
["Lorain","On","Olmsted loam, sandstone substratum","Olmstead",5,0.24,"NHEL"]
["Lorain","Or","Orrville silt loam","Orrville",5,0.37,"NHEL"]
["Lorain","OtA","Oshtemo sandy loam, 0 to 2 percent slopes","Oshtemo",5,0.24,"NHEL"]
["Lorain","OtB","Oshtemo sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Lorain","OtC","Oshtemo sandy loam, 6 to 12 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Lorain","Qu","Quarries","Quarries"]
["Lorain","RdA","Rawson loam, 0 to 2 percent slopes","Rawson",4,0.32,"NHEL"]
["Lorain","RdB","Rawson loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Lorain","RdC2","Rawson loam, 6 to 12 percent slopes, moderately eroded","Rawson",4,0.32,"PHEL"]
["Lorain","Sb","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Lorain","Sd","Sebring silt loam, sandstone substratum","Sebring",5,0.37,"NHEL"]
["Lorain","Se","Senecaville silt loam","Senecaville",5,0.32,"NHEL"]
["Lorain","SkA","Shinrock silt loam, 0 to 2 percent slopes","Shinrock",3,0.37,"NHEL"]
["Lorain","SkB","Shinrock silt loam, 2 to 6 percent slopes","Shinrock",3,0.37,"PHEL"]
["Lorain","Sw","Stafford fine sandy loam","Stafford",4,0.17,"NHEL"]
["Lorain","Tg","Tioga fine sandy loam","Tioga",5,0.37,"NHEL"]
["Lorain","TrA","Trumbull silty clay loam, 0 to 2 percent slopes","Trumbull",3,0.37,"NHEL"]
["Lorain","TyB","Tyner loamy sand, 1 to 6 percent slopes","Tyner",5,0.17,"NHEL"]
["Lorain","TyC","Tyner loamy sand, 6 to 12 percent slopes","Tyner",5,0.17,"PHEL"]
["Lorain","UpC","Upshur silt loam, 2 to 8 percent slopes","Upshur",3,0.43,"PHEL"]
["Lorain","UpF","Upshur silt loam, 25 to 70 percent slopes","Upshur",3,0.43,"HEL"]
["Lorain","W","Water","Water"]
["Lorain","WeB","Weikert channery fine sandy loam, 1 to 6 percent slopes","Weikert",2,0.28000000000000003,"PHEL"]
[null,"Select","none","none"]
["Mahoning","BeB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Mahoning","BgB","Bogart loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Mahoning","BgC","Bogart loam, 6 to 12 percent slopes","Bogart",5,0.32,"PHEL"]
["Mahoning","BtB","Bogart loam, till substratum, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Mahoning","BtC2","Bogart loam, till substratum, 6 to 12 percent slopes, moderately eroded","Bogart",5,0.32,"PHEL"]
["Mahoning","Ca","Canadice silty clay loam","Canadice",5,0.49,"NHEL"]
["Mahoning","CdB","Canfield silt loam, 2 to 6 percent slopes","Canfield",4,0.37,"PHEL"]
["Mahoning","CdC","Canfield silt loam, 6 to 12 percent slopes","Canfield",4,0.37,"PHEL"]
["Mahoning","CdC2","Canfield silt loam, 6 to 12 percent slopes, moderately eroded","Canfield",4,0.37,"PHEL"]
["Mahoning","CeB","Canfield-Urban land complex","Canfield",4,0.37,"PHEL"]
["Mahoning","CgB","Cardington silt loam, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Mahoning","CgC2","Cardington silt loam, 6 to 12 percent slopes, moderately eroded","Cardington",4,0.37,"PHEL"]
["Mahoning","Ch","Carlisle muck","Carlisle",2,null,"NHEL"]
["Mahoning","Ck","Chagrin loam","Chagrin",5,0.32,"NHEL"]
["Mahoning","ClB","Chili gravelly loam, 2 to 6 percent slopes","Chili",4,0.24,"PHEL"]
["Mahoning","ClC","Chili gravelly loam, 6 to 12 percent slopes","Chili",4,0.24,"PHEL"]
["Mahoning","ClD","Chili gravelly loam, 12 to 18 percent slopes","Chili",4,0.24,"HEL"]
["Mahoning","CmB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Mahoning","CmC","Chili loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Mahoning","CnE","Chili and Conotton gravelly soils, 18 to 25 percent slopes","Chili",4,0.24,"HEL"]
["Mahoning","CnF","Chili and Conotton gravelly soils, 25 to 50 percent slopes","Chili",4,0.24,"HEL"]
["Mahoning","CoB","Chili-Urban land complex, undulating","Chili",4,0.32,"PHEL"]
["Mahoning","CoC","Chili-Urban land complex, rolling","Chili",4,0.32,"PHEL"]
["Mahoning","Ct","Condit silt loam","Condit",5,0.37,"NHEL"]
["Mahoning","Da","Damascus loam","Damascus",5,0.32,"NHEL"]
["Mahoning","Dc","Damascus loam, till substratum","Damascus",5,0.32,"NHEL"]
["Mahoning","DkC","Dekalb very stony loam, 2 to 12 percent slopes","Dekalb",2,0.24,"PHEL"]
["Mahoning","DkE","Dekalb very stony loam, 12 to 25 percent slopes","Dekalb",2,0.24,"HEL"]
["Mahoning","DkF","Dekalb very stony loam, 25 to 50 percent slopes","Dekalb",2,0.24,"HEL"]
["Mahoning","ElB","Ellsworth silt loam, 2 to 6 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Mahoning","ElC","Ellsworth silt loam, 6 to 12 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Mahoning","ElC2","Ellsworth silt loam, 6 to 12 percent slopes, moderately eroded","Ellsworth",3,0.43,"PHEL"]
["Mahoning","ElD2","Ellsworth silt loam, 12 to 18 percent slopes, moderately eroded","Ellsworth",3,0.43,"HEL"]
["Mahoning","ElE2","Ellsworth silt loam, 18 to 25 percent slopes, moderately eroded","Ellsworth",3,0.43,"HEL"]
["Mahoning","ElF","Ellsworth silt loam, 25 to 50 percent slopes","Ellsworth",3,0.43,"HEL"]
["Mahoning","EsF3","Ellsworth silty clay loam, 25 to 50 percent slopes, severely eroded","Ellsworth",2,0.43,"HEL"]
["Mahoning","EuB","Ellsworth-Urban land complex","Ellsworth",3,0.43,"PHEL"]
["Mahoning","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Mahoning","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Mahoning","FhB","Fitchville silt loam, till substratum, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Mahoning","FlB","Fitchville-Urban land complex","Fitchville",5,0.37,"PHEL"]
["Mahoning","Fr","Frenchtown silt loam","Frenchtown",3,0.37,"NHEL"]
["Mahoning","GbB","Geeburg silt loam, 2 to 6 percent slopes","Geeburg",3,0.43,"PHEL"]
["Mahoning","GbB2","Geeburg silt loam, 2 to 6 percent slopes, moderately eroded","Geeburg",3,0.43,"PHEL"]
["Mahoning","GbC","Geeburg silt loam, 6 to 12 percent slopes","Geeburg",3,0.43,"PHEL"]
["Mahoning","GbD","Geeburg silt loam, 12 to 18 percent slopes","Geeburg",3,0.43,"HEL"]
["Mahoning","GeC2","Geeburg silty clay loam, 6 to 12 percent slopes, moderately eroded","Geeburg",3,0.43,"PHEL"]
["Mahoning","GeC3","Geeburg silty clay loam, 6 to 12 percent slopes, severely eroded","Geeburg",2,0.43,"HEL"]
["Mahoning","GeD2","Geeburg silty clay loam, 12 to 18 percent slopes, moderately eroded","Geeburg",3,0.43,"HEL"]
["Mahoning","GeE2","Geeburg silty clay loam, 18 to 25 percent slopes, moderately eroded","Geeburg",3,0.43,"HEL"]
["Mahoning","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Mahoning","GfC2","Glenford silt loam, 6 to 12 percent slopes, moderately eroded","Glenford",5,0.37,"PHEL"]
["Mahoning","Gp","Gravel Pits","Gravel"]
["Mahoning","HoB","Hornell silt loam, 2 to 6 percent slopes","Hornell",3,0.43,"PHEL"]
["Mahoning","JtA","Jimtown loam, 0 to 2 percent slopes","Jimtown",4,0.32,"NHEL"]
["Mahoning","JtB","Jimtown loam, 2 to 6 percent slopes","Jimtown",4,0.32,"PHEL"]
["Mahoning","JuB","Jimtown loam, till substratum, 2 to 6 percent slopes","Jimtown",4,0.32,"PHEL"]
["Mahoning","JwB","Jimtown-Urban land complex","Jimtown",4,0.32,"PHEL"]
["Mahoning","Km","Kerston muck","Kerston",2,null,"NHEL"]
["Mahoning","Lb","Lobdell loam","Lobdell",5,0.37,"NHEL"]
["Mahoning","Lc","Lorain silty clay loam","Lorain",5,0.32,"NHEL"]
["Mahoning","LdB","Loudonville loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Mahoning","LdC2","Loudonville loam, 6 to 12 percent slopes, moderately eroded","Loudonville",4,0.32,"PHEL"]
["Mahoning","LdD2","Loudonville loam, 12 to 18 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Mahoning","LdE2","Loudonville loam, 18 to 25 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Mahoning","LrB","Loudonville-Urban land complex, undulating","Loudonville",4,0.32,"PHEL"]
["Mahoning","LrC","Loudonville-Urban land complex, rolling","Loudonville",4,0.32,"PHEL"]
["Mahoning","Ls","Luray silt loam","Luray",5,0.32,"NHEL"]
["Mahoning","Ly","Luray silty clay loam","Luray",5,0.32,"NHEL"]
["Mahoning","Ma","Made Land","Made"]
["Mahoning","MgA","Mahoning silt loam, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Mahoning","MgB","Mahoning silt loam, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Mahoning","MhB","Mahoning-Urban land complex","Mahoning",3,0.43,"PHEL"]
["Mahoning","Mn","Marengo silty clay loam","Marengo",5,0.28000000000000003,"NHEL"]
["Mahoning","MsB","Muskingum channery silt loam, 2 to 6 percent slopes","Muskingum",3,0.37,"PHEL"]
["Mahoning","MsC2","Muskingum channery silt loam, 6 to 12 percent slopes, moderately eroded","Muskingum",3,0.37,"PHEL"]
["Mahoning","MsD2","Muskingum channery silt loam, 12 to 18 percent slopes, moderately eroded","Muskingum",3,0.37,"HEL"]
["Mahoning","MsE2","Muskingum channery silt loam, 18 to 25 percent slopes, moderately eroded","Muskingum",3,0.37,"HEL"]
["Mahoning","MsF2","Muskingum channery silt loam, 25 to 50 percent slopes, moderately eroded","Muskingum",3,0.37,"HEL"]
["Mahoning","Od","Olmsted loam","Olmstead",5,0.24,"NHEL"]
["Mahoning","Ov","Orrville silt loam","Orrville",5,0.37,"NHEL"]
["Mahoning","Pa","Papakating silt loam","Papakating",5,0.28000000000000003,"NHEL"]
["Mahoning","Pc","Papakating silty clay loam","Papakating",5,0.28000000000000003,"NHEL"]
["Mahoning","Qu","quarry","Quarry"]
["Mahoning","RaA","Ravenna silt loam, 0 to 2 percent slopes","Ravena",3,0.37,"NHEL"]
["Mahoning","RaB","Ravenna silt loam, 2 to 6 percent slopes","Ravena",3,0.37,"PHEL"]
["Mahoning","ReA","Remsen silt loam, 0 to 2 percent slopes","Remsen",3,0.43,"NHEL"]
["Mahoning","ReB","Remsen silt loam, 2 to 6 percent slopes","Remsen",3,0.43,"PHEL"]
["Mahoning","RmB","Remsen-Urban land complex","Remsen",3,0.43,"PHEL"]
["Mahoning","RsB","Rittman silt loam, 2 to 6 percent slopes","Rittman",4,0.43,"PHEL"]
["Mahoning","RsC","Rittman silt loam, 6 to 12 percent slopes","Rittman",4,0.43,"PHEL"]
["Mahoning","RsC2","Rittman silt loam, 6 to 12 percent slopes, moderately eroded","Rittman",4,0.43,"PHEL"]
["Mahoning","RsD2","Rittman silt loam, 12 to 18 percent slopes, moderately eroded","Rittman",4,0.43,"HEL"]
["Mahoning","RuB","Rittman-Urban land complex","Rittman",4,0.43,"PHEL"]
["Mahoning","Sb","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Mahoning","Se","Sebring silt loam, till substratum","Sebring",5,0.37,"NHEL"]
["Mahoning","Sg","Sebring-Urban land complex","Sebring",5,0.37,"NHEL"]
["Mahoning","SsB ","Strip mine spoils, shale and sandstone materials, undulating","Strip Mine"]
["Mahoning","SsC","Strip mine spoils, shale and sandstone materials, rolling ","Strip Mine"]
["Mahoning","SsF","Strip mine spoils, shale and sandstone materials, steep","Strip Mine"]
["Mahoning","StB","Strip mine spoils, loamy till materials, undulating","Strip Mine"]
["Mahoning","StC","Strip mine spoils, loamy till materials, rolling","Strip Mine"]
["Mahoning","StF","Strip mine spoils loamy till materials, steep","Strip Mine"]
["Mahoning","SuB","Strip mine spoils, clayey till materials, undulating","Strip Mine"]
["Mahoning","TrA","Trumbull silt loam, 0 to 2 percent slopes","Trumbull",3,0.37,"NHEL"]
["Mahoning","TrB","Trumbull silt loam, 2 to 6 percent slopes","Trumbull",3,0.37,"PHEL"]
["Mahoning","Tu","Trumbull-Urban land complex","Trumbull",3,0.37,"NHEL"]
["Mahoning","W","Water","Water"]
["Mahoning","WaA","Wadsworth silt loam, 0 to 2 percent slopes","Wadsworth",4,0.43,"NHEL"]
["Mahoning","WaB","Wadsworth silt loam, 2 to 6 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Mahoning","WbB","Wadsworth-Urban land complex","Wadsworth",4,0.43,"PHEL"]
["Mahoning","Wc","Wayland silt loam","Wayland",5,0.43,"NHEL"]
["Mahoning","WrF2","Wooster loam, 25 to 50 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
["Mahoning","WsB","Wooster silt loam, 2 to 6 percent slopes","Wooster",4,0.37,"PHEL"]
["Mahoning","WsC2","Wooster silt loam, 6 to 12 percent slopes, moderately eroded","Wooster",4,0.37,"PHEL"]
["Mahoning","WsD2","Wooster silt loam, 12 to 18 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
["Mahoning","WsE2","Wooster silt loam, 18 to 25 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
[null,"Select","none","none"]
["Medina","BnA","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Medina","BnB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Medina","BoA","Bennington-Tiro silt loams, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Medina","BrF","Berks silt loam, 25 to 70 percent slopes","Berks",3,0.24,"HEL"]
["Medina","BtA","Bogart loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Medina","BtB","Bogart loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Medina","Ca","Canadice silty clay loam","Canadice",5,0.49,"NHEL"]
["Medina","CcA","Caneadea silt loam, 0 to 2 percent slopes","Caneadea",3,0.43,"NHEL"]
["Medina","CcB","Caneadea silt loam, 2 to 6 percent slopes","Caneadea",3,0.43,"PHEL"]
["Medina","CdA","Canfield silt loam, 0 to 2 percent slopes","Canfield",4,0.37,"NHEL"]
["Medina","CdB","Canfield silt loam, 2 to 6 percent slopes","Canfield",4,0.37,"PHEL"]
["Medina","CdB2","Canfield silt loam, 2 to 6 percent slopes, moderately eroded","Canfield",4,0.37,"PHEL"]
["Medina","CdC2","Canfield silt loam, 6 to 12 percent slopes, moderately eroded","Canfield",4,0.37,"PHEL"]
["Medina","CeC","Canfield-Urban land complex, rolling","Canfield",4,0.37,"PHEL"]
["Medina","CfB","Cardington fine sandy loam, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Medina","CgB","Cardington silt loam, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Medina","CgC2","Cardington silt loam, 6 to 12 percent slopes, moderately eroded","Cardington",4,0.37,"PHEL"]
["Medina","CgE2","Cardington silt loam, 12 to 25 percent slopes, moderately eroded","Cardington",4,0.37,"HEL"]
["Medina","Ch","Carlisle muck","Carlisle",2,null,"NHEL"]
["Medina","Cm","Chagrin silt loam","Chagrin",5,0.32,"NHEL"]
["Medina","CnA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Medina","CnB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Medina","CnC","Chili loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Medina","CoC2","Chili gravelly loam, 6 to 12 percent slopes, moderately eroded","Chili",4,0.24,"PHEL"]
["Medina","CoE2","Chili gravelly loam, 12 to 25 percent slopes, moderately eroded","Chili",4,0.24,"PHEL"]
["Medina","CoF2","Chili gravelly loam, 25 to 70 percent slopes, moderately eroded","Chili",4,0.24,"HEL"]
["Medina","CpA","Chili silt loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Medina","CpB","Chili silt loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Medina","CpC","Chili silt loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Medina","CuB","Chili-Urban land complex, undulating","Chili",4,0.32,"PHEL"]
["Medina","Cy","Condit silt loam","Condit",5,0.37,"NHEL"]
["Medina","C.F. ","Cut and Fill Land","Cut"]
["Medina","ElB","Ellsworth silt loam, 2 to 6 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Medina","ElB2","Ellsworth silt loam, 2 to 6 percent slopes, moderately eroded","Ellsworth",3,0.43,"PHEL"]
["Medina","ElC","Ellsworth silt loam, 6 to 12 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Medina","ElC2","Ellsworth silt loam, 6 to 12 percent slopes, moderately eroded","Ellsworth",3,0.43,"PHEL"]
["Medina","ElE2","Ellsworth silt loam, 12 to 25 percent slopes, moderately eroded","Ellsworth",3,0.43,"HEL"]
["Medina","ElF","Ellsworth silt loam, 25 to 70 percent slopes","Ellsworth",3,0.43,"HEL"]
["Medina","EsB","Ellsworth silt loam, sandstone substratum, 2 to 6 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Medina","EsC2","Ellsworth silt loam, sandstone substratum, 6 to 12 percent slopes, moderately eroded","Ellsworth",3,0.43,"PHEL"]
["Medina","EuB","Ellsworth-Urban land complex, undulating","Ellsworth",3,0.43,"PHEL"]
["Medina","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Medina","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Medina","FlA","Fitchville silt loam, low terrace, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Medina","G.P.","Gravel pit","Gravel"]
["Medina","GbC","Geeburg silt loam, 6 to 18 percent slopes","Geeburg",3,0.43,"PHEL"]
["Medina","GfA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Medina","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Medina","GfC2","Glenford silt loam, 6 to 12 percent slopes, moderately eroded","Glenford",5,0.37,"PHEL"]
["Medina","HsA","Haskins loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Medina","HsB","Haskins loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Medina","Hy","Holly silt loam","Holly",5,0.28000000000000003,"NHEL"]
["Medina","JtA","Jimtown loam, 0 to 2 percent slopes","Jimtown",4,0.32,"NHEL"]
["Medina","JtB","Jimtown loam, 2 to 6 percent slopes","Jimtown",4,0.32,"PHEL"]
["Medina","Ju","Jimtown-Urban land complex","Jimtown",4,0.32,"NHEL"]
["Medina","Ld","Linwood muck","Linwood",2,null,"NHEL"]
["Medina","Le","Lobdell silt loam","Lobdell",5,0.37,"NHEL"]
["Medina","Ln","Lorain silty clay loam","Lorain",5,0.32,"NHEL"]
["Medina","LoB","Loudonville silt loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Medina","LoC","Loudonville silt loam, 6 to 12 percent slopes","Loudonville",4,0.32,"PHEL"]
["Medina","LoC2","Loudonville silt loam, 6 to 12 percent slopes, moderately eroded","Loudonville",4,0.32,"PHEL"]
["Medina","LoE2","Loudonville silt loam, 12 to 25 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Medina","Ly","Luray silt loam","Luray",5,0.32,"NHEL"]
["Medina","M.L.","Made land","Made"]
["Medina","MgA","Mahoning silt loam, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Medina","MgB","Mahoning silt loam, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Medina","MlA","Mahoning silt loam, sandstone substratum, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Medina","MlB","Mahoning silt loam, sandstone substratum, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Medina","MnA","Mahoning-Urban land complex, nearly level","Mahoning",3,0.43,"NHEL"]
["Medina","Mr","Miner silty clay loam","Miner",5,0.32,"NHEL"]
["Medina","Od","Olmsted loam","Olmstead",5,0.24,"NHEL"]
["Medina","Or","Orrville silt loam","Orrville",5,0.37,"NHEL"]
["Medina","Os","Orrville silt loam, bedrock substratum","Orrville",5,0.37,"NHEL"]
["Medina","OtB","Oshtemo sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Medina","QU.","Quarry","Quarry"]
["Medina","ReA","Ravenna silt loam, 0 to 2 percent slopes","Ravenna",3,0.37,"NHEL"]
["Medina","ReB","Ravenna silt loam, 2 to 6 percent slopes","Ravenna",3,0.37,"PHEL"]
["Medina","RnA","Ravenna-Urban land complex, nearly level","Ravenna",3,0.37,"NHEL"]
["Medina","RoB","Rawson loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Medina","RsB","Rittman silt loam, 2 to 6 percent slopes","Rittman",4,0.43,"PHEL"]
["Medina","RsB2","Rittman silt loam, 2 to 6 percent slopes, moderately eroded","Rittman",4,0.43,"PHEL"]
["Medina","RsC","Rittman silt loam, 6 to 12 percent slopes","Rittman",4,0.43,"PHEL"]
["Medina","RsC2","Rittman silt loam, 6 to 12 percent slopes, moderately eroded","Rittman",4,0.43,"PHEL"]
["Medina","RsE2","Rittman silt loam, 12 to 25 percent slopes, moderately eroded","Rittman",4,0.43,"HEL"]
["Medina","RsF","Rittman silt loam, 25 to 70 percent slopes","Rittman",4,0.43,"HEL"]
["Medina","ScF","Schaffenaker loamy sand, 25 to 70 percent slopes","Schaffenaker",3,0.17,"HEL"]
["Medina","Sg","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Medina","St","Sebring silt loam, till substratum","Sebring",5,0.37,"NHEL"]
["Medina","W","Water","Water"]
["Medina","WaA","Wadsworth silt loam, 0 to 2 percent slopes","Wadsworth",4,0.43,"NHEL"]
["Medina","WaB","Wadsworth silt loam, 2 to 6 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Medina","WbB","Wadsworth-Urban land complex, undulating","Wadsworth",4,0.43,"PHEL"]
["Medina","Wc","Wallkill silt loam","Wallkill",5,0.32,"NHEL"]
["Medina","Wt","Willette muck","Willette",2,null,"NHEL"]
["Medina","WuB","Wooster silt loam, 2 to 6 percent slopes","Wooster",4,0.37,"PHEL"]
["Medina","WuB2","Wooster silt loam, 2 to 6 percent slopes, moderately eroded","Wooster",4,0.37,"PHEL"]
["Medina","WuC2","Wooster silt loam, 6 to 12 percent slopes, moderately eroded","Wooster",4,0.37,"PHEL"]
["Medina","WuE2","Wooster silt loam, 12 to 25 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
["Medina","WuF","Wooster silt loam, 25 to 70 percent slopes","Wooster",4,0.37,"HEL"]
[null,"Select","none","none"]
["Portage","BgA","Bogart silt loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Portage","BgB","Bogart silt loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Portage","BhB","Bogart-Haskins complex, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Portage","Bp","Borrow pits","Borrow"]
["Portage","Ca","Canadice silt loam","Canadice",5,0.49,"NHEL"]
["Portage","CcA","Caneadea silt loam, 0 to 2 percent slopes","Caneadea",3,0.43,"NHEL"]
["Portage","CcB","Caneadea silt loam, 2 to 6 percent slopes","Caneadea",3,0.43,"PHEL"]
["Portage","CdA","Canfield silt loam, 0 to 2 percent slopes","Canfield",4,0.37,"NHEL"]
["Portage","CdB","Canfield silt loam, 2 to 6 percent slopes","Canfield",4,0.37,"PHEL"]
["Portage","CdC","Canfield silt loam, 6 to 12 percent slopes","Canfield",4,0.37,"PHEL"]
["Portage","CdC2","Canfield silt loam, 6 to 12 percent slopes, moderately eroded","Canfield",4,0.37,"PHEL"]
["Portage","CfB","Canfield-Urban land complex, undulating","Canfield",4,0.37,"PHEL"]
["Portage","CfC","Canfield-Urban land complex, rolling","Canfield",4,0.37,"PHEL"]
["Portage","Cg","Carlisle muck","Carlisle",2,null,"NHEL"]
["Portage","CnA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Portage","CnB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Portage","CnC","Chili loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Portage","CoC2","Chili gravelly loam, 6 to 12 percent slopes, moderately eroded","Chili",4,0.24,"PHEL"]
["Portage","CpA","Chili silt loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Portage","CpB","Chili silt loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Portage","CpC","Chili silt loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Portage","CtD","Chili-Oshtemo complex, 12 to 18 percent slopes","Chili",4,0.32,"HEL"]
["Portage","CtE","Chili-Oshtemo complex, 18 to 25 percent slopes","Chili",4,0.32,"HEL"]
["Portage","CtF","Chili-Oshtemo complex, 25 to 50 percent slopes","Chili",4,0.32,"HEL"]
["Portage","CuB","Chili-Urban land complex, undulating","Chili",4,0.32,"PHEL"]
["Portage","CuC","Chili-Urban land complex, rolling","Chili",4,0.32,"PHEL"]
["Portage","CwC2","Chili-Wooster complex, 6 to 12 percent slopes, moderately eroded","Chili",4,0.32,"PHEL"]
["Portage","CwD2","Chili-Wooster complex, 12 to 18 percent slopes, moderately eroded","Chili",4,0.32,"HEL"]
["Portage","CwE","Chili-Wooster complex, 18 to 30 percent slopes","Chili",4,0.32,"HEL"]
["Portage","Da","Damascus loam","Damascus",5,0.32,"NHEL"]
["Portage","DkB","Dekalb channery loam, 2 to 6 percent slopes","Dekalb",2,0.24,"PHEL"]
["Portage","DkC","Dekalb channery loam, 6 to 12 percent slopes","Dekalb",2,0.24,"PHEL"]
["Portage","DkD","Dekalb channery loam 12 to 25 percent slopes","Dekalb",2,0.24,"HEL"]
["Portage","DkF","Dekalb channery loam, 25 to 70 percent slopes","Dekalb",2,0.24,"HEL"]
["Portage","ElB","Ellsworth silt loam, 2 to 6 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Portage","ElB2","Ellsworth silt loam, 2 to 6 percent slopes, moderately eroded","Ellsworth",3,0.43,"PHEL"]
["Portage","ElC","Ellsworth silt loam, 6 to 12 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Portage","ElC2","Ellsworth silt loam, 6 to 12 percent slopes, moderately eroded","Ellsworth",3,0.43,"PHEL"]
["Portage","ElD2","Ellsworth silt loam, 12 to 18 percent slopes, moderately eroded","Ellsworth",3,0.43,"HEL"]
["Portage","ElE2","Ellsworth silt loam, 18 to 40 percent slopes, moderately eroded","Ellsworth",3,0.43,"HEL"]
["Portage","EsB","Ellsworth silt loam, sandstone substratum, 2 to 6 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Portage","EuB","Ellsworth-Urban land complex, undulating","Ellsworth",3,0.43,"PHEL"]
["Portage","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Portage","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Portage","FnA","Fitchville-Urban land complex, nearly level","Fitchville",5,0.37,"NHEL"]
["Portage","Fr","Frenchtown silt loam","Frenchtown",3,0.37,"NHEL"]
["Portage","GbB","Geeburg silt loam, 2 to 6 percent slopes","Geeburg",3,0.43,"PHEL"]
["Portage","GbB2","Geeburg silt loam, 2 to 6 percent slopes, moderately eroded","Geeburg",3,0.43,"PHEL"]
["Portage","GbC2","Geeburg silt loam, 6 to 12 percent slopes, moderately eroded","Geeburg",3,0.43,"PHEL"]
["Portage","GbD2","Geeburg silt loam, 12 to 18 percent slopes, moderately eroded","Geeburg",3,0.43,"HEL"]
["Portage","GcB","Geeburg-Urban land complex, undulating","Geeburg",3,0.43,"PHEL"]
["Portage","GeF","Geeburg and Glenford silt loams, steep","Geeburg",3,0.43,"HEL"]
["Portage","GfA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Portage","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Portage","GfC2","Glenford silt loam, 6 to 12 percent slopes, moderately eroded","Glenford",5,0.37,"PHEL"]
["Portage","GfD2","Glenford silt loam, 12 to 18 percent slopes, moderately eroded","Glenford",5,0.37,"HEL"]
["Portage","Gp","Gravel Pits","Gravel"]
["Portage","HaB","Haskins loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Portage","Ho","Holly silt loam","Holly",5,0.28000000000000003,"NHEL"]
["Portage","HrB","Hornell silt loam, 3 to 8 percent slopes","Hornell",3,0.43,"PHEL"]
["Portage","JtA","Jimtown loam, 0 to 2 percent slopes","Jimtown",4,0.32,"NHEL"]
["Portage","JtB","Jimtown loam, 2 to 6 percent slopes","Jimtown",4,0.32,"PHEL"]
["Portage","LaB","Lakin loamy sand, 2 to 6 percent slopes","Lakin",5,0.17,"NHEL"]
["Portage","LaC","Lakin loamy sand, 6 to 12 percent slopes","Lakin",5,0.17,"PHEL"]
["Portage","Ld","Linwood muck","Linwood",2,null,"NHEL"]
["Portage","Ln","Lorain silty clay loam","Lorain",5,0.32,"NHEL"]
["Portage","LoB","Loudonville silt loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Portage","LoC","Loudonville silt loam, 6 to 12 percent slopes","Loudonville",4,0.32,"PHEL"]
["Portage","LoC2","Loudonville silt loam, 6 to 12 percent slopes, moderately eroded","Loudonville",4,0.32,"PHEL"]
["Portage","LoD2","Loudonville silt loam, 12 to 18 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Portage","LoE","Loudonville silt loam, 18 to 25 percent slopes","Loudonville",4,0.32,"HEL"]
["Portage","MgA","Mahoning silt loam, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Portage","MgB","Mahoning silt loam, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Portage","MnB","Mahoning-Urban land complex, undulating","Mahoning",3,0.43,"PHEL"]
["Portage","MtA","Mitiwanga silt loam, 0 to 2 percent slopes","Mitiwanga",4,0.32,"NHEL"]
["Portage","MtB","Mitiwanga silt loam, 2 to 6 percent slopes","Mitiwanga",4,0.32,"PHEL"]
["Portage","MvB","Mitiwanga silt loam, moderately well drained variant, 2 to 6 percent slopes","Mitiwanga",4,0.32,"PHEL"]
["Portage","MvC","Mitiwanga silt loam, moderately well drained variant, 6 to 12 percent slopes","Mitiwanga",4,0.32,"PHEL"]
["Portage","Od","Olmsted loam","Olmstead",5,0.24,"NHEL"]
["Portage","Or","Orrville silt loam","Orrville",5,0.37,"NHEL"]
["Portage","OsB","Oshtemo sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Portage","OsC","Oshtemo sandy loam, 6 to 12 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Portage","Qu","Quarries","Quarries"]
["Portage","ReA","Ravenna silt loam, 0 to 2 percent slopes","Ravenna",3,0.37,"NHEL"]
["Portage","ReB","Ravenna silt loam, 2 to 6 percent slopes","Ravenna",3,0.37,"PHEL"]
["Portage","RmA","Remsen silt loam, 0 to 2 percent slopes","Remsen",3,0.43,"NHEL"]
["Portage","RmB","Remsen silt loam, 2 to 6 percent slopes","Remsen",3,0.43,"PHEL"]
["Portage","RsB","Rittman silt loam, 2 to 6 percent slopes","Rittman",4,0.43,"PHEL"]
["Portage","RsC","Rittman silt loam, 6 to 12 percent slopes","Rittman",4,0.43,"PHEL"]
["Portage","RsC2","Rittman silt loam, 6 to 12 percent slopes, moderately eroded","Rittman",4,0.43,"PHEL"]
["Portage","RsD2","Rittman silt loam, 12 to 18 percent slopes, moderately eroded","Rittman",4,0.43,"HEL"]
["Portage","RsE2","Rittman silt loam, 18 to 25 percent slopes, moderately eroded","Rittman",4,0.43,"HEL"]
["Portage","Sb","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Portage","Sv","Sebring silt loam, dark surface variant","Sebring",5,0.37,"NHEL"]
["Portage","Tg","Tioga loam","Tioga",5,0.37,"NHEL"]
["Portage","TrA","Trumbull silt loam, 0 to 2 percent slopes","Trumbull",3,0.37,"NHEL"]
["Portage","TuB","Typic Udorthents, strip mined, undulating","Udorthents"]
["Portage","TuD","Typic Udorthents, strip mined, hilly","Udorthents"]
["Portage","Ur","Urban land","Urban"]
["Portage","W","Water","Water"]
["Portage","WaA","Wadsworth silt loam, 0 to 2 percent slopes","Wadsworth",4,0.43,"NHEL"]
["Portage","WaB","Wadsworth silt loam, 2 to 6 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Portage","Wc","Wallkill silt loam","Wallkill",5,0.32,"NHEL"]
["Portage","WhA","Wheeling silt loam, 0 to 2 percent slopes","Wheeling",4,0.37,"NHEL"]
["Portage","WhB","Wheeling silt loam, 2 to 6 percent slopes","Wheeling",4,0.37,"PHEL"]
["Portage","WuB","Wooster silt loam, 2 to 6 percent slopes","Wooster",4,0.37,"PHEL"]
["Portage","WuC","Wooster silt loam, 6 to 12 percent slopes","Wooster",4,0.37,"PHEL"]
["Portage","WuC2","Wooster silt loam, 6 to 12 percent slopes, moderately eroded","Wooster",4,0.37,"PHEL"]
["Portage","WuD2","Wooster silt loam, 12 to 18 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
["Portage","WuE2","Wooster silt loam, 18 to 50 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
[null,"Select","none","none"]
["Richland","AdB","Alexandria silt loam, 2 to 6 percent slopes","Alexandria",4,0.37,"PHEL"]
["Richland","AdC","Alexandria silt loam, 6 to 12 percent slopes","Alexandria",4,0.37,"HEL"]
["Richland","AdC2","Alexandria silt loam, 6 to 12 percent slopes, moderately eroded","Alexandria",4,0.37,"HEL"]
["Richland","AdD","Alexandria silt loam, 12 to 18 percent slopes","Alexandria",4,0.37,"HEL"]
["Richland","AdD2","Alexandria silt loam, 12 to 18 percent slopes, moderately eroded","Alexandria",4,0.37,"HEL"]
["Richland","AdE","Alexandria silt loam, 18 to 25 percent slopes","Alexandria",4,0.37,"HEL"]
["Richland","AdE2","Alexandria silt loam, 18 to 25 percent slopes, moderately eroded","Alexandria",4,0.37,"HEL"]
["Richland","AdF","Alexandria silt loam, 25 to 40 percent slopes","Alexandria",4,0.37,"HEL"]
["Richland","AeD3","Alexandria silty clay loam, 12 to 18 percent slopes, severely eroded","Alexandria",4,0.37,"HEL"]
["Richland","Ag","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Richland","BeB","Belmore loam, 2 to 6 percent slopes","Belmore",4,0.32,"PHEL"]
["Richland","BeC","Belmore loam, 6 to 12 percent slopes","Belmore",4,0.32,"PHEL"]
["Richland","BeD","Belmore loam, 12 to 18 percent slopes","Belmore",4,0.32,"HEL"]
["Richland","BnA","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Richland","BnB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Richland","BnB2","Bennington silt loam, 2 to 6 percent slopes, moderately eroded","Bennington",3,0.43,"HEL"]
["Richland","BpB","Bennington-Fitchville silt loams, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Richland","BrB","Berks channery silt loam, 2 to 6 percent slopes","Berks",3,0.24,"PHEL"]
["Richland","BrC","Berks channery silt loam, 6 to 12 percent slopes","Berks",3,0.24,"PHEL"]
["Richland","BrD","Berks channery silt loam, 12 to 18 percent slopes","Berks",3,0.24,"HEL"]
["Richland","BsF","Berks-Rock outcrop complex, steep","Berks",3,0.24,"HEL"]
["Richland","BtA","Bogart loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Richland","BtB","Bogart loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Richland","BvA","Bogart silt loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Richland","BvB","Bogart silt loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Richland","CdB","Canfield silt loam, 2 to 6 percent slopes","Canfield",4,0.37,"PHEL"]
["Richland","CdB2","Canfield silt loam, 2 to 6 percent slopes, moderately eroded","Canfield",4,0.37,"PHEL"]
["Richland","CdC","Canfield silt loam, 6 to 12 percent slopes","Canfield",4,0.37,"HEL"]
["Richland","CdC2","Canfield silt loam, 6 to 12 percent slopes, moderately eroded","Canfield",4,0.37,"HEL"]
["Richland","CgB","Cardington silt loam, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Richland","CgB2","Cardington silt loam, 2 to 6 percent slopes, moderately eroded","Cardington",4,0.37,"PHEL"]
["Richland","CgC","Cardington silt loam, 6 to 12 percent slopes","Cardington",4,0.37,"HEL"]
["Richland","CgC2","Cardington silt loam, 6 to 12 percent slopes, moderately eroded","Cardington",4,0.37,"HEL"]
["Richland","ChC3","Cardington silty clay loam, 6 to 12 percent slopes, severely eroded","Cardington",4,0.37,"HEL"]
["Richland","Ck","Carlisle muck","Carlisle",2,null,"NHEL"]
["Richland","CnB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Richland","CnC","Chili loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Richland","CoD","Chili and Conotton soils, 12 to 18 percent slopes","Chili",4,0.24,"HEL"]
["Richland","CoD3","Chili and Conotton soils, 12 to 18 percent slopes, severely eroded","Chili",3,0.24,"HEL"]
["Richland","CoE","Chili and Conotton soils, 18 to 25 percent slopes","Chili",4,0.24,"HEL"]
["Richland","CoF","Chili and Conotton soils, 25 to 40 percent slopes","Chili",4,0.24,"HEL"]
["Richland","Cr","Condit silt loam","Condit",5,0.37,"NHEL"]
["Richland","CtC","Conotton gravelly loam, 2 to 12 percent slopes","Conotton",3,0.24,"PHEL"]
["Richland","Cz","Cut and fill land","Cut"]
["Richland","DmB","Digby loam, 1 to 4 percent slopes","Digby",4,0.32,"PHEL"]
["Richland","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Richland","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Richland","FdA","Fitchville-Bennington silt loams, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Richland","FgA","Fitchville silt loam, gravelly subsoil variant, 0 to 2 percent slopes","Fitchville",4,0.37,"NHEL"]
["Richland","FgB","Fitchville silt loam, gravelly subsoil variant, 2 to 6 percent slopes","Fitchville",4,0.37,"PHEL"]
["Richland","Fr","Frenchtown silt loam","Frenchtown",3,0.37,"NHEL"]
["Richland","GfA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Richland","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Richland","GfC","Glenford silt loam, 6 to 12 percent slopes","Glenford",5,0.37,"HEL"]
["Richland","Gp","Gravel Pits","Gravel"]
["Richland","GrB","Gresham silt loam, 2 to 6 percent slopes","Gresham",4,0.37,"PHEL"]
["Richland","HaB","Haney loam, 2 to 6 percent slopes","Haney",4,0.32,"PHEL"]
["Richland","HfB","Hanover silt loam, 2 to 6 percent slopes","Hanover",5,0.37,"PHEL"]
["Richland","HfC","Hanover silt loam, 6 to 12 percent slopes","Hanover",5,0.37,"HEL"]
["Richland","HfC2","Hanover silt loam, 6 to 12 percent slopes, moderately eroded","Hanover",5,0.37,"HEL"]
["Richland","HfC3","Hanover silt loam, 6 to 12 percent slopes, severely eroded","Hanover",4,0.37,"HEL"]
["Richland","HfD","Hanover silt loam, 12 to 18 percent slopes","Hanover",5,0.37,"HEL"]
["Richland","HfD2","Hanover silt loam, 12 to 18 percent slopes, moderately eroded","Hanover",5,0.37,"HEL"]
["Richland","HfE","Hanover silt loam, 18 to 25 percent slopes","Hanover",5,0.37,"HEL"]
["Richland","Ho","Holly silt loam","Holly",5,0.28000000000000003,"NHEL"]
["Richland","La","Landes fine sandy loam","Landes",5,0.2,"NHEL"]
["Richland","LfB","Latham silt loam, 2 to 6 percent slopes","Latham",3,0.43,"PHEL"]
["Richland","LfC","Latham silt loam, 6 to 12 percent slopes","Latham",3,0.43,"HEL"]
["Richland","Lk","Linwood muck","Linwood",2,null,"NHEL"]
["Richland","Lo","Lobdell silt loam","Lobdell",5,0.37,"NHEL"]
["Richland","LrB","Lordstown silt loam, 2 to 6 percent slopes","Lordstown",3,0.28000000000000003,"PHEL"]
["Richland","LrC","Lordstown silt loam, 6 to 12 percent slopes","Lordstown",3,0.28000000000000003,"PHEL"]
["Richland","LrD","Lordstown silt loam, 12 to 18 percent slopes","Lordstown",3,0.28000000000000003,"HEL"]
["Richland","LtE","Lordstown and Loudonville silt loams, 18 to 25 percent slopes","Lordstown",3,0.28000000000000003,"HEL"]
["Richland","LtF","Lordstown and Loudonville silt loams, 25 to 40 percent slopes","Lordstown",3,0.28000000000000003,"HEL"]
["Richland","LvB","Loudonville silt loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Richland","LvC","Loudonville silt loam, 6 to 12 percent slopes","Loudonville",4,0.32,"PHEL"]
["Richland","LvD","Loudonville silt loam, 12 to 18 percent slopes","Loudonville",4,0.32,"HEL"]
["Richland","Ly","Luray silty clay loam","Luray",5,0.32,"NHEL"]
["Richland","MeB","Mentor silt loam, 2 to 6 percent slopes","Mentor",5,0.37,"PHEL"]
["Richland","MeC","Mentor silt loam, 6 to 12 percent slopes","Mentor",5,0.37,"HEL"]
["Richland","Or","Orrville loam, moderately shallow variant","Orrville",4,0.32,"NHEL"]
["Richland","Pa","Pewamo silt loam","Pewamo",5,0.24,"NHEL"]
["Richland","Pc","Pewamo silt loam, overwash","Pewamo",5,0.24,"NHEL"]
["Richland","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Richland","Qu","Quarry","Quarry"]
["Richland","ReA","Ravenna silt loam, 0 to 2 percent slopes","Ravenna",3,0.37,"NHEL"]
["Richland","ReB","Ravenna silt loam, 2 to 6 percent slopes","Ravenna",3,0.37,"PHEL"]
["Richland","RsB","Rittman silt loam, 2 to 6 percent slopes","Rittman",4,0.43,"PHEL"]
["Richland","RsB2","Rittman silt loam, 2 to 6 percent slopes, moderately eroded","Rittman",4,0.43,"PHEL"]
["Richland","RsC","Rittman silt loam, 6 to 12 percent slopes","Rittman",4,0.43,"HEL"]
["Richland","RsC2","Rittman silt loam, 6 to 12 percent slopes, moderately eroded","Rittman",4,0.43,"HEL"]
["Richland","RsD","Rittman silt loam, 12 to 18 percent slopes","Rittman",4,0.43,"HEL"]
["Richland","RsD2","Rittman silt loam, 12 to 18 percent slopes, moderately eroded","Rittman",4,0.43,"HEL"]
["Richland","RtC3","Rittman silty clay loam, 6 to 12 percent slopes, severely eroded","Rittman",3,0.43,"HEL"]
["Richland","RtD3","Rittman silty clay loam, 12 to 18 percent slopes, severely eroded","Rittman",3,0.43,"HEL"]
["Richland","SaC","Schaffenaker loamy sand, 2 to 12 percent slopes","Schaffenaker",3,0.17,"PHEL"]
["Richland","SaD","Schaffenaker loamy sand, 12 to 18 percent slopes","Schaffenaker",3,0.17,"HEL"]
["Richland","SaE","Schaffenaker loamy sand, 18 to 40 percent slopes","Schaffenaker",3,0.17,"HEL"]
["Richland","Se","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Richland","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Richland","Sk","Shoals loam, coarse subsoil variant","Shoals",2,0.32,"NHEL"]
["Richland","So","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Richland","TmA","Tiro silt loam, 0 to 2 percent slopes","Tiro",4,0.37,"NHEL"]
["Richland","TmB","Tiro silt loam, 2 to 6 percent slopes","Tiro",4,0.37,"PHEL"]
["Richland","TvB","Titusville silt loam, 2 to 6 percent slopes","Titusville",4,0.37,"PHEL"]
["Richland","TvC","Titusville silt loam, 6 to 12 percent slopes","Titusville",4,0.37,"HEL"]
["Richland","Ur","Urban land","Urban"]
["Richland","W","Water","Water"]
["Richland","WaA","Wadsworth silt loam, 0 to 2 percent slopes","Wadsworth",4,0.43,"NHEL"]
["Richland","WaB","Wadsworth silt loam, 2 to 6 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Richland","Wc","Wallkill silt loam","Wallkill",5,0.32,"NHEL"]
["Richland","WhA","Wheeling silt loam, 0 to 2 percent slopes","Wheeling",4,0.37,"NHEL"]
["Richland","WhB","Wheeling silt loam, 2 to 6 percent slopes","Wheeling",4,0.37,"PHEL"]
["Richland","WhC","Wheeling silt loam, 6 to 12 percent slopes","Wheeling",4,0.37,"PHEL"]
["Richland","WmD","Wheeling and Mentor silt loams, 12 to 18 percent slopes","Wheeling",4,0.37,"HEL"]
["Richland","WsB","Wooster silt loam, 2 to 6 percent slopes","Wooster",4,0.37,"PHEL"]
["Richland","WsB2","Wooster silt loam, 2 to 6 percent slopes, moderately eroded","Wooster",4,0.37,"PHEL"]
["Richland","WsC","Wooster silt loam, 6 to 12 percent slopes","Wooster",4,0.37,"HEL"]
["Richland","WsC2","Wooster silt loam, 6 to 12 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
["Richland","WsD","Wooster silt loam, 12 to 18 percent slopes","Wooster",4,0.37,"HEL"]
["Richland","WsD2","Wooster silt loam, 12 to 18 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
["Richland","WsD3","Wooster silt loam, 12 to 18 percent slopes, severely eroded","Wooster",4,0.37,"HEL"]
["Richland","WsE","Wooster silt loam, 18 to 25 percent slopes","Wooster",4,0.37,"HEL"]
["Richland","WsE3","Wooster silt loam, 18 to 40 percent slopes, severely eroded","Wooster",4,0.37,"HEL"]
["Richland","WsF","Wooster silt loam, 25 to 40 percent slopes","Wooster",4,0.37,"HEL"]
["Richland","WtB","Wooster-Chili soils, 2 to 6 percent slopes","Wooster",4,0.37,"PHEL"]
["Richland","WtC","Wooster-Chili soils, 6 to 12 percent slopes","Wooster",4,0.37,"PHEL"]
[null,"Select","none","none"]
["Stark","Ad","Alluvial land","Alluvial",null,null,"NHEL"]
["Stark","An","Alluvial land-Urban land complex","Alluvial",null,null,"NHEL"]
["Stark","ArB","Arkport fine sandy loam, 0 to 6 percent slopes","Arkport",3,0.17,"PHEL"]
["Stark","ArC","Arkport fine sandy loam, 6 to 12 percent slopes","Arkport",3,0.17,"PHEL"]
["Stark","ArD","Arkport fine sandy loam, 12 to 18 percent slopes","Arkport",3,0.17,"HEL"]
["Stark","BgA","Bogart loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Stark","BgB","Bogart loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Stark","BoA","Bogart silt loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Stark","BoB","Bogart silt loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Stark","BoC","Bogart silt loam, 6 to 12 percent slopes","Bogart",5,0.32,"PHEL"]
["Stark","Bu","Bogart-Urban land complex","Bogart",5,0.32,"PHEL"]
["Stark","Bv","Borrow pits","Borrow"]
["Stark","BwC2","Brooke silty clay loam, 4 to 12 percent slopes, moderately eroded","Brooke",3,0.37,"PHEL"]
["Stark","BwE2","Brooke silty clay loam, 12 to 25 percent slopes, moderately eroded","Brooke",3,0.37,"HEL"]
["Stark","Ca","Canadice silt loam","Canadice",5,0.49,"NHEL"]
["Stark","CdA","Canfield silt loam, 0 to 2 percent slopes","Canfield",4,0.37,"NHEL"]
["Stark","CdB","Canfield silt loam, 2 to 6 percent slopes","Canfield",4,0.37,"PHEL"]
["Stark","CdC","Canfield silt loam, 6 to 12 percent slopes","Canfield",4,0.37,"PHEL"]
["Stark","CdC2","Canfield silt loam, 6 to 12 percent slopes, moderately eroded","Canfield",4,0.37,"PHEL"]
["Stark","CdD","Canfield silt loam, 12 to 18 percent slopes","Canfield",4,0.37,"HEL"]
["Stark","CdD2","Canfield silt loam, 12 to 18 percent slopes, moderately eroded","Canfield",4,0.37,"HEL"]
["Stark","CeB","Canfield-Urban land complex, undulating","Canfield",4,0.37,"PHEL"]
["Stark","CeC","Canfield-Urban land complex, rolling","Canfield",4,0.37,"PHEL"]
["Stark","CfB","Canfield silt loam, moderately shallow variant, 2 to 6 percent slopes","Canfield",3,0.37,"PHEL"]
["Stark","CfC","Canfield silt loam, moderately shallow variant, 6 to 12 percent slopes","Canfield",3,0.37,"PHEL"]
["Stark","Ch","Carlisle muck","Carlisle",2,null,"NHEL"]
["Stark","Ck","Chagrin loam, alkaline phase","Chagrin",5,0.32,"NHEL"]
["Stark","Cm","Chagrin silt loam, alkaline phase","Chagrin",5,0.32,"NHEL"]
["Stark","CnA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Stark","CnB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Stark","CoC","Chili gravelly loam, 6 to 12 percent slopes","Chili",4,0.24,"PHEL"]
["Stark","CoC2","Chili gravelly loam, 6 to 12 percent slopes, moderately eroded","Chili",4,0.24,"PHEL"]
["Stark","CoD2","Chili gravelly loam, 12 to 18 percent slopes, moderately eroded","Chili",4,0.24,"HEL"]
["Stark","CoE2","Chili gravelly loam, 18 to 25 percent slopes, moderately eroded","Chili",4,0.24,"HEL"]
["Stark","CpA","Chili silt loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Stark","CpB","Chili silt loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Stark","CpC","Chili silt loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Stark","CpC2","Chili silt loam, 6 to 12 percent slopes, moderately eroded","Chili",4,0.32,"PHEL"]
["Stark","CuB","Chili-Urban land complex, undulating","Chili",4,0.32,"PHEL"]
["Stark","CuC","Chili-Urban land complex, rolling","Chili",4,0.32,"PHEL"]
["Stark","CuF","Chili-Urban land complex, steep","Chili",4,0.32,"HEL"]
["Stark","CvF2","Chili and Conotton gravelly loams, 25 to 50 percent slopes, moderately eroded","Chili",4,0.24,"HEL"]
["Stark","CwA","Conotton loam, 0 to 2 percent slopes","Conotton",3,0.24,"NHEL"]
["Stark","CyB","Conotton gravelly loam, 2 to 6 percent slopes","Conotton",3,0.24,"PHEL"]
["Stark","CyC","Conotton gravelly loam, 6 to 12 percent slopes","Conotton",3,0.24,"PHEL"]
["Stark","CyD2","Conotton gravelly loam, 12 to 18 percent slopes, moderately eroded","Conotton",3,0.24,"HEL"]
["Stark","CyE2","Conotton gravelly loam, 18 to 25 percent slopes, moderately eroded","Conotton",3,0.24,"HEL"]
["Stark","Cz","Cut and Fill land","Cut"]
["Stark","DkB","Dekalb sandy loam, 2 to 6 percent slopes","Dekalb",2,0.24,"PHEL"]
["Stark","DkC","Dekalb sandy loam, 6 to 12 percent slopes","Dekalb",2,0.24,"PHEL"]
["Stark","DkE2","Dekalb sandy loam, 12 to 25 percent slopes, moderately eroded","Dekalb",2,0.24,"HEL"]
["Stark","DkF2","Dekalb sandy loam, 25 to 50 percent slopes, moderately eroded","Dekalb",2,0.24,"HEL"]
["Stark","Ed","Edwards muck","Edwards",2,null,"NHEL"]
["Stark","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Stark","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Stark","FcC","Fitchville silt loam, 6 to 12 percent slopes","Fitchville",5,0.37,"PHEL"]
["Stark","Fu","Fitchville-Urban land complex","Fitchville",5,0.37,"PHEL"]
["Stark","GbC2","Geeburg silt loam, 6 to 12 percent slopes, moderately eroded","Geeburg",3,0.43,"PHEL"]
["Stark","GbE2","Geeburg silt loam, 12 to 25 percent, moderately eroded","Geeburg",3,0.43,"HEL"]
["Stark","GdB","Gilpin silt loam, 2 to 6 percent slopes","Gilpin",3,0.32,"PHEL"]
["Stark","GdC","Gilpin silt loam, 6 to 12 percent slopes","Gilpin",3,0.32,"PHEL"]
["Stark","GdD","Gilpin silt loam, 12 to 18 percent slopes","Gilpin",3,0.32,"HEL"]
["Stark","Ge","Ginat silt loam","Ginat",4,0.43,"NHEL"]
["Stark","GfA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Stark","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Stark","GfC","Glenford silt loam, 6 to 12 percent slopes","Glenford",5,0.37,"PHEL"]
["Stark","GfC2","Glenford silt loam, 6 to 12 percent slopes, moderately eroded","Glenford",5,0.37,"PHEL"]
["Stark","GfD2","Glenford silt loam, 12 to 18 percent slopes, moderately eroded","Glenford",5,0.37,"HEL"]
["Stark","Gp","Gravel Pits","Gravel"]
["Stark","KeB","Keene silt loam, 2 to 6 percent slopes","Keene",4,0.37,"PHEL"]
["Stark","KeC","Keene silt loam, 6 to 12 percent slopes","Keene",4,0.37,"PHEL"]
["Stark","KeC2","Keene silt loam, 6 to 12 percent slopes, moderately eroded","Keene",4,0.37,"PHEL"]
["Stark","KeD","Keene silt loam, 12 to 18 percent slopes","Keene",4,0.37,"HEL"]
["Stark","KeD2","Keene silt loam, 12 to 18 percent slopes, moderately eroded","Keene",4,0.37,"HEL"]
["Stark","KeE","Keene silt loam, 18 to 25 percent slopes","Keene",4,0.37,"HEL"]
["Stark","Kk","Killbuck silt loam","Killbuck",5,0.37,"NHEL"]
["Stark","LaB","Latham silt loam, 2 to 6 percent slopes","Latham",3,0.43,"PHEL"]
["Stark","LaC","Latham silt loam, 6 to 12 percent slopes","Latham",3,0.43,"PHEL"]
["Stark","LaC2","Latham silt loam, 6 to 12 percent slopes, moderately eroded","Latham",3,0.43,"PHEL"]
["Stark","LaD","Latham silt loam, 12 to 18 percent slopes","Latham",3,0.43,"HEL"]
["Stark","LaD2","Latham silt loam, 12 to 18 percent slopes, moderately eroded","Latham",3,0.43,"HEL"]
["Stark","LaF","Latham silt loam, 18 to 35 percent slopes","Latham",3,0.43,"HEL"]
["Stark","LcA","Licking silt loam, 0 to 2 percent slopes","Licking",3,0.43,"NHEL"]
["Stark","LcB","Licking silt loam, 2 to 6 percent slopes","Licking",3,0.43,"PHEL"]
["Stark","LcC","Licking silt loam, 6 to 12 percent slopes","Licking",3,0.43,"PHEL"]
["Stark","LcC2","Licking silt loam, 6 to 12 percent slopes, moderately eroded","Licking",3,0.43,"PHEL"]
["Stark","LcE2","Licking silt loam, 12 to 25 percent slopes, moderately eroded","Licking",3,0.43,"HEL"]
["Stark","Ld","Linwood muck","Linwood",2,null,"NHEL"]
["Stark","Le","Lobdell silt loam, alkaline phase","Lobdell",5,0.37,"NHEL"]
["Stark","LoB","Loudonville silt loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Stark","LoC","Loudonville silt loam, 6 to 12 percent slopes","Loudonville",4,0.32,"PHEL"]
["Stark","LoC2","Loudonville silt loam, 6 to 12 percent slopes, moderately eroded","Loudonville",4,0.32,"PHEL"]
["Stark","LoD","Loudonville silt loam, 12 to 18 percent slopes","Loudonville",4,0.32,"HEL"]
["Stark","LoD2","Loudonville silt loam, 12 to 18 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Stark","LoE2","Loudonville silt loam, 18 to 25 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Stark","LoF2","Loudonville silt loam, 25 to 35 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Stark","LuB","Loudonville-Urban land complex, undulating","Loudonville",4,0.32,"PHEL"]
["Stark","LuC","Loudonville-Urban land complex, rolling","Loudonville",4,0.32,"PHEL"]
["Stark","Ly","Luray silt loam","Luray",5,0.32,"NHEL"]
["Stark","Lz","Luray silt loam, gravelly subsoil variant","Luray",5,0.32,"NHEL"]
["Stark","Ma","Made land","Made"]
["Stark","MeA","Mentor silt loam, 0 to 2 percent slopes","Mentor",5,0.37,"NHEL"]
["Stark","MeB","Mentor silt loam, 2 to 6 percent slopes","Mentor",5,0.37,"PHEL"]
["Stark","MeC","Mentor silt loam, 6 to 12 percent slopes","Mentor",5,0.37,"PHEL"]
["Stark","MeD","Mentor silt loam, 12 to 18 percent slopes","Mentor",5,0.37,"HEL"]
["Stark","Mg","Montgomery silty clay loam","Montgomery",5,0.37,"NHEL"]
["Stark","MsB","Muskingum silt loam, 2 to 6 percent slopes","Muskingum",3,0.37,"PHEL"]
["Stark","MsC","Muskingum silt loam, 6 to 12 percent slopes","Muskingum",3,0.37,"PHEL"]
["Stark","MsD","Muskingum silt loam, 12 to 18 percent slopes","Muskingum",3,0.37,"HEL"]
["Stark","MvE","Muskingum and Gilpin silt loams, 18 to 25 percent slopes","Muskingum",3,0.37,"HEL"]
["Stark","MvE3","Muskingum and Gilpin silt loams, 18 to 25 percent slopes, severely eroded","Muskingum",3,0.37,"HEL"]
["Stark","MvF","Muskingum and Gilpin silt loams, 25 to 35 percent slopes","Muskingum",3,0.37,"HEL"]
["Stark","MvG","Muskingum and Gilpin silt loams, 35 to 50 percent slopes","Muskingum",3,0.37,"HEL"]
["Stark","MwF","Muskingum and Gilpin-Urban land complex, steep","Muskingum",3,0.37,"HEL"]
["Stark","PlB","Plainfield loamy sand, 0 to 6 percent slopes","Plainfield",5,0.17,"PHEL"]
["Stark","PlC","Plainfield loamy sand, 6 to 12 percent slopes","Plainfield",5,0.17,"PHEL"]
["Stark","Qu","Quarries","Quarries"]
["Stark","RaB","Rainsboro silt loam, 2 to 6 percent slopes","Rainsboro",4,0.43,"PHEL"]
["Stark","RaC","Rainsboro silt loam, 6 to 12 percent slopes","Rainsboro",4,0.43,"PHEL"]
["Stark","RcC","Ramsey channery sandy loam, 6 to 12 percent slopes","Ramsey",1,0.24,"HEL"]
["Stark","RcD","Ramsey channery sandy loam, 12 to 18 percent slopes","Ramsey",1,0.24,"HEL"]
["Stark","RcE2","Ramsey channery sandy loam, 18 to 25 percent slopes, moderately eroded","Ramsey",1,0.24,"HEL"]
["Stark","RcF2","Ramsey channery sandy loam, 25 to 50 percent slopes, moderately eroded","Ramsey",1,0.24,"HEL"]
["Stark","ReA","Ravenna silt loam, 0 to 2 percent slopes","Ravenna",3,0.37,"NHEL"]
["Stark","ReB","Ravenna silt loam, 2 to 6 percent slopes","Ravenna",3,0.37,"PHEL"]
["Stark","Rn","Ravenna-Urban land complex","Ravenna",3,0.37,"PHEL"]
["Stark","RoA","Remsen silt loam, 0 to 2 percent slopes","Remsen",3,0.43,"NHEL"]
["Stark","RoB","Remsen silt loam, 2 to 6 percent slopes","Remsen",3,0.43,"PHEL"]
["Stark","Rr","Remsen-Urban land complex","Remsen",3,0.43,"PHEL"]
["Stark","RsB","Rittman silt loam, 2 to 6 percent slopes","Rittman",4,0.43,"PHEL"]
["Stark","RsC","Rittman silt loam, 6 to 12 percent slopes","Rittman",4,0.43,"PHEL"]
["Stark","RsC2","Rittman silt loam, 6 to 12 percent slopes, moderately eroded","Rittman",4,0.43,"PHEL"]
["Stark","RsD2","Rittman silt loam, 12 to 18 percent slopes, moderately eroded","Rittman",4,0.43,"HEL"]
["Stark","Sb","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Stark","Se","Sebring silt loam, till substratum","Sebring",5,0.37,"NHEL"]
["Stark","Sg","Sebring-Urban land complex","Sebring",5,0.37,"NHEL"]
["Stark","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Stark","Sl","Sloan silt loam","Sloan",5,0.37,"NHEL"]
["Stark","SoC","Strip mine spoil, sandstone and shale materials, undulating","Strip Mine"]
["Stark","SoE","Strip mine spoil, sandstone and shale materials, rolling","Strip Mine"]
["Stark","SoF","Strip mine spoil, sandstone and shale materials, steep","Strip Mine"]
["Stark","SsC","Strip mine spoil, acid clay shale materials, undulating","Strip Mine"]
["Stark","SsE","Strip mine spoil, acid clay shale materials, rolling","Strip Mine"]
["Stark","SsF","Strip mine spoil, acid clay shale materials, steep","Strip Mine"]
["Stark","StC","Strip mine spoil, nonacid materials, undulating","Strip Mine"]
["Stark","StD","Strip mine spoil, nonacid materials, rolling","Strip Mine"]
["Stark","StF","Strip mine spoil, nonacid materials, steep","Strip Mine"]
["Stark","TlC","Tilsit silt loam, 6 to 12 percent slopes","Tilsit",3,0.43,"PHEL"]
["Stark","TlD","Tilsit silt loam, 12 to 18 percent slopes","Tilsit",3,0.43,"HEL"]
["Stark","Tr","Trumbull silt loam","Trumbull",3,0.37,"NHEL"]
["Stark","Ur","Urban land","Urban"]
["Stark","W","Water","Water"]
["Stark","WaA","Wadsworth silt loam, 0 to 2 percent slopes","Wadsworth",4,0.43,"NHEL"]
["Stark","WaB","Wadsworth silt loam, 2 to 6 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Stark","WaC","Wadsworth silt loam, 6 to 12 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Stark","WaC2","Wadsworth silt loam, 6 to 12 percent slopes, moderately eroded","Wadsworth",4,0.43,"PHEL"]
["Stark","WbB","Wadsworth silt loam, moderately shallow variant, 2 to 6 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Stark","Wc","Wallkill silt loam, clayey subsoil variant","Wallkill",5,0.28000000000000003,"NHEL"]
["Stark","Wd","Wayland silt loam","Wayland",5,0.43,"NHEL"]
["Stark","WeC","Weikert channery silt loam, 6 to 12 percent slopes","Weikert",2,0.28000000000000003,"PHEL"]
["Stark","WeD","Weikert channery silt loam, 12 to 18 percent slopes","Weikert",2,0.28000000000000003,"HEL"]
["Stark","WeE2","Weikert channery silt loam, 18 to 25 percent slopes, moderately eroded","Weikert",2,0.28000000000000003,"HEL"]
["Stark","WeF2","Weikert channery silt loam, 25 to 50 percent slopes, moderately eroded","Weikert",2,0.28000000000000003,"HEL"]
["Stark","WhA","Weinbach silt loam, 0 to 2 percent slopes","Weinbach",4,0.43,"NHEL"]
["Stark","WhB","Weinbach silt loam, 2 to 6 percent slopes","Weinbach",4,0.43,"PHEL"]
["Stark","Wk","Weinbach-Urban land complex","Weinbach",4,0.43,"NHEL"]
["Stark","WlB","Wellston silt loam, 2 to 6 percent slopes","Wellston",4,0.37,"PHEL"]
["Stark","WlC","Wellston silt loam, 6 to 12 percent slopes","Wellston",4,0.37,"PHEL"]
["Stark","WmA","Wheeling loam, 0 to 2 percent slopes","Wheeling",4,0.37,"NHEL"]
["Stark","WmB","Wheeling loam, 2 to 6 percent slopes","Wheeling",4,0.37,"PHEL"]
["Stark","WmC2","Wheeling loam, 6 to 12 percent slopes, moderately eroded","Wheeling",4,0.37,"PHEL"]
["Stark","WrA","Wheeling silt loam, 0 to 2 percent slopes","Wheeling",4,0.37,"NHEL"]
["Stark","WrB","Wheeling silt loam, 2 to 6 percent slopes","Wheeling",4,0.37,"PHEL"]
["Stark","WrC","Wheeling silt loam, 6 to 12 percent slopes","Wheeling",4,0.37,"PHEL"]
["Stark","WrC2","Wheeling silt loam, 6 to 12 percent slopes, moderately eroded","Wheeling",4,0.37,"PHEL"]
["Stark","WsD2","Wheeling soils, 12 to 18 percent slopes, moderately eroded","Wheeling",4,0.37,"HEL"]
["Stark","Wt","Willette muck","Willette",2,null,"NHEL"]
["Stark","WuB","Wooster silt loam, 2 to 6 percent slopes","Wooster",4,0.37,"PHEL"]
["Stark","WuC","Wooster silt loam, 6 to 12 percent slopes","Wooster",4,0.37,"PHEL"]
["Stark","WuC2","Wooster silt loam, 6 to 12 percent slopes, moderately eroded","Wooster",4,0.37,"PHEL"]
["Stark","WuD2","Wooster silt loam, 12 to 18 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
["Stark","WuE2","Wooster silt loam, 18 to 25 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
["Stark","WuF2","Wooster silt loam, 25 to 50 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
["Stark","WvD","Wooster-Urban land complex, steep","Wooster",4,0.37,"HEL"]
[null,"Select","none","none"]
["Summit","BeF","Berks channery silt loam, 25 to 70 percent slopes","Berks",3,0.24,"HEL"]
["Summit","BgA","Bogart loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Summit","BgB","Bogart loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Summit","BhB","Bogart-Haskins loams, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Summit","Bp","Borrow Pits","Borrow"]
["Summit","C.F.","Cut and fill land","Cut"]
["Summit","Ca","Canadice silty clay loam","Canadice",5,0.49,"NHEL"]
["Summit","CcA","Caneadea silt loam, 0 to 2 percent slopes","Caneadea",3,0.43,"NHEL"]
["Summit","CcB","Caneadea silt loam, 2 to 6 percent slopes","Caneadea",3,0.43,"PHEL"]
["Summit","CdA","Canfield silt loam, 0 to 2 percent slopes","Canfield",4,0.37,"NHEL"]
["Summit","CdB","Canfield silt loam, 2 to 6 percent slopes","Canfield",4,0.37,"PHEL"]
["Summit","CdC","Canfield silt loam, 6 to 12 percent slopes","Canfield",4,0.37,"PHEL"]
["Summit","CdC2","Canfield silt loam, 6 to 12 percent slopes, moderately eroded","Canfield",4,0.37,"PHEL"]
["Summit","CeB","Canfield silt loam, sandstone substratum, 2 to 6 percent slopes","Canfield",4,0.37,"PHEL"]
["Summit","CfB","Canfield-Urban land complex, undulating","Canfield",4,0.37,"PHEL"]
["Summit","CfC","Canfield-Urban land complex, rolling","Canfield",4,0.37,"PHEL"]
["Summit","Cg","Carlisle muck","Carlisle",2,null,"NHEL"]
["Summit","Ch","Chagrin silt loam","Chagrin",5,0.32,"NHEL"]
["Summit","Ck","Chagrin silt loam, alkaline","Chagrin",5,0.32,"NHEL"]
["Summit","Cm","Chagrin-Urban land complex","Chagrin",5,0.32,"NHEL"]
["Summit","CnA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Summit","CnB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Summit","CnC","Chili loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Summit","CoC2","Chili gravelly loam, 6 to 12 percent slopes, moderately eroded","Chili",4,0.24,"PHEL"]
["Summit","CoD2","Chili gravelly loam, 12 to 18 percent slopes, moderately eroded","Chili",4,0.24,"PHEL"]
["Summit","CpA","Chili silt loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Summit","CpB","Chili silt loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Summit","CpC","Chili silt loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Summit","CuB","Chili-Urban land complex, undulating","Chili",4,0.32,"PHEL"]
["Summit","CuC","Chili-Urban land complex, rolling","Chili",4,0.32,"PHEL"]
["Summit","CwC2","Chili-Wooster complex, 6 to 12 percent slopes, moderately eroded","Chili",4,0.32,"PHEL"]
["Summit","CwD2","Chili-Wooster complex, 12 to 18 percent slopes, moderately eroded","Chili",4,0.32,"HEL"]
["Summit","CwE2","Chili-Wooster complex, 18 to 25 percent slopes, moderately eroded","Chili",4,0.32,"HEL"]
["Summit","Cx","Clay pits and quarries","Clay"]
["Summit","CyD","Conotton-Oshtemo complex, 12 to 18 percent slopes","Conotton",3,0.24,"HEL"]
["Summit","CyE","Conotton-Oshtemo complex, 18 to 25 percent slopes","Conotton",3,0.24,"HEL"]
["Summit","CyF","Conotton-Oshtemo complex, 25 to 50 percent slopes","Conotton",3,0.24,"HEL"]
["Summit","Da","Damascus loam","damascus",5,0.32,"NHEL"]
["Summit","DkC","Dekalb sandy loam, 6 to 12 percent slopes","Dekalb",2,0.24,"PHEL"]
["Summit","DkD","Dekalb sandy loam, 12 to 18 percent slopes","Dekalb",2,0.24,"HEL"]
["Summit","DkE","Dekalb sandy loam, 18 to 25 percent slopes","Dekalb",2,0.24,"HEL"]
["Summit","DkF","Dekalb sandy loam, 25 to 70 percent slopes","Dekalb",2,0.24,"HEL"]
["Summit","ElB","Ellsworth silt loam, 2 to 6 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Summit","ElC","Ellsworth silt loam, 6 to 12 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Summit","ElC2","Ellsworth silt loam, 6 to 12 percent slopes, moderately eroded","Ellsworth",3,0.43,"PHEL"]
["Summit","ElE2","Ellsworth silt loam, 12 to 25 percent slopes, moderately eroded","Ellsworth",3,0.43,"HEL"]
["Summit","ElF2","Ellsworth silt loam, 25 to 50 percent slopes, moderately eroded","Ellsworth",3,0.43,"HEL"]
["Summit","EsB","Ellsworth silt loam, sandstone substratum, 2 to 6 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Summit","EsC","Ellsworth silt loam, sandstone substratum, 6 to 12 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Summit","EuB","Ellsworth-Urban land complex, undulating","Ellsworth",3,0.43,"PHEL"]
["Summit","EuC","Ellsworth-Urban land complex, rolling","Ellsworth",3,0.43,"HEL"]
["Summit","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Summit","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Summit","Fn","Fitchville-Urban land complex","Fitchville",5,0.37,"NHEL"]
["Summit","Fr","Frenchtown silt loam","Frenchtown",3,0.37,"NHEL"]
["Summit","GbB","Geeburg silt loam, 2 to 6 percent slopes","Geeburg",3,0.43,"PHEL"]
["Summit","GbC2","Geeburg silt loam, 6 to 12 percent slopes, moderately eroded","Geeburg",3,0.43,"PHEL"]
["Summit","GbD2","Geeburg silt loam, 12 to 18 percent slopes, moderately eroded","Geeburg",3,0.43,"HEL"]
["Summit","GfA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Summit","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Summit","GfC2","Glenford silt loam, 6 to 12 percent slopes, moderately eroded","Glenford",5,0.37,"PHEL"]
["Summit","GfD2","Glenford silt loam, 12 to 18 percent slopes, moderately eroded","Glenford",5,0.37,"HEL"]
["Summit","GoB","Glenford-Urban land complex, undulating","Glenford",5,0.37,"PHEL"]
["Summit","GoC","Glenford-Urban land complex, rolling","Glenford",5,0.37,"PHEL"]
["Summit","HcB","Haskins-Caneadea complex, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Summit","Ho","Holly silt loam","Holly",5,0.28000000000000003,"NHEL"]
["Summit","Hy","Holly silt loam, alkaline","Holly",5,0.28000000000000003,"NHEL"]
["Summit","JtA","Jimtown loam, 0 to 2 percent slopes","Jimtown",4,0.32,"NHEL"]
["Summit","JtB","Jimtown loam, 2 to 6 percent slopes","Jimtown",4,0.32,"PHEL"]
["Summit","Ju","Jimtown-Urban land complex","Jimtown",4,0.32]
["Summit","Ld","Linwood muck","Linwood",2,null,"NHEL"]
["Summit","Le","Lobdell silt loam","Lobdell",5,0.37,"NHEL"]
["Summit","Ln","Lorain silty clay loam","Lorain",5,0.32,"NHEL"]
["Summit","LoB","Loudonville silt loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Summit","LoC","Loudonville silt loam, 6 to 12 percent slopes","Loudonville",4,0.32,"PHEL"]
["Summit","LoC2","Loudonville silt loam, 6 to 12 percent slopes, moderately eroded","Loudonville",4,0.32,"PHEL"]
["Summit","LoD","Loudonville silt loam, 12 to 18 percent slopes","Loudonville",4,0.32,"HEL"]
["Summit","LoE","Loudonville silt loam, 18 to 25 percent slopes","Loudonville",4,0.32,"HEL"]
["Summit","LuC","Loudonville-Urban land complex, rolling","Loudonville",4,0.32,"PHEL"]
["Summit","Ly","Luray silt loam","Luray",5,0.32,"NHEL"]
["Summit","Ma","Made land, chemical waste","Made"]
["Summit","Md","Made land, sanitary fill","Made"]
["Summit","MgA","Mahoning silt loam, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Summit","MgB","Mahoning silt loam, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Summit","MlB","Mahoning silt loam, sandstone substratum, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Summit","Mn","Mahoning-Urban land complex","Mahoning",3,0.43,"PHEL"]
["Summit","MtB","Mitiwanga silt loam, 2 to 6 percent slopes","Mitiwanga",4,0.32,"PHEL"]
["Summit","Od","Olmsted loam","Olmstead",5,0.24,"NHEL"]
["Summit","Or","Orrville silt loam","Orrville",5,0.37,"NHEL"]
["Summit","OsA","Oshtemo sandy loam, 0 to 2 percent slopes","Oshtemo",5,0.24,"NHEL"]
["Summit","OsB","Oshtemo sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Summit","OsC","Oshtemo sandy loam, 6 to 12 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Summit","ReA","Ravenna silt loam, 0 to 2 percent slopes","Ravenna",3,0.37,"NHEL"]
["Summit","ReB","Ravenna silt loam, 2 to 6 percent slopes","Ravenna",3,0.37,"PHEL"]
["Summit","Rn","Ravenna-Urban land complex","Ravenna",3,0.37,"PHEL"]
["Summit","RsB","Rittman silt loam, 2 to 6 percent slopes","Rittman",4,0.43,"PHEL"]
["Summit","RsC","Rittman silt loam, 6 to 12 percent slopes","Rittman",4,0.43,"PHEL"]
["Summit","RsC2","Rittman silt loam, 6 to 12 percent slopes, moderately eroded","Rittman",4,0.43,"PHEL"]
["Summit","RsD","Rittman silt loam, 12 to 18 percent slopes","Rittman",4,0.43,"HEL"]
["Summit","RsD2","Rittman silt loam, 12 to 18 percent slopes, moderately eroded","Rittman",4,0.43,"HEL"]
["Summit","RsE2","Rittman silt loam, 18 to 25 percent slopes, moderately eroded","Rittman",4,0.43,"HEL"]
["Summit","RtB","Rittman silt loam, sandstone substratum, 2 to 6 percent slopes","Rittman",4,0.43,"PHEL"]
["Summit","RtC","Rittman silt loam, sandstone substratum 6 to 12 percent slopes","Rittman",4,0.43,"PHEL"]
["Summit","RuB","Rittman-Urban land complex, undulating","Rittman",4,0.43,"PHEL"]
["Summit","RuC","Rittman-Urban land complex, rolling","Rittman",4,0.43,"HEL"]
["Summit","Rv","Rough broken land, clay and silt","Rough"]
["Summit","Rw","Rough broken land, silt and sand","Rough"]
["Summit","Sb","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Summit","Sc","Shale rock land","Shale"]
["Summit","So","Sloan silt loam","Sloan",5,0.37,"NHEL"]
["Summit","Tg","Tioga loam","Tioga",5,0.37,"NHEL"]
["Summit","Tr","Trumbull silt loam","Trumbull",3,0.37,"NHEL"]
["Summit","Ur","Urban land","Urban"]
["Summit","W","Water","Water"]
["Summit","WaA","Wadsworth silt loam, 0 to 2 percent slopes","Wadsworth",4,0.43,"NHEL"]
["Summit","WaB","Wadsworth silt loam, 2 to 6 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Summit","Wb","Wadsworth-Urban land complex","Wadsworth",4,0.43,"PHEL"]
["Summit","Wc","Wallkill silt loam","Wallkill",5,0.32,"NHEL"]
["Summit","WrA","Wheeling silt loam, 0 to 2 percent slopes","Wheeling",4,0.37,"NHEL"]
["Summit","WrB","Wheeling silt loam, 2 to 6 percent slopes","Wheeling",4,0.37,"PHEL"]
["Summit","Wt","Willette muck","Willette",2,null,"NHEL"]
["Summit","WuB","Wooster silt loam, 2 to 6 percent slopes","Wooster",4,0.37,"PHEL"]
["Summit","WuC","Wooster silt loam, 6 to 12 percent slopes","Wooster",4,0.37,"PHEL"]
["Summit","WuC2","Wooster silt loam, 6 to 12 percent slopes, moderately eroded","Wooster",4,0.37,"PHEL"]
["Summit","WuD","Wooster silt loam, 12 to 18 percent slopes","Wooster",4,0.37,"HEL"]
["Summit","WuD2","Wooster silt loam, 12 to 18 percent, moderately eroded","Wooster",4,0.37,"HEL"]
["Summit","WuE2","Wooster silt loam, 18 to 25 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
["Summit","WuF2","Wooster silt loam, 25 to 50 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
["Summit","WvC2","Wooster silt loam, sandstone substratum, 6 to 12 percent slopes, moderately eroded","Wooster",4,0.37,"PHEL"]
["Summit","WvD2","Wooster silt loam, sandstone substratum, 12 to 18 percent slopes, moderately eroded","Wooster",4,0.37,"HEL"]
["Summit","WwD","Wooster-Urban land complex, hilly","Wooster",4,0.37,"HEL"]
[null,"Select","none","none"]
["Trumbull","BrF","Brecksville silt loam, 25 to 50 percent slopes","Brecksville",4,0.43,"HEL"]
["Trumbull","CaB","Cambridge silt loam, 2 to 6 percent slopes","Cambridge",4,0.43,"PHEL"]
["Trumbull","CaC","Cambridge silt loam, 6 to 12 percent slopes","Cambridge",4,0.43,"PHEL"]
["Trumbull","Cb","Canadice silty clay loam","Canadice",5,0.49,"NHEL"]
["Trumbull","CcA","Caneadea silt loam, 0 to 2 percent slopes","Caneadea",3,0.43,"NHEL"]
["Trumbull","CcB","Caneadea silt loam, 2 to 6 percent slopes","Caneadea",3,0.43,"PHEL"]
["Trumbull","CdA","Caneadea-Canadice complex, 0 to 2 percent slopes","Caneadea",3,0.43,"NHEL"]
["Trumbull","CeA","Caneadea-Urban land complex, 0 to 2 percent slopes","Caneadea",3,0.43,"NHEL"]
["Trumbull","CfB","Canfield silt loam, 2 to 6 percent slopes","Canfield",4,0.37,"PHEL"]
["Trumbull","CfC","Canfield silt loam, 6 to 12 percent slopes","Canfield",4,0.37,"PHEL"]
["Trumbull","CgB","Canfield-Urban land complex, 2 to 8 percent slopes","Canfield",4,0.37,"PHEL"]
["Trumbull","Ch","Carlisle muck, ponded","Carlisle",2,null,"NHEL"]
["Trumbull","CnA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Trumbull","CnB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Trumbull","CnC","Chili loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Trumbull","CoD","Chili gravelly loam, 12 to 18 percent slopes","Chili",4,0.24,"HEL"]
["Trumbull","CrF","Chili-Oshtemo complex, 25 to 50 percent slopes","Chili",4,0.24,"HEL"]
["Trumbull","CsB","Chili-Urban land complex, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Trumbull","CsC","Chili-Urban land complex, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Trumbull","Ct","Condit silt loam","Condit",5,0.37,"NHEL"]
["Trumbull","Da","Damascus loam","damascus",5,0.32,"NHEL"]
["Trumbull","DrA","Darien silt loam, 0 to 2 percent slopes","Darien",3,0.37,"NHEL"]
["Trumbull","DrB","Darien silt loam, 2 to 6 percent slopes","Darien",3,0.37,"PHEL"]
["Trumbull","Du","Dumps","Dumps"]
["Trumbull","EhB","Ellsworth silt loam, 2 to 6 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Trumbull","EhB2","Ellsworth silt loam, 2 to 6 percent slopes, eroded","Ellsworth",3,0.43,"PHEL"]
["Trumbull","EhC2","Ellsworth silt loam, 6 to 12 percent slopes, eroded","Ellsworth",3,0.43,"HEL"]
["Trumbull","EhD2","Ellsworth silt loam, 12 to 18 percent slopes, eroded","Ellsworth",3,0.43,"HEL"]
["Trumbull","EhF","Ellsworth silt loam, 25 to 50 percent slopes","Ellsworth",3,0.43,"HEL"]
["Trumbull","ExB","Ellsworth-Urban land complex, 2 to 8 percent slopes","Ellsworth",3,0.43,"PHEL"]
["Trumbull","EyB","Elnora loamy fine sand, 2 to 6 percent slopes","Elnora",4,0.17,"NHEL"]
["Trumbull","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Trumbull","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Trumbull","FdA","Fitchville-Urban land complex, 0 to 3 percent slopes","Fitchville",5,0.37,"NHEL"]
["Trumbull","GbB","Geeburg silt loam, 2 to 6 percent slopes","Geeburg",3,0.43,"PHEL"]
["Trumbull","GbB2","Geeburg silt loam, 2 to 6 percent slopes, eroded","Geeburg",3,0.43,"PHEL"]
["Trumbull","GbC","Geeburg silt loam, 6 to 12 percent slopes","Geeburg",3,0.43,"HEL"]
["Trumbull","GbC2","Geeburg silt loam, 6 to 12 percent slopes, eroded","Geeburg",3,0.43,"HEL"]
["Trumbull","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Trumbull","GfC","Glenford silt loam, 6 to 12 percent slopes","Glenford",5,0.37,"PHEL"]
["Trumbull","GnB","Glenford-Urban land complex, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Trumbull","HaA","Haskins loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Trumbull","HaB","Haskins loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Trumbull","HbB","Haskins-Urban land complex, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Trumbull","Ho","Holly silt loam, frequently flooded","Holly",5,0.28000000000000003,"NHEL"]
["Trumbull","JtA","Jimtown loam, 0 to 2 percent slopes","Jimtown",4,0.32,"NHEL"]
["Trumbull","JtB","Jimtown loam, 2 to 6 percent slopes","Jimtown",4,0.32,"PHEL"]
["Trumbull","JuA","Jimtown-Urban land complex, 0 to 3 percent slopes","Jimtown",4,0.32,"NHEL"]
["Trumbull","LaB","Lakin loamy fine sand, 2 to 8 percent slopes","Lakin",5,0.17,"PHEL"]
["Trumbull","Lo","Lorain silty clay loam","Lorain",5,0.32,"NHEL"]
["Trumbull","Lp","Lorain silty clay loam, loamy substratum","Lorain",5,0.32,"NHEL"]
["Trumbull","LrB","Lordstown loam, 2 to 6 percent slopes","Lordstown",3,0.28000000000000003,"PHEL"]
["Trumbull","LrC","Lordstown loam, 6 to 12 percent slopes","Lordstown",3,0.28000000000000003,"PHEL"]
["Trumbull","LxF","Lordstown-Rock outcrop complex, 18 to 50 percent slopes","Lordstown",3,0.28000000000000003,"HEL"]
["Trumbull","LyB","Loudonville silt loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Trumbull","LyC","Loudonville silt loam, 6 to 12 percent slopes","Loudonville",4,0.32,"PHEL"]
["Trumbull","LyC2","Loudonville silt loam, 6 to 12 percent slopes, eroded","Loudonville",4,0.32,"PHEL"]
["Trumbull","LyD","Loudonville silt loam, 12 to 18 percent slopes","Loudonville",4,0.32,"HEL"]
["Trumbull","LzB","Loudonville-Urban land complex, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Trumbull","LzC","Loudonville-Urban land complex, 6 to 18 percent slopes","Loudonville",4,0.32,"PHEL"]
["Trumbull","MgA","Mahoning silt loam, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Trumbull","MgB","Mahoning silt loam, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Trumbull","MhA","Mahoning silt loam, shale substratum, 0 to 2 percent slopes","Mahoning",3,0.43,"NHEL"]
["Trumbull","MhB","Mahoning silt loam, shale substratum, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Trumbull","MhC","Mahoning silt loam, shale substratum, 6 to 12 percent slopes","Mahoning",3,0.43,"PHEL"]
["Trumbull","MkB","Mahoning-Urban land complex, 2 to 6 percent slopes","Mahoning",3,0.43,"PHEL"]
["Trumbull","MtA","Mitiwanga silt loam, 0 to 2 percent slopes","Mitiwanga",4,0.32,"NHEL"]
["Trumbull","MtB","Mitiwanga silt loam, 2 to 6 percent slopes","Mitiwanga",4,0.32,"PHEL"]
["Trumbull","Or","Orrville silt loam, frequently flooded","Orrville",5,0.37,"NHEL"]
["Trumbull","OsB","Oshtemo sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Trumbull","OsC","Oshtemo sandy loam, 6 to 12 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Trumbull","Pg","Pits, gravel","Pits"]
["Trumbull","Pr","Pits, quarry","Pits"]
["Trumbull","PsA","Platea silt loam, 0 to 2 percent slopes","Platea",3,0.43,"NHEL"]
["Trumbull","PsB","Platea silt loam, 2 to 6 percent slopes","Platea",3,0.43,"PHEL"]
["Trumbull","PsC","Platea silt loam, 6 to 12 percent slopes","Platea",3,0.43,"HEL"]
["Trumbull","RaA","Ravenna silt loam, 0 to 2 percent slopes","Ravenna",3,0.37,"NHEL"]
["Trumbull","RaB","Ravenna silt loam, 2 to 6 percent slopes","Ravenna",3,0.37,"PHEL"]
["Trumbull","RdB","Rawson silt loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Trumbull","RmA","Remsen silt loam, 0 to 2 percent slopes","Remsen",3,0.43,"NHEL"]
["Trumbull","RmB","Remsen silt loam, 2 to 6 percent slopes","Remsen",3,0.43,"PHEL"]
["Trumbull","RoB","Remsen-Urban land complex, 2 to 6 percent slopes","Remsen",3,0.43,"PHEL"]
["Trumbull","RsB","Rittman silt loam, 2 to 6 percent slopes","Rittman",4,0.43,"PHEL"]
["Trumbull","RsC","Rittman silt loam, 6 to 12 percent slopes","Rittman",4,0.43,"PHEL"]
["Trumbull","RtB","Rittman-Urban land complex, 4 to 10 percent slopes","Rittman",4,0.43,"PHEL"]
["Trumbull","Sb","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Trumbull","Sc","Sebring silt loam, till substratum","Sebring",5,0.37,"NHEL"]
["Trumbull","SeB","Seward loamy fine sand, 2 to 6 percent slopes","Seward",4,0.17,"NHEL"]
["Trumbull","Tg","Tioga loam, occasionally flooded","Tioga",5,0.37,"NHEL"]
["Trumbull","Th","Tioga loam, frequently flooded","Tioga",5,0.37,"NHEL"]
["Trumbull","Tr","Trumbull silty clay loam","Trumbull",3,0.37,"NHEL"]
["Trumbull","Ud","Udorthents, loamy","Udorthents"]
["Trumbull","Ur","Urban land","Urban"]
["Trumbull","VeA","Venango silt loam, 0 to 2 percent slopes","Venango",4,0.37,"NHEL"]
["Trumbull","VeB","Venango silt loam, 2 to 6 percent slopes","Venango",4,0.37,"PHEL"]
["Trumbull","W","Water","Water"]
["Trumbull","WbA","Wadsworth silt loam, 0 to 2 percent slopes","Wadsworth",4,0.43,"NHEL"]
["Trumbull","WbB","Wadsworth silt loam, 2 to 6 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Trumbull","WeA","Wadsworth-Urban land complex, 0 to 2 percent slopes","Wadsworth",4,0.43,"NHEL"]
["Trumbull","WeB","Wadsworth-Urban land complex, 2 to 6 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Trumbull","WuF","Wooster silt loam, 25 to 50 percent slopes","Wooster",4,0.37,"HEL"]
[null,"Select","none","none"]
["Wayne","AdD","Alexandria silt loam, 12 to 18 percent slopes","Alexandria",4,0.37,"HEL"]
["Wayne","AdF","Alexandria silt loam, 18 to 50 percent slopes","Alexandria",4,0.37,"HEL"]
["Wayne","BnA","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Wayne","BnB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Wayne","BrD","Berks silt loam, 12 to 18 percent slopes","Berks",3,0.24,"HEL"]
["Wayne","BrE","Berks silt loam, 18 to 25 percent slopes","Berks",3,0.24,"HEL"]
["Wayne","BrF","Berks silt loam, 25 to 70 percent slopes","Berks",3,0.24,"HEL"]
["Wayne","BsB","Bethesda silty clay loam, 2 to 12 percent slopes","Bethesda",3,0.43,"PHEL"]
["Wayne","BsF","Bethesda silty clay loam, 18 to 70 percent slopes","Bethesda",3,0.43,"HEL"]
["Wayne","BtA","Bogart loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Wayne","BtB","Bogart loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Wayne","CdA","Canfield silt loam, 0 to 2 percent slopes","Canfield",4,0.37,"NHEL"]
["Wayne","CdB","Canfield silt loam, 2 to 6 percent slopes","Canfield",4,0.37,"PHEL"]
["Wayne","CdB2","Canfield silt loam, 2 to 6 percent slopes, eroded","Canfield",4,0.37,"PHEL"]
["Wayne","CdC","Canfield silt loam, 6 to 12 percent slopes","Canfield",4,0.37,"PHEL"]
["Wayne","CdC2","Canfield silt loam, 6 to 12 percent slopes, eroded","Canfield",4,0.37,"PHEL"]
["Wayne","CfB","Canfield-Urban land complex, 2 to 6 percent slopes","Canfield",4,0.37,"PHEL"]
["Wayne","CgB","Cardington silt loam, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Wayne","CgB2","Cardington silt loam, 2 to 6 percent slopes, eroded","Cardington",4,0.37,"PHEL"]
["Wayne","CgC","Cardington silt loam, 6 to 12 percent slopes","Cardington",4,0.37,"PHEL"]
["Wayne","CgC2","Cardington silt loam, 6 to 12 percent slopes, eroded","Cardington",4,0.37,"PHEL"]
["Wayne","Ch","Carlisle muck","Carlisle",2,null,"NHEL"]
["Wayne","Ck","Carlisle muck, ponded","Carlisle",2,null,"NHEL"]
["Wayne","CnA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Wayne","CnB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Wayne","CnC","Chili loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Wayne","CoD2","Chili gravelly loam, 12 to 25 percent slopes, eroded","Chili",4,0.24,"HEL"]
["Wayne","CoF","Chili gravelly loam, 25 to 70 percent slopes","Chili",4,0.24,"HEL"]
["Wayne","CrB","Chili-Urban land complex, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Wayne","Cs","Condit silt loam","Condit",5,0.37,"NHEL"]
["Wayne","CtC","Coshocton silt loam, 6 to 12 percent slopes","Coshocton",4,0.37,"PHEL"]
["Wayne","DkD","Dekalb channery loam, 12 to 18 percent slopes","Dekalb",2,0.24,"HEL"]
["Wayne","DkE","Dekalb channery loam, 18 to 25 percent slopes","Dekalb",2,0.24,"HEL"]
["Wayne","EuA","Euclid silt loam, occasionally flooded","Euclid",5,0.37,"NHEL"]
["Wayne","FaB","Fairpoint silty clay loam, 2 to 12 percent slopes","Fairpont",3,0.43,"PHEL"]
["Wayne","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Wayne","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Wayne","FfA","Fitchville-Urban land complex, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Wayne","GfA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Wayne","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Wayne","GfC","Glenford silt loam, 6 to 12 percent slopes","Glenford",5,0.37,"PHEL"]
["Wayne","GfC2","Glenford silt loam, 6 to 12 percent slopes, eroded","Glenford",5,0.37,"PHEL"]
["Wayne","GfD","Glenford silt loam, 12 to 18 percent slopes","Glenford",5,0.37,"HEL"]
["Wayne","HdA","Haskins silt loam, 0 to 3 percent slopes","Haskins",4,0.37,"NHEL"]
["Wayne","JtA","Jimtown loam, 0 to 2 percent slopes","Jimtown",4,0.32,"NHEL"]
["Wayne","JtB","Jimtown loam, 2 to 6 percent slopes","Jimtown",4,0.32,"PHEL"]
["Wayne","Kb","Killbuck silt loam, frequently flooded","Killbuck",5,0.37,"NHEL"]
["Wayne","Ld","Linwood muck","Linwood",2,null,"NHEL"]
["Wayne","Le","Lobdell silt loam, occasionally flooded","Lobdell",5,0.37,"NHEL"]
["Wayne","LnB","Loudonville silt loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Wayne","LnC2","Loudonville silt loam, 6 to 12 percent slopes, eroded","Loudonville",4,0.32,"PHEL"]
["Wayne","LnD","Loudonville silt loam, 12 to 18 percent slopes","Loudonville",4,0.32,"HEL"]
["Wayne","Ly","Luray silty clay loam","Luray",5,0.32,"NHEL"]
["Wayne","McB","Mechanicsburg silt loam, 2 to 6 percent slopes","Mechanicsburg",5,0.37,"PHEL"]
["Wayne","McC2","Mechanicsburg silt loam, 6 to 12 percent slopes, eroded","Mechanicsburg",5,0.37,"PHEL"]
["Wayne","McD","Mechanicsburg silt loam, 12 to 18 percent slopes","Mechanicsburg",5,0.37,"HEL"]
["Wayne","Md","Melvin silt loam, frequently flooded","Melvin",5,0.43,"NHEL"]
["Wayne","Mg","Melvin silt loam, ponded","Melvin",5,0.43,"NHEL"]
["Wayne","MtB","Mitiwanga silt loam, 1 to 4 percent slopes","Mitiwanga",4,0.32,"PHEL"]
["Wayne","Or","Orrville silt loam, occasionally flooded","Orrville",5,0.37,"NHEL"]
["Wayne","OtB","Oshtemo sandy loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Wayne","Pg","Pits, gravel","Pits"]
["Wayne","Pr","Pits, quarry","Pits"]
["Wayne","ReA","Ravenna silt loam, 0 to 2 percent slopes","Ravenna",3,0.37,"NHEL"]
["Wayne","ReB","Ravenna silt loam, 2 to 6 percent slopes","Ravenna",3,0.37,"PHEL"]
["Wayne","RgB","Rawson silt loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Wayne","RhB","Riddles silt loam, 2 to 6 percent slopes","Riddles",5,0.32,"PHEL"]
["Wayne","RhC","Riddles silt loam, 6 to 12 percent slopes","Riddles",5,0.32,"PHEL"]
["Wayne","RhD2","Riddles silt loam, 12 to 18 percent, eroded","Riddles",5,0.32,"HEL"]
["Wayne","RhE","Riddles silt loam, 18 to 25 percent slopes","Riddles",5,0.32,"HEL"]
["Wayne","RsB","Rittman silt loam, 2 to 6 percent slopes","Rittman",4,0.43,"PHEL"]
["Wayne","RsB2","Rittman silt loam, 2 to 6 percent slopes, eroded","Rittman",4,0.43,"PHEL"]
["Wayne","RsC","Rittman silt loam, 6 to 12 percent slopes","Rittman",4,0.43,"PHEL"]
["Wayne","RsC2","Rittman silt loam, 6 to 12 percent slopes, eroded","Rittman",4,0.43,"PHEL"]
["Wayne","RsD2","Rittman silt loam, 12 to 18 percent slopes, eroded","Rittman",4,0.43,"HEL"]
["Wayne","RtB","Rittman-Urban land complex, 2 to 6 percent slopes","Rittman",4,0.43,"PHEL"]
["Wayne","Sb","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Wayne","Tg","Tioga silt loam, occasionally flooded","Tioga",5,0.37,"NHEL"]
["Wayne","TrA","Tiro silt loam, 0 to 2 percent slopes","Tioga",4,0.37,"NHEL"]
["Wayne","Ud","Udorthents, loamy","Udorthents"]
["Wayne","W","Water","Water"]
["Wayne","WaA","Wadsworth silt loam, 0 to 2 percent slopes","Wadsworth",4,0.43,"NHEL"]
["Wayne","WaB","Wadsworth silt loam, 2 to 6 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Wayne","Wc","Wallkill silt loam","Wallkill",5,0.32,"NHEL"]
["Wayne","WuB","Wooster-Riddles silt loams, 2 to 6 percent slopes","Wooster",4,0.37,"PHEL"]
["Wayne","WuC","Wooster-Riddles silt loams, 6 to 12 percent slopes","Wooster",4,0.37,"PHEL"]
["Wayne","WuC2","Wooster-Riddles silt loams, 6 to 12 percent slopes, eroded","Wooster",4,0.37,"PHEL"]
["Wayne","WuD2","Wooster-Riddles silt loams, 12 to 18 percent slopes, eroded","Wooster",4,0.37,"HEL"]
["Wayne","WyC","Wooster-Urban land complex, 6 to 12 percent slopes","Wooster",4,0.37,"PHEL"]

{"sheet":"Area 3","index":4,"n_rows":1483,"n_cols":7,"rows_kept":1483,"cut":false,"hidden":false,"merged":[]}
["County","symbol","map unit name","Component","T","Kw","HEL"]
[null,"Select","none","none"]
["Belmont","AeC","Allegheny variant loam, 8 to 15 percent slopes","Allegheny",5,0.32,"PHEL"]
["Belmont","As","Ashton silt loam, occasionally flooded","Ashton",5,0.32,"NHEL"]
["Belmont","BaB","Barkcamp gravelly sandy loam, 0 to 8 percent slopes","Barkcamp",5,0.24,"PHEL"]
["Belmont","BaD","Barkcamp gravelly sandy loam, 8 to 40 percent slopes","Barkcamp",5,0.24,"PHEL"]
["Belmont","BaF","Barkcamp very stony sandy loam, 40 to 70 percent slopes","Barkcamp",5,0.24,"HEL"]
["Belmont","BcB","Barkcamp clay loam, 0 to 8 percent slopes","Barkcamp",3,0.32,"PHEL"]
["Belmont","BcD","Barkcamp clay loam, 8 to 25 percent slopes","Barkcamp",3,0.32,"HEL"]
["Belmont","BeB","Bethesda silt loam, 0 to 8 percent slopes","Bethesda",3,0.43,"PHEL"]
["Belmont","BeD","Bethesda silt loam, 8 to 25 percent slopes","Bethesda",3,0.43,"HEL"]
["Belmont","BhB","Bethesda shaly silty clay loam, 0 to 8 percent slopes","Bethesda",5,0.32,"PHEL"]
["Belmont","BhD","Bethesda shaly silty clay loam, 8 to 25 percent slopes","Bethesda",5,0.32,"PHEL"]
["Belmont","BhE","Bethesda shaly silty clay loam, 25 to 40 percent slopes","Bethesda",5,0.32,"HEL"]
["Belmont","BhF","Bethesda very cobbly silty clay loam, 40 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Belmont","BsC","Brookside silty clay loam, 8 to 15 percent slopes","Brookside",5,0.37,"PHEL"]
["Belmont","BsD","Brookside silty clay loam, 15 to 25 percent slopes","Brookside",5,0.37,"HEL"]
["Belmont","BsE","Brookside silty clay loam, 25 to 40 percent slopes","Brookside",5,0.37,"HEL"]
["Belmont","BuB","Brookside-Urban land complex, 3 to 15 percent slopes","Brookside",5,0.37,"PHEL"]
["Belmont","BuD","Brookside-Urban land complex, 15 to 40 percent slopes","Brookside",5,0.37,"HEL"]
["Belmont","Cg","Chagrin silt loam, occasionally flooded","Chagrin",5,0.32,"NHEL"]
["Belmont","ChB","Chili gravelly loam, 3 to 8 percent slopes","Chili",4,0.24,"PHEL"]
["Belmont","CmB","Chili-Urban land complex, 0 to 8 percent slopes","Chili",4,0.24,"PHEL"]
["Belmont","CuB","Culleoka silt loam, 3 to 8 percent slopes","Culleoka",3,0.32,"PHEL"]
["Belmont","CuC","Culleoka silt loam, 8 to 15 percent slopes","Culleoka",3,0.32,"HEL"]
["Belmont","DkB","Dekalb loam, 3 to 8 percent slopes","Dekalb",2,0.24,"PHEL"]
["Belmont","DkC","Dekalb loam, 8 to 15 percent slopes","Dekalb",2,0.24,"HEL"]
["Belmont","DkD","Dekalb loam, 15 to 25 percent slopes","Dekalb",2,0.24,"HEL"]
["Belmont","DkE","Dekalb loam, 25 to 40 percent slopes","Dekalb",2,0.24,"HEL"]
["Belmont","DmF","Dekalb moderately channery loam, 40 to 70 percent slopes","Dekalb",2,0.24,"HEL"]
["Belmont","Dp","Dumps","Dumps"]
["Belmont","Ds","Dumps, mine","Dumps"]
["Belmont","DuB","Duncannon-Urban land complex, 0 to 15 percent slopes","Duncannon",4,0.37,"PHEL"]
["Belmont","EbB","Elba silty clay loam, 3 to 8 percent slopes","Elba",3,0.43,"PHEL"]
["Belmont","EbC","Elba silty clay loam, 8 to 15 percent slopes","Elba",3,0.43,"HEL"]
["Belmont","EbD","Elba silty clay loam, 15 to 25 percent slopes","Elba",3,0.43,"HEL"]
["Belmont","EbE","Elba silty clay loam, 25 to 40 percent slopes","Elba",3,0.43,"HEL"]
["Belmont","ElB","Elkinsville silt loam, 3 to 8 percent slopes","Elkinsville",5,0.37,"PHEL"]
["Belmont","ElC","Elkinsville silt loam, 8 to 15 percent slopes","Elkinsville",5,0.37,"PHEL"]
["Belmont","ElD","Elkinsville silt loam, 15 to 25 percent slopes","Elkinsville",5,0.37,"HEL"]
["Belmont","FbB","Fairpoint gravelly clay loam, 0 to 8 percent slopes","Fairpoint",3,0.43,"PHEL"]
["Belmont","FbD","Fairpoint gravelly clay loam, 8 to 25 percent slopes","Fairpoint",3,0.43,"PHEL"]
["Belmont","FcB","Fairpoint silty clay loam, 0 to 8 percent slopes","Fairpoint",3,0.43,"PHEL"]
["Belmont","FcD","Fairpoint silty clay loam, 8 to 25 percent slopes","Fairpoint",3,0.43,"HEL"]
["Belmont","FtA","Fitchville silt loam, 0 to 3 percent slopes","Fitchville",5,0.37,"NHEL"]
["Belmont","He","Hartshorn silt loam, occasionally flooded","Hartshorn",3,0.32,"NHEL"]
["Belmont","LeB","Lowell silt loam, 3 to 8 percent slopes","Lowell",3,0.37,"PHEL"]
["Belmont","LeC","Lowell silt loam, 8 to 15 percent slopes","Lowell",3,0.37,"HEL"]
["Belmont","LeD","Lowell silt loam, 15 to 25 percent slopes","Lowell",3,0.37,"HEL"]
["Belmont","LeE","Lowell silt loam, 25 to 40 percent slopes","Lowell",3,0.37,"HEL"]
["Belmont","LeF","Lowell silt loam, 40 to 70 percent slopes","Lowell",3,0.37,"HEL"]
["Belmont","LoB","Lowell-Westmoreland silt loams, 3 to 8 percent slopes","Lowell",3,0.37,"PHEL"]
["Belmont","LoC","Lowell-Westmoreland silt loams, 8 to 15 percent slopes","Lowell",3,0.37,"HEL"]
["Belmont","LoD","Lowell-Westmoreland silt loams, 15 to 25 percent slopes","Lowell",3,0.37,"HEL"]
["Belmont","LoE","Lowell-Westmoreland silt loams, 25 to 40 percent slopes","Lowell",3,0.37,"HEL"]
["Belmont","LoF","Lowell-Westmoreland silt loams, 40 to 70 percent slopes","Lowell",3,0.37,"HEL"]
["Belmont","LpF","Lowell-Westmoreland silt loams, benched, 30 to 70 percent slopes","Lowell",3,0.37,"HEL"]
["Belmont","MnB","Morristown clay loam, 0 to 8 percent slopes","Morristown",3,0.43,"PHEL"]
["Belmont","MnD","Morristown clay loam, 8 to 25 percent slopes","Morristown",3,0.43,"HEL"]
["Belmont","MnE","Morristown clay loam, 25 to 40 percent slopes","Morristown",3,0.43,"HEL"]
["Belmont","MoB","Morristown stony clay loam, 0 to 8 percent slopes","Morristown",5,0.32,"PHEL"]
["Belmont","MoD","Morristown stony clay loam, 8 to 25 percent slopes","Morristown",5,0.32,"PHEL"]
["Belmont","MoE","Morristown stony clay loam, 25 to 40 percent slopes","Morristown",5,0.32,"HEL"]
["Belmont","MoF","Morristown very stony clay loam, 40 to 70 percent slopes","Morristown",5,0.32,"HEL"]
["Belmont","Ne","Newark silt loam, frequently flooded","Newark",5,0.32,"NHEL"]
["Belmont","Nm","Newark silt loam, ponded","Newark",5,0.32,"NHEL"]
["Belmont","Nn","Newark Variant silt loam, frequently flooded","Newark",5,0.37,"NHEL"]
["Belmont","No","Nolin variant silt loam, occasionally flooded","Nolin",5,0.37,"NHEL"]
["Belmont","Nu","Nolin variant-Urban land complex","Nolin",5,0.37,"NHEL"]
["Belmont","OtB","Otwell silt loam, 3 to 8 percent slopes","Otwell",3,0.43,"PHEL"]
["Belmont","OtC","Otwell silt loam, 8 to 15 percent slopes","Otwell",3,0.43,"HEL"]
["Belmont","RcC","Richland loam, 8 to 15 percent slopes","Richland",5,0.37,"PHEL"]
["Belmont","RcD","Richland loam, 15 to 25 percent slopes","Richland",5,0.37,"HEL"]
["Belmont","RcE","Richland moderately stony loam, 25 to 40 percent slopes","Richland",5,0.37,"HEL"]
["Belmont","RhB","Richland silt loam, 3 to 8 percent slopes","Richland",5,0.37,"PHEL"]
["Belmont","Uc","Udorthents-Pits complex","Udorthents"]
["Belmont","Ud","Udorthents-Urban land complex","Udorthents"]
["Belmont","W","Water","Water"]
["Belmont","WhB","Wellston silt loam, 3 to 8 percent slopes","Wellston",4,0.37,"PHEL"]
["Belmont","WhC","Wellston silt loam, 8 to 15 percent slopes","Wellston",4,0.37,"PHEL"]
["Belmont","WkB","Westmore silt loam, 3 to 8 percent slopes","Westmore",4,0.37,"PHEL"]
["Belmont","WkC","Westmore silt loam, 8 to 15 percent slopes","Westmore",4,0.37,"PHEL"]
["Belmont","WkD","Westmore silt loam, 15 to 25 percent slopes","Westmore",4,0.37,"HEL"]
["Belmont","WmB","Westmoreland silt loam, 3 to 8 percent slopes","Westmoreland",3,0.37,"PHEL"]
["Belmont","WmC","Westmoreland silt loam, 8 to 15 percent slopes","Westmoreland",3,0.37,"HEL"]
["Belmont","WmD","Westmoreland silt loam, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Belmont","WmE","Westmoreland silt loam, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Belmont","WmF","Westmoreland silt loam, 40 to 70 percent slopes","Westmoreland",3,0.37,"HEL"]
["Belmont","WoC","Westmoreland-Upshur complex, 8 to 15 percent slopes","Westmoreland",3,0.37,"PHEL"]
["Belmont","WoD","Westmoreland-Upshur complex, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Belmont","ZnB","Zanesville silt loam, 3 to 8 percent slopes","Zanesville",3,0.43,"PHEL"]
["Belmont","ZnC","Zanesville silt loam, 8 to 15 percent slopes","Zanesville",3,0.43,"HEL"]
[null,"Select","none","none"]
["Carroll","BkB","Berks shaly silt loam, 3 to 8 percent slopes","Berks",3,0.24,"PHEL"]
["Carroll","BkC","Berks shaly silt loam, 8 to 15 percent slopes","Berks",3,0.24,"HEL"]
["Carroll","BkD","Berks shaly silt loam, 15 to 25 percent slopes","Berks",3,0.24,"HEL"]
["Carroll","BkE","Berks shaly silt loam, 25 to 40 percent slopes","Berks",3,0.24,"HEL"]
["Carroll","BkF","Berks shaly silt loam, 40 to 70 percent slopes","Berks",3,0.24,"HEL"]
["Carroll","BnD","Bethesda channery clay loam, 8 to 25 percent slopes","Bethesda",5,0.32,"PHEL"]
["Carroll","BnF","Bethesda channery clay loam, 25 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Carroll","BrA","Boyer loam, 0 to 4 percent slopes","Boyer",4,0.17,"NHEL"]
["Carroll","ChA","Chili silt loam, 0 to 3 percent slopes","Chili",4,0.32,"NHEL"]
["Carroll","ChB","Chili silt loam, 3 to 8 percent slopes","Chili",4,0.32,"PHEL"]
["Carroll","ChC","Chili silt loam, 8 to 15 percent slopes","Chili",4,0.32,"PHEL"]
["Carroll","CnB","Coshocton silt loam, 3 to 8 percent slopes","Coshocton",4,0.37,"PHEL"]
["Carroll","CoB","Coshocton-Keene silt loams, 3 to 8 percent slopes","Coshocton",4,0.37,"PHEL"]
["Carroll","CuB","Culleoka silt loam, 3 to 8 percent slopes","Culleoka",3,0.32,"PHEL"]
["Carroll","EbB","Elba silty clay loam, 3 to 8 percent slopes","Elba",3,0.43,"PHEL"]
["Carroll","EbC2","Elba silty clay loam, 8 to 15 percent slopes, eroded","Elba",3,0.43,"HEL"]
["Carroll","EcD2","Elba-Upshur silty clay loams, 15 to 25 percent slopes, eroded","Elba",3,0.43,"HEL"]
["Carroll","Ek","Elkinsville silt loam, rarely flooded","Elkinsville",5,0.37,"NHEL"]
["Carroll","FaD","Fairpoint channery clay loam, 8 to 25 percent slopes","Fairpoint",3,0.43,"PHEL"]
["Carroll","FaF","Fairpoint channery clay loam, 25 to 70 percent slopes","Fairpoint",3,0.43,"HEL"]
["Carroll","FcA","Fitchville silt loam, 0 to 3 percent slopes","Fitchville",5,0.37,"NHEL"]
["Carroll","FcB","Fitchville silt loam, 3 to 8 percent slopes","Fitchville",5,0.37,"PHEL"]
["Carroll","GfB","Glenford silt loam, 3 to 8 percent slopes","Glenford",5,0.37,"PHEL"]
["Carroll","GfC","Glenford silt loam, 8 to 15 percent slopes","Glenford",5,0.37,"PHEL"]
["Carroll","GuB","Guernsey silty clay loam, 3 to 8 percent slopes","Guernsey",3,0.43,"PHEL"]
["Carroll","GuC2","Guernsey silty clay loam, 8 to 15 percent slopes, eroded","Guernsey",3,0.43,"HEL"]
["Carroll","HeB","Hazleton loam, 3 to 8 percent slopes","Hazleton",3,0.17,"PHEL"]
["Carroll","HeC","Hazleton loam, 8 to 15 percent slopes","Hazleton",3,0.17,"PHEL"]
["Carroll","HeD","Hazleton loam, 15 to 25 percent slopes","Hazleton",3,0.17,"HEL"]
["Carroll","HeE","Hazleton loam, 25 to 40 percent slopes","Hazleton",3,0.17,"HEL"]
["Carroll","Ho","Holly silt loam, ponded","Holly",5,0.28000000000000003,"NHEL"]
["Carroll","JwA","Jimtown silt loam, 0 to 3 percent slopes","Jimtown",4,0.32,"NHEL"]
["Carroll","LbB","Library Variant silt loam, 3 to 8 percent slopes","Library",5,0.43,"PHEL"]
["Carroll","Lo","Lorain silty clay loam, silty substratum","Lorain",5,0.32,"NHEL"]
["Carroll","MrD","Morristown shaly silty clay loam, 8 to 25 percent slopes","Morristown",5,0.32,"PHEL"]
["Carroll","Or","Orrville silt loam, occasionally flooded","Orrville",5,0.37,"NHEL"]
["Carroll","OsB","Oshtemo sandy loam, 3 to 8 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Carroll","OtB","Oshtemo sandy loam, loamy substratum, 3 to 8 percent slopes","Oshtemo",5,0.24,"PHEL"]
["Carroll","Pe","Peoga silt loam, rarely flooded","Peoga",4,0.43,"NHEL"]
["Carroll","Pg","Pits, gravel","Pits"]
["Carroll","RgB","Rigley sandy loam, 3 to 8 percent slopes","Rigley",4,0.24,"PHEL"]
["Carroll","RgC","Rigley sandy loam, 8 to 15 percent slopes","Rigley",4,0.24,"PHEL"]
["Carroll","RgD","Rigley sandy loam, 15 to 25 percent slopes","Rigley",4,0.24,"HEL"]
["Carroll","RgE","Rigley sandy loam, 25 to 40 percent slopes","Rigley",4,0.24,"HEL"]
["Carroll","Sb","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Carroll","Tg","Tioga silt loam, occasionally flooded","Tioga",5,0.37,"NHEL"]
["Carroll","UpC2","Upshur silty clay loam, 8 to 15 percent slopes, eroded","Upshur",3,0.43,"HEL"]
["Carroll","W","Water","Water"]
["Carroll","WhB","Wellston silt loam, 3 to 8 percent slopes","Wellston",4,0.37,"PHEL"]
["Carroll","WkC","Westmoreland silt loam, 8 to 15 percent slopes","Westmoreland",3,0.37,"HEL"]
["Carroll","WkD","Westmoreland silt loam, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Carroll","WkE","Westmoreland silt loam, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Carroll","WmC","Westmoreland-Coshocton silt loams, 8 to 15 percent slopes","Westmoreland",3,0.37,"HEL"]
["Carroll","WmD","Westmoreland-Coshocton silt loams, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
[null,"select","none","none"]
["Coshocton","AaB","Aaron silt loam, 2 to 6 percent slopes","Aaron",3,0.37,"PHEL"]
["Coshocton","AaC2","Aaron silt loam 6 to 15 percent slopes, eroded","Aaron",3,0.37,"HEL"]
["Coshocton","AfB","Alford silt loam, 2 to 6 percent slopes","Alford",5,0.37,"PHEL"]
["Coshocton","AfC2","Alford silt loam, 6 to 15 percent slopes, eroded","Alford",5,0.37,"HEL"]
["Coshocton","BgB","Bethesda loam, 0 to 8 percent slopes","Bethesda",3,0.43,"PHEL"]
["Coshocton","BgD","Bethesda loam, 8 to 25 percent slopes","Bethesda",3,0.43,"HEL"]
["Coshocton","BgE","Bethesda loam, 25 to 40 percent slopes","Bethesda",3,0.43,"HEL"]
["Coshocton","BhB","Bethesda channery loam, 0 to 8 percent slopes","Bethesda",5,0.32,"PHEL"]
["Coshocton","BhD","Bethesda channery loam, 8 to 25 percent slopes","Bethesda",5,0.32,"HEL"]
["Coshocton","BhF","Bethesda channery loam, 25 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Coshocton","BrD","Brownsville channery silt loam, 15 to 25 percent slopes","Brownsville",5,0.2,"HEL"]
["Coshocton","BrE","Brownsville channery silt loam, 25 to 35 percent slopes","Brownsville",5,0.2,"HEL"]
["Coshocton","BrF","Brownsville channery silt loam, 35 to 70 percent slopes","Brownsville",5,0.2,"HEL"]
["Coshocton","BtF","Brownsville-Rock outcrop complex, 35 to 70 percent slopes","Brownsville",5,0.2,"HEL"]
["Coshocton","CdA","Caneadea silt loam, 0 to 2 percent slopes","Caneadea",3,0.43,"NHEL"]
["Coshocton","CfA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Coshocton","CfB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Coshocton","CfC","Chili loam, 6 to 15 percent slopes","Chili",4,0.32,"HEL"]
["Coshocton","CfD","Chili loam, 15 to 25 percent slopes","Chili",4,0.32,"HEL"]
["Coshocton","CfE","Chili loam, 25 to 35 percent slopes","Chili",4,0.32,"HEL"]
["Coshocton","CgA","Chili-Urban land complex, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Coshocton","CgB","Chili-Urban land complex, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Coshocton","ChA","Cidermill silt loam, 0 to 2 percent slopes","Cidermill",4,0.37,"NHEL"]
["Coshocton","ChB","Cidermill silt loam, 2 to 6 percent slopes","Cidermill",4,0.37,"PHEL"]
["Coshocton","CkC","Clarksburg silt loam, 6 to 15 percent slopes","Clarksburg",3,0.37,"HEL"]
["Coshocton","CkD","Clarksburg silt loam, 15 to 25 percent slopes","Clarksburg",3,0.37,"HEL"]
["Coshocton","CoB","Coshocton silt loam, 2 to 6 percent slopes","Coshocton",4,0.37,"PHEL"]
["Coshocton","CoC2","Coshocton silt loam, 6 to 15 percent slopes, eroded","Coshocton",4,0.37,"HEL"]
["Coshocton","CoD","Coshocton silt loam, 15 to 25 percent slopes","Coshocton",4,0.37,"HEL"]
["Coshocton","CoE","Coshocton silt loam, 25 to 35 percent slopes","Coshocton",4,0.37,"HEL"]
["Coshocton","CpC","Coshocton silt loam, 6 to 15 percent slopes, very stony","Coshocton",4,0.37,"HEL"]
["Coshocton","CpD","Coshocton silt loam, 15 to 25 percent slopes, very stony","Coshocton",4,0.37,"HEL"]
["Coshocton","CrD","Coshocton-Rigley complex, 15 to 25 percent slopes","Coshocton",4,0.37,"HEL"]
["Coshocton","CrE","Coshocton-Rigley complex, 25 to 35 percent slopes","Coshocton",4,0.37,"HEL"]
["Coshocton","CsD","Coshocton-Westmoreland complex, 15 to 25 percent slopes","Coshocton",4,0.37,"HEL"]
["Coshocton","CsE","Coshocton-Westmoreland complex, 25 to 35 percent slopes","Coshocton",4,0.37,"HEL"]
["Coshocton","DeC","Dekalb channery sandy loam, 6 to 15 percent slopes, stony","Dekalb",2,0.24,"HEL"]
["Coshocton","Ds","Dumps, mine","Dumps"]
["Coshocton","EuA","Euclid silt loam, occasionally flooded","Euclid",5,0.37,"NHEL"]
["Coshocton","FaB","Fairpoint loam, 0 to 8 percent slopes","Fairpoint",3,0.43,"PHEL"]
["Coshocton","FaD","Fairpoint loam, 8 to 25 percent slopes","Fairpoint",3,0.43,"HEL"]
["Coshocton","FaE","Fairpoint loam, 25 to 35 percent slopes","Fairpoint",3,0.43,"HEL"]
["Coshocton","FeB","Farmerstown loam, 0 to 8 percent slopes","Farmerstown",4,0.43,"PHEL"]
["Coshocton","FeC","Farmerstown loam, 8 to 20 percent slopes","Farmerstown",4,0.43,"HEL"]
["Coshocton","FhA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Coshocton","FhB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Coshocton","GdB","Germano sandy loam, 2 to 6 percent slopes","Germano",4,0.24,"PHEL"]
["Coshocton","GdC2","Germano sandy loam, 6 to 15 percent slopes, eroded","Germano",4,0.24,"HEL"]
["Coshocton","GhB","Gilpin silt loam, 2 to 6 percent slopes","Gilpin",3,0.32,"PHEL"]
["Coshocton","GhC","Gilpin silt loam, 6 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Coshocton","GhD","Gilpin silt loam, 15 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Coshocton","GnA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Coshocton","GnB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Coshocton","GnC","Glenford silt loam, 6 to 15 percent slopes","Glenford",5,0.37,"HEL"]
["Coshocton","GpA","Glenford silt loam, occasionally flooded","Glenford",5,0.37,"NHEL"]
["Coshocton","GuC","Guernsey silt loam, 6 to 15 percent slopes","Guernsey",3,0.43,"HEL"]
["Coshocton","GuD","Guernsey silt loam, 15 to 25 percent slopes","Guernsey",3,0.43,"HEL"]
["Coshocton","HaD","Hazleton channery sandy loam, 15 to 25 percent slopes","Hazleton",3,0.17,"HEL"]
["Coshocton","HaE","Hazleton channery sandy loam, 25 to 35 percent slopes","Hazleton",3,0.17,"HEL"]
["Coshocton","HaF","Hazleton channery sandy loam, 35 to 70 percent slopes","Hazleton",3,0.17,"HEL"]
["Coshocton","HeF","Hazleton channery sandy loam, 25 to 70 percent slopes, very bouldery","Hazleton",3,0.17,"HEL"]
["Coshocton","HoB","Homewood silt loam, 2 to 6 percent slopes","Homewood",4,0.37,"PHEL"]
["Coshocton","HoC","Homewood silt loam, 6 to 15 percent slopes","Homewood",4,0.37,"HEL"]
["Coshocton","Ht","Huntington silt loam, rarely flooded","Huntington",5,0.28000000000000003,"NHEL"]
["Coshocton","JmA","Jimtown loam, 0 to 2 percent slopes","Jimtown",4,0.32,"NHEL"]
["Coshocton","KeB","Keene silt loam, 2 to 6 percent slopes","Keene",4,0.37,"PHEL"]
["Coshocton","KeC","Keene silt loam, 6 to 15 percent slopes","Keene",4,0.37,"HEL"]
["Coshocton","La","Landes sandy loam, rarely flooded","Landes",5,0.2,"NHEL"]
["Coshocton","Lb","Landes loam, occasionally flooded","Landes",5,0.28000000000000003,"NHEL"]
["Coshocton","Lo","Lobdell silt loam, occasionally flooded","Lobdell",5,0.37,"NHEL"]
["Coshocton","LrB","Loudon silt loam, 2 to 6 percent slopes","Loudon",3,0.43,"PHEL"]
["Coshocton","LrC","Loudon silt loam, 6 to 15 percent slopes","Loudon",3,0.43,"HEL"]
["Coshocton","LvC","Loudonville silt loam, 6 to 15 percent slopes","Loudonville",4,0.32,"HEL"]
["Coshocton","LvD","Loudonville silt loam, 15 to 20 percent slopes","Loudonville",4,0.32,"HEL"]
["Coshocton","MaB","Markland silt loam, 2 to 6 percent slopes","Markland",3,0.43,"PHEL"]
["Coshocton","MaC","Markland silt loam, 6 to 15 percent slopes","Markland",3,0.43,"HEL"]
["Coshocton","MaD2","Markland silt loam, 15 to 35 percent slopes, eroded","Markland",3,0.43,"HEL"]
["Coshocton","Mg","Melvin silt loam, frequently flooded","Melvin",5,0.43,"NHEL"]
["Coshocton","Mh","Melvin silt loam, ponded","Melvin",5,0.43,"NHEL"]
["Coshocton","MnA","Mentor silt loam, 0 to 2 percent slopes","Mentor",5,0.37,"NHEL"]
["Coshocton","MnB","Mentor silt loam, 2 to 6 percent slopes","Mentor",5,0.37,"PHEL"]
["Coshocton","MnC","Mentor silt loam, 6 to 15 percent slopes","Mentor",5,0.37,"HEL"]
["Coshocton","MnD","Mentor silt loam, 15 to 25 percent slopes","Mentor",5,0.37,"HEL"]
["Coshocton","Ne","Newark silt loam, occasionally flooded","Newark",5,0.32,"NHEL"]
["Coshocton","Nf","Newark silt loam, frequently flooded","Newark",5,0.32,"NHEL"]
["Coshocton","Nn","Nolin silt loam, rarely flooded","Nolin",5,0.43,"NHEL"]
["Coshocton","No","Nolin silt loam, occasionally flooded","Nolin",5,0.43,"NHEL"]
["Coshocton","Or","Orrville silt loam, occasionally flooded","Orrville",5,0.37,"NHEL"]
["Coshocton","Pg","Pits, gravel","Pits"]
["Coshocton","Ph","Pits, quarry","Pits"]
["Coshocton","RcC","Richland silt loam, 6 to 15 percent slopes","Richland",5,0.37,"HEL"]
["Coshocton","RcD","Richland silt loam, 15 to 25 percent slopes","Richland",5,0.37,"HEL"]
["Coshocton","RgC","Rigley sandy loam, 6 to 15 percent slopes","Rigley",4,0.24,"HEL"]
["Coshocton","RgD","Rigley sandy loam, 15 to 25 percent slopes","Rigley",4,0.24,"HEL"]
["Coshocton","RgE","Rigley sandy loam, 25 to 35 percent slopes","Rigley",4,0.24,"HEL"]
["Coshocton","RhD","Rigley sandy loam, 12 to 25 percent slopes, very stony","Rigley",4,0.24,"HEL"]
["Coshocton","Se","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Coshocton","Th","Tioga fine sandy loam, rarely flooded","Tioga",5,0.37,"NHEL"]
["Coshocton","Tk","Tioga fine sandy loam, occasionally flooded","Tioga",5,0.37,"NHEL"]
["Coshocton","Tm","Tioga fine sandy loam, frequently flooded","Tioga",5,0.37,"NHEL"]
["Coshocton","To","Tioga-Urban land complex, rarely flooded","Tioga",5,0.37,"NHEL"]
["Coshocton","TsB","Titusville silt loam, 2 to 6 percent slopes","Titusville",4,0.37,"PHEL"]
["Coshocton","TsC","Titusville silt loam, 6 to 15 percent slopes","Titusville",4,0.37,"HEL"]
["Coshocton","Ug","Udorthents, loamy","Udorthents"]
["Coshocton","Uh","Udorthents, loamy-skeletal","Udorthents"]
["Coshocton","Up","Udorthents-Pits complex","Udorthents"]
["Coshocton","W","Water","Water"]
["Coshocton","WaA","Watertown sandy loam, 0 to 2 percent slopes","Watertown",4,0.17,"NHEL"]
["Coshocton","WaB","Watertown sandy loam, 2 to 6 percent slopes","Watertown",4,0.17,"NHEL"]
["Coshocton","WaC","Watertown sandy loam, 6 to 15 percent slopes","Watertown",4,0.17,"PHEL"]
["Coshocton","WaD","Watertown sandy loam, 15 to 25 percent slopes","Watertown",4,0.17,"HEL"]
["Coshocton","WaF","Watertown sandy loam, 25 to 70 percent slopes","Watertown",4,0.17,"HEL"]
["Coshocton","Wb","Wappinger sandy loam, rarely flooded","Wappinger",4,0.49,"NHEL"]
["Coshocton","WeC","Wellston silt loam, 6 to 15 percent slopes","Wellston",4,0.37,"HEL"]
["Coshocton","WhC","Westmoreland silt loam, 6 to 15 percent slopes","Westmoreland",3,0.37,"HEL"]
["Coshocton","WhD","Westmoreland silt loam, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Coshocton","WhE","Westmoreland silt loam, 25 to 35 percent slopes","Westmoreland",3,0.37,"HEL"]
["Coshocton","WnA","Wheeling silt loam, 0 to 2 percent slopes","Wheeling",4,0.37,"NHEL"]
["Coshocton","WnB","Wheeling silt loam, 2 to 6 percent slopes","Wheeling",4,0.37,"PHEL"]
["Coshocton","Zp","Zipp silty clay loam, frequently flooded","Zipp",5,0.28000000000000003,"NHEL"]
[null,"Select","none","none"]
["Guernsey","AaB","Aaron silt loam, 2 to 8 percent slopes","Aaron",3,0.37,"PHEL"]
["Guernsey","AaC","Aaron silt loam, 8 to 15 percent slopes","Aaron",3,0.37,"HEL"]
["Guernsey","AbB","Aaron-Upshur complex, 2 to 8 percent slopes","Aaron",3,0.37,"PHEL"]
["Guernsey","AbC2","Aaron-Upshur complex, 8 to 15 percent slopes, eroded","Aaron",3,0.37,"HEL"]
["Guernsey","AgC","Allegheny loam, 8 to 15 percent slopes","Allegheny",4,0.32,"HEL"]
["Guernsey","BaD","Barkcamp loam, 8 to 25 percent slopes","Barkcamp",3,0.32,"HEL"]
["Guernsey","BcB","Barkcamp very flaggy sandy loam, 0 to 8 percent slopes, very stony","Barkcamp",5,0.24,"PHEL"]
["Guernsey","BcD","Barkcamp very flaggy sandy loam, 8 to 40 percent slopes, very stony","Barkcamp",5,0.24,"HEL"]
["Guernsey","BeC","Berks channery silt loam, 8 to 15 percent slopes","Berks",3,0.24,"HEL"]
["Guernsey","BeD","Berks channery silt loam, 15 to 25 percent slopes","Berks",3,0.24,"HEL"]
["Guernsey","BeE","Berks channery silt loam, 25 to 40 percent slopes","Berks",3,0.24,"HEL"]
["Guernsey","BeF","Berks channery silt loam, 40 to 70 percent slopes","Berks",3,0.24,"HEL"]
["Guernsey","BgB","Bethesda clay loam, 0 to 8 percent slopes","Bethesda",3,0.43,"PHEL"]
["Guernsey","BgD","Bethesda clay loam, 8 to 25 percent slopes","Bethesda",3,0.43,"HEL"]
["Guernsey","BgE","Bethesda clay loam, 25 to 40 percent slopes","Bethesda",3,0.43,"HEL"]
["Guernsey","BhB","Bethesda channery loam, 0 to 8 percent slopes","Bethesda",5,0.32,"PHEL"]
["Guernsey","BhD","Bethesda channery loam, 8 to 25 percent slopes","Bethesda",5,0.32,"HEL"]
["Guernsey","BhF","Bethesda channery loam, 25 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Guernsey","BsD","Brookside silt loam, 15 to 25 percent slopes","Brookside",5,0.37,"HEL"]
["Guernsey","BtC","Brookside-Vandalia complex, 8 to 15 percent slopes","Brookside",5,0.37,"HEL"]
["Guernsey","BtD","Brookside-Vandalia complex, 15 to 25 percent slopes","Brookside",5,0.37,"HEL"]
["Guernsey","BtE","Brookside-Vandalia complex, 25 to 40 percent slopes","Brookside",5,0.37,"HEL"]
["Guernsey","Ca","Chagrin loam, occasionally flooded","Chagrin",5,0.32,"NHEL"]
["Guernsey","ChD","Clarksburg channery silt loam, 15 to 25 percent slopes","Clarksburg",3,0.37,"HEL"]
["Guernsey","CkC","Claysville-Guernsey complex, 8 to 15 percent slopes","Claysville",5,0.28000000000000003,"HEL"]
["Guernsey","CoD","Coshocton loam, 15 to 25 percent slopes","Coshocton",4,0.37,"HEL"]
["Guernsey","CsC2","Coshocton silt loam, 8 to 15 percent slopes, eroded","Coshocton",4,0.37,"HEL"]
["Guernsey","DkC","Dekalb channery loam, 8 to 15 percent slopes","Dekalb",2,0.24,"HEL"]
["Guernsey","DkD","Dekalb channery loam, 15 to 25 percent slopes","Dekalb",2,0.24,"HEL"]
["Guernsey","DkE","Dekalb channery loam, 25 to 40 percent slopes","Dekalb",2,0.24,"HEL"]
["Guernsey","DmF","Dekalb channery loam, 25 to 70 percent slopes, very stony","Dekalb",2,0.24,"HEL"]
["Guernsey","Dp","Dumps","Dumps"]
["Guernsey","Ds","Dumps, mine","Dumps"]
["Guernsey","EbC","Elba silty clay loam, 8 to 15 percent slopes","Elba",3,0.43,"HEL"]
["Guernsey","EbD","Elba silty clay loam, 15 to 25 percent slopes","Elba",3,0.43,"HEL"]
["Guernsey","EbE","Elba silty clay loam, 25 to 40 percent slopes","Elba",3,0.43,"HEL"]
["Guernsey","EkF","Elba-Berks complex, 40 to 70 percent slopes","Elba",3,0.43,"HEL"]
["Guernsey","EnB","Enoch loam, 0 to 8 percent slopes","Enoch",3,0.37,"PHEL"]
["Guernsey","EnD","Enoch loam, 8 to 25 percent slopes","Enoch",3,0.37,"HEL"]
["Guernsey","EuA","Euclid silt loam, rarely flooded","Euclid",5,0.37,"NHEL"]
["Guernsey","FcB","Fairpoint silty clay loam, 0 to 8 percent slopes","Fairpoint",3,0.43,"PHEL"]
["Guernsey","FcD","Fairpoint silty clay loam, 8 to 25 percent slopes","Fairpoint",3,0.43,"HEL"]
["Guernsey","FcE","Fairpoint silty clay loam, 25 to 40 percent slopes","Fairpoint",3,0.43,"HEL"]
["Guernsey","FtA","Fitchville silt loam, 0 to 3 percent slopes","Fitchville",5,0.37,"NHEL"]
["Guernsey","GdB","Gilpin silt loam, 2 to 8 percent slopes","Gilpin",3,0.32,"PHEL"]
["Guernsey","GdC","Gilpin silt loam, 8 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Guernsey","GdD","Gilpin silt loam, 15 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Guernsey","GnA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Guernsey","GnB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Guernsey","GpA","Glenford-Urban land complex, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Guernsey","GrC","Guernsey silt loam, 8 to 15 percent slopes","Guernsey",3,0.43,"HEL"]
["Guernsey","GrD2","Guernsey silt loam, 15 to 25 percent slopes, eroded","Guernsey",3,0.43,"HEL"]
["Guernsey","GuC","Guernsey-Upshur complex, 8 to 15 percent slopes","Guernsey",3,0.43,"HEL"]
["Guernsey","GuD","Guernsey-Upshur complex, 15 to 25 percent slopes","Guernsey",3,0.43,"HEL"]
["Guernsey","HaF","Hazleton channery loam, 25 to 70 percent slopes, stony","Hazleton",3,0.17,"HEL"]
["Guernsey","HbE","Hazleton channery loam, 25 to 40 percent slopes","Hazleton",3,0.17,"HEL"]
["Guernsey","He","Hartshorn silt loam, occasionally flooded","Hartshorn",3,0.32,"NHEL"]
["Guernsey","Ho","Holton silt loam, occasionally flooded","Holton",5,0.37,"NHEL"]
["Guernsey","KaB","Kanawha loam, 2 to 6 percent slopes","Kanawha",5,0.32,"PHEL"]
["Guernsey","KeB","Keene silt loam, 1 to 8 percent slopes","Keene",4,0.37,"PHEL"]
["Guernsey","KeC","Keene silt loam, 8 to 15 percent slopes","Keene",4,0.37,"HEL"]
["Guernsey","Lc","Lindside silt loam, occasionally flooded","Lindside",5,0.28000000000000003,"NHEL"]
["Guernsey","Ld","Lindside silt loam, frequently flooded","Lindside",5,0.28000000000000003,"NHEL"]
["Guernsey","LoC","Lowell silt loam, 8 to 15 percent slopes","Lowell",3,0.37,"HEL"]
["Guernsey","LoD","Lowell silt loam, 15 to 25 percent slopes","Lowell",3,0.37,"HEL"]
["Guernsey","LuE","Lowell-Upshur complex, 25 to 40 percent slopes","Lowell",3,0.37,"HEL"]
["Guernsey","LwC","Lowell-Westmoreland complex, 8 to 15 percent slopes","Lowell",3,0.37,"HEL"]
["Guernsey","LwD","Lowell-Westmoreland complex, 15 to 25 percent slopes","Lowell",3,0.37,"HEL"]
["Guernsey","LwE","Lowell-Westmoreland complex, 25 to 40 percent slopes","Lowell",3,0.37,"HEL"]
["Guernsey","LwF","Lowell-Westmoreland complex, 40 to 70 percent slopes","Lowell",3,0.37,"HEL"]
["Guernsey","McA","McGary silt loam, 0 to 3 percent slopes","McGary",3,0.43,"NHEL"]
["Guernsey","Md","Melvin silt loam, ponded","Melvin",5,0.43,"NHEL"]
["Guernsey","MeB","Mentor silt loam, 2 to 8 percent slopes","Mentor",5,0.37,"PHEL"]
["Guernsey","MeC","Mentor silt loam, 8 to 15 percent slopes","Mentor",5,0.37,"HEL"]
["Guernsey","MeD","Mentor silt loam, 15 to 25 percent slopes","Mentor",5,0.37,"HEL"]
["Guernsey","MfB","Mentor-Urban land complex, 2 to 8 percent slopes","Mentor",5,0.37,"PHEL"]
["Guernsey","MnB","Morristown silty clay loam, 0 to 8 percent slopes","Morristown",3,0.43,"PHEL"]
["Guernsey","MnD","Morristown silty clay loam, 8 to 25 percent slopes","Morristown",3,0.43,"HEL"]
["Guernsey","MoF","Morristown channery clay loam, 40 to 70 percent slopes","Morristown",5,0.32,"HEL"]
["Guernsey","Nd","Newark silt loam, occasionally flooded","Newark",5,0.32,"NHEL"]
["Guernsey","Ne","Newark silt loam, frequently flooded","Newark",5,0.32,"NHEL"]
["Guernsey","No","Nolin silt loam, frequently flooded","Nolin",5,0.43,"NHEL"]
["Guernsey","OmB","Omulga silt loam, 1 to 6 percent slopes","Omulga",3,0.43,"PHEL"]
["Guernsey","OmC","Omulga silt loam, 6 to 15 percent slopes","Omulga",3,0.43,"HEL"]
["Guernsey","Or","Orrville silt loam, occasionally flooded","Orrville",5,0.37,"NHEL"]
["Guernsey","RcC","Richland channery loam, 8 to 15 percent slopes","Richland",5,0.37,"HEL"]
["Guernsey","RcD","Richland channery loam, 15 to 25 percent slopes","Richland",5,0.37,"HEL"]
["Guernsey","Sa","Sarahsville silty clay loam, frequently flooded","Sarahsville",3,0.43,"NHEL"]
["Guernsey","SeB","Sees silty clay loam, 2 to 6 percent slopes","Sees",3,0.37,"PHEL"]
["Guernsey","Ub","Udorthents, loamy-Rock outcrop complex","Udorthents"]
["Guernsey","Uc","Udorthents-Pits complex","Udorthents"]
["Guernsey","Ud","Udorthents-Urban land complex","Udorthents"]
["Guernsey","UpB","Upshur silt loam, 2 to 6 percent slopes","Upshur",3,0.43,"PHEL"]
["Guernsey","UrC","Upshur silty clay loam, 6 to 15 percent slopes","Upshur",3,0.43,"HEL"]
["Guernsey","UrD","Upshur silty clay loam, 15 to 25 percent slopes","Upshur",3,0.43,"HEL"]
["Guernsey","UrD3","Upshur silty clay loam, 15 to 25 percent slopes, severely eroded","Upshur",2,0.43,"HEL"]
["Guernsey","VaD2","Vandalia silty clay loam, 15 to 25 percent slopes, eroded","Vandalia",4,0.37,"HEL"]
["Guernsey","VtC","Vincent silt loam, 6 to 15 percent slopes","Vincent",3,0.43,"HEL"]
["Guernsey","VwB","Vincent silty clay loam, 2 to 6 percent slopes","Vincent",3,0.43,"PHEL"]
["Guernsey","W","Water","Water"]
["Guernsey","WhB","Wellston silt loam, 2 to 8 percent slopes","Wellston",4,0.37,"PHEL"]
["Guernsey","WhC","Wellston silt loam, 8 to 15 percent slopes","Wellston",4,0.37,"HEL"]
["Guernsey","WkB","Westmore silt loam, 2 to 8 percent slopes","Westmore",4,0.37,"PHEL"]
["Guernsey","WkC2","Westmore silt loam, 8 to 15 percent slopes, eroded","Westmore",4,0.37,"HEL"]
["Guernsey","WmC","Westmoreland silt loam, 8 to 15 percent slopes","Westmoreland",3,0.37,"HEL"]
["Guernsey","WmD","Westmoreland silt loam, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Guernsey","WmE","Westmoreland silt loam, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Guernsey","WnF","Westmoreland-Berks complex, 40 to 70 percent slopes","Westmoreland",3,0.37,"HEL"]
["Guernsey","WrC","Westmoreland-Urban land complex, 6 to 15 percent slopes","Westmoreland",3,0.37,"HEL"]
["Guernsey","WrD","Westmoreland-Urban land complex, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Guernsey","WtB","Woodsfield silt loam, 1 to 8 percent slopes","Woodsfield",3,0.43,"PHEL"]
["Guernsey","WtC","Woodsfield silt loam, 8 to 15 percent slopes","Woodsfield",3,0.43,"HEL"]
["Guernsey","ZnB","Zanesville silt loam, 2 to 6 percent slopes","Zanesville",3,0.43,"PHEL"]
["Guernsey","ZnC","Zanesville silt loam, 6 to 15 percent slopes","Zanesville",3,0.43,"HEL"]
["Guernsey","Zp","Zipp silty clay loam, frequently flooded","Zipp",5,0.28000000000000003,"NHEL"]
["Guernsey","Zs","Zipp silty clay loam, ponded","Zipp",5,0.28000000000000003,"NHEL"]
[null,"Select","none","none"]
["Harrison","AaB","Aaron silt loam, 2 to 6 percent slopes","Aaron",3,0.37,"PHEL"]
["Harrison","AbC2","Aaron silty clay loam, 6 to 15 percent slopes, eroded","Aaron",3,0.37,"HEL"]
["Harrison","BkC","Berks channery silt loam, 6 to 15 percent slopes","Berks",3,0.24,"PHEL"]
["Harrison","BkD","Berks channery silt loam, 15 to 25 percent slopes","Berks",3,0.24,"HEL"]
["Harrison","BkE","Berks channery silt loam, 25 to 40 percent slopes","Berks",3,0.24,"HEL"]
["Harrison","BkF","Berks channery silt loam, 40 to 70 percent slopes","Berks",3,0.24,"HEL"]
["Harrison","BmC","Berks-Aaron complex, 6 to 15 percent slopes","Berks",3,0.24,"HEL"]
["Harrison","BnD","Berks-Guernsey complex, 15 to 25 percent slopes","Berks",3,0.24,"HEL"]
["Harrison","BnE","Berks-Guernsey complex, 25 to 40 percent slopes","Berks",3,0.24,"HEL"]
["Harrison","BpB","Bethesda channery silty clay loam, 0 to 8 percent slopes","Bethesda",5,0.32,"PHEL"]
["Harrison","BpD","Bethesda channery silty clay loam, 8 to 25 percent slopes","Bethesda",5,0.32,"HEL"]
["Harrison","BpF","Bethesda channery silty clay loam, 25 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Harrison","BsD","Brookside silty clay loam, 15 to 25 percent slopes","Brookside",5,0.37,"HEL"]
["Harrison","Ca","Canadice silty clay loam","Canadice",5,0.49,"NHEL"]
["Harrison","CcA","Caneadea silty clay loam, 0 to 2 percent slopes","Caneadea",3,0.43,"NHEL"]
["Harrison","CnB","Coshocton silt loam, 2 to 6 percent slopes","Coshocton",4,0.37,"PHEL"]
["Harrison","CnC","Coshocton silt loam, 6 to 15 percent slopes","Coshocton",4,0.37,"HEL"]
["Harrison","CnD","Coshocton silt loam, 15 to 25 percent slopes","Coshocton",4,0.37,"HEL"]
["Harrison","DkC","Dekalb channery loam, 6 to 15 percent slopes","Dekalb",2,0.24,"HEL"]
["Harrison","Dm","Dumps, mine","Dumps"]
["Harrison","FaB","Fairpoint silty clay loam, 0 to 8 percent slopes","Fairpoint",3,0.43,"PHEL"]
["Harrison","FaD","Fairpoint silty clay loam, 8 to 25 percent slopes","Fairpoint",3,0.43,"HEL"]
["Harrison","FaE","Fairpoint silty clay loam, 25 to 40 percent slopes","Fairpoint",3,0.43,"HEL"]
["Harrison","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Harrison","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Harrison","GeC","Germano fine sandy loam, 6 to 15 percent slopes","Germano",4,0.24,"PHEL"]
["Harrison","GeD","Germano fine sandy loam, 15 to 25 percent slopes","Germano",4,0.24,"HEL"]
["Harrison","GnB","Gilpin silt loam, 2 to 6 percent slopes","Gilpin",3,0.32,"PHEL"]
["Harrison","GnC","Gilpin silt loam, 6 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Harrison","GnD","Gilpin silt loam, 15 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Harrison","GoC","Gilpin-Coshocton complex, 6 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Harrison","GoD","Gilpin-Coshocton complex, 15 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Harrison","GpC","Gilpin-Lowell complex, 6 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Harrison","GpD","Gilpin-Lowell complex, 15 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Harrison","GsB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Harrison","GsC","Glenford silt loam, 6 to 15 percent slopes","Glenford",5,0.37,"HEL"]
["Harrison","GtC","Guernsey silt loam, 6 to 15 percent slopes","Guernsey",3,0.43,"HEL"]
["Harrison","GuD2","Guernsey silty clay loam, 15 to 25 percent slopes, eroded","Guernsey",3,0.43,"HEL"]
["Harrison","GuE2","Guernsey silty clay loam, 25 to 40 percent slopes, eroded","Guernsey",3,0.43,"HEL"]
["Harrison","HeD","Hazleton channery sandy loam, 15 to 25 percent slopes","Hazleton",3,0.17,"HEL"]
["Harrison","HeE","Hazleton channery sandy loam, 25 to 40 percent slopes","Hazleton",3,0.17,"HEL"]
["Harrison","HeF","Hazleton channery sandy loam, 40 to 70 percent slopes","Hazleton",3,0.17,"HEL"]
["Harrison","KeB","Keene silt loam, 2 to 6 percent slopes","Keene",4,0.37,"PHEL"]
["Harrison","LnC","Lowell silt loam, 6 to 15 percent slopes","Lowell",3,0.37,"HEL"]
["Harrison","LoD2","Lowell silty clay loam, 15 to 25 percent slopes, eroded","Lowell",3,0.37,"HEL"]
["Harrison","LoE2","Lowell silty clay loam, 25 to 40 percent slopes, eroded","Lowell",3,0.37,"HEL"]
["Harrison","Me","Melvin silt loam, ponded","Melvin",5,0.43,"NHEL"]
["Harrison","MnB","Morristown silty clay loam, 0 to 8 percent slopes","Morristown",3,0.43,"PHEL"]
["Harrison","MnD","Morristown silty clay loam, 8 to 25 percent slopes","Morristown",3,0.43,"HEL"]
["Harrison","MoB","Morristown channery silty clay loam, 0 to 8 percent slopes, stony","Morristown",5,0.32,"PHEL"]
["Harrison","MoD","Morristown channery silty clay loam, 8 to 25 percent slopes, stony","Morristown",5,0.32,"HEL"]
["Harrison","MoE","Morristown channery silty clay loam, 25 to 40 percent slopes, stony","Morristown",5,0.32,"HEL"]
["Harrison","MrF","Morristown channery silt loam, 25 to 70 percent slopes, bouldery","Morristown",5,0.32,"HEL"]
["Harrison","No","Nolin silt loam, occasionally flooded","Nolin",5,0.43,"NHEL"]
["Harrison","Np","Nolin silt loam, frequently flooded","Nolin",5,0.43,"NHEL"]
["Harrison","OmB","Omulga silt loam, 2 to 6 percent slopes","Omulga",3,0.43,"PHEL"]
["Harrison","OmC","Omulga silt loam, 6 to 15 percent slopes","Omulga",3,0.43,"HEL"]
["Harrison","Or","Orrville silt loam, occasionally flooded","Orrville",5,0.37,"NHEL"]
["Harrison","OsB","Oshtemo loam, 2 to 6 percent slopes","Oshtemo",5,0.24,"NHEL"]
["Harrison","Pe","Peoga silt loam, rarely flooded","Peoga",4,0.43,"NHEL"]
["Harrison","RcB","Richland silt loam, 2 to 6 percent slopes","Richland",5,0.37,"PHEL"]
["Harrison","RcC","Richland silt loam, 6 to 15 percent slopes","Richland",5,0.37,"HEL"]
["Harrison","RgD","Rigley loam, 15 to 25 percent slopes","Rigley",4,0.24,"HEL"]
["Harrison","RgE","Rigley loam, 25 to 40 percent slopes","Rigley",4,0.24,"HEL"]
["Harrison","Tg","Tioga silt loam, occasionally flooded","Tioga",5,0.37,"NHEL"]
["Harrison","Ua","Udorthents","Udorthents"]
["Harrison","Uc","Udorthents-Pits complex","Udorthents"]
["Harrison","UpC2","Upshur silty clay loam, 6 to 15 percent slopes, eroded","Upshur",3,0.43,"HEL"]
["Harrison","UpD2","Upshur silty clay loam, 15 to 25 percent slopes, eroded","Upshur",3,0.43,"HEL"]
["Harrison","W","Water","water"]
["Harrison","WhC","Westmoreland silt loam, 6 to 15 percent slopes","Westmoreland",3,0.37,"HEL"]
["Harrison","WhD","Westmoreland silt loam, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Harrison","WhE","Westmoreland silt loam, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Harrison","WmE","Westmoreland-Coshocton complex, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Harrison","WnE","Westmoreland-Dekalb complex, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Harrison","WnF","Westmoreland-Dekalb complex, 40 to 70 percent slopes","Westmoreland",3,0.37,"HEL"]
["Harrison","WoF","Westmoreland-Dekalb complex, 25 to 70 percent slopes, extremely bouldery","Westmoreland",3,0.37,"HEL"]
[null,"Select","none","none"]
["Holmes","AmE","Amanda loam, 18 to 25 percent slopes","Amanda",4,0.37,"HEL"]
["Holmes","AwB","Amanda-Wooster complex, 2 to 6 percent slopes","Amanda",4,0.37,"PHEL"]
["Holmes","AwC2","Amanda-Wooster complex, 6 to 12 percent slopes, eroded","Amanda",4,0.37,"HEL"]
["Holmes","AwD2","Amanda-Wooster complex, 12 to 18 percent slopes, eroded","Amanda",4,0.37,"HEL"]
["Holmes","BkD","Berks silt loam, 15 to 25 percent slopes, very stony","Berks",3,0.24,"HEL"]
["Holmes","BkE","Berks silt loam, 25 to 35 percent slopes, very stony","Berks",3,0.24,"HEL"]
["Holmes","BkF","Berks silt loam, 35 to 70 percent slopes, very stony","Berks",3,0.24,"HEL"]
["Holmes","BnB","Bethesda very channery clay loam, 0 to 8 percent slopes","Bethesda",5,0.32,"PHEL"]
["Holmes","BnC","Bethesda very channery clay loam, 8 to 20 percent slopes","Bethesda",5,0.32,"HEL"]
["Holmes","BnF","Bethesda very channery clay loam, 20 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Holmes","BtA","Bogart silt loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Holmes","BtB","Bogart silt loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Holmes","BvD","Brownsville channery silt loam, 15 to 25 percent slopes","Brownsville",5,0.2,"PHEL"]
["Holmes","BvE","Brownsville channery silt loam, 25 to 35 percent slopes","Brownsville",5,0.2,"HEL"]
["Holmes","BvF","Brownsville channery silt loam, 35 to 70 percent slopes","Brownsville",5,0.2,"HEL"]
["Holmes","ByF","Brownsville-Rock outcrop complex, 35 to 70 percent slopes","Brownsville",5,0.2,"HEL"]
["Holmes","CdB","Canfield silt loam, 2 to 6 percent slopes","Canfield",4,0.37,"PHEL"]
["Holmes","CdC","Canfield silt loam, 6 to 12 percent slopes","Canfield",4,0.37,"PHEL"]
["Holmes","CdC2","Canfield silt loam, 6 to 12 percent slopes, eroded","Canfield",4,0.37,"PHEL"]
["Holmes","Ce","Carlisle muck","Carlisle",2,null,"NHEL"]
["Holmes","CgB","Centerburg silt loam, 2 to 6 percent slopes","Centerburg",4,0.37,"PHEL"]
["Holmes","CgC2","Centerburg silt loam, 6 to 12 percent slopes, eroded","Centerburg",4,0.37,"PHEL"]
["Holmes","CnA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Holmes","CnB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Holmes","CnC2","Chili loam, 6 to 12 percent slopes, eroded","Chili",4,0.32,"PHEL"]
["Holmes","CnD2","Chili loam, 12 to 18 percent slopes, eroded","Chili",4,0.32,"HEL"]
["Holmes","CnE","Chili loam, 18 to 25 percent slopes","Chili",4,0.32,"HEL"]
["Holmes","CnF","Chili loam, 25 to 70 percent slopes","Chili",4,0.32,"HEL"]
["Holmes","CoE","Chili-Amanda complex, 18 to 25 percent slopes","Chili",4,0.32,"HEL"]
["Holmes","CpA","Cidermill silt loam, 0 to 2 percent slopes","Cidermill",4,0.37,"NHEL"]
["Holmes","CpB","Cidermill silt loam, 2 to 6 percent slopes","Cidermill",4,0.37,"PHEL"]
["Holmes","CtB","Coshocton silt loam, 2 to 6 percent slopes","Coshocton",4,0.37,"PHEL"]
["Holmes","CtC2","Coshocton silt loam, 6 to 15 percent slopes, eroded","Coshocton",4,0.37,"HEL"]
["Holmes","CtD2","Coshocton silt loam, 15 to 25 percent slopes, eroded","Coshocton",4,0.37,"HEL"]
["Holmes","CtE","Coshocton silt loam, 25 to 40 percent slopes","Coshocton",4,0.37,"HEL"]
["Holmes","CvD","Coshocton silt loam, 12 to 25 percent slopes, very stony","Coshocton",4,0.37,"HEL"]
["Holmes","EuA","Euclid silt loam, occasionally flooded","Euclid",5,0.37,"NHEL"]
["Holmes","FaB","Fairpoint silt loam, 0 to 8 percent slopes","Fairpoint",3,0.43,"PHEL"]
["Holmes","FaC","Fairpoint silt loam, 8 to 20 percent slopes","Fairpoint",3,0.43,"HEL"]
["Holmes","FcB","Farmerstown silt loam, 0 to 8 percent slopes","Farmerstown",4,0.43,"PHEL"]
["Holmes","FcC","Farmerstown silt loam, 8 to 20 percent slopes","Farmerstown",4,0.43,"HEL"]
["Holmes","FhA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Holmes","FhB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Holmes","GhB","Gilpin silt loam, 3 to 8 percent slopes","Gilpin",3,0.32,"PHEL"]
["Holmes","GhC","Gilpin silt loam, 8 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Holmes","GnA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Holmes","GnB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Holmes","GnC2","Glenford silt loam, 6 to 12 percent slopes, eroded","Glenford",5,0.37,"PHEL"]
["Holmes","HtC","Hazleton loam, 8 to 15 percent slopes","Hazleton",3,0.17,"HEL"]
["Holmes","HtD","Hazleton loam, 15 to 25 percent slopes","Hazleton",3,0.17,"HEL"]
["Holmes","HtE","Hazleton loam, 25 to 40 percent slopes","Hazleton",3,0.17,"HEL"]
["Holmes","HvF","Hazleton loam, 25 to 70 percent slopes, very bouldery","Hazleton",3,0.17,"HEL"]
["Holmes","KeB","Keene silt loam, 2 to 6 percent slopes","Keene",4,0.37,"PHEL"]
["Holmes","Kk","Killbuck silt loam, frequently flooded","Killbuck",5,0.37,"NHEL"]
["Holmes","Lo","Lobdell silt loam, occasionally flooded","Lobdell",5,0.37,"NHEL"]
["Holmes","LvB","Loudonville silt loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Holmes","LvC","Loudonville silt loam, 6 to 12 percent slopes","Loudonville",4,0.32,"PHEL"]
["Holmes","LvD","Loudonville silt loam, 12 to 18 percent slopes","Loudonville",4,0.32,"HEL"]
["Holmes","LvE","Loudonville silt loam, 18 to 25 percent slopes","Loudonville",4,0.32,"HEL"]
["Holmes","Ly","Luray silty clay loam","Luray",5,0.32,"NHEL"]
["Holmes","McC","Mechanicsburg silt loam, 6 to 12 percent slopes","Mechanicsburg",5,0.37,"HEL"]
["Holmes","McD","Mechanicsburg silt loam, 12 to 18 percent slopes","Mechanicsburg",5,0.37,"HEL"]
["Holmes","Md","Melvin silt loam, frequently flooded","Melvin",5,0.43,"NHEL"]
["Holmes","Mg","Melvin silt loam, ponded","Melvin",5,0.43,"NHEL"]
["Holmes","Or","Orrville silt loam, occasionally flooded","Orrville",5,0.37,"NHEL"]
["Holmes","Pg","Pits, gravel","Pits"]
["Holmes","Pu","Pits, quarry","Pits"]
["Holmes","ReA","Ravenna silt loam, 0 to 2 percent slopes","Ravenna",3,0.37,"NHEL"]
["Holmes","ReB","Ravenna silt loam, 2 to 6 percent slopes","Ravenna",3,0.37,"PHEL"]
["Holmes","RgB","Rigley sandy loam, 3 to 8 percent slopes","Rigley",4,0.24,"PHEL"]
["Holmes","RgC","Rigley sandy loam, 8 to 15 percent slopes","Rigley",4,0.24,"PHEL"]
["Holmes","RgD","Rigley sandy loam, 15 to 25 percent slopes","Rigley",4,0.24,"HEL"]
["Holmes","ScD","Schaffenaker loamy sand, 12 to 25 percent slopes","Schaffenaker",3,0.17,"HEL"]
["Holmes","Se","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Holmes","Tg","Tioga loam, occasionally flooded","Tioga",5,0.37,"NHEL"]
["Holmes","Ud","Udorthents, loamy","Udorthents"]
["Holmes","Up","Udorthents-Pits complex","Udorthents"]
["Holmes","W","Water","Water"]
["Holmes","WeC2","Westmoreland silt loam, 8 to 15 percent slopes, eroded","Westmoreland",3,0.37,"HEL"]
["Holmes","WeD2","Westmoreland silt loam, 15 to 25 percent slopes, eroded","Westmoreland",3,0.37,"HEL"]
["Holmes","WeE","Westmoreland silt loam, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Holmes","WgC2","Westmoreland-Coshocton complex, 8 to 15 percent slopes, eroded","Westmoreland",3,0.37,"HEL"]
["Holmes","WgD2","Westmoreland-Coshocton complex, 15 to 25 percent slopes, eroded","Westmoreland",3,0.37,"HEL"]
["Holmes","WsB","Wooster silt loam, 2 to 6 percent slopes","Wooster",4,0.37,"PHEL"]
["Holmes","WsC","Wooster silt loam, 6 to 12 percent slopes","Wooster",4,0.37,"PHEL"]
["Holmes","WsC2","Wooster silt loam, 6 to 12 percent slopes, eroded","Wooster",4,0.37,"PHEL"]
["Holmes","WsD2","Wooster silt loam, 12 to 18 percent slopes, eroded","Wooster",4,0.37,"HEL"]
["Holmes","WtB","Wooster-Chili complex, 2 to 6 percent slopes","Wooster",4,0.37,"PHEL"]
["Holmes","WtC2","Wooster-Chili complex, 6 to 12 percent slopes, eroded","Wooster",4,0.37,"PHEL"]
["Holmes","WtD2","Wooster-Chili complex, 12 to 18 percent slopes, eroded","Wooster",4,0.37,"HEL"]
[null,"Select","none","none"]
["Jefferson","BkB","Berks shaly silt loam, 3 to 8 percent slopes","Berks",3,0.24,"PHEL"]
["Jefferson","BkC","Berks shaly silt loam, 8 to 15 percent slopes","Berks",3,0.24,"PHEL"]
["Jefferson","BkD","Berks shaly silt loam, 15 to 25 percent slopes","Berks",3,0.24,"HEL"]
["Jefferson","BmC","Berks-Guernsey complex, 8 to 15 percent slopes","Berks",3,0.24,"PHEL"]
["Jefferson","BmD","Berks-Guernsey complex, 15 to 25 percent slopes","Berks",3,0.24,"HEL"]
["Jefferson","BmE","Berks-Guernsey complex, 25 to 40 percent slopes","Berks",3,0.24,"HEL"]
["Jefferson","BnD","Bethesda silt loam, 8 to 25 percent slopes","Bethesda",3,0.43,"HEL"]
["Jefferson","BpC","Bethesda very channery clay loam, 3 to 15 percent slopes","Bethesda",5,0.32,"PHEL"]
["Jefferson","BpF","Bethesda very channery clay loam, 25 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Jefferson","BsC","Brookside silty clay loam, 8 to 15 percent slopes","Brookside",5,0.37,"PHEL"]
["Jefferson","BsD","Brookside silty clay loam, 15 to 25 percent slopes","Brookside",5,0.37,"HEL"]
["Jefferson","BsE","Brookside silty clay loam, 25 to 40 percent slopes","Brookside",5,0.37,"HEL"]
["Jefferson","CkD","Clarksburg silt loam, 15 to 25 percent slopes","Clarksburg",3,0.37,"HEL"]
["Jefferson","CmD","Clarksburg-Urban land complex, 15 to 25 percent slopes","Clarksburg",3,0.37,"HEL"]
["Jefferson","CnB","Coshocton silt loam, 1 to 7 percent slopes","Coshocton",4,0.37,"PHEL"]
["Jefferson","DkE","Dekalb channery loam, 25 to 40 percent slopes","Dekalb",2,0.24,"HEL"]
["Jefferson","DkF","Dekalb channery loam, 40 to 70 percent slopes","Dekalb",2,0.24,"HEL"]
["Jefferson","Ds","Dumps, mine","Dumps"]
["Jefferson","EbC2","Elba silty clay loam, 8 to 15 percent slopes, eroded","Elba",3,0.43,"HEL"]
["Jefferson","EbD2","Elba silty clay loam, 15 to 25 percent slopes, eroded","Elba",3,0.43,"HEL"]
["Jefferson","FaC","Fairpoint silt loam, 3 to 15 percent slopes","Fairpoint",3,0.43,"PHEL"]
["Jefferson","FbC","Fairpoint very shaly clay loam, 3 to 15 percent slopes","Fairpoint",3,0.43,"PHEL"]
["Jefferson","FbF","Fairpoint very shaly clay loam, 25 to 70 percent slopes","Fairpoint",3,0.43,"HEL"]
["Jefferson","FcB","Fitchville variant silt loam, 1 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Jefferson","GnB","Gilpin silt loam, 3 to 8 percent slopes","Gilpin",3,0.32,"PHEL"]
["Jefferson","GnC","Gilpin silt loam, 8 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Jefferson","GnD","Gilpin silt loam, 15 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Jefferson","GoC","Gilpin-Coshocton silt loams, 8 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Jefferson","GoD","Gilpin-Coshocton silt loams, 15 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Jefferson","GpC","Gilpin-Lowell silt loams, 8 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Jefferson","GpD","Gilpin-Lowell silt loams, 15 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Jefferson","GsB","Glenford silt loam, 1 to 7 percent slopes","Glenford",5,0.37,"PHEL"]
["Jefferson","GsC","Glenford silt loam, 7 to 15 percent slopes","Glenford",5,0.37,"HEL"]
["Jefferson","GuB","Guernsey silt loam, 1 to 7 percent slopes","Guernsey",3,0.43,"PHEL"]
["Jefferson","GvC2","Guernsey silty clay loam, 7 to 15 percent slopes, eroded","Guernsey",3,0.43,"HEL"]
["Jefferson","HfE","Hazleton-Summitville complex, 15 to 40 percent slopes","Hazleton",3,0.17,"HEL"]
["Jefferson","HgE","Hazleton-Westmoreland complex, 25 to 40 percent slopes","Hazleton",3,0.17,"HEL"]
["Jefferson","HgF","Hazleton-Westmoreland complex, 40 to 70 percent slopes","Hazleton",3,0.17,"HEL"]
["Jefferson","KeB","Keene silt loam, 1 to 7 percent slopes","Keene",4,0.37,"PHEL"]
["Jefferson","LnB","Lowell silt loam, 1 to 7 percent slopes","Lowell",3,0.37,"PHEL"]
["Jefferson","LnC","Lowell silt loam, 7 to 15 percent slopes","Lowell",3,0.37,"HEL"]
["Jefferson","LoD2","Lowell silty clay loam, 15 to 25 percent slopes, eroded","Lowell",3,0.37,"HEL"]
["Jefferson","LoE","Lowell silty clay loam, 25 to 40 percent slopes","Lowell",3,0.37,"HEL"]
["Jefferson","LoF","Lowell silty clay loam, 40 to 70 percent slopes","Lowell",3,0.37,"HEL"]
["Jefferson","Me","Melvin silt loam, ponded","Melvin",5,0.43,"NHEL"]
["Jefferson","MnA","Morristown silty clay loam, 0 to 3 percent slopes","Morristown",3,0.43,"PHEL"]
["Jefferson","MnC","Morristown silty clay loam, 3 to 15 percent slopes","Morristown",3,0.43,"PHEL"]
["Jefferson","MnE","Morristown silty clay loam, 15 to 40 percent slopes","Morristown",3,0.43,"HEL"]
["Jefferson","MoA","Morristown shaly silty clay loam, 0 to 3 percent slopes, stony","Morristown",5,0.32,"NHEL"]
["Jefferson","MoC","Morristown shaly silty clay loam, 3 to 15 percent slopes, stony","Morristown",5,0.32,"PHEL"]
["Jefferson","MrF","Morristown shaly silty clay loam, 25 to 70 percent slopes, bouldery","Morristown",5,0.32,"HEL"]
["Jefferson","No","Nolin silt loam, occasionally flooded","Nolin",5,0.43,"NHEL"]
["Jefferson","OmB","Omulga silt loam, 1 to 7 percent slopes","Omulga",3,0.43,"PHEL"]
["Jefferson","OmC","Omulga silt loam, 7 to 15 percent slopes","Omulga",3,0.43,"HEL"]
["Jefferson","Or","Orrville silt loam, occasionally flooded","Orrville",5,0.37,"NHEL"]
["Jefferson","PeB","Pekin silt loam, 1 to 7 percent slopes","Pekin",4,0.43,"PHEL"]
["Jefferson","RcB","Richland silt loam, 1 to 7 percent slopes","Richland",5,0.37,"PHEL"]
["Jefferson","RcC","Richland silt loam, 7 to 15 percent slopes","Richland",5,0.37,"HEL"]
["Jefferson","RgC","Rigley sandy loam, 8 to 15 percent slopes","Rigley",4,0.24,"HEL"]
["Jefferson","RgD","Rigley sandy loam, 15 to 25 percent slopes","Rigley",4,0.24,"HEL"]
["Jefferson","StB","Steinsburg-Rigley variant fine sandy loams, 3 to 8 percent slopes","Steinsburg",2,0.28000000000000003,"PHEL"]
["Jefferson","StC","Steinsburg-Rigley variant fine sandy loams, 8 to 15 percent slopes","Steinsburg",2,0.28000000000000003,"HEL"]
["Jefferson","StD","Steinsburg-Rigley variant fine sandy loams, 15 to 25 percent slopes","Steinsburg",2,0.28000000000000003,"HEL"]
["Jefferson","Tf","Tioga loam, rarely flooded","Tioga",5,0.37,"NHEL"]
["Jefferson","Tg","Tioga silt loam, occasionally flooded","Tioga",5,0.37,"NHEL"]
["Jefferson","Ub","Udorthents, loamy","Udorthents"]
["Jefferson","Uc","Udorthents-Pits complex","Udorthents"]
["Jefferson","Ud","Udorthents-Urban land complex","Udorthents"]
["Jefferson","UpC2","Upshur silty clay loam, 8 to 15 percent slopes, eroded","Upshur",3,0.43,"HEL"]
["Jefferson","Ur","Urban land","Urban"]
["Jefferson","UsA","Urban land-Chavies complex, 0 to 3 percent slopes","Urban"]
["Jefferson","UtC","Urban land-Gilpin-Lowell complex, 8 to 15 percent slopes","Urban",null,null,"HEL"]
["Jefferson","UtD","Urban land-Gilpin-Lowell complex, 15 to 25 percent slopes","Urban",null,null,"HEL"]
["Jefferson","UvC","Urban land-Omulga complex, 3 to 15 percent slopes","Urban"]
["Jefferson","UwB","Urban land-Steinsburg complex, 3 to 8 percent slopes","Urban"]
["Jefferson","W","Water","Water"]
["Jefferson","WeB","Wellston silt loam, 1 to 7 percent slopes","Wellston",4,0.37,"PHEL"]
["Jefferson","WkC","Westmoreland silt loam, 8 to 15 percent slopes","Westmoreland",3,0.37,"HEL"]
["Jefferson","WkD","Westmoreland silt loam, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Jefferson","WtE","Westmoreland-Berks complex, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Jefferson","WtF","Westmoreland-Berks complex, 40 to 70 percent slopes","Westmoreland",3,0.37,"HEL"]
["Jefferson","WuF","Westmoreland-Lowell complex, 40 to 70 percent slopes","Westmoreland",3,0.37,"HEL"]
["Jefferson","WvA","Wheeling silt loam, 0 to 3 percent slopes","Wheeling",4,0.37,"NHEL"]
[null,"Select","none","none"]
["Knox","AdD2","Amanda silt loam, 12 to 18 percent slopes, eroded","Amanda",4,0.37,"HEL"]
["Knox","AdF2","Amanda silt loam, 18 to 40 percent slopes, eroded","Amanda",4,0.37,"HEL"]
["Knox","BnA","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Knox","BnB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Knox","BoA","Bogart silt loam, 0 to 2 percent slopes","Bogart",5,0.32,"NHEL"]
["Knox","BoB","Bogart silt loam, 2 to 6 percent slopes","Bogart",5,0.32,"PHEL"]
["Knox","BrC","Brownsville channery silt loam, 6 to 12 percent slopes","Brownsville",5,0.2,"PHEL"]
["Knox","BrD","Brownsville channery silt loam, 12 to 18 percent slopes","Brownsville",5,0.2,"PHEL"]
["Knox","BsE","Brownsville-Westmoreland complex, 18 to 25 percent slopes","Brownsville",5,0.2,"HEL"]
["Knox","BsF","Brownsville-Westmoreland complex, 25 to 40 percent slopes","Brownsville",5,0.2,"HEL"]
["Knox","BuG","Brownsville-Rock outcrop complex, 35 to 60 percent slopes","Brownsville",5,0.2,"HEL"]
["Knox","CaB","Canfield silt loam, 2 to 6 percent slopes","Canfield",4,0.37,"PHEL"]
["Knox","CaC","Canfield silt loam, 6 to 12 percent slopes","Canfield",4,0.37,"PHEL"]
["Knox","CdB","Centerburg silt loam, 2 to 6 percent slopes","Centerburg",4,0.37,"PHEL"]
["Knox","CdB2","Centerburg silt loam, 2 to 6 percent slopes, eroded","Centerburg",4,0.37,"PHEL"]
["Knox","CdC","Centerburg silt loam, 6 to 12 percent slopes","Centerburg",4,0.37,"PHEL"]
["Knox","CdC2","Centerburg silt loam, 6 to 12 percent slopes, eroded","Centerburg",4,0.37,"PHEL"]
["Knox","ChB","Chili gravelly loam, 2 to 6 percent slopes","Chili",4,0.24,"PHEL"]
["Knox","ChC","Chili gravelly loam, 6 to 12 percent slopes","Chili",4,0.24,"PHEL"]
["Knox","ChD","Chili gravelly loam, 12 to 18 percent slopes","Chili",4,0.24,"HEL"]
["Knox","ChE","Chili gravelly loam, 18 to 25 percent slopes","Chili",4,0.24,"HEL"]
["Knox","CmA","Chili silt loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Knox","CmB","Chili silt loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Knox","CnC","Chili-Homewood silt loams, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Knox","CnD","Chili-Homewood silt loams, 12 to 18 percent slopes","Chili",4,0.32,"HEL"]
["Knox","Cr","Condit silt loam","Condit",5,0.37,"NHEL"]
["Knox","CvB","Coshocton silt loam, 2 to 6 percent slopes","Coshocton",4,0.37,"PHEL"]
["Knox","CvC","Coshocton silt loam, 6 to 12 percent slopes","Coshocton",4,0.37,"PHEL"]
["Knox","CvD","Coshocton silt loam, 12 to 18 percent slopes","Coshocton",4,0.37,"HEL"]
["Knox","CzA","Crane silt loam, 1 to 4 percent slopes","Crane",5,0.28000000000000003,"NHEL"]
["Knox","DAM","Dam","Dam"]
["Knox","Du","Dumps","Dumps"]
["Knox","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Knox","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Knox","FoA","Fox gravelly loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Knox","FoB","Fox gravelly loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Knox","FoC","Fox gravelly loam, 6 to 12 percent slopes","Fox",4,0.37,"PHEL"]
["Knox","FoD","Fox gravelly loam, 12 to 25 percent slopes","Fox",4,0.37,"HEL"]
["Knox","GhB","Gilpin silt loam, 2 to 6 percent slopes","Gilpin",3,0.32,"PHEL"]
["Knox","GhC","Gilpin silt loam, 6 to 12 percent slopes","Gilpin",3,0.32,"PHEL"]
["Knox","GnA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Knox","GnB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Knox","GnC","Glenford silt loam, 6 to 12 percent slopes","Glenford",5,0.37,"PHEL"]
["Knox","GrB","Gresham silt loam, 2 to 6 percent slopes","Gresham",4,0.37,"PHEL"]
["Knox","Ho","Holly silt loam, frequently flooded","Holly",5,0.28000000000000003,"NHEL"]
["Knox","HwB","Homewood silt loam, 2 to 6 percent slopes","Homewood",4,0.37,"PHEL"]
["Knox","HwC","Homewood silt loam, 6 to 12 percent slopes","Homewood",4,0.37,"PHEL"]
["Knox","HwD2","Homewood silt loam, 12 to 18 percent slopes, eroded","Homewood",4,0.37,"HEL"]
["Knox","HwE2","Homewood silt loam, 18 to 25 percent slopes, eroded","Homewood",4,0.37,"HEL"]
["Knox","JmA","Jimtown silt loam, 0 to 2 percent slopes","Jimtown",4,0.32,"NHEL"]
["Knox","JmB","Jimtown silt loam, 2 to 6 percent slopes","Jimtown",4,0.32,"PHEL"]
["Knox","La","Landes fine sandy loam, occasionally flooded","Landes",5,0.2,"NHEL"]
["Knox","Ln","Linwood muck","Linwood",2,null,"NHEL"]
["Knox","Lo","Lobdell silt loam, occasionally flooded","Lobdell",5,0.37,"NHEL"]
["Knox","LvB","Loudonville silt loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Knox","LvC","Loudonville silt loam, 6 to 12 percent slopes","Loudonville",4,0.32,"PHEL"]
["Knox","LvD","Loudonville silt loam, 12 to 18 percent slopes","Loudonville",4,0.32,"HEL"]
["Knox","LvE","Loudonville silt loam, 18 to 25 percent slopes","Loudonville",4,0.32,"HEL"]
["Knox","Ly","Luray silty clay loam","Luray",5,0.32,"NHEL"]
["Knox","Md","Medway silt loam, occasionally flooded","Medway",5,0.32,"NHEL"]
["Knox","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Knox","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Knox","Or","Orrville silt loam, occasionally flooded","Orrville",5,0.37,"NHEL"]
["Knox","Pc","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Knox","Pg","Pits, gravel","Pits"]
["Knox","Pu","Pits, quarry","Pits"]
["Knox","RgB","Rigley sandy loam, 2 to 6 percent slopes","Rigley",4,0.24,"PHEL"]
["Knox","RgC","Rigley sandy loam, 6 to 12 percent slopes","Rigley",4,0.24,"PHEL"]
["Knox","RgD","Rigley sandy loam, 12 to 18 percent slopes","Rigley",4,0.24,"HEL"]
["Knox","RhE","Rigley-Coshocton complex, 18 to 25 percent slopes","Rigley",4,0.24,"HEL"]
["Knox","RmB","Rittman silt loam, 2 to 6 percent slopes","Rittman",4,0.43,"PHEL"]
["Knox","RmC2","Rittman silt loam, 6 to 12 percent slopes, eroded","Rittman",4,0.43,"PHEL"]
["Knox","ScD","Schaffenaker loamy sand, 12 to 25 percent slopes","Schaffenaker",3,0.17,"HEL"]
["Knox","SdF","Schaffenaker very bouldery loamy sand, 25 to 60 percent slopes","Schaffenaker",3,0.17,"HEL"]
["Knox","Se","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Knox","Sh","Shoals silt loam, occasionally flooded","Shoals",5,0.37,"NHEL"]
["Knox","Sn","Sloan silt loam, occasionally flooded","Sloan",5,0.37,"NHEL"]
["Knox","Tg","Tioga fine sandy loam, occasionally flooded","Tioga",5,0.37,"NHEL"]
["Knox","TvB","Titusville silt loam, 2 to 6 percent slopes","Titusville",4,0.37,"PHEL"]
["Knox","TvC","Titusville silt loam, 6 to 12 percent slopes","Titusville",4,0.37,"PHEL"]
["Knox","Ud","Udorthents, loamy","Udorthents"]
["Knox","W","Water","Water"]
["Knox","WaB","Wadsworth silt loam, 1 to 4 percent slopes","Wadsworth",4,0.43,"PHEL"]
["Knox","WeD","Westmoreland silt loam, 12 to 18 percent slopes","Westmoreland",3,0.37,"HEL"]
["Knox","WsB","Wooster silt loam, 2 to 6 percent slopes","Wooster",4,0.37,"PHEL"]
["Knox","WsC","Wooster silt loam, 6 to 12 percent slopes","Wooster",4,0.37,"PHEL"]
["Knox","WsD2","Wooster silt loam, 12 to 18 percent slopes, eroded","Wooster",4,0.37,"HEL"]
["Knox","WsE2","Wooster silt loam, 18 to 40 percent slopes, eroded","Wooster",4,0.37,"HEL"]
[null,"Select","none","none"]
["Licking","Ab","Abandoned Canal","Abandoned"]
["Licking","AfA","Alford silt loam, 0 to 2 percent slopes","Alford",5,0.37,"NHEL"]
["Licking","AfB","Alford silt loam, 2 to 6 percent slopes","Alford",5,0.37,"PHEL"]
["Licking","AfC2","Alford silt loam, 6 to 12 percent slopes, eroded","Alford",5,0.37,"PHEL"]
["Licking","AhB","Alford-Urban land complex, 2 to 6 percent slopes","Alford",5,0.37,"PHEL"]
["Licking","Ak","Algiers silt loam, frequently flooded","Algiers",5,0.37,"NHEL"]
["Licking","AmB2","Amanda silt loam, 2 to 6 percent slopes, eroded","Amanda",4,0.37,"PHEL"]
["Licking","AmC2","Amanda silt loam, 6 to 12 percent slopes, eroded","Amanda",4,0.37,"PHEL"]
["Licking","AmD2","Amanda silt loam, 12 to 18 percent slopes, eroded","Amanda",4,0.37,"HEL"]
["Licking","AmE","Amanda silt loam, 18 to 25 percent slopes","Amanda",4,0.37,"HEL"]
["Licking","AmF","Amanda silt loam, 25 to 50 percent slopes","Amanda",4,0.37,"HEL"]
["Licking","AvC2","Amanda variant silt loam, 6 to 12 percent slopes, eroded","Amanda",5,0.37,"PHEL"]
["Licking","AvD2","Amanda variant silt loam, 12 to 18 percent slopes, eroded","Amanda",5,0.37,"HEL"]
["Licking","BeA","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Licking","BeB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Licking","BfA","Bennington-Urban land complex, 0 to 3 percent slopes","Bennington",3,0.43,"NHEL"]
["Licking","BgB","Berks channery silt loam, 2 to 6 percent slopes","Berks",3,0.24,"PHEL"]
["Licking","BgD","Berks channery silt loam, 12 to 18 percent slopes","Berks",3,0.24,"HEL"]
["Licking","BrC","Brownsville channery silt loam, 6 to 12 percent slopes","Brownsville",5,0.2,"PHEL"]
["Licking","BrD","Brownsville channery silt loam, 12 to 18 percent slopes","Brownsville",5,0.2,"PHEL"]
["Licking","BrE","Brownsville channery silt loam, 18 to 25 percent slopes","Brownsville",5,0.2,"HEL"]
["Licking","BrF","Brownsville channery silt loam, 25 to 35 percent slopes","Brownsville",5,0.2,"HEL"]
["Licking","BrG","Brownsville channery silt loam, 35 to 70 percent slopes","Brownsville",5,0.2,"HEL"]
["Licking","Ca","Carlisle muck","Carlisle",2,null,"NHEL"]
["Licking","CeB","Centerburg silt loam, 2 to 6 percent slopes","Centerburg",4,0.37,"PHEL"]
["Licking","CeC2","Centerburg silt loam, 6 to 12 percent slopes, eroded","Centerburg",4,0.37,"PHEL"]
["Licking","CfB","Centerburg-Urban land complex, 2 to 6 percent slopes","Centerburg",4,0.37,"PHEL"]
["Licking","CfC","Centerburg-Urban land complex, 6 to 12 percent slopes","Centerburg",4,0.37,"PHEL"]
["Licking","ChA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Licking","ChB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Licking","ChC2","Chili loam, 6 to 12 percent slopes, eroded","Chili",4,0.32,"PHEL"]
["Licking","ChD2","Chili loam, 12 to 18 percent slopes, eroded","Chili",4,0.32,"HEL"]
["Licking","ChE2","Chili loam, 18 to 25 percent slopes, eroded","Chili",4,0.32,"HEL"]
["Licking","CkB","Cincinnati silt loam, 2 to 6 percent slopes","Cincinnati",4,0.37,"PHEL"]
["Licking","CkC2","Cincinnati silt loam, 6 to 12 percent slopes, eroded","Cincinnati",4,0.37,"PHEL"]
["Licking","CmC2","Clarksburg silt loam, 6 to 12 percent slopes, eroded","Clarksburg",3,0.37,"PHEL"]
["Licking","CmD2","Clarksburg silt loam, 12 to 18 percent slopes, eroded","Clarksburg",3,0.37,"HEL"]
["Licking","Cn","Condit silt loam","Condit",5,0.37,"NHEL"]
["Licking","CoB","Coshocton silt loam, 2 to 6 percent slopes","Coshocton",4,0.37,"PHEL"]
["Licking","CoC2","Coshocton silt loam, 6 to 12 percent slopes, eroded","Coshocton",4,0.37,"PHEL"]
["Licking","CoD2","Coshocton silt loam, 12 to 18 percent slopes, eroded","Coshocton",4,0.37,"HEL"]
["Licking","CoE2","Coshocton silt loam, 18 to 25 percent slopes, eroded","Coshocton",4,0.37,"HEL"]
["Licking","CrA","Crane silt loam, 0 to 2 percent slopes","Crane",5,0.28000000000000003,"NHEL"]
["Licking","FaD","Fairpoint silty clay loam, 8 to 25 percent slopes","Fairpoint",3,0.43,"HEL"]
["Licking","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Licking","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Licking","FoD2","Fox gravelly loam, 12 to 18 percent slopes, eroded","Fox",4,0.37,"HEL"]
["Licking","FoE2","Fox gravelly loam, 18 to 25 percent slopes, eroded","Fox",4,0.37,"HEL"]
["Licking","FrB","Frankstown variant-Mertz complex, 2 to 6 percent slopes, very stony","Frankstown",4,0.28000000000000003,"PHEL"]
["Licking","GfA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Licking","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Licking","GnB","Guernsey silt loam, 2 to 6 percent slopes","Guernsey",3,0.43,"PHEL"]
["Licking","GnC2","Guernsey silt loam, 6 to 12 percent slopes, eroded","Guernsey",3,0.43,"HEL"]
["Licking","GnD","Guernsey silt loam, 12 to 18 percent slopes","Guernsey",3,0.43,"HEL"]
["Licking","HeF","Hazleton-Rock outcrop complex, 25 to 70 percent slopes","Hazleton",3,0.17,"HEL"]
["Licking","HkC2","Hickory silt loam, 6 to 12 percent slopes, eroded","Hickory",5,0.37,"PHEL"]
["Licking","HkD2","Hickory silt loam, 12 to 18 percent slopes, eroded","Hickory",5,0.37,"HEL"]
["Licking","HoB","Homewood silt loam, 2 to 6 percent slopes","Homewood",4,0.37,"PHEL"]
["Licking","HoC2","Homewood silt loam, 6 to 12 percent slopes, eroded","Homewood",4,0.37,"PHEL"]
["Licking","HoD2","Homewood silt loam, 12 to 18 percent slopes, eroded","Homewood",4,0.37,"HEL"]
["Licking","HoE2","Homewood silt loam, 18 to 25 percent slopes, eroded","Homewood",4,0.37,"HEL"]
["Licking","KeB","Keene silt loam, 2 to 6 percent slopes","Keene",4,0.37,"PHEL"]
["Licking","KeC2","Keene silt loam, 6 to 12 percent slopes, eroded","Keene",4,0.37,"PHEL"]
["Licking","KeD2","Keene silt loam, 12 to 18 percent slopes, eroded","Keene",4,0.37,"HEL"]
["Licking","Kk","Killbuck silt loam, frequently flooded","Killbuck",5,0.37,"NHEL"]
["Licking","Lu","Luray silty clay loam","Luray",5,0.32,"NHEL"]
["Licking","McB","Mechanicsburg silt loam, 2 to 6 percent slopes","Mechanicsburg",5,0.37,"PHEL"]
["Licking","McC2","Mechanicsburg silt loam, 6 to 12 percent slopes, eroded","Mechanicsburg",5,0.37,"PHEL"]
["Licking","McD2","Mechanicsburg silt loam, 12 to 18 percent slopes, eroded","Mechanicsburg",5,0.37,"HEL"]
["Licking","McE","Mechanicsburg silt loam, 18 to 25 percent slopes","Mechanicsburg",5,0.37,"HEL"]
["Licking","Md","Medway silt loam, occasionally flooded","Medway",5,0.32,"NHEL"]
["Licking","Me","Melvin silt loam, frequently flooded","Melvin",5,0.43,"NHEL"]
["Licking","MnA","Mentor silt loam, 0 to 2 percent slopes","Mentor",5,0.37,"NHEL"]
["Licking","MnB","Mentor silt loam, 2 to 6 percent slopes","Mentor",5,0.37,"PHEL"]
["Licking","MnC2","Mentor silt loam, 6 to 12 percent slopes, eroded","Mentor",5,0.37,"PHEL"]
["Licking","MnD2","Mentor silt loam, 12 to 18 percent slopes, eroded","Mentor",5,0.37,"HEL"]
["Licking","MrE","Mertz very cherty silt loam, 18 to 35 percent slopes, very stony","Mertz",4,0.28000000000000003,"HEL"]
["Licking","NeC2","Negley loam, 6 to 12 percent slopes, eroded","Negley",3,0.32,"PHEL"]
["Licking","NeD2","Negley loam, 12 to 18 percent slopes, eroded","Negley",3,0.32,"HEL"]
["Licking","NeE","Negley loam, 18 to 25 percent slopes","Negley",3,0.32,"HEL"]
["Licking","NeF","Negley loam, 25 to 70 percent slopes","Negley",3,0.32,"HEL"]
["Licking","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Licking","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Licking","OcC2","Ockley silt loam, 6 to 12 percent slopes, eroded","Ockley",5,0.37,"PHEL"]
["Licking","OeA","Ockley-Urban land complex, 0 to 3 percent slopes","Ockley",5,0.37,"NHEL"]
["Licking","OeC","Ockley-Urban land complex, 6 to 12 percent slopes","Ockley",5,0.37,"PHEL"]
["Licking","Or","Orrville silt loam, occasionally flooded","Orrville",5,0.37,"NHEL"]
["Licking","PaC2","Parke silt loam, 6 to 12 percent slopes, eroded","Parke",5,0.37,"PHEL"]
["Licking","Pe","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Licking","Pf","Pewamo-Urban land complex","Pewamo",5,0.24,"NHEL"]
["Licking","Pg","Pits, gravel","Pits"]
["Licking","RgC","Rigley fine sandy loam, 6 to 12 percent slopes","Rigley",4,0.24,"PHEL"]
["Licking","RgD","Rigley fine sandy loam, 12 to 18 percent slopes","Rigley",4,0.24,"HEL"]
["Licking","RgE","Rigley fine sandy loam, 18 to 25 percent slopes","Rigley",4,0.24,"HEL"]
["Licking","RgF","Rigley fine sandy loam, 25 to 35 percent slopes","Rigley",4,0.24,"HEL"]
["Licking","RhE","Rigley-Coshocton complex, 18 to 25 percent slopes","Rigley",4,0.24,"HEL"]
["Licking","RsA","Rush silt loam, 0 to 2 percent slopes","Rush",5,0.37,"NHEL"]
["Licking","Se","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Licking","Sh","Shoals silt loam, occasionally flooded","Shoals",5,0.37,"NHEL"]
["Licking","SkA","Sleeth silt loam, 0 to 2 percent slopes","Sleeth",5,0.32,"NHEL"]
["Licking","So","Sloan silt loam, frequently flooded","Sloan",5,0.37,"NHEL"]
["Licking","St","Stonelick loam, occasionally flooded","Stonelick",5,0.24,"NHEL"]
["Licking","Su","Stonelick-Urban land complex, occasionally flooded","Stonelick",5,0.24,"NHEL"]
["Licking","Tg","Tioga fine sandy loam, occasionally flooded","Tioga",5,0.37,"NHEL"]
["Licking","TsB","Titusville silt loam, 2 to 6 percent slopes","Titusville",4,0.37,"PHEL"]
["Licking","TsC2","Titusville silt loam, 6 to 12 percent slopes, eroded","Titusville",4,0.37,"PHEL"]
["Licking","Uf","Udorthents, loamy","Udorthents"]
["Licking","W","Water","Water"]
["Licking","Wa","Wallkill silt loam, clayey substratum, frequently flooded","Wallkill",5,0.32,"NHEL"]
["Licking","Ws","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
["Licking","Wt","Westland-Urban land complex","Westland",5,0.28000000000000003,"NHEL"]
[null,"Select","none","none"]
["Monroe","AsA","Ashton silt loam, 0 to 3 percent slopes","Ashton",5,0.32,"NHEL"]
["Monroe","BwD2","Brooke silty clay loam, 12 to 18 percent slopes, moderately eroded","Brooke",3,0.37,"HEL"]
["Monroe","BwE2","Brooke silty clay loam, 18 to 35 percent slopes, moderately eroded","Brooke",3,0.37,"HEL"]
["Monroe","CaB","Captina silt loam, 2 to 6 percent slopes","Captina",5,0.43,"PHEL"]
["Monroe","CaC2","Captina silt loam, 6 to 12 percent slopes, moderately eroded","Captina",5,0.43,"PHEL"]
["Monroe","CaD2","Captina silt loam, 12 to 18 percent slopes, moderately eroded","Captina",5,0.43,"HEL"]
["Monroe","Cg","Chagrin silt loam","Chagrin",5,0.32,"NHEL"]
["Monroe","CoA","Conotton gravelly loam, 0 to 2 percent slopes","Conotton",3,0.24,"NHEL"]
["Monroe","CoD","Conotton gravelly loam, 6 to 18 percent slopes","Conotton",3,0.24,"PHEL"]
["Monroe","CrC2","Coolville-Rarden silt loams, 6 to 12 percent slopes, moderately eroded","Coolville",4,0.43,"PHEL"]
["Monroe","CrD2","Coolville-Rarden silt loams, 12 to 18 percent slopes, moderately eroded","Coolville",4,0.43,"HEL"]
["Monroe","DkC2","Dekalb loam, 6 to 12 percent slopes, moderately eroded","Dekalb",2,0.24,"PHEL"]
["Monroe","DkD2","Dekalb loam, 12 to 18 percent slopes, moderately eroded","Dekalb",2,0.24,"HEL"]
["Monroe","DkE2","Dekalb loam, 18 to 35 percent slopes, moderately eroded","Dekalb",2,0.24,"HEL"]
["Monroe","GdE","Gilpin and Dekalb very stony soils, 12 to 35 percent slopes","Gilpin",3,0.32,"HEL"]
["Monroe","GdG","Gilpin and Dekalb very stony soils, 35 to 70 percent slopes","Gilpin",3,0.32,"HEL"]
["Monroe","GkB2","Gilpin-Upshur complex, 2 to 6 percent slopes, moderately eroded","Gilpin",3,0.32,"PHEL"]
["Monroe","GkC2","Gilpin-Upshur complex, 6 to 12 percent slopes, moderately eroded","Gilpin",3,0.32,"PHEL"]
["Monroe","GkD","Gilpin-Upshur complex, 12 to 18 percent slopes","Gilpin",3,0.32,"HEL"]
["Monroe","GkD2","Gilpin-Upshur complex, 12 to 18 percent slopes, moderately eroded","Gilpin",3,0.32,"HEL"]
["Monroe","GkE2","Gilpin-Upshur complex, 18 to 35 percent slopes, moderately eroded","Gilpin",3,0.32,"HEL"]
["Monroe","GkE3","Gilpin-Upshur complex, 18 to 35 percent slopes, severely eroded","Gilpin",3,0.32,"HEL"]
["Monroe","GkG","Gilpin-Upshur complex, 35 to 70 percent slopes","Gilpin",3,0.32,"HEL"]
["Monroe","GkG3","Gilpin-Upshur complex, 35 to 70 percent slopes, severely eroded","Gilpin",3,0.32,"HEL"]
["Monroe","GlE","Gilpin-Upshur complex, steep, benched","Gilpin",3,0.32,"HEL"]
["Monroe","GlG","Gilpin-Upshur complex, very steep, benched","Gilpin",3,0.32,"HEL"]
["Monroe","GnE","Gilpin-Upshur very stony complex, 12 to 35 percent slopes","Gilpin",3,0.32,"HEL"]
["Monroe","GnG","Gilpin-Upshur very stony complex, 35 to 70 percent slopes","Gilpin",3,0.32,"HEL"]
["Monroe","GoB2","Gilpin-Westmoreland silt loams, 2 to 6 percent slopes, moderately eroded","Gilpin",3,0.32,"PHEL"]
["Monroe","GoC2","Gilpin-Westmoreland silt loams, 6 to 12 percent slopes, moderately eroded","Gilpin",3,0.32,"PHEL"]
["Monroe","GoD2","Gilpin-Westmoreland silt loams, 12 to 18 percent slopes, moderately eroded","Gilpin",3,0.32,"HEL"]
["Monroe","GoD3","Gilpin-Westmoreland silt loams, 12 to 18 percent slopes, severely eroded","Gilpin",3,0.32,"HEL"]
["Monroe","GoE2","Gilpin-Westmoreland silt loams, 18 to 35 percent slopes, moderately eroded","Gilpin",3,0.32,"HEL"]
["Monroe","GoE3","Gilpin-Westmoreland silt loams, 18 to 35 percent slopes, severely eroded","Gilpin",3,0.32,"HEL"]
["Monroe","GoG2","Gilpin-Westmoreland silt loams, 35 to 70 percent slopes, moderately eroded","Gilpin",3,0.32,"HEL"]
["Monroe","GpG","Gilpin-Westmoreland silt loams, very steep, benched","Gilpin",3,0.32,"HEL"]
["Monroe","GrC2","Guernsey-Upshur complex, 6 to 12 percent slopes, moderately eroded","Guernsey",3,0.43,"PHEL"]
["Monroe","GrD2","Guernsey-Upshur complex, 12 to 18 percent slopes, moderately eroded","Guernsey",3,0.43,"HEL"]
["Monroe","GrE2","Guernsey-Upshur complex, 18 to 35 percent slopes, moderately eroded","Guernsey",3,0.43,"HEL"]
["Monroe","GrG2","Guernsey-Upshur complex, 35 to 70 percent slopes, moderately eroded","Guernsey",3,0.43,"HEL"]
["Monroe","GsG","Guernsey-Upshur complex, 18 to 70 percent slopes, landslip","Guernsey",3,0.43,"HEL"]
["Monroe","GuE","Guernsey-Upshur complex, steep, benched","Guernsey",3,0.43,"HEL"]
["Monroe","GuG","Guernsey-Upshur complex, very steep, benched","Guernsey",3,0.43,"HEL"]
["Monroe","GwC2","Guernsey-Westmore silt loams, 6 to 12 percent slopes, moderately eroded","Guernsey",3,0.43,"PHEL"]
["Monroe","GwD2","Guernsey-Westmore silt loams, 12 to 18 percent slopes, moderately eroded","Guernsey",3,0.43,"HEL"]
["Monroe","GwE2","Guernsey-Westmore silt loams, 18 to 35 percent slopes, moderately eroded","Guernsey",3,0.43,"HEL"]
["Monroe","GwE3","Guernsey-Westmore silt loams, 18 to 35 percent slopes, severely eroded","Guernsey",3,0.43,"HEL"]
["Monroe","GwG2","Guernsey-Westmore silt loams, 35 to 70 percent slopes, moderately eroded","Guernsey",3,0.43,"HEL"]
["Monroe","Gy","Gullied land, Gilpin-Upshur material","Gullied"]
["Monroe","HcB","Hackers silt loam, 3 to 8 percent slopes","Hackers",4,0.32,"PHEL"]
["Monroe","He","Hartshorn silt loam","Hartshorn",3,0.32,"NHEL"]
["Monroe","Hr","Hartshorn silt loam, wet variant","Hartshorn",4,0.37,"NHEL"]
["Monroe","Hu","Huntington silt loam","Huntington",5,0.28000000000000003,"NHEL"]
["Monroe","KeB","Keene silt loam, 2 to 6 percent slopes","Keene",4,0.37,"PHEL"]
["Monroe","KeC2","Keene silt loam, 6 to 12 percent slopes, moderately eroded","Keene",4,0.37,"PHEL"]
["Monroe","KlD2","Keene-Latham silt loam, 12 to 18 percent slopes, moderately eroded","Keene",4,0.37,"HEL"]
["Monroe","LdE2","Latham-Keene silt loams, 18 to 35 percent slopes, moderately eroded","Latham",3,0.43,"HEL"]
["Monroe","Lh","Lindside silt loam","Lindside",5,0.28000000000000003,"NHEL"]
["Monroe","Ma","Made land","Made"]
["Monroe","Nn","Newark silt loam","Newark",5,0.32,"NHEL"]
["Monroe","RcD2","Rarden-Coolville silt loams, 12 to 18 percent slopes, moderately eroded","Rarden",3,0.43,"HEL"]
["Monroe","ScB","Sciotoville silt loam, 0 to 4 percent slopes","Sciotoville",4,0.37,"PHEL"]
["Monroe","SsD","Sees-Woolper silt loams, 12 to 18 percent slopes","Sees",3,0.37,"HEL"]
["Monroe","SsE","Sees-Woolper silt loams, 18 to 35 percent slopes","sees",3,0.37,"HEL"]
["Monroe","St","Strip mine spoils","Strip Mine"]
["Monroe","UpC2","Upshur silt loam, 6 to 12 percent slopes, moderately eroded","Upshur",3,0.43,"PHEL"]
["Monroe","UpD2","Upshur silt loam, 12 to 18 percent slopes, moderately eroded","Upshur",3,0.43,"HEL"]
["Monroe","UrC3","Upshur clay, 6 to 12 percent slopes, severely eroded","Upshur",2,0.43,"HEL"]
["Monroe","UrD3","Upshur clay, 12 to 18 percent slopes, severely eroded","Upshur",2,0.43,"HEL"]
["Monroe","VaD","Vandalia silt loam, 12 to 18 percent slopes","Vandalia",4,0.37,"HEL"]
["Monroe","VdE","Vandalia-Sees silt loams, 18 to 35 percent slopes","Vandalia",4,0.37,"HEL"]
["Monroe","VsE2","Vandalia-Sees very stony silt loams, 18 to 35 percent slopes, moderately eroded","Vandalia",4,0.37,"HEL"]
["Monroe","W","Water","Water"]
["Monroe","WhB2","Wellston silt loam, 2 to 6 percent slopes, moderately eroded","Wellston",4,0.37,"PHEL"]
["Monroe","WhC2","Wellston silt loam, 6 to 12 percent slopes, moderately eroded","Wellston",4,0.37,"PHEL"]
["Monroe","WhD2","Wellston silt loam, 12 to 18 percent slopes, moderately eroded","Wellston",4,0.37,"HEL"]
["Monroe","WrA","Wheeling silt loam, 0 to 2 percent slopes","Wheeling",4,0.37,"NHEL"]
["Monroe","WrB","Wheeling silt loam, 2 to 6 percent slopes","Wheeling",4,0.37,"PHEL"]
["Monroe","WrC2","Wheeling silt loam, 6 to 18 percent slopes, moderately eroded","Wheeling",4,0.37,"PHEL"]
["Monroe","WtB","Woodsfield silt loam, 2 to 6 percent slopes","Woodsfield",3,0.43,"PHEL"]
["Monroe","WtC2","Woodsfield silt loam, 6 to 12 percent slopes, moderately eroded","Woodsfield",3,0.43,"PHEL"]
["Monroe","WtD2","Woodsfield silt loam, 12 to 18 percent slopes, moderately eroded","Woodsfield",3,0.43,"HEL"]
["Monroe","WxB","Woolper silt loam, 2 to 6 percent slopes","Woolper",3,0.37,"PHEL"]
["Monroe","WyC","Woolper and Sees silt loams, 6 to 12 percent slopes","Woolper",3,0.37,"PHEL"]
["Monroe","ZnB","Zanesville silt loam, 2 to 6 percent slopes","Zanesville",3,0.43,"PHEL"]
["Monroe","ZnB2","Zanesville silt loam, 2 to 6 percent slopes, moderately eroded","Zanesville",3,0.43,"PHEL"]
["Monroe","ZnC","Zanesville silt loam, 6 to 12 percent slopes","Zanesville",3,0.43,"PHEL"]
["Monroe","ZnC2","Zanesville silt loam, 6 to 12 percent slopes, moderately eroded","Zanesville",3,0.43,"PHEL"]
["Monroe","ZnD2","Zanesville silt loam, 12 to 18 percent slopes, moderately eroded","Zanesville",3,0.43,"HEL"]
["Monroe","ZoB","Zanesville-Woodsfield silt loams, 2 to 6 percent slopes","Zanesville",3,0.43,"PHEL"]
["Monroe","ZoB2","Zanesville-Woodsfield silt loams, 2 to 6 percent slopes, moderately eroded","Zanesville",3,0.43,"PHEL"]
["Monroe","ZoC","Zanesville-Woodsfield silt loams, 6 to 12 percent slopes","Zanesville",3,0.43,"PHEL"]
["Monroe","ZoC2","Zanesville-Woodsfield silt loams, 6 to 12 percent slopes, moderately eroded","Zanesville",3,0.43,"PHEL"]
["Monroe","ZoD2","Zanesville-Woodsfield silt loams, 12 to 18 percent slopes, moderately eroded","Zanesville",3,0.43,"HEL"]
[null,"Select","none","none"]
["Morgan","AaC2","Aaron silt loam, 6 to 12 percent slopes, eroded","Aaron",3,0.37,"HEL"]
["Morgan","AgC2","Aaron-Gilpin complex, 6 to 12 percent slopes, eroded","Aaron",3,0.37,"HEL"]
["Morgan","BaF","Barkcamp channery sandy loam, 20 to 70 percent slopes","Barkcamp",5,0.24,"HEL"]
["Morgan","BdF","Berks channery silt loam, 35 to 70 percent slopes","Berks",3,0.24,"HEL"]
["Morgan","BeF","Berks-Westmoreland complex, 35 to 70 percent slopes","Berks",3,0.24,"HEL"]
["Morgan","BkF","Bethesda channery loam, 20 to 70 percent slopes","Bethesda",3,0.43,"HEL"]
["Morgan","BrD","Brookside silty clay loam, 12 to 20 percent slopes","Brookside",5,0.37,"HEL"]
["Morgan","BrE","Brookside silty clay loam, 20 to 35 percent slopes","Brookside",5,0.37,"HEL"]
["Morgan","Ca","Chagrin silt loam, frequently flooded","Chagrin",5,0.32,"NHEL"]
["Morgan","CeB","Chavies loam, 0 to 6 percent slopes","Chavies",4,0.24,"PHEL"]
["Morgan","CgC","Claysville-Guernsey complex, 8 to 15 percent slopes","Claysville",5,0.28000000000000003,"HEL"]
["Morgan","CoB","Conotton gravelly loam, 0 to 6 percent slopes","Conotton",3,0.24,"PHEL"]
["Morgan","CoC2","Conotton gravelly loam, 6 to 12 percent slopes, eroded","Conotton",3,0.24,"PHEL"]
["Morgan","Ds","Dumps, mine","Dumps"]
["Morgan","EbE2","Elba silty clay loam, 20 to 35 percent slopes, eroded","Elba",3,0.43,"HEL"]
["Morgan","EuA","Euclid silt loam, rarely flooded","Euclid",5,0.37,"NHEL"]
["Morgan","GdC2","Gilpin silt loam, 6 to 12 percent slopes, eroded","Gilpin",3,0.32,"PHEL"]
["Morgan","GhD2","Gilpin-Upshur complex, 12 to 20 percent slopes, eroded","Gilpin",3,0.32,"HEL"]
["Morgan","GhE2","Gilpin-Upshur complex, 20 to 35 percent slopes, eroded","Gilpin",3,0.32,"HEL"]
["Morgan","GhF","Gilpin-Upshur complex, 35 to 70 percent slopes","Gilpin",3,0.32,"HEL"]
["Morgan","GnB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Morgan","GsD2","Guernsey-Upshur complex, 12 to 20 percent slopes, eroded","Guernsey",3,0.43,"HEL"]
["Morgan","LcB","Licking silt loam, 0 to 6 percent slopes","Licking",3,0.43,"PHEL"]
["Morgan","LcC2","Licking silt loam, 6 to 12 percent slopes","Licking",3,0.43,"HEL"]
["Morgan","Ld","Lobdell silt loam, channery substratum, occasionally flooded","Lobdell",5,0.37,"NHEL"]
["Morgan","LoD2","Lowell silt loam, 12 to 20 percent slopes, eroded","Lowell",3,0.37,"HEL"]
["Morgan","LrE2","Lowell-Gilpin complex, 20 to 35 percent slopes, eroded","Lowell",3,0.37,"HEL"]
["Morgan","LrF","Lowell-Gilpin complex, 35 to 70 percent slopes","Lowell",3,0.37,"HEL"]
["Morgan","MaD2","Markland silty clay loam, 12 to 25 percent slopes, eroded","Markland",3,0.43,"HEL"]
["Morgan","Md","Melvin silt loam, ponded","Melvin",5,0.43,"NHEL"]
["Morgan","MeB","Mentor silt loam, 0 to 6 percent slopes","Mentor",5,0.37,"PHEL"]
["Morgan","MnB","Morristown silty clay loam, 0 to 6 percent slopes","Morristown",3,0.43,"PHEL"]
["Morgan","MnD","Morristown silty clay loam, 6 to 20 percent slopes","Morristown",3,0.43,"HEL"]
["Morgan","MnE","Morristown silty clay loam, 20 to 35 percent slopes","Morristown",3,0.43,"HEL"]
["Morgan","MpB","Morristown channery clay loam, 0 to 6 percent slopes","Morristown",5,0.32,"PHEL"]
["Morgan","MpD","Morristown channery clay loam, 6 to 20 percent slopes","Morristown",5,0.32,"HEL"]
["Morgan","MrF","Morristown channery clay loam, 20 to 70 percent slopes, very stony","Morristown",5,0.32,"HEL"]
["Morgan","Ne","Newark silt loam, frequently flooded","Newark",5,0.32,"NHEL"]
["Morgan","No","Nolin silt loam, occasionally flooded","Nolin",5,0.43,"NHEL"]
["Morgan","Np","Nolin silt loam, frequently flooded","Nolin",5,0.43,"NHEL"]
["Morgan","OmB","Omulga silt loam, 2 to 6 percent slopes","Omulga",3,0.43,"PHEL"]
["Morgan","OmC2","Omulga silt loam, 6 to 12 percent slopes","Omulga",3,0.43,"HEL"]
["Morgan","Pg","Pits, gravel","Pits"]
["Morgan","RvE","Richland-Vandalia complex, 20 to 35 percent slopes","Richland",5,0.37,"HEL"]
["Morgan","StF","Steinsburg loam, 25 to 70 percent slopes","Steinsburg",2,0.28000000000000003,"HEL"]
["Morgan","Ud","Udorthents","Udorthents"]
["Morgan","UpC2","Upshur silty clay loam, 6 to 12 percent slopes, eroded","Upshur",3,0.43,"HEL"]
["Morgan","UpD2","Upshur silty clay loam, 12 to 20 percent slopes, eroded","Upshur",3,0.43,"HEL"]
["Morgan","VaE2","Vandalia silt loam, 20 to 35 percent slopes, eroded","Vandalia",4,0.37,"HEL"]
["Morgan","VbD2","Vandalia-Brookside complex, 12 to 20 percent slopes, eroded","Vandalia",4,0.37,"HEL"]
["Morgan","W","Water","Water"]
["Morgan","WeB","Wellston silt loam, 2 to 6 percent slopes","Wellston",4,0.37,"PHEL"]
["Morgan","WeC2","Wellston silt loam, 6 to 12 percent slopes, eroded","Wellston",4,0.37,"PHEL"]
["Morgan","WfB","Westgate silt loam, 2 to 6 percent slopes","Westgate",4,0.43,"PHEL"]
["Morgan","WfC2","Westgate silt loam, 6 to 12 percent slopes, eroded","Westgate",4,0.43,"HEL"]
["Morgan","WgD2","Westmoreland-Guernsey complex, 12 to 20 percent slopes, eroded","Westmoreland",3,0.37,"HEL"]
["Morgan","WgE2","Westmoreland-Guernsey complex, 20 to 35 percent slopes, eroded","Westmoreland",3,0.37,"HEL"]
["Morgan","WgF","Westmoreland-Guernsey complex, 35 to 70 percent slopes","Westmoreland",3,0.37,"HEL"]
["Morgan","WyB","Woodsfield silt loam, 2 to 6 percent slopes","woodsfield",3,0.43,"PHEL"]
["Morgan","WyC2","Woodsfield silt loam, 6 to 12 percent slopes, eroded","woodsfield",3,0.43,"HEL"]
["Morgan","ZnB","Zanesville silt loam, 2 to 6 percent slopes","Zanesville",3,0.43,"PHEL"]
["Morgan","ZnC2","Zanesville silt loam, 6 to 12 percent slopes, eroded","Zanesville",3,0.43,"HEL"]
[null,"Select","none","none"]
["Muskingum","AaB","Aaron silt loam, 2 to 8 percent slopes","Aaron",3,0.37,"PHEL"]
["Muskingum","AaC2","Aaron silt loam, 8 to 15 percent slopes, eroded","Aaron",3,0.37,"HEL"]
["Muskingum","AaD2","Aaron silt loam, 15 to 25 percent slopes, eroded","Aaron",3,0.37,"HEL"]
["Muskingum","AcB","Aaron-Upshur complex, 2 to 6 percent slopes","Aaron",3,0.37,"PHEL"]
["Muskingum","AfB","Alford silt loam, 2 to 8 percent slopes","Alford",5,0.37,"PHEL"]
["Muskingum","AfC2","Alford silt loam, 8 to 15 percent slopes, eroded","Alford",5,0.37,"PHEL"]
["Muskingum","BeB","Berks channery silt loam, 2 to 8 percent slopes","Berks",3,0.24,"PHEL"]
["Muskingum","BeD2","Berks channery silt loam, 15 to 25 percent slopes, eroded","Berks",3,0.24,"HEL"]
["Muskingum","BeE","Berks channery silt loam, 25 to 40 percent slopes","Berks",3,0.24,"HEL"]
["Muskingum","BkF","Berks-Westmoreland complex, 40 to 70 percent slopes","Berks",3,0.24,"HEL"]
["Muskingum","BoB","Bethesda shaly silt loam, 1 to 15 percent slopes","Bethesda",5,0.32,"PHEL"]
["Muskingum","BoD","Bethesda shaly silt loam, 15 to 25 percent slopes","Bethesda",5,0.32,"HEL"]
["Muskingum","BpF","Bethesda flaggy silt loam, 25 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Muskingum","BsC2","Brookside silty clay loam, 8 to 15 percent slopes, eroded","Brookside",5,0.37,"HEL"]
["Muskingum","BsE","Brookside silty clay loam, 15 to 40 percent slopes","Brookside",5,0.37,"HEL"]
["Muskingum","Cb","Chagrin loam, rarely flooded","Chagrin",5,0.32,"NHEL"]
["Muskingum","CcA","Chavies loam, 0 to 2 percent slopes","Chavies",4,0.24,"NHEL"]
["Muskingum","CcB","Chavies loam, 2 to 6 percent slopes","Chavies",4,0.24,"PHEL"]
["Muskingum","CeA","Chili loam, 0 to 3 percent slopes","Chili",4,0.32,"NHEL"]
["Muskingum","CeB","Chili loam, 3 to 8 percent slopes","Chili",4,0.32,"PHEL"]
["Muskingum","ChA","Chili gravelly loam, 0 to 3 percent slopes","Chili",4,0.24,"NHEL"]
["Muskingum","ChB","Chili gravelly loam, 3 to 8 percent slopes","Chili",4,0.24,"PHEL"]
["Muskingum","ChC","Chili gravelly loam, 8 to 15 percent slopes","Chili",4,0.24,"PHEL"]
["Muskingum","CkA","Cidermill silt loam, 0 to 3 percent slopes","Cidermill",4,0.37,"NHEL"]
["Muskingum","CnB","Cincinnati silt loam, 2 to 6 percent slopes","Cincinnati",4,0.37,"PHEL"]
["Muskingum","CnC2","Cincinnati silt loam, 6 to 15 percent slopes, eroded","Cincinnati",4,0.37,"PHEL"]
["Muskingum","CpC2","Clarksburg silt loam, 8 to 15 percent slopes, eroded","Clarksburg",3,0.37,"PHEL"]
["Muskingum","CrC","Claysville-Guernsey silty clay loams, 8 to 15 percent slopes","Claysville",5,0.28000000000000003,"HEL"]
["Muskingum","CsC2","Coshocton silt loam, 8 to 15 percent slopes, eroded","Coshocton",4,0.37,"PHEL"]
["Muskingum","CsD","Coshocton silt loam, 15 to 25 percent slopes","Coshocton",4,0.37,"HEL"]
["Muskingum","CtE","Coshocton-Westmoreland silt loams, 25 to 40 percent slopes","Coshocton",4,0.37,"HEL"]
["Muskingum","Ds","Dumps and Pits, mine","Dumps"]
["Muskingum","FaB","Fairpoint silty clay loam, 1 to 15 percent slopes","Fairpoint",3,0.43,"PHEL"]
["Muskingum","FaD","Fairpoint silty clay loam, 15 to 25 percent slopes","Fairpoint",3,0.43,"HEL"]
["Muskingum","FaE","Fairpoint silty clay loam, 25 to 50 percent slopes","Fairpoint",3,0.43,"HEL"]
["Muskingum","FbF","Fairpoint channery silty clay loam, 25 to 70 percent slopes","Fairpoint",3,0.43,"HEL"]
["Muskingum","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Muskingum","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Muskingum","FkB","Frankstown variant-Mertz complex, 3 to 8 percent slopes","Frankstown",4,0.37,"PHEL"]
["Muskingum","GdB","Gilpin silt loam, 2 to 8 percent slopes","Gilpin",3,0.32,"PHEL"]
["Muskingum","GdC2","Gilpin silt loam, 8 to 15 percent slopes, eroded","Gilpin",3,0.32,"HEL"]
["Muskingum","GeD2","Gilpin-Upshur complex, 15 to 25 percent slopes, eroded","Gilpin",3,0.32,"HEL"]
["Muskingum","GeE2","Gilpin-Upshur complex, 25 to 40 percent slopes, eroded","Gilpin",3,0.32,"HEL"]
["Muskingum","GfA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Muskingum","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Muskingum","GfC2","Glenford silt loam, 6 to 15 percent slopes, eroded","Glenford",5,0.37,"PHEL"]
["Muskingum","GtC2","Guernsey-Upshur silty clay loams, 6 to 15 percent slopes, eroded","Guernsey",3,0.43,"HEL"]
["Muskingum","GtD2","Guernsey-Upshur silty clay loams, 15 to 25 percent slopes, eroded","Guernsey",3,0.43,"HEL"]
["Muskingum","HaC2","Homewood silt loam, 8 to 15 percent slopes, eroded","Homewood",4,0.37,"PHEL"]
["Muskingum","HaD2","Homewood silt loam, 15 to 20 percent slopes, eroded","Homewood",4,0.37,"HEL"]
["Muskingum","JtA","Jimtown loam, 0 to 3 percent slopes","Jimtown",4,0.32,"NHEL"]
["Muskingum","KeB","Keene silt loam, 2 to 6 percent slopes","Keene",4,0.37,"PHEL"]
["Muskingum","KeC2","Keene silt loam, 6 to 15 percent slopes, eroded","Keene",4,0.37,"PHEL"]
["Muskingum","Km","Killbuck silt loam, occasionally flooded","Killbuck",5,0.37,"NHEL"]
["Muskingum","LaC","Lakin loamy fine sand, 8 to 15 percent slopes","Lakin",5,0.17,"PHEL"]
["Muskingum","LcD","Lakin-Alford complex, 15 to 25 percent slopes","Lakin",5,0.17,"HEL"]
["Muskingum","Lk","Lindside silt loam, occasionally flooded","Lindside",5,0.28000000000000003,"NHEL"]
["Muskingum","Lm","Lobdell loam, channery substratum, occasionally flooded","Lobdell",5,0.37,"NHEL"]
["Muskingum","Lo","Lorain silty clay","Lorain",5,0.32,"NHEL"]
["Muskingum","LpC2","Lowell silt loam, 8 to 15 percent slopes, eroded","Lowell",3,0.37,"HEL"]
["Muskingum","LpD2","Lowell silt loam, 15 to 25 percent slopes, eroded","Lowell",3,0.37,"HEL"]
["Muskingum","LrE2","Lowell-Gilpin complex, 25 to 40 percent slopes, eroded","Lowell",3,0.37,"HEL"]
["Muskingum","LrF","Lowell-Gilpin complex, 40 to 70 percent slopes","Lowell",3,0.37,"HEL"]
["Muskingum","Lu","Luray silty clay loam","Luray",5,0.32,"NHEL"]
["Muskingum","MaB","Markland silt loam, 2 to 6 percent slopes","Markland",3,0.43,"PHEL"]
["Muskingum","MbC2","Markland silty clay loam, 6 to 15 percent slopes, eroded","Markland",3,0.43,"PHEL"]
["Muskingum","McD2","Markland-Glenford complex, 15 to 35 percent slopes, eroded","Markland",3,0.43,"HEL"]
["Muskingum","MdA","McGary silt loam, 0 to 3 percent slopes","McGary",3,0.43,"NHEL"]
["Muskingum","Me","Melvin silt loam, frequently flooded","Melvin",5,0.43,"NHEL"]
["Muskingum","MkD","Mertz very cherty silt loam, 15 to 35 percent slopes","Mertz",4,0.28000000000000003,"HEL"]
["Muskingum","MrB","Morristown shaly silty clay loam, 1 to 15 percent slopes","Morristown",5,0.32,"PHEL"]
["Muskingum","MrD","Morristown shaly silty clay loam, 15 to 25 percent slopes","Morristown",5,0.32,"HEL"]
["Muskingum","MrF","Morristown shaly silty clay loam, 25 to 70 percent slopes","Morristown",5,0.32,"HEL"]
["Muskingum","MsB","Morristown silty clay loam, 1 to 8 percent slopes","Morristown",3,0.43,"PHEL"]
["Muskingum","MsC","Morristown silty clay loam, 8 to 15 percent slopes","Morristown",3,0.43,"HEL"]
["Muskingum","MsD","Morristown silty clay loam, 15 to 25 percent slopes","Morristown",3,0.43,"HEL"]
["Muskingum","MsE","Morristown silty clay loam, 25 to 50 percent slopes","Morristown",3,0.43,"HEL"]
["Muskingum","Ne","Newark silt loam, frequently flooded","Newark",5,0.32,"NHEL"]
["Muskingum","No","Nolin silt loam, occasionally flooded","Nolin",5,0.43,"NHEL"]
["Muskingum","OmB","Omulga silt loam, 2 to 6 percent slopes","Omulga",3,0.43,"PHEL"]
["Muskingum","OmC","Omulga silt loam, 6 to 15 percent slopes","Omulga",3,0.43,"HEL"]
["Muskingum","RaB","Rawson silt loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Muskingum","RfC","Rigley loam, 8 to 15 percent slopes","Rigley",4,0.24,"PHEL"]
["Muskingum","RgD","Rigley channery loam, 15 to 25 percent slopes","Rigley",4,0.24,"HEL"]
["Muskingum","RhE","Rigley-Coshocton complex, 25 to 40 percent slopes","Rigley",4,0.24,"HEL"]
["Muskingum","RoF","Rodman gravelly sandy loam, 25 to 70 percent slopes","Rodman",3,0.15,"HEL"]
["Muskingum","Se","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Muskingum","St","Stonelick loam, occasionally flooded","Stonelick",5,0.24,"NHEL"]
["Muskingum","Ta","Tioga fine sandy loam, rarely flooded","Tioga",5,0.37,"NHEL"]
["Muskingum","Tf","Tioga fine sandy loam, occasionally flooded","Tioga",5,0.37,"NHEL"]
["Muskingum","Ud","Udorthents, loamy, hilly","Udorthents"]
["Muskingum","Ug","Udorthents, sandy, rolling","Udorthents"]
["Muskingum","Uh","Udorthents, sandy-skeletal, steep","Udorthents"]
["Muskingum","Uk","Udorthents-Pits complex","Udorthents"]
["Muskingum","UsB","Urban land-Glenford complex, 2 to 8 percent slopes","Urban"]
["Muskingum","UtA","Urban land-Nolin complex, rarely flooded","Urban"]
["Muskingum","UvB","Urban land-Watertown complex, 1 to 15 percent slopes","Urban"]
["Muskingum","UwC","Urban land-Wellston complex, 5 to 15 percent slopes","Urban"]
["Muskingum","W","Water","Water"]
["Muskingum","WaB","Watertown sandy loam, 1 to 8 percent slopes","Watertown",4,0.17,"PHEL"]
["Muskingum","WaC","Watertown sandy loam, 8 to 15 percent slopes","Watertown",4,0.17,"PHEL"]
["Muskingum","WhB","Wellston silt loam, 2 to 8 percent slopes","Wellston",4,0.37,"PHEL"]
["Muskingum","WhC2","Wellston silt loam, 8 to 15 percent slopes, eroded","Wellston",4,0.37,"PHEL"]
["Muskingum","WmB","Westgate silt loam, 2 to 6 percent slopes","Westgate",4,0.43,"PHEL"]
["Muskingum","WmC2","Westgate silt loam, 6 to 15 percent slopes, eroded","Westgate",4,0.43,"PHEL"]
["Muskingum","WtC2","Westmoreland silt loam, 8 to 15 percent slopes, eroded","Westmoreland",3,0.37,"HEL"]
["Muskingum","WtD2","Westmoreland silt loam, 15 to 25 percent slopes, eroded","Westmoreland",3,0.37,"HEL"]
["Muskingum","WtE","Westmoreland silt loam, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Muskingum","WuC2","Westmoreland-Guernsey silt loams, 8 to 15 percent slopes, eroded","Westmoreland",3,0.37,"HEL"]
["Muskingum","WuD2","Westmoreland-Guernsey silt loams, 15 to 25 percent slopes, eroded","Westmoreland",3,0.37,"HEL"]
["Muskingum","WuE2","Westmoreland-Guernsey silt loams, 25 to 40 percent slopes, eroded","Westmoreland",3,0.37,"HEL"]
["Muskingum","WvD","Westmoreland-Urban land complex, 15 to 35 percent slopes","Westmoreland",3,0.37,"HEL"]
["Muskingum","ZnB","Zanesville silt loam, 2 to 6 percent slopes","Zanesville",3,0.43,"PHEL"]
["Muskingum","ZnC2","Zanesville silt loam, 6 to 15 percent slopes, eroded","Zanesville",3,0.43,"PHEL"]
[null,"Select","none","none"]
["Noble","BaB","Barkcamp channery sandy loam, 0 to 8 percent slopes, very stony","Barkcamp",5,0.24,"PHEL"]
["Noble","BaF","Barkcamp channery sandy loam, 25 to 70 percent slopes, very stony","Barkcamp",5,0.24,"HEL"]
["Noble","BkC","Berks shaly silt loam, 8 to 15 percent slopes","Berks",3,0.24,"PHEL"]
["Noble","BkD","Berks shaly silt loam, 15 to 25 percent slopes","Berks",3,0.24,"HEL"]
["Noble","BkE","Berks shaly silt loam, 25 to 35 percent slopes","Berks",3,0.24,"HEL"]
["Noble","BkF","Berks shaly silt loam, 35 to 70 percent slopes","Berks",3,0.24,"HEL"]
["Noble","BnD","Bethesda silty clay loam, 15 to 25 percent slopes","Bethesda",3,0.43,"HEL"]
["Noble","BoB","Bethesda very shaly silty clay loam, 0 to 8 percent slopes","Bethesda",5,0.32,"PHEL"]
["Noble","BoF","Bethesda very shaly silty clay loam, 25 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Noble","BsC2","Brookside silt loam, 8 to 15 percent slopes, eroded","Brookside",5,0.37,"PHEL"]
["Noble","BsD2","Brookside silt loam, 15 to 25 percent slopes, eroded","Brookside",5,0.37,"HEL"]
["Noble","BtD2","Brookside-Vandalia complex, 15 to 25 percent slopes, eroded","Brookside",5,0.37,"HEL"]
["Noble","BtE2","Brookside-Vandalia complex, 25 to 35 percent slopes, eroded","Brookside",5,0.37,"HEL"]
["Noble","Ch","Chagrin silt loam, occasionally flooded","Chagrin",5,0.32,"NHEL"]
["Noble","DkE","Dekalb channery loam, 25 to 40 percent slopes","Dekalb",2,0.24,"HEL"]
["Noble","DkF","Dekalb channery loam, 40 to 70 percent slopes","Dekalb",2,0.24,"HEL"]
["Noble","EbD2","Elba silty clay loam, 15 to 25 percent slopes, eroded","Elba",3,0.43,"HEL"]
["Noble","EbE2","Elba silty clay loam, 25 to 40 percent slopes, eroded","Elba",3,0.43,"HEL"]
["Noble","EbF2","Elba silty clay loam, 40 to 70 percent slopes, eroded","Elba",3,0.43,"HEL"]
["Noble","EdD2","Elba-Guernsey silty clay loams, 15 to 25 percent slopes, eroded","Elba",3,0.43,"HEL"]
["Noble","EdE2","Elba-Guernsey silty clay loams, 25 to 35 percent slopes, eroded","Elba",3,0.43,"HEL"]
["Noble","EnB","Enoch shaly silty clay loam, 0 to 8 percent slopes, very stony","Enoch",3,0.37,"PHEL"]
["Noble","EnD","Enoch shaly silty clay loam, 15 to 25 percent slopes, very stony","Enoch",3,0.37,"HEL"]
["Noble","EnF","Enoch shaly silty clay loam, 25 to 70 percent slopes, very stony","Enoch",3,0.37,"HEL"]
["Noble","GdC","Gilpin silt loam, 8 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Noble","GdD","Gilpin silt loam, 15 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Noble","GdE","Gilpin silt loam, 25 to 35 percent slopes","Gilpin",3,0.32,"HEL"]
["Noble","GdF","Gilpin silt loam, 35 to 70 percent slopes","Gilpin",3,0.32,"HEL"]
["Noble","GkD2","Gilpin-Upshur complex, 15 to 25 percent slopes, eroded","Gilpin",3,0.32,"HEL"]
["Noble","GkE2","Gilpin-Upshur complex, 25 to 35 percent slopes, eroded","Gilpin",3,0.32,"HEL"]
["Noble","GkF2","Gilpin-Upshur complex, 35 to 70 percent slopes, eroded","Gilpin",3,0.32,"HEL"]
["Noble","GuB","Guernsey silt loam, 1 to 6 percent slopes","Guernsey",3,0.43,"PHEL"]
["Noble","GuC","Guernsey silt loam, 6 to 15 percent slopes","Guernsey",3,0.43,"PHEL"]
["Noble","GuD","Guernsey silt loam, 15 to 25 percent slopes","Guernsey",3,0.43,"HEL"]
["Noble","GwD2","Guernsey-Upshur silty clay loams, 15 to 25 percent slopes, eroded","Guernsey",3,0.43,"HEL"]
["Noble","LoC","Lowell silt loam, 8 to 15 percent slopes","Lowell",3,0.37,"HEL"]
["Noble","LoD","Lowell silt loam, 15 to 25 percent slopes","Lowell",3,0.37,"HEL"]
["Noble","LpE2","Lowell silty clay loam, 25 to 40 percent slopes, eroded","Lowell",3,0.37,"HEL"]
["Noble","LtE2","Lowell-Elba silty clay loams, 25 to 40 percent slopes, eroded","Lowell",3,0.37,"HEL"]
["Noble","LtF2","Lowell-Elba silty clay loams, 40 to 70 percent slopes, eroded","Lowell",3,0.37,"HEL"]
["Noble","LuE","Lowell-Gilpin silt loams, 25 to 35 percent slopes","Lowell",3,0.37,"HEL"]
["Noble","LuF","Lowell-Gilpin silt loams, 35 to 70 percent slopes","Lowell",3,0.37,"HEL"]
["Noble","LvD2","Lowell-Upshur silty clay loams, 15 to 25 percent slopes, eroded","Lowell",3,0.37,"HEL"]
["Noble","LvE2","Lowell-Upshur silty clay loams, 25 to 40 percent slopes, eroded","Lowell",3,0.37,"HEL"]
["Noble","LvF2","Lowell-Upshur silty clay loams, 40 to 70 percent slopes, eroded","Lowell",3,0.37,"HEL"]
["Noble","MoB","Morristown silty clay loam, 0 to 8 percent slopes","Morristown",3,0.43,"PHEL"]
["Noble","MoC","Morristown silty clay loam, 8 to 15 percent slopes","Morristown",3,0.43,"HEL"]
["Noble","MoD","Morristown silty clay loam, 15 to 25 percent slopes","Morristown",3,0.43,"HEL"]
["Noble","MrB","Morristown channery silty clay loam, 0 to 8 percent slopes","Morristown",5,0.32,"PHEL"]
["Noble","MrD","Morristown channery silty clay loam, 8 to 25 percent slopes","Morristown",5,0.32,"PHEL"]
["Noble","MrF","Morristown channery silty clay loam, 25 to 70 percent slopes","Morristown",5,0.32,"HEL"]
["Noble","Ne","Newark silt loam, occasionally flooded","Newark",5,0.32,"NHEL"]
["Noble","Ng","Newark silt loam, frequently flooded","Newark",5,0.32,"NHEL"]
["Noble","No","Nolin silt loam, frequently flooded","Nolin",5,0.43,"NHEL"]
["Noble","OmB","Omulga silt loam, 1 to 6 percent slopes","Omulga",3,0.43,"PHEL"]
["Noble","OmC","Omulga silt loam, 6 to 15 percent slopes","Omulga",3,0.43,"PHEL"]
["Noble","Sa","Sarahsville silty clay, frequently flooded","Sarahsville",3,0.32,"NHEL"]
["Noble","Uc","Udorthents-Pits complex","Udorthents"]
["Noble","Uc","Udorthents-Pits complex","Udorthents"]
["Noble","UpB","Upshur silt loam, 3 to 8 percent slopes","Upshur",3,0.43,"PHEL"]
["Noble","UpC","Upshur silt loam, 8 to 15 percent slopes","Upshur",3,0.43,"HEL"]
["Noble","UrC3","Upshur silty clay, 8 to 15 percent slopes, severely eroded","Upshur",2,0.43,"HEL"]
["Noble","UrD3","Upshur silty clay, 15 to 25 percent slopes, severely eroded","Upshur",2,0.43,"HEL"]
["Noble","UrE3","Upshur silty clay, 25 to 40 percent slopes, severely eroded","Upshur",2,0.43,"HEL"]
["Noble","VaD2","Vandalia silty clay loam, 15 to 25 percent slopes, eroded","vandalia",4,0.37,"HEL"]
["Noble","VaE2","Vandalia silty clay loam, 25 to 40 percent slopes, eroded","vandalia",4,0.37,"HEL"]
["Noble","VcC2","Vandalia-Guernsey silty clay loams, 8 to 15 percent slopes, eroded","vandalia",4,0.37,"PHEL"]
["Noble","VcD2","Vandalia-Guernsey silty clay loams, 15 to 25 percent slopes, eroded","vandalia",4,0.37,"HEL"]
["Noble","VcE2","Vandalia-Guernsey silty clay loams, 25 to 35 percent slopes, eroded","vandalia",4,0.37,"HEL"]
["Noble","W","Water","Water"]
["Noble","WoB","Woodsfield silt loam, 1 to 6 percent slopes","woodsfield",3,0.43,"PHEL"]
["Noble","WoC","Woodsfield silt loam, 6 to 15 percent slopes","woodsfield",3,0.43,"PHEL"]
["Noble","WoD","Woodsfield silt loam, 15 to 25 percent slopes","woodsfield",3,0.43,"HEL"]
["Noble","ZaB","Zanesville silt loam, 1 to 6 percent slopes","Zanesville",3,0.43,"PHEL"]
["Noble","ZaC","Zanesville silt loam, 6 to 15 percent slopes","Zanesville",3,0.43,"HEL"]
[null,"Select","none","none"]
["Perry","AfB","Alford silt loam, 1 to 8 percent slopes","Alford",5,0.37,"PHEL"]
["Perry","AfC","Alford silt loam, 8 to 15 percent slopes","Alford",5,0.37,"PHEL"]
["Perry","AfD","Alford silt loam, 15 to 25 percent slopes","Alford",5,0.37,"HEL"]
["Perry","AmB2","Amanda silt loam, 2 to 6 percent slopes, eroded","Amanda",4,0.37,"PHEL"]
["Perry","AmC2","Amanda silt loam, 6 to 12 percent slopes, eroded","Amanda",4,0.37,"PHEL"]
["Perry","AmD2","Amanda silt loam, 12 to 18 percent slopes, eroded","Amanda",4,0.37,"HEL"]
["Perry","BeA","Bennington silt loam, 0 to 3 percent slopes","Bennington",3,0.43,"PHEL"]
["Perry","BhB","Bethesda silt loam, 0 to 8 percent slopes","Bethesda",3,0.43,"PHEL"]
["Perry","BhD","Bethesda silt loam, 8 to 20 percent slopes","Bethesda",3,0.43,"HEL"]
["Perry","BkB","Bethesda channery loam, 0 to 8 percent slopes","Bethesda",5,0.32,"PHEL"]
["Perry","BkD","Bethesda channery loam, 8 to 20 percent slopes","Bethesda",5,0.32,"PHEL"]
["Perry","BkF","Bethesda channery loam, 40 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Perry","BvF","Brownsville silt loam, 40 to 70 percent slopes","Brownsville",5,0.28000000000000003,"HEL"]
["Perry","CdB","Centerburg silt loam, 2 to 6 percent slopes","Centerburg",4,0.37,"PHEL"]
["Perry","CkB","Cincinnati silt loam, 1 to 8 percent slopes","Cincinnati",4,0.37,"PHEL"]
["Perry","CkC2","Cincinnati silt loam, 8 to 15 percent slopes, eroded","Cincinnati",4,0.37,"PHEL"]
["Perry","DkC","Dekalb loam, 8 to 15 percent slopes","Dekalb",2,0.24,"HEL"]
["Perry","DkD","Dekalb loam, 15 to 25 percent slopes","Dekalb",2,0.24,"HEL"]
["Perry","DkE","Dekalb loam, 25 to 40 percent slopes","Dekalb",2,0.24,"HEL"]
["Perry","DmF","Dekalb loam, 40 to 70 percent slopes, very stony","Dekalb",2,0.24,"HEL"]
["Perry","Ds","Dumps, mine","Dumps"]
["Perry","EnE","Enoch shaly clay loam, 20 to 40 percent slopes","Enoch",3,0.37,"HEL"]
["Perry","EuA","Euclid silt loam, rarely flooded","Euclid",5,0.37,"NHEL"]
["Perry","FbD","Fairpoint channery clay loam, 8 to 20 percent slopes","Fairpoint",3,0.43,"PHEL"]
["Perry","FbF","Fairpoint channery clay loam, 40 to 70 percent slopes","Fairpoint",3,0.43,"HEL"]
["Perry","FtA","Fitchville silt loam, 0 to 3 percent slopes","Fitchville",5,0.37,"NHEL"]
["Perry","GdC","Gilpin silt loam, 8 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Perry","GdD","Gilpin silt loam, 15 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Perry","GnB","Glenford silt loam, 1 to 8 percent slopes","Glenford",5,0.37,"PHEL"]
["Perry","GwC","Guernsey-Westmoreland silt loams, 8 to 15 percent slopes","Guernsey",3,0.43,"HEL"]
["Perry","GwD","Guernsey-Westmoreland silt loams, 15 to 25 percent slopes","Guernsey",3,0.43,"HEL"]
["Perry","GwE","Guernsey-Westmoreland silt loams, 25 to 40 percent slopes","Guernsey",3,0.43,"HEL"]
["Perry","HaD2","Homewood-Westmoreland silt loams, 15 to 25 percent slopes, eroded","Homewood",4,0.37,"HEL"]
["Perry","HaE2","Homewood-Westmoreland silt loams, 25 to 40 percent slopes, eroded","Homewood",4,0.37,"HEL"]
["Perry","Km","Killbuck silt loam, frequently flooded","Killbuck",5,0.37,"NHEL"]
["Perry","LaB","Lakin loamy sand, 1 to 8 percent slopes","Lakin",5,0.17,"PHEL"]
["Perry","Ln","Linwood muck","Linwood",2,null,"NHEL"]
["Perry","Lu","Luray silt loam","Luray",5,0.32,"NHEL"]
["Perry","Mc","Melvin silt loam, ponded","Melvin",5,0.43,"NHEL"]
["Perry","MeB","Mentor silt loam, gravelly substratum, 1 to 8 percent slopes","Mentor",5,0.37,"PHEL"]
["Perry","MeC","Mentor silt loam, gravelly substratum, 8 to 15 percent slopes","Mentor",5,0.37,"PHEL"]
["Perry","Ne","Newark silt loam, frequently flooded","Newark",5,0.32,"NHEL"]
["Perry","No","Nolin silt loam, occasionally flooded","Nolin",5,0.43,"NHEL"]
["Perry","OcA","Ockley loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Perry","OcB","Ockley loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Perry","OcC2","Ockley loam, 6 to 12 percent slopes, eroded","Ockley",5,0.37,"PHEL"]
["Perry","Pg","Peoga silt loam, rarely flooded","Peoga",4,0.43,"NHEL"]
["Perry","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Perry","Uc","Udorthents-Pits complex","Udorthents"]
["Perry","Ud","Udorthents","Udorthents"]
["Perry","UpC","Upshur silty clay loam, 8 to 15 percent slopes","Upshur",3,0.43,"HEL"]
["Perry","UpD","Upshur silty clay loam, 15 to 25 percent slopes","Upshur",3,0.43,"HEL"]
["Perry","W","Water","Water"]
["Perry","WhB","Wellston silt loam, 1 to 8 percent slopes","Wellston",4,0.37,"PHEL"]
["Perry","WhC","Wellston silt loam, 8 to 15 percent slopes","Wellston",4,0.37,"PHEL"]
["Perry","WkB","Westmore silt loam, 1 to 8 percent slopes","Westmore",4,0.37,"PHEL"]
["Perry","WkC","Westmore silt loam, 8 to 15 percent slopes","Westmore",4,0.37,"PHEL"]
["Perry","WmC","Westmoreland silt loam, 8 to 15 percent slopes","Westmoreland",3,0.37,"HEL"]
["Perry","WmD","Westmoreland silt loam, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Perry","WmE","Westmoreland silt loam, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Perry","WnE","Westmoreland loam, 20 to 40 percent slopes, very bouldery","Westmoreland",3,0.37,"HEL"]
["Perry","WsF","Westmoreland-Guernsey silt loams, 40 to 70 percent slopes","Westmoreland",3,0.37,"HEL"]
["Perry","WtC","Woodsfield silt loam, 8 to 15 percent slopes","woodsfield",3,0.43,"HEL"]
["Perry","ZnB","Zanesville silt loam, 1 to 8 percent slopes","Zanesville",3,0.43,"PHEL"]
["Perry","ZnC","Zanesville silt loam, 8 to 15 percent slopes","Zanesville",3,0.43,"HEL"]
[null,"Select","none","none"]
["Tuscarawas","BeB","Berks silt loam, 3 to 8 percent slopes","Berks",3,0.24,"PHEL"]
["Tuscarawas","BkC","Berks shaly silt loam, 8 to 15 percent slopes","Berks",3,0.24,"PHEL"]
["Tuscarawas","BkD","Berks shaly silt loam, 15 to 25 percent slopes","Berks",3,0.24,"HEL"]
["Tuscarawas","BkE","Berks shaly silt loam, 25 to 40 percent slopes","Berks",3,0.24,"HEL"]
["Tuscarawas","BkF","Berks shaly silt loam, 40 to 70 percent slopes","Berks",3,0.24,"HEL"]
["Tuscarawas","BnB","Bethesda channery clay loam, 0 to 8 percent slopes","Bethesda",5,0.32,"PHEL"]
["Tuscarawas","BnC","Bethesda channery clay loam, 8 to 15 percent slopes","Bethesda",5,0.32,"PHEL"]
["Tuscarawas","BnD","Bethesda channery clay loam, 15 to 25 percent slopes","Bethesda",5,0.32,"HEL"]
["Tuscarawas","BnF","Bethesda channery clay loam, 25 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Tuscarawas","BtA","Bogart variant loam, 0 to 3 percent slopes","Bogart",5,0.32,"NHEL"]
["Tuscarawas","BtB","Bogart variant loam, 3 to 8 percent slopes","Bogart",5,0.32,"PHEL"]
["Tuscarawas","Ca","Canadice silty clay loam","Canadice",5,0.49,"NHEL"]
["Tuscarawas","CcA","Caneadea silty clay loam, 0 to 3 percent slopes","Caneadea",3,0.43,"PHEL"]
["Tuscarawas","CdB","Canfield silt loam, 3 to 8 percent slopes","Canfield",4,0.37,"PHEL"]
["Tuscarawas","CdC","Canfield silt loam, 8 to 15 percent slopes","Canfield",4,0.37,"PHEL"]
["Tuscarawas","CkB","Chili gravelly loam, 3 to 8 percent slopes","Chili",4,0.24,"PHEL"]
["Tuscarawas","CkC","Chili gravelly loam, 8 to 15 percent slopes","Chili",4,0.24,"PHEL"]
["Tuscarawas","CmA","Chili silt loam, 0 to 3 percent slopes","Chili",4,0.32,"NHEL"]
["Tuscarawas","CnB","Chili-Urban land complex, undulating","Chili",4,0.24,"PHEL"]
["Tuscarawas","CoA","Conotton gravelly loam, 0 to 3 percent slopes","Conotton",3,0.24,"NHEL"]
["Tuscarawas","CoB","Conotton gravelly loam, 3 to 8 percent slopes","Conotton",3,0.24,"PHEL"]
["Tuscarawas","CoD","Conotton gravelly loam, 15 to 25 percent slopes","Conotton",3,0.24,"HEL"]
["Tuscarawas","CpB","Coshocton silt loam, 3 to 8 percent slopes","Coshocton",4,0.37,"PHEL"]
["Tuscarawas","CsC","Coshocton-Guernsey silt loams, 8 to 15 percent slopes","Coshocton",4,0.37,"PHEL"]
["Tuscarawas","CsD","Coshocton-Guernsey silt loams, 15 to 25 percent slopes","Coshocton",4,0.37,"HEL"]
["Tuscarawas","CsE","Coshocton-Guernsey silt loams, 25 to 40 percent slopes","Coshocton",4,0.37,"HEL"]
["Tuscarawas","CtC","Coshocton-Guernsey very stony silt loams, 8 to 15 percent slopes","Coshocton",4,0.37,"PHEL"]
["Tuscarawas","CtD","Coshocton-Guernsey very stony silt loams, 15 to 25 percent slopes","Coshocton",4,0.37,"HEL"]
["Tuscarawas","EkA","Elkinsville silt loam, 0 to 3 percent slopes","Elkinsville",5,0.37,"NHEL"]
["Tuscarawas","FcA","Fitchville silt loam, 0 to 3 percent slopes","Fitchville",5,0.37,"NHEL"]
["Tuscarawas","FcB","Fitchville silt loam, 3 to 8 percent slopes","Fitchville",5,0.37,"PHEL"]
["Tuscarawas","FdA","Fitchville silt loam, clayey substratum, 0 to 3 percent slopes","Fitchville",5,0.37,"NHEL"]
["Tuscarawas","FdB","Fitchville silt loam, clayey substratum, 3 to 8 percent slopes","Fitchville",5,0.37,"PHEL"]
["Tuscarawas","FeB","Fitchville-Urban land complex, undulating","Fitchville",5,0.37,"PHEL"]
["Tuscarawas","GfB","Glenford silt loam, 3 to 8 percent slopes","Glenford",5,0.37,"PHEL"]
["Tuscarawas","GfC","Glenford silt loam, 8 to 15 percent slopes","Glenford",5,0.37,"PHEL"]
["Tuscarawas","GgB","Guernsey silt loam, 3 to 8 percent slopes","Guernsey",3,0.43,"PHEL"]
["Tuscarawas","GgC","Guernsey silt loam, 8 to 15 percent slopes","Guernsey",3,0.43,"HEL"]
["Tuscarawas","GgD","Guernsey silt loam, 15 to 25 percent slopes","Guernsey",3,0.43,"HEL"]
["Tuscarawas","HeC","Hazleton channery loam, 8 to 15 percent slopes","Hazleton",3,0.17,"PHEL"]
["Tuscarawas","HeD","Hazleton channery loam, 15 to 25 percent slopes","Hazleton",3,0.17,"HEL"]
["Tuscarawas","HeE","Hazleton channery loam, 25 to 40 percent slopes","Hazleton",3,0.17,"HEL"]
["Tuscarawas","HeF","Hazleton channery loam, 40 to 60 percent slopes","Hazleton",3,0.17,"HEL"]
["Tuscarawas","HgF","Hazleton extremely bouldery loam, 25 to 60 percent slopes","Hazleton",3,0.17,"HEL"]
["Tuscarawas","KeB","Keene silt loam, 3 to 8 percent slopes","Keene",4,0.37,"PHEL"]
["Tuscarawas","KeC","Keene silt loam, 8 to 15 percent slopes","Keene",4,0.37,"PHEL"]
["Tuscarawas","Ln","Linwood mucky silt loam, ponded","Linwood",2,0.24,"NHEL"]
["Tuscarawas","Mc","Melvin silt loam, frequently flooded","Melvin",5,0.43,"NHEL"]
["Tuscarawas","MrB","Morristown loam, 0 to 8 percent slopes","Morristown",3,0.43,"PHEL"]
["Tuscarawas","MrC","Morristown loam, 8 to 15 percent slopes","Morristown",3,0.43,"HEL"]
["Tuscarawas","MrD","Morristown loam, 15 to 25 percent slopes","Morristown",3,0.43,"HEL"]
["Tuscarawas","MrF","Morristown loam, 25 to 70 percent slopes","Morristown",3,0.43,"HEL"]
["Tuscarawas","No","Nolin silt loam, occasionally flooded","Nolin",5,0.43,"NHEL"]
["Tuscarawas","Or","Orrville silt loam, occasionally flooded","Orrville",5,0.37,"NHEL"]
["Tuscarawas","Pt","Pits, gravel","Pits"]
["Tuscarawas","Pu","Pits, quarry","Pits"]
["Tuscarawas","PwB","Plainfield loamy sand, 3 to 8 percent slopes","Plainfield",5,0.17,"PHEL"]
["Tuscarawas","RgC","Rigley sandy loam, 8 to 15 percent slopes","Rigley",4,0.24,"PHEL"]
["Tuscarawas","RgD","Rigley sandy loam, 15 to 25 percent slopes","Rigley",4,0.24,"HEL"]
["Tuscarawas","RgE","Rigley sandy loam, 25 to 40 percent slopes","Rigley",4,0.24,"HEL"]
["Tuscarawas","RuA","Rush silt loam, 0 to 3 percent slopes","Rush",5,0.37,"NHEL"]
["Tuscarawas","Se","Sebring silt loam","Sebring",5,0.37,"NHEL"]
["Tuscarawas","ShC3","Shinrock silty clay loam, 8 to 20 percent slopes, severely eroded","Shinrock",2,0.37,"HEL"]
["Tuscarawas","SpA","Sparta loamy fine sand, 0 to 3 percent slopes","Sparta",5,0.17,"NHEL"]
["Tuscarawas","To","Tioga loam, occasionally flooded","Tioga",5,0.37,"NHEL"]
["Tuscarawas","Ua","Udorthents, hilly","Udorthents"]
["Tuscarawas","UpC","Upshur silt loam, 8 to 15 percent slopes","Upshur",3,0.43,"HEL"]
["Tuscarawas","W","Water","Water"]
["Tuscarawas","WbA","Weinbach silt loam, 0 to 3 percent slopes","Weinbach",4,0.43,"NHEL"]
["Tuscarawas","WhC","Westmoreland silt loam, 8 to 15 percent slopes","Westmoreland",3,0.37,"PHEL"]
["Tuscarawas","WhD","Westmoreland silt loam, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Tuscarawas","WhE","Westmoreland silt loam, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Tuscarawas","WhF","Westmoreland silt loam, 40 to 60 percent slopes","Westmoreland",3,0.37,"HEL"]
["Tuscarawas","WnC","Westmoreland-Guernsey silt loams, 8 to 15 percent slopes","Westmoreland",3,0.37,"PHEL"]
["Tuscarawas","WnD","Westmoreland-Guernsey silt loams, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Tuscarawas","WnE","Westmoreland-Guernsey silt loams, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Tuscarawas","WrA","Wheeling loam, 0 to 3 percent slopes","Wheeling",4,0.37,"NHEL"]
["Tuscarawas","WsA","Wheeling-Urban land complex, nearly level","Wheeling",4,0.37,"NHEL"]
[null,"Select","none","none"]
["Washington","AfB","Alford silt loam, 2 to 6 percent slopes","Alford",5,0.37,"PHEL"]
["Washington","AfC","Alford silt loam, 6 to 12 percent slopes","Alford",5,0.37,"PHEL"]
["Washington","AlB","Allegheny silt loam, 2 to 6 percent slopes","Allegheny",4,0.32,"PHEL"]
["Washington","AlC","Allegheny silt loam, 6 to 12 percent slopes","Allegheny",4,0.32,"PHEL"]
["Washington","AlD","Allegheny silt loam, 12 to 18 percent slopes","Allegheny",4,0.32,"HEL"]
["Washington","AlG","Allegheny silt loam, 18 to 50 percent slopes","Allegheny",4,0.32,"HEL"]
["Washington","AsA","Ashton silt loam, 0 to 2 percent slopes","Ashton",5,0.32,"NHEL"]
["Washington","AsB","Ashton silt loam, 2 to 6 percent slopes","Ashton",5,0.32,"PHEL"]
["Washington","BeC","Belpre clay, 6 to 12 percent slopes","Belpre",3,0.32,"PHEL"]
["Washington","BeD","Belpre clay, 12 to 18 percent slopes","Belpre",3,0.32,"HEL"]
["Washington","BeE","Belpre clay, 18 to 25 percent slopes","Belpre",3,0.32,"HEL"]
["Washington","BeF","Belpre clay, 25 to 35 percent slopes","Belpre",3,0.32,"HEL"]
["Washington","BsC","Brookside silty clay loam, 6 to 12 percent slopes","Brookside",5,0.37,"PHEL"]
["Washington","BsD","Brookside silty clay loam, 12 to 18 percent slopes","Brookside",5,0.37,"HEL"]
["Washington","BsE","Brookside silty clay loam, 18 to 25 percent slopes","Brookside",5,0.37,"HEL"]
["Washington","BtF","Brookside bouldery silty clay loam, 18 to 35 percent slopes","Brookside",5,0.37,"HEL"]
["Washington","Cg","Chagrin silt loam","Chagrin",5,0.32,"NHEL"]
["Washington","ChA","Chili loam, 0 to 2 percent slopes","Chili",4,0.32,"NHEL"]
["Washington","ChB","Chili loam, 2 to 6 percent slopes","Chili",4,0.32,"PHEL"]
["Washington","ChC","Chili loam, 6 to 12 percent slopes","Chili",4,0.32,"PHEL"]
["Washington","ClC","Clymer silt loam, 6 to 12 percent slopes","Clymer",3,0.24,"PHEL"]
["Washington","ClD","Clymer silt loam, 12 to 18 percent slopes","Clymer",3,0.24,"HEL"]
["Washington","CoA","Conotton gravelly loam, 1 to 6 percent slopes","Conotton",3,0.24,"PHEL"]
["Washington","CpE","Conotton-Chili gravelly loams, 18 to 25 percent slopes","Conotton",3,0.24,"HEL"]
["Washington","DkC","Dekalb loam, 6 to 12 percent slopes","Dekalb",2,0.24,"PHEL"]
["Washington","DkD","Dekalb loam, 12 to 18 percent slopes","Dekalb",2,0.24,"HEL"]
["Washington","DkE","Dekalb loam, 18 to 25 percent slopes","Dekalb",2,0.24,"HEL"]
["Washington","DkF","Dekalb loam, 25 to 35 percent slopes","Dekalb",2,0.24,"HEL"]
["Washington","DsG","Dekalb and Gilpin stony soils, 25 to 70 percent slopes","Dekalb",2,0.24,"HEL"]
["Washington","DtB","Duncannon silt loam, 2 to 6 percent slopes","Ducannon",4,0.37,"PHEL"]
["Washington","DtC","Duncannon silt loam, 6 to 12 percent slopes","Ducannon",4,0.37,"PHEL"]
["Washington","DuD","Duncannon-Lakin complex, 12 to 18 percent slopes","Ducannon",4,0.37,"HEL"]
["Washington","DuE","Duncannon-Lakin complex, 18 to 25 percent slopes","Ducannon",4,0.37,"HEL"]
["Washington","ElD","Elba-Belpre complex, 12 to 18 percent slopes","Elba",3,0.43,"HEL"]
["Washington","ElE","Elba-Belpre complex, 18 to 25 percent slopes","Elba",3,0.43,"HEL"]
["Washington","ElF","Elba-Belpre complex, 25 to 35 percent slopes","Elba",3,0.43,"HEL"]
["Washington","Fa","Fill land, sandy, gravelly and channery materials","Fill"]
["Washington","Fb","Fill land, loamy materials","Fill"]
["Washington","Fc","Fill land, clayey materials","Fill"]
["Washington","GaB","Gallia silt loam, 2 to 6 percent slopes","Gallia",5,0.37,"PHEL"]
["Washington","GaC","Gallia silt loam, 6 to 12 percent slopes","Gallia",5,0.37,"PHEL"]
["Washington","GaD","Gallia silt loam, 12 to 18 percent slopes","Gallia",5,0.37,"HEL"]
["Washington","GdB","Gilpin silt loam, 2 to 6 percent slopes","Gilpin",3,0.32,"PHEL"]
["Washington","GdC","Gilpin silt loam, 6 to 12 percent slopes","Gilpin",3,0.32,"PHEL"]
["Washington","GdD","Gilpin silt loam, 12 to 18 percent slopes","Gilpin",3,0.32,"HEL"]
["Washington","GdE","Gilpin silt loam, 18 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Washington","GdF","Gilpin silt loam, 25 to 35 percent slopes","Gilpin",3,0.32,"HEL"]
["Washington","GkC","Gilpin-Summitville-Upshur complex, 6 to 12 percent slopes","Gilpin",3,0.32,"PHEL"]
["Washington","GkD","Gilpin-Summitville-Upshur complex, 12 to 18 percent slopes","Gilpin",3,0.32,"HEL"]
["Washington","GkD3","Gilpin-Summitville-Upshur complex, 12 to 18 percent slopes, severely eroded","Gilpin",3,0.32,"HEL"]
["Washington","GkE","Gilpin-Summitville-Upshur complex, 18 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Washington","GkE3","Gilpin-Summitville-Upshur complex, 18 to 25 percent slopes, severely eroded","Gilpin",3,0.32,"HEL"]
["Washington","GkF","Gilpin-Summitville-Upshur complex, 25 to 35 percent slopes","Gilpin",3,0.32,"HEL"]
["Washington","GlF","Gilpin-Summitville-Upshur complex, 25 to 35 percent slopes, benched","Gilpin",3,0.32,"HEL"]
["Washington","GlG","Gilpin-Summitville-Upshur complex, 35 to 70 percent slopes, benched","Gilpin",3,0.32,"HEL"]
["Washington","GnA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Washington","GnB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Washington","HcA","Hackers silt loam, 0 to 2 percent slopes","Hackers",4,0.32,"NHEL"]
["Washington","HcB","Hackers silt loam, 2 to 6 percent slopes","Hackers",4,0.32,"PHEL"]
["Washington","HcC","Hackers silt loam, 6 to 12 percent slopes","Hackers",4,0.32,"PHEL"]
["Washington","He","Hartshorn silt loam","Hartshorn",3,0.32,"NHEL"]
["Washington","HgB","Hayter loam, 2 to 6 percent slopes","Hayter",4,0.28000000000000003,"PHEL"]
["Washington","HgC","Hayter loam, 6 to 12 percent slopes","Hayter",4,0.28000000000000003,"PHEL"]
["Washington","HgD","Hayter loam, 12 to 18 percent slopes","Hayter",4,0.28000000000000003,"HEL"]
["Washington","HgE","Hayter loam, 18 to 25 percent slopes","Hayter",4,0.28000000000000003,"HEL"]
["Washington","HgF","Hayter loam, 25 to 35 percent slopes","Hayter",4,0.28000000000000003,"HEL"]
["Washington","HhE","Hayter very stony soils, 18 to 30 percent slopes","Hayter",4,0.28000000000000003,"HEL"]
["Washington","HkE","Hayter-Vandalia channery loams, 12 to 25 percent slopes","Hayter",4,0.28000000000000003,"HEL"]
["Washington","HkF","Hayter-Vandalia stony complex, 25 to 50 percent slopes","Hayter",4,0.28000000000000003,"HEL"]
["Washington","Hu","Huntington silt loam","Huntington",5,0.28000000000000003,"NHEL"]
["Washington","KeB","Keene silt loam, 2 to 6 percent slopes","Keene",4,0.37,"PHEL"]
["Washington","KeC","Keene silt loam, 6 to 12 percent slopes","Keene",4,0.37,"PHEL"]
["Washington","LbC","Lakin loamy fine sand, 3 to 12 percent slopes","Lakin",5,0.17,"PHEL"]
["Washington","LbD","Lakin loamy fine sand, 12 to 18 percent slopes","Lakin",5,0.17,"PHEL"]
["Washington","LcB","Licking silt loam, 2 to 6 percent slopes","Licking",3,0.43,"PHEL"]
["Washington","LcC","Licking silt loam, 6 to 12 percent slopes","Licking",3,0.43,"PHEL"]
["Washington","LcD","Licking silt loam, 12 to 18 percent slopes","Licking",3,0.43,"HEL"]
["Washington","LoC","Lowell-Upshur complex, 6 to 12 percent slopes","Lowell",3,0.37,"PHEL"]
["Washington","LoD","Lowell-Upshur complex, 12 to 18 percent slopes","Lowell",3,0.37,"HEL"]
["Washington","LoE","Lowell-Upshur complex, 18 to 25 percent slopes","Lowell",3,0.37,"HEL"]
["Washington","LoF","Lowell-Upshur complex, 25 to 35 percent slopes","Lowell",3,0.37,"HEL"]
["Washington","MbB","Markland silt loam, 2 to 6 percent slopes","Markland",3,0.43,"PHEL"]
["Washington","MbC","Markland silt loam, 6 to 12 percent slopes","Markland",3,0.43,"PHEL"]
["Washington","MbD2","Markland silt loam, 12 to 18 percent slopes, moderately eroded","Markland",3,0.43,"HEL"]
["Washington","MbG","Markland silt loam, 18 to 50 percent slopes","Markland",3,0.43,"HEL"]
["Washington","McA","McGary silt loam, 0 to 2 percent slopes","McGary",3,0.43,"NHEL"]
["Washington","Md","Melvin silt loam,","Melvin",5,0.43,"NHEL"]
["Washington","MeA","Mentor silt loam, 0 to 2 percent slopes","Melvin",5,0.37,"NHEL"]
["Washington","MeB","Mentor silt loam, 2 to 6 percent slopes","Mentor",5,0.37,"PHEL"]
["Washington","MeC","Mentor silt loam, 6 to 12 percent slopes","Mentor",5,0.37,"PHEL"]
["Washington","Mp","Moshannon silt loam","Moshannon",5,0.37,"NHEL"]
["Washington","Nn","Newark silt loam","Newark",5,0.32,"NHEL"]
["Washington","No","Nolin silt loam","Nolin",5,0.43,"NHEL"]
["Washington","OtB","Otwell silt loam, 2 to 6 percent slopes","Otwell",3,0.43,"PHEL"]
["Washington","OtC","Otwell silt loam, 6 to 12 percent slopes","Otwell",3,0.43,"PHEL"]
["Washington","OvB","Otwell-Vincent silt loams, 2 to 6 percent slopes","Otwell",3,0.43,"PHEL"]
["Washington","OvC","Otwell-Vincent silt loams, 6 to 12 percent slopes","Otwell",3,0.43,"PHEL"]
["Washington","Pe","Peoga silt loam","Peoga",4,0.43,"NHEL"]
["Washington","Pg","Pits, gravel","Pits"]
["Washington","Pu","Pits, quarry","Pits"]
["Washington","SaB","Sparta loamy sand, 0 to 6 percent slopes","Sparta",5,0.17,"NHEL"]
["Washington","SM","Strip mine spoil, calcareous","Strip Mine"]
["Washington","SP","Strip mine spoil, acidic (toxic)","Strip Mine"]
["Washington","SuD","Summitville silt loam, 10 to 20 percent slopes","Summitville",3,0.37,"HEL"]
["Washington","TaA","Taggart silt loam, 0 to 2 percent slopes","Taggart",5,0.37,"NHEL"]
["Washington","Tg","Tioga fine sandy loam","Tioga",5,0.37,"NHEL"]
["Washington","UpB","Upshur silty clay loam, 2 to 6 percent slopes","Upshur",3,0.43,"PHEL"]
["Washington","UpC","Upshur silty clay loam, 6 to 12 percent slopes","Upshur",3,0.43,"PHEL"]
["Washington","UpD","Upshur silty clay loam, 12 to 18 percent slopes","Upshur",3,0.43,"HEL"]
["Washington","UpE","Upshur silty clay loam, 18 to 25 percent slopes","Upshur",3,0.43,"HEL"]
["Washington","UrD3","Upshur clay, 12 to 18 percent slopes, severely eroded","Upshur",2,0.43,"HEL"]
["Washington","UrE3","Upshur clay, 18 to 25 percent slopes, severely eroded","Upshur",2,0.43,"HEL"]
["Washington","UsF","Upshur-Gilpin complex, 25 to 35 percent slopes","Upshur",3,0.43,"HEL"]
["Washington","UsF3","Upshur-Gilpin complex, 25 to 35 percent slopes, severely eroded","Upshur",2,0.43,"HEL"]
["Washington","UTG","Upshur association, very stony, 25 to 70 percent slopes","Upshur",3,0.43,"HEL"]
["Washington","UX","Urban land","Urban"]
["Washington","VaC","Vandalia silty clay loam, 6 to 12 percent slopes","Vandalia",4,0.37,"PHEL"]
["Washington","VaD","Vandalia silty clay loam, 12 to 18 percent slopes","Vandalia",4,0.37,"HEL"]
["Washington","VaE","Vandalia silty clay loam, 18 to 25 percent slopes","Vandalia",4,0.37,"HEL"]
["Washington","VaF","Vandalia silty clay loam, 25 to 35 percent slopes","Vandalia",4,0.37,"HEL"]
["Washington","VtB","Vincent silt loam, 2 to 6 percent slopes","Vincent",3,0.43,"PHEL"]
["Washington","VtC","Vincent silt loam, 6 to 12 percent slopes","Vincent",3,0.43,"PHEL"]
["Washington","VtD","Vincent silt loam, 12 to 18 percent slopes","Vincent",3,0.43,"HEL"]
["Washington","W","Water","Water"]
["Washington","WaB","Watertown gravelly loamy sand, 2 to 6 percent slopes","Watertown",4,0.17,"PHEL"]
["Washington","WbA","Watertown sandy loam, 0 to 2 percent slopes","Watertown",4,0.17,"NHEL"]
["Washington","WbB","Watertown sandy loam, 2 to 6 percent slopes","Watertown",4,0.17,"PHEL"]
["Washington","WbC","Watertown sandy loam, 6 to 12 percent slopes","Watertown",4,0.17,"PHEL"]
["Washington","WhB","Wellston silt loam, 2 to 6 percent slopes","Wellston",4,0.37,"PHEL"]
["Washington","WhC","Wellston silt loam, 6 to 12 percent slopes","Wellston",4,0.37,"PHEL"]
["Washington","WhD","Wellston silt loam, 12 to 18 percent slopes","Wellston",4,0.37,"HEL"]
["Washington","WkF","Westmore-Lowell-Elba complex, 25 to 35 percent slopes","Westmore",4,0.37,"HEL"]
["Washington","WkG","Westmore-Lowell-Elba complex, 35 to 70 percent slopes","Westmore",4,0.37,"HEL"]
["Washington","WlF","Westmore-Lowell-Elba complex, 25 to 35 percent slopes, benched","Westmore",4,0.37,"HEL"]
["Washington","WlG","Westmore-Lowell-Elba complex, 35 to 70 percent slopes, benched","Westmore",4,0.37,"HEL"]
["Washington","WrA","Wheeling silt loam, 0 to 2 percent slopes","Wheeling",4,0.37,"NHEL"]
["Washington","WrB","Wheeling silt loam, 2 to 6 percent slopes","Wheeling",4,0.37,"PHEL"]
["Washington","WrC","Wheeling silt loam, 6 to 12 percent slopes","Wheeling",4,0.37,"PHEL"]
["Washington","WrD","Wheeling silt loam, 12 to 18 percent slopes","Wheeling",4,0.37,"HEL"]
["Washington","WrF","Wheeling silt loam, 18 to 35 percent slopes","Wheeling",4,0.37,"HEL"]
["Washington","WtB","Woodsfield silt loam, 2 to 6 percent slopes","Woodsfield",3,0.43,"PHEL"]
["Washington","WtC","Woodsfield silt loam, 6 to 12 percent slopes","Woodsfield",3,0.43,"PHEL"]
["Washington","WtD","Woodsfield silt loam, 12 to 18 percent slopes","Woodsfield",3,0.43,"HEL"]
["Washington","WzB","Woodsfield-Zanesville silt loams, 2 to 6 percent slopes","Woodsfield",3,0.43,"PHEL"]
["Washington","WzC","Woodsfield-Zanesville silt loams, 6 to 12 percent slopes","Woodsfield",3,0.43,"PHEL"]
["Washington","WzD","Woodsfield-Zanesville silt loams, 12 to 18 percent slopes","Woodsfield",3,0.43,"HEL"]
["Washington","ZnB","Zanesville silt loam, 2 to 6 percent slopes","Zanesville",3,0.43,"PHEL"]
["Washington","ZnC","Zanesville silt loam, 6 to 12 percent slopes","Zanesville",3,0.43,"PHEL"]
["Washington","ZnD","Zanesville silt loam, 12 to 18 percent slopes","Zanesville",3,0.43,"HEL"]

{"sheet":"Area 4","index":5,"n_rows":1468,"n_cols":7,"rows_kept":1468,"cut":false,"hidden":false,"merged":[]}
["County","symbol","map unit name","Component","T","Kw","HEL"]
[null,"Select","none","none"]
["Butler","AvA","Avonburg silt loam, 0 to 2 percent slopes","Avonburg",4,0.43,"NHEL"]
["Butler","Bt","Brenton silt loam","Brenton",5,0.28000000000000003,"NHEL"]
["Butler","CdD2","Casco and Rodman gravelly loams, 6 to 18 percent slopes, moderately eroded","Casco",3,0.24,"PHEL"]
["Butler","CdE","Casco and Rodman gravelly loams, 18 to 35 percent slopes","Casco",3,0.24,"HEL"]
["Butler","CeB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Butler","CnC2","Cincinnati silt loam, 6 to 12 percent slopes, moderately eroded","Cincinnati",4,0.37,"PHEL"]
["Butler","CrA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Butler","DaA","Dana silt loam, 0 to 2 percent slopes","Dana",5,0.32,"NHEL"]
["Butler","DaB","Dana silt loam, 2 to 6 percent slopes","Dana",5,0.32,"PHEL"]
["Butler","DbB","Dana silt loam, bedrock substratum, 2 to 8 percent slopes","Dana",5,0.32,"PHEL"]
["Butler","EcE2","Eden silty clay loam, 15 to 25 percent slopes, moderately eroded","Eden",3,0.43,"HEL"]
["Butler","EcF2","Eden silty clay loam, 25 to 50 percent slopes, moderately eroded","Eden",3,0.43,"HEL"]
["Butler","Ee","Eel silt loam","Eel",5,0.37,"NHEL"]
["Butler","ElA","Eldean loam, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Butler","ElB2","Eldean loam, 2 to 6 percent slopes, moderately eroded","Eldean",4,0.37,"PHEL"]
["Butler","ElC2","Eldean loam, 6 to 12 percent slopes, moderately eroded","Eldean",4,0.37,"PHEL"]
["Butler","EnA","Eldean gravelly loam, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Butler","EnB2","Eldean gravelly loam, 2 to 6 percent slopes, moderately eroded","Eldean",4,0.37,"PHEL"]
["Butler","EuA","Eldean-Urban land complex, nearly level","Eldean",4,0.37,"NHEL"]
["Butler","EuB","Eldean-Urban land complex, gently sloping","Eldean",4,0.37,"PHEL"]
["Butler","FcA","Fincastle silt loam, 0 to 2 percent slopes","Fincastle",5,0.37,"NHEL"]
["Butler","FcB","Fincastle silt loam, 2 to 6 percent slopes","Fincastle",5,0.37,"PHEL"]
["Butler","FdA","Fincastle silt loam, bedrock substratum, 0 to 2 percent slopes","Fincastle",5,0.37,"NHEL"]
["Butler","FdB","Fincastle silt loam, bedrock substratum, 2 to 6 percent slopes","Fincastle",5,0.37,"PHEL"]
["Butler","Gn","Genesee loam","Genesee",5,0.37,"NHEL"]
["Butler","Go","Genesee-Urban land complex","Genesee",5,0.37,"NHEL"]
["Butler","HeE2","Hennepin-Miamian silt loams, 18 to 25 percent slopes, moderately eroded","Hennepin",4,0.32,"HEL"]
["Butler","HeF","Hennepin-Miamian silt loams, 25 to 50 percent slopes","Hennepin",4,0.32,"HEL"]
["Butler","HoA","Henshaw silt loam, 0 to 2 percent slopes","Henshaw",4,0.43,"NHEL"]
["Butler","La","Landes sandy loam","Landes",5,0.2,"NHEL"]
["Butler","Lg","Lanier fine sandy loam","Lanier",5,0.2,"NHEL"]
["Butler","MlB2","Miamian silt loam, 2 to 6 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Butler","MlC2","Miamian silt loam, 6 to 12 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Butler","MlD2","Miamian silt loam, 12 to 18 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Butler","MnC3","Miamian clay loam, 6 to 12 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Butler","MnD3","Miamian clay loam, 12 to 18 percent slopes, severely eroded","Miamian",4,0.37,"HEL"]
["Butler","MsC2","Miamian-Russell silt loams, 6 to 12 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Butler","MsD2","Miamian-Russell silt loams, 12 to 18 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Butler","MtC2","Miamian-Russell silt loams, bedrock substratum, 6 to 12 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Butler","MuC","Miamian-Urban land complex, sloping","Miamian",5,0.37,"PHEL"]
["Butler","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Butler","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Butler","Pa","Patton silty clay loam","Patton",5,0.28000000000000003,"NHEL"]
["Butler","Pg","Pits, gravel","Pits"]
["Butler","PrB","Princeton sandy loam, 2 to 8 percent slopes","Princeton",5,0.24,"PHEL"]
["Butler","Ra","Ragsdale silty clay loam","Ragsdale",5,0.28000000000000003,"NHEL"]
["Butler","RdA","Raub silt loam, 0 to 2 percent slopes","Raub",5,0.28000000000000003,"NHEL"]
["Butler","RdB","Raub silt loam, 2 to 6 percent slopes","Raub",5,0.28000000000000003,"PHEL"]
["Butler","Rh","Riverwash","Riverwash"]
["Butler","Rn","Ross loam","Ross",5,0.32,"NHEL"]
["Butler","RpB","Rossmoyne silt loam, 2 to 6 percent slopes","Rossmoyne",4,0.37,"PHEL"]
["Butler","RtB","Russell silt loam, 2 to 6 percent slopes","Russell",5,0.37,"PHEL"]
["Butler","RvB","Russell-Miamian silt loams, 2 to 6 percent slopes","Russell",5,0.37,"PHEL"]
["Butler","RvB2","Russell-Miamian silt loams, 2 to 6 percent slopes, moderately eroded","Russell",5,0.37,"PHEL"]
["Butler","RwB","Russell-Miamian silt loams, bedrock substratum, 2 to 6 percent slopes","Russell",5,0.37,"PHEL"]
["Butler","RwB2","Russell-Miamian silt loams, bedrock substratum, 2 to 6 percent slopes, moderately eroded","Russell",5,0.37,"PHEL"]
["Butler","RxB","Russell-Urban land complex, gently sloping","Russell",5,0.37,"PHEL"]
["Butler","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Butler","SlA","Sleeth silt loam, 0 to 2 percent slopes","Sleeth",5,0.32,"NHEL"]
["Butler","St","Stonelick fine sandy loam","Stonelick",5,0.24,"NHEL"]
["Butler","ThA","Thackery silt loam, 0 to 2 percent slopes","Thackery",4,0.37,"NHEL"]
["Butler","TpA","Tippecanoe silt loam, 0 to 2 percent slopes","Tippecanoe",5,0.32,"NHEL"]
["Butler","Ud","Udorthents","Udorthents"]
["Butler","Uf","Udorthents and Dumps","Udorthents"]
["Butler","UnA","Uniontown silt loam, 0 to 2 percent slopes","Uniontown",4,0.37,"NHEL"]
["Butler","UnB","Uniontown silt loam, 2 to 6 percent slopes","Uniontown",4,0.37,"PHEL"]
["Butler","UpA","Urban land-Eldean complex, nearly level","Urban"]
["Butler","UsA","Urban land-Patton complex, nearly level","Urban"]
["Butler","W","Water","Water"]
["Butler","WbA","Warsaw loam, 0 to 3 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
["Butler","WeA","Wea silt loam, 0 to 2 percent slopes","Wea",5,0.32,"NHEL"]
["Butler","WeB","Wea silt loam, 2 to 6 percent slopes","Wea",5,0.32,"PHEL"]
["Butler","WuB","Wynn-Urban land complex, gently sloping","Wynn",4,0.37,"PHEL"]
["Butler","WuC","Wynn-Urban land complex, sloping","Wynn",4,0.37,"PHEL"]
["Butler","WyB","Wynn silt loam, 2 to 6 percent slopes","Wynn",4,0.37,"PHEL"]
["Butler","WyB2","Wynn silt loam, 2 to 6 percent slopes, moderately eroded","Wynn",4,0.37,"PHEL"]
["Butler","WyC2","Wynn silt loam, 6 to 12 percent slopes, moderately eroded","Wynn",4,0.37,"PHEL"]
["Butler","WzC3","Wynn silty clay loam, 6 to 12 percent slopes, severely eroded","Wynn",3,0.37,"PHEL"]
["Butler","XeA","Xenia silt loam, 0 to 2 percent slopes","Xenia",5,0.37,"NHEL"]
["Butler","XeB","Xenia silt loam, 2 to 6 percent slopes","Xenia",5,0.37,"PHEL"]
["Butler","XeB2","Xenia silt loam, 2 to 6 percent slopes, moderately eroded","Xenia",5,0.37,"PHEL"]
["Butler","XfA","Xenia silt loam, bedrock substratum, 0 to 2 percent slopes","Xenia",5,0.37,"NHEL"]
["Butler","XfB","Xenia silt loam, bedrock substratum, 2 to 6 percent slopes","Xenia",5,0.37,"PHEL"]
["Butler","XfB2","Xenia silt loam, bedrock substratum, 2 to 6 percent slopes, moderately eroded","Xenia",5,0.37,"PHEL"]
[null,"Select","none","none"]
["Champaign","Ag","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Champaign","BsA","Brookston silty clay loam, 0 to 2 percent slopes","Brookston",5,0.28000000000000003,"NHEL"]
["Champaign","BsB","Brookston silty clay loam, 2 to 6 percent slopes","Brookston",5,0.28000000000000003,"PHEL"]
["Champaign","Ca","Carlisle muck","Carlisle",2,null,"NHEL"]
["Champaign","CcB","Casco loam, 2 to 6 percent slopes","Casco",3,0.24,"PHEL"]
["Champaign","CcC2","Casco loam, 6 to 12 percent slopes, moderately eroded","Casco",3,0.24,"PHEL"]
["Champaign","CgD2","Casco gravelly loam, 12 to 18 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Champaign","CmD2","Casco-Miami-Fox complex, 12 to 18 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Champaign","CnA","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Champaign","CnB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Champaign","CnB2","Celina silt loam, 2 to 6 percent slopes, moderately eroded","Celina",5,0.37,"PHEL"]
["Champaign","CnC2","Celina silt loam, 6 to 12 percent slopes, moderately eroded","Celina",5,0.37,"PHEL"]
["Champaign","CoB","Celina bouldery silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Champaign","CrA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Champaign","CrB","Crosby silt loam, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Champaign","CsB","Crosby bouldery silt loam, 0 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Champaign","Ed","Edwards muck","Edwards",2,null,"NHEL"]
["Champaign","Ee","Eel silt loam","Eel",5,0.37,"NHEL"]
["Champaign","FlB","Fox loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Champaign","FmB","Fox sandy loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Champaign","FnA","Fox silt loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Champaign","FnB","Fox silt loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Champaign","FnB2","Fox silt loam, 2 to 6 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Champaign","FnC2","Fox silt loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Champaign","FoC2","Fox-Miami silt loams, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Champaign","Gn","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Champaign","Gp","Gravel pit","Gravel"]
["Champaign","HeA","Henshaw silt loam, 0 to 2 percent slopes","Henshaw",4,0.43,"NHEL"]
["Champaign","HeB","Henshaw silt loam, 2 to 6 percent slopes","Henshaw",4,0.43,"PHEL"]
["Champaign","HoA","Homer silt loam, 0 to 2 percent slopes","Homer",4,0.37,"NHEL"]
["Champaign","IoA","Ionia silt loam, 0 to 2 percent slopes","Ionia",4,0.32,"NHEL"]
["Champaign","IoB","Ionia silt loam, 2 to 6 percent slopes","Ionia",4,0.32,"PHEL"]
["Champaign","KaA","Kane silt loam, 0 to 2 percent slopes","Kane",4,0.28000000000000003,"NHEL"]
["Champaign","KeA","Kendallville silt loam, 0 to 2 percent slopes","Kendallville",3,0.37,"NHEL"]
["Champaign","KeB","Kendallville silt loam, 2 to 6 percent slopes","Kendallville",3,0.37,"PHEL"]
["Champaign","KeC2","Kendallville silt loam, 6 to 12 percent slopes, moderately eroded","Kendallville",3,0.37,"PHEL"]
["Champaign","KeD2","Kendallville silt loam, 12 to 18 percent slopes, moderately eroded","Kendallville",3,0.37,"HEL"]
["Champaign","Ln","Linwood muck","Linwood",2,null,"NHEL"]
["Champaign","Lp","Lippincott silty clay loam","Lippincott",5,0.28000000000000003,"NHEL"]
["Champaign","Ma","Made land","Made"]
["Champaign","MbC","Miami bouldery silt loam, 2 to 12 percent slopes","Miami",5,0.37,"PHEL"]
["Champaign","MlA","Miami silt loam, 0 to 2 percent slopes","Miami",5,0.37,"NHEL"]
["Champaign","MlB","Miami silt loam, 2 to 6 percent slopes","Miami",5,0.37,"PHEL"]
["Champaign","MlB2","Miami silt loam, 2 to 6 percent slopes, moderately eroded","Miami",5,0.37,"PHEL"]
["Champaign","MlC","Miami silt loam, 6 to 12 percent slopes","Miami",5,0.37,"PHEL"]
["Champaign","MlC2","Miami silt loam, 6 to 12 percent slopes, moderately eroded","Miami",5,0.37,"PHEL"]
["Champaign","MlD","Miami silt loam, 12 to 18 percent slopes","Miami",5,0.37,"HEL"]
["Champaign","MlD2","Miami silt loam, 12 to 18 percent slopes, moderately eroded","Miami",5,0.37,"HEL"]
["Champaign","MlE","Miami silt loam, 18 to 25 percent slopes","Miami",5,0.37,"HEL"]
["Champaign","MlE2","Miami silt loam, 18 to 25 percent slopes, moderately eroded","Miami",5,0.37,"HEL"]
["Champaign","MmC3","Miami soils, 6 to 12 percent slopes, severely eroded","Miami",4,0.37,"PHEL"]
["Champaign","MmD3","Miami soils, 12 to 18 percent slopes, severely eroded","Miami",4,0.37,"HEL"]
["Champaign","MmE3","Miami soils, 18 to 25 percent slopes, severely eroded","Miami",4,0.37,"HEL"]
["Champaign","MoF2","Miami and Lewisburg silt loams, 25 to 50 percent slopes, moderately eroded","Miami",5,0.37,"HEL"]
["Champaign","MrF2","Miami-Rodman complex, 25 to 50 percent slopes, moderately eroded","Miami",5,0.37,"HEL"]
["Champaign","MsE2","Miami-Casco-Rodman complex, 18 to 25 percent slopes, moderately eroded","Miami",5,0.37,"HEL"]
["Champaign","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Champaign","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Champaign","Pa","Patton silty clay loam","Patton",5,0.28000000000000003,"NHEL"]
["Champaign","Qu","Quarry","Quarry"]
["Champaign","RgD2","Rodman gravelly loam, 12 to 18 percent slopes, moderately eroded","Rodman",3,0.2,"HEL"]
["Champaign","RgF2","Rodman gravelly loam, 18 to 50 percent slopes, moderately eroded","Rodman",3,0.2,"HEL"]
["Champaign","Rn","Ross silt loam","Ross",5,0.32,"NHEL"]
["Champaign","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Champaign","Sm","Shoals silt loam, till subsoil variant","Shoals",5,0.37,"NHEL"]
["Champaign","So","Sloan silt loam","Sloan",5,0.37,"NHEL"]
["Champaign","Sv","Sloan silt loam, gravelly subsoil variant","Sloan",4,0.28000000000000003,"NHEL"]
["Champaign","UnB","Uniontown silt loam, 2 to 6 percent slopes","Uniontown",4,0.37,"PHEL"]
["Champaign","W","Water","Water"]
["Champaign","Wa","Wallkill silt loam","Wallkill",5,0.32,"NHEL"]
["Champaign","Wn","Warners silt loam","Warners",5,0.43,"NHEL"]
["Champaign","WrA","Warsaw silt loam, 0 to 2 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
["Champaign","WrB","Warsaw silt loam, 2 to 6 percent slopes","Warsaw",4,0.28000000000000003,"PHEL"]
["Champaign","WsA","Wea silt loam, 0 to 3 percent slopes","Wea",5,0.32,"NHEL"]
[null,"Select","none","none"]
["Clark","Ad","Adrian muck, drained","Adrian",2,null,"NHEL"]
["Clark","Ae","Adrian muck, undrained","Adrian",2,null,"NHEL"]
["Clark","Ca","Carlisle muck, drained","Carlisle",2,null,"NHEL"]
["Clark","Cb","Carlisle muck, undrained","Carlisle",2,null,"NHEL"]
["Clark","CcD2","Casco gravelly loam, 12 to 20 percent slopes, eroded","Casco",3,0.24,"HEL"]
["Clark","CeA","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Clark","CeB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Clark","ChA","Celina-Strawn complex, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Clark","ChB","Celina-Strawn complex, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Clark","CrA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Clark","CrB","Crosby silt loam, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Clark","DAM","Dam","Dam"]
["Clark","DoE","Donnelsville channery silt loam, 18 to 30 percent slopes","Donnelsville",3,0.17,"HEL"]
["Clark","DpF","Donnelsville-Rock outcrop complex, 30 to 70 percent slopes","Donnelsville",3,0.12,"HEL"]
["Clark","Dr","Drummer silty clay loam, gravelly substratum","Drummer",4,0.28000000000000003,"NHEL"]
["Clark","EmA","Eldean silt loam, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Clark","EmB","Eldean silt loam, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Clark","EmB2","Eldean silt loam, 2 to 6 percent slopes, eroded","Eldean",4,0.37,"PHEL"]
["Clark","EmC2","Eldean silt loam, 6 to 12 percent slopes, eroded","Eldean",4,0.37,"HEL"]
["Clark","EnC2","Eldean-Casco complex, 6 to 12 percent slopes, eroded","Eldean",4,0.37,"HEL"]
["Clark","EpB2","Eldean-Miamian complex, 2 to 6 percent slopes, eroded","Eldean",4,0.37,"PHEL"]
["Clark","EpC2","Eldean-Miamian complex, 6 to 12 percent slopes, eroded","Eldean",4,0.37,"HEL"]
["Clark","EpC3","Eldean-Miamian complex, 6 to 12 percent slopes, severely eroded","Eldean",3,0.37,"HEL"]
["Clark","EpD2","Eldean-Miamian complex, 12 to 18 percent slopes, eroded","Eldean",4,0.37,"HEL"]
["Clark","EpD3","Eldean-Miamian complex, 12 to 18 percent slopes, severely eroded","Eldean",3,0.37,"HEL"]
["Clark","EpE2","Eldean-Miamian complex, 18 to 30 percent slopes, eroded","Eldean",4,0.37,"HEL"]
["Clark","EsE3","Eldean-Rodman complex, 18 to 30 percent slopes, severely eroded","Eldean",3,0.37,"HEL"]
["Clark","EuB","Eldean-Urban land complex, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Clark","EuC","Eldean-Urban land complex, 6 to 12 percent slopes","Eldean",4,0.37,"HEL"]
["Clark","Ge","Genesee silt loam, till substratum, rarely flooded","Genesee",5,0.37,"NHEL"]
["Clark","Gn","Genesee silt loam, till substratum, occasionally flooded","Genesee",5,0.37,"NHEL"]
["Clark","Ko","Kokomo silty clay loam","Kokomo",5,0.32,"NHEL"]
["Clark","Lg","Linwood muck, undrained","Linwood",2,null,"NHEL"]
["Clark","Lh","Linwood mucky silt loam, drained","Linwood",2,0.24,"NHEL"]
["Clark","Lm","Lippincott mucky silt loam","Lippincott",5,0.28000000000000003,"NHEL"]
["Clark","Lp","Lippincott silty clay loam","Lippincott",5,0.28000000000000003,"NHEL"]
["Clark","Lu","Lippincott-Urban land complex","Lippincott",5,0.28000000000000003,"NHEL"]
["Clark","MgB2","Miamian silty clay loam, limestone substratum, 2 to 6 percent slopes, eroded","Miamian",5,0.37,"PHEL"]
["Clark","MgC2","Miamian silty clay loam, limestone substratum, 6 to 12 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Clark","MgE2","Miamian silty clay loam, limestone substratum, 18 to 30 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Clark","MhA","Miamian silt loam, 0 to 2 percent slopes","Miamian",5,0.37,"NHEL"]
["Clark","MhB","Miamian silt loam, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Clark","MhB2","Miamian silt loam, 2 to 6 percent slopes, eroded","Miamian",5,0.37,"PHEL"]
["Clark","MhC","Miamian silt loam, 6 to 12 percent slopes","Miamian",5,0.37,"HEL"]
["Clark","MhC2","Miamian silt loam, 6 to 12 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Clark","MhD2","Miamian silt loam, 12 to 18 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Clark","MhE","Miamian silt loam, 18 to 30 percent slopes","Miamian",5,0.37,"HEL"]
["Clark","MhE2","Miamian silt loam, 18 to 30 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Clark","MkB2","Miamian silty clay loam, 2 to 6 percent slopes, eroded","Miamian",5,0.37,"PHEL"]
["Clark","MkC2","Miamian silty clay loam, 6 to 12 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Clark","MkD2","Miamian silty clay loam, 12 to 18 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Clark","MmC3","Miamian clay loam, 6 to 12 percent slopes, severely eroded","Miamian",4,0.37,"HEL"]
["Clark","MmD3","Miamian clay loam, 12 to 18 percent slopes, severely eroded","Miamian",4,0.37,"HEL"]
["Clark","MmE3","Miamian clay loam, 18 to 30 percent slopes, severely eroded","Miamian",4,0.37,"HEL"]
["Clark","MnB","Miamian-Urban land complex, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Clark","MnC","Miamian-Urban land complex, 6 to 12 percent slopes","Miamian",5,0.37,"HEL"]
["Clark","Mo","Milford silty clay loam, sandy substratum","Milford",5,0.28000000000000003,"NHEL"]
["Clark","Ms","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Clark","MtA","Milton silt loam, 0 to 2 percent slopes","Milton",4,0.37,"NHEL"]
["Clark","MtB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Clark","MvC2","Milton silty clay loam, 6 to 12 percent slopes, eroded","Milton",4,0.37,"HEL"]
["Clark","MxB","Milton-Urban land complex, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Clark","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Clark","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Clark","Pa","Patton silty clay loam","Patton",5,0.28000000000000003,"NHEL"]
["Clark","Pg","Pits, gravel","Pits"]
["Clark","Ph","Pits, quarry","Pits"]
["Clark","Pl","Pits, lime","Pits"]
["Clark","RaA","Randolph silt loam, 0 to 2 percent slopes","Randolph",3,0.37,"NHEL"]
["Clark","RgE","Rodman gravelly loam, 18 to 35 percent slopes","Rodman",3,0.2,"HEL"]
["Clark","Rn","Ross silt loam, occasionally flooded","Ross",5,0.32,"NHEL"]
["Clark","Ro","Ross silty clay loam, rarely flooded","Ross",5,0.32,"NHEL"]
["Clark","RuA","Rush silt loam, 0 to 2 percent slopes","Rush",5,0.37,"NHEL"]
["Clark","ScA","Savona silt loam, 0 to 2 percent slopes","Savona",4,0.37,"NHEL"]
["Clark","So","Sloan silt loam, sandy substratum, occasionally flooded","Sloan",5,0.37,"NHEL"]
["Clark","StB2","Strawn silty clay loam, 2 to 6 percent slopes, eroded","Strawn",5,0.37,"PHEL"]
["Clark","StC2","Strawn silty clay loam, 6 to 12 percent slopes, eroded","Strawn",5,0.37,"HEL"]
["Clark","StD2","Strawn silty clay loam, 12 to 18 percent slopes, eroded","Strawn",5,0.37,"HEL"]
["Clark","StE2","Strawn silty clay loam, 18 to 35 percent slopes, eroded","Strawn",5,0.37,"HEL"]
["Clark","SuA","Strawn-Crosby complex, 0 to 2 percent slopes","Strawn",5,0.37,"NHEL"]
["Clark","SuB","Strawn-Crosby complex, 2 to 6 percent slopes","Strawn",5,0.37,"PHEL"]
["Clark","ThA","Thackery silt loam, 0 to 2 percent slopes","Thackery",4,0.37,"NHEL"]
["Clark","Tr","Tremont silty clay loam, rarely flooded","Tremont",4,0.28000000000000003,"NHEL"]
["Clark","Ts","Tremont silt loam, occasionally flooded","Tremont",4,0.28000000000000003,"NHEL"]
["Clark","Ud","Udorthents, loamy","Udorthents"]
["Clark","Ur","Urban land","Urban"]
["Clark","W","Water","Water"]
["Clark","Wc","Wallkill silt loam, occasionally flooded","Wallkill",5,0.32,"NHEL"]
["Clark","WeA","Warsaw silt loam, 0 to 3 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
["Clark","WpA","Waupecan silt loam, 0 to 2 percent slopes","Waupecan",4,0.32,"NHEL"]
["Clark","WrA","Waynetown silt loam, 0 to 2 percent slopes","Waynetown",5,0.37,"NHEL"]
["Clark","Wt","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
[null,"Select","none","none"]
["Clermont","AdC","Alluvial land, sloping","Alluvial"]
["Clermont","AvA","Avonburg silt loam, 0 to 2 percent slopes","Avonburg",4,0.43,"NHEL"]
["Clermont","AvB","Avonburg silt loam, 2 to 6 percent slopes","Avonburg",4,0.43,"PHEL"]
["Clermont","AvB2","Avonburg silt loam, 2 to 6 percent slopes, moderately eroded","Avonburg",4,0.43,"PHEL"]
["Clermont","AwA","Avonburg-Urban land complex, nearly level","Avonburg",4,0.43,"NHEL"]
["Clermont","Bc","Blanchester silt loam","Blanchester",5,0.37,"NHEL"]
["Clermont","CcB","Cincinnati silt loam, 2 to 6 percent slopes","Cincinnati",4,0.37,"PHEL"]
["Clermont","CcB2","Cincinnati silt loam, 2 to 6 percent slopes, moderately eroded","Cincinnati",4,0.37,"PHEL"]
["Clermont","CcC2","Cincinnati silt loam, 6 to 12 percent slopes, moderately eroded","Cincinnati",4,0.37,"PHEL"]
["Clermont","CcD2","Cincinnati silt loam, 12 to 18 percent slopes, moderately eroded","Cincinnati",4,0.37,"HEL"]
["Clermont","CkD3","Cincinnati and Hickory soils, 12 to 25 percent slopes, severely eroded","Cincinnati",3,0.37,"HEL"]
["Clermont","Ct","Clermont silt loam","Clermont",5,0.37,"NHEL"]
["Clermont","Cu","Cut and fill land","Cut"]
["Clermont","EaD2","Eden flaggy silty clay loam, 12 to 18 percent slopes, moderately eroded","Eden",3,0.43,"HEL"]
["Clermont","EaE2","Eden flaggy silty clay loam, 18 to 25 percent slopes, moderately eroded","Eden",3,0.43,"HEL"]
["Clermont","EaF2","Eden flaggy silty clay loam, 25 to 50 percent slopes, moderately eroded","Eden",3,0.43,"HEL"]
["Clermont","EbC2","Edenton loam, 6 to 12 percent slopes, moderately eroded","Edenton",3,0.43,"HEL"]
["Clermont","EbD2","Edenton loam, 12 to 18 percent slopes, moderately eroded","Edenton",3,0.43,"HEL"]
["Clermont","EbE2","Edenton loam, 18 to 25 percent slopes, moderately eroded","Edenton",3,0.43,"HEL"]
["Clermont","EbG2","Edenton loam, 25 to 50 percent slopes, moderately eroded","Edenton",3,0.43,"HEL"]
["Clermont","EcE3","Edenton clay loam, 12 to 25 percent slopes, severely eroded","Edenton",2,0.43,"HEL"]
["Clermont","EdG3","Edenton and Fairmount soils, 25 to 50 percent slopes, severely eroded","Edenton",2,0.43,"HEL"]
["Clermont","Ee","Eel silt loam","Eel",5,0.37,"NHEL"]
["Clermont","FaE2","Fairmount very flaggy silty clay loam, 18 to 25 percent slopes, moderately eroded","Fairmount",2,0.37,"HEL"]
["Clermont","FaG2","Fairmount very flaggy silty clay loam, 25 to 50 percent slopes, moderately eroded","Fairmount",2,0.37,"HEL"]
["Clermont","FnB","Fox silt loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Clermont","FnC2","Fox silt loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Clermont","FuB","Fox-Urban land complex, gently sloping","Fox",4,0.37,"PHEL"]
["Clermont","Gn","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Clermont","GpB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Clermont","GpC2","Glenford silt loam, 6 to 12 percent slopes, moderately eroded","Glenford",5,0.37,"PHEL"]
["Clermont","GpE2","Glenford silt loam, 18 to 25 percent slopes, moderately eroded","Glenford",5,0.37,"HEL"]
["Clermont","Gr","Gravel pits","Gravel"]
["Clermont","HkD2","Hickory loam, 12 to 18 percent slopes, moderately eroded","Hickory",5,0.37,"HEL"]
["Clermont","HkF2","Hickory loam, 18 to 35 percent slopes, moderately eroded","Hickory",5,0.37,"HEL"]
["Clermont","HlG3","Hickory clay loam, 25 to 50 percent slopes, severely eroded","Hickory",4,0.37,"HEL"]
["Clermont","Hu","Huntington silt loam","Huntington",5,0.28000000000000003,"NHEL"]
["Clermont","Lg","Lanier sandy loam","Lanier",5,0.2,"NHEL"]
["Clermont","Ln","Lindside silt loam","Lindside",5,0.28000000000000003,"NHEL"]
["Clermont","Mb","Mahalasville silty clay loam","Mahalasville",5,0.28000000000000003,"NHEL"]
["Clermont","MdB","Markland silt loam, 2 to 6 percent slopes","Markland",3,0.43,"PHEL"]
["Clermont","MgA","McGary silt loam, 0 to 2 percent slopes","McGary",3,0.43,"NHEL"]
["Clermont","Mh","Medway silt loam, overwash","Medway",5,0.32,"NHEL"]
["Clermont","Ne","Newark silt loam","Newark",5,0.32,"NHEL"]
["Clermont","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Clermont","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Clermont","OdA","Ockley-Urban land complex, nearly level","Ockley",5,0.37,"NHEL"]
["Clermont","Rh","Riverwash","Riverwash"]
["Clermont","RkD2","Rodman and Casco loams, 12 to 18 percent slopes, moderately eroded","Rodman",3,0.2,"HEL"]
["Clermont","RkE2","Rodman and Casco loams, 18 to 25 percent slopes, moderately eroded","Rodman",3,0.2,"HEL"]
["Clermont","Rn","Ross silt loam","Ross",5,0.32,"NHEL"]
["Clermont","RpA","Rossmoyne silt loam, 0 to 2 percent slopes","Rossmoyne",4,0.37,"NHEL"]
["Clermont","RpB","Rossmoyne silt loam, 2 to 6 percent slopes","Rossmoyne",4,0.37,"PHEL"]
["Clermont","RpB2","Rossmoyne silt loam, 2 to 6 percent slopes, moderately eroded","Rossmoyne",4,0.37,"PHEL"]
["Clermont","RpC2","Rossmoyne silt loam, 6 to 12 percent slopes, moderately eroded","Rossmoyne",4,0.37,"PHEL"]
["Clermont","RsC3","Rossmoyne silty clay loam, 6 to 12 percent slopes, severely eroded","Rossmoyne",3,0.37,"PHEL"]
["Clermont","RtB","Rossmoyne-Urban land complex, gently sloping","Rossmoyne",4,0.37,"PHEL"]
["Clermont","RtC","Rossmoyne-Urban land complex, sloping","Rossmoyne",4,0.37,"HEL"]
["Clermont","SaA","Sardinia silt loam, 0 to 2 percent slopes","Sardinia",5,0.37,"NHEL"]
["Clermont","SaB","Sardinia silt loam, 2 to 6 percent slopes","Sardinia",5,0.37,"PHEL"]
["Clermont","SeC2","Sees silty clay loam, 4 to 12 percent slopes, moderately eroded","Sees",3,0.37,"PHEL"]
["Clermont","SeD2","Sees silty clay loam, 12 to 18 percent slopes, moderately eroded","Sees",3,0.37,"HEL"]
["Clermont","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Clermont","St","Stonelick sandy loam","Stonelick",5,0.24,"NHEL"]
["Clermont","W","Water","Water"]
["Clermont","WvB","Williamsburg and Martinsville silt loams, 2 to 6 percent slopes","Williamsburg",5,0.32,"PHEL"]
["Clermont","WvC2","Williamsburg and Martinsville silt loams, 6 to 12 percent slopes, moderately eroded","Williamsburg",5,0.32,"PHEL"]
["Clermont","WvD2","Williamsburg and Martinsville silt loams, 12 to 18 percent slopes, moderately eroded","Williamsburg",5,0.32,"HEL"]
[null,"Select","none","none"]
["Clinton","AgA0","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Clinton","AvA1","Avonburg silt loam, 0 to 2 percent slopes","Avonburg",4,0.43,"NHEL"]
["Clinton","AvB1","Avonburg silt loam, 2 to 6 percent slopes","Avonburg",4,0.43,"PHEL"]
["Clinton","AvB2","Avonburg silt loam, 2 to 6 percent slopes, moderately eroded","Avonburg",4,0.43,"PHEL"]
["Clinton","BbA1","Birkbeck silt loam, 0 to 2 percent slopes","Birkbeck",5,0.37,"NHEL"]
["Clinton","BbB1","Birkbeck silt loam, 2 to 6 percent slopes","Birkbeck",5,0.37,"PHEL"]
["Clinton","BbB2","Birkbeck silt loam, 2 to 6 percent slopes, moderately eroded","Birkbeck",5,0.37,"PHEL"]
["Clinton","BcA0","Blanchester silt loam","Blanchester",5,0.37,"NHEL"]
["Clinton","BrA0","Brookston silty clay loam","Brookston",5,0.28000000000000003,"NHEL"]
["Clinton","BsA+","Brookston silt loam, overwashed","Brookston",5,0.28000000000000003,"NHEL"]
["Clinton","BsA0","Brookston silt loam","Brookston",5,0.28000000000000003,"NHEL"]
["Clinton","CcB1","Cincinnati silt loam, 2 to 6 percent slopes","Cincinnati",4,0.37,"PHEL"]
["Clinton","CcB2","Cincinnati silt loam, 2 to 6 percent slopes, moderately eroded","Cincinnati",4,0.37,"PHEL"]
["Clinton","CcC1","Cincinnati silt loam, 6 to 12 percent slopes","Cincinnati",4,0.37,"PHEL"]
["Clinton","CcC2","Cincinnati silt loam, 6 to 12 percent slopes, moderately eroded","Cincinnati",4,0.37,"PHEL"]
["Clinton","CeA1","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Clinton","CeB1","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Clinton","CeB2","Celina silt loam, 2 to 6 percent slopes, moderately eroded","Celina",5,0.37,"PHEL"]
["Clinton","CeC2","Celina silt loam, 6 to 12 percent slopes, moderately eroded","Celina",5,0.37,"PHEL"]
["Clinton","CfF2","Casco and Rodman soils, 25 to 50 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Clinton","CgE2","Casco, Rodman, and Fox soils, 18 to 25 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Clinton","CrA1","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Clinton","CrB1","Crosby silt loam, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Clinton","CrB2","Crosby silt loam, 2 to 6 percent slopes, moderately eroded","Crosby",3,0.43,"PHEL"]
["Clinton","CtA1","Clermont silt loam","Clermont",5,0.37,"NHEL"]
["Clinton","DeA1","Delmar silt loam","Delmar",4,0.37,"NHEL"]
["Clinton","EdB2","Edenton silt loam, 2 to 6 percent slopes, moderately eroded","Edenton",3,0.43,"PHEL"]
["Clinton","EdC2","Edenton silt loam, 6 to 12 percent slopes, moderately eroded","Edenton",3,0.43,"PHEL"]
["Clinton","EdD2","Edenton silt loam, 12 to 18 percent slopes, moderately eroded","Edenton",3,0.43,"HEL"]
["Clinton","EeA0","Eel silt loam","Eel",5,0.37,"NHEL"]
["Clinton","EfE2","Edenton and Fairmount soils, 18 to 25 percent slopes, moderately eroded","Edenton",3,0.43,"HEL"]
["Clinton","EfE3","Edenton and Fairmount soils, 18 to 25 percent slopes, severely eroded","Edenton",2,0.43,"HEL"]
["Clinton","EfF2","Edenton and Fairmount soils, 25 to 50 percent slopes, moderately eroded","Edenton",3,0.43,"HEL"]
["Clinton","EmA0","Eel loam","Eel",5,0.37,"NHEL"]
["Clinton","EsC3","Edenton soils, 6 to 12 percent slopes, severely eroded","Edenton",2,0.43,"PHEL"]
["Clinton","EsD3","Edenton soils, 12 to 18 percent slopes, severely eroded","Edenton",2,0.43,"HEL"]
["Clinton","FcD2","Fox and Casco soils, 12 to 18 percent slopes, moderately eroded","Fox",4,0.37,"HEL"]
["Clinton","FdD3","Fox, Casco, and Rodman soils, 12 to 25 percent slopes, severely eroded","Fox",3,0.37,"HEL"]
["Clinton","FnA1","Fincastle silt loam, 0 to 2 percent slopes","Fincastle",5,0.37,"NHEL"]
["Clinton","FnB1","Fincastle silt loam, 2 to 6 percent slopes","Fincastle",5,0.37,"PHEL"]
["Clinton","FnB2","Fincastle silt loam, 2 to 6 percent slopes, moderately eroded","Fincastle",5,0.37,"PHEL"]
["Clinton","FxA1","Fox silt loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Clinton","FxB1","Fox silt loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Clinton","FxB2","Fox silt loam, 2 to 6 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Clinton","FxC2","Fox silt loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Clinton","GeA0","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Clinton","GmA0","Genesee loam, sandy substratum","Genesee",5,0.37,"NHEL"]
["Clinton","GnA0","Genesee loam","Genesee",5,0.37,"NHEL"]
["Clinton","GsA0","Genesee silt loam, sandy substratum","Genesee",5,0.37,"NHEL"]
["Clinton","Gu","Gullied land","Gullied",null,null,"HEL"]
["Clinton","HeF1","Hennepin and Miami soils, 25 to 50 percent slopes","Hennepin",4,0.32,"HEL"]
["Clinton","HeF2","Hennepin and Miami soils, 25 to 50 pecent slopes, moderately eroded","Hennepin",4,0.32,"HEL"]
["Clinton","HeF3","Hennepin and Miami soils, 25 to 50 percent slopes, severely eroded","Hennepin",4,0.32,"HEL"]
["Clinton","HnA1","Henshaw silt loam","Henshaw",4,0.43,"NHEL"]
["Clinton","KoA+","Kokomo silt loam, overwashed","Kokomo",3,0.32,"NHEL"]
["Clinton","MdA0","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Clinton","MeB3","Miami soils, 2 to 6 percent slopes, severely eroded","Miami",4,0.37,"PHEL"]
["Clinton","MeC3","Miami soils, 6 to 12 percent slopes, severely eroded","Miami",4,0.37,"PHEL"]
["Clinton","MeD3","Miami soils, 12 to 18 percent slopes, severely eroded","Miami",4,0.37,"HEL"]
["Clinton","MhE1","Miami and Hennepin silt loams, 18 to 25 percent slopes","Miami",5,0.37,"HEL"]
["Clinton","MhE2","Miami and Hennepin silt loams, 18 to 25 percent slopes, moderately eroded","Miami",5,0.37,"HEL"]
["Clinton","MmB1","Miami silt loam, 2 to 6 percent slopes","Miami",5,0.37,"PHEL"]
["Clinton","MmB2","Miami silt loam, 2 to 6 percent slopes, moderately eroded","Miami",5,0.37,"PHEL"]
["Clinton","MmC1","Miami silt loam, 6 to 12 percent slopes","Miami",5,0.37,"PHEL"]
["Clinton","MmC2","Miami silt loam, 6 to 12 percent slopes, moderately eroded","Miami",5,0.37,"PHEL"]
["Clinton","MmD1","Miami silt loam, 12 to 18 percent slopes","Miami",5,0.37,"HEL"]
["Clinton","MmD2","Miami silt loam, 12 to 18 percent slopes, moderately eroded","Miami",5,0.37,"HEL"]
["Clinton","MnA1","Milton silt loam, 0 to 2 percent slopes","Milton",4,0.37,"NHEL"]
["Clinton","MnB1","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Clinton","MnB2","Milton silt loam, 2 to 6 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Clinton","MnC2","Milton silt loam, 6 to 12 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Clinton","MnD2","Milton silt loam, 12 to 18 percent slopes, moderately eroded","Milton",4,0.37,"HEL"]
["Clinton","MpE3","Miami and Hennepin soils, 18 to 25 percent slopes, severely eroded","Miami",4,0.37,"HEL"]
["Clinton","MsD3","Milton soils, shallow, 12 to 18 percent slopes, severely eroded","Milton",3,0.37,"HEL"]
["Clinton","MsF3","Milton soils, shallow, 25 to 50 percent slopes, severely eroded","Milton",3,0.37,"HEL"]
["Clinton","MtB1","Milton silt loam, shallow, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Clinton","MtC2","Milton silt loam, shallow, 6 to 12 percent slopes, moderately eroded","Milton",4,0.37,"HEL"]
["Clinton","MtD2","Milton silt loam, shallow, 12 to 18 percent slopes, moderately eroded","Milton",4,0.37,"HEL"]
["Clinton","MtE2","Milton silt loam, shallow, 18 to 25 percent slopes, moderately eroded","Milton",4,0.37,"HEL"]
["Clinton","MtF2","Milton silt loam, shallow, 25 to 50 percent slopes, moderately eroded","Milton",4,0.37,"HEL"]
["Clinton","MwA0","Medway loam","Medway",5,0.32,"NHEL"]
["Clinton","MyA0","Medway silt loam","Medway",5,0.32,"NHEL"]
["Clinton","OcA1","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Clinton","OcB1","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Clinton","OcB2","Ockley silt loam, 2 to 6 percent slopes, moderately eroded","Ockley",5,0.37,"PHEL"]
["Clinton","OcC2","Ockley silt loam, 6 to 12 percent slopes, moderately eroded","Ockley",5,0.37,"PHEL"]
["Clinton","OmA1","Ockley silt loam, mixed substratum, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Clinton","OmB1","Ockley silt loam, mixed substratum, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Clinton","OmB2","Ockley silt loam, mixed substratum, 2 to 6 percent slopes, moderately eroded","Ockley",5,0.37,"PHEL"]
["Clinton","OmC2","Ockley silt loam, mixed substratum, 6 to 12 percent slopes, moderately eroded","Ockley",5,0.37,"PHEL"]
["Clinton","PaA+","Bonpas silt loam, overwashed","Bonpas",5,0.28000000000000003,"NHEL"]
["Clinton","PcA0","Bonpas silty clay loam","Bonpas",5,0.28000000000000003,"NHEL"]
["Clinton","RaA0","Ragsdale silt loam","Ragsdale",5,0.28000000000000003,"NHEL"]
["Clinton","RbA1","Raub silt loam","Raub",5,0.28000000000000003,"NHEL"]
["Clinton","ReA1","Reesville silt loam, 0 to 2 percent slopes","Reesville",5,0.37,"NHEL"]
["Clinton","ReB1","Reesville silt loam, 2 to 6 percent slopes","Reesville",5,0.37,"PHEL"]
["Clinton","RgA0","Ragsdale silty clay loam","Ragsdale",5,0.28000000000000003,"NHEL"]
["Clinton","RhF1","Russell and Hennepin silt loams, 25 to 50 percent slopes","Russell",5,0.37,"HEL"]
["Clinton","RhF2","Russell and Hennepin silt loams, 25 to 50 percent slopes, moderately eroded","Russell",5,0.37,"HEL"]
["Clinton","RmA1","Rossmoyne silt loam, 0 to 2 percent slopes","Rossmoyne",4,0.37,"NHEL"]
["Clinton","RmB1","Rossmoyne silt loam, 2 to 6 percent slopes","Rossmoyne",4,0.37,"PHEL"]
["Clinton","RmB2","Rossmoyne silt loam, 2 to 6 percent slopes, moderately eroded","Rossmoyne",4,0.37,"PHEL"]
["Clinton","RmC2","Rossmoyne silt loam, 6 to 12 percent slopes, moderately eroded","Rossmoyne",4,0.37,"PHEL"]
["Clinton","RmD2","Rossmoyne silt loam, 12 to 18 percent slopes, moderately eroded","Rossmoyne",4,0.37,"HEL"]
["Clinton","RnC3","Rossmoyne soils, 6 to 12 percent slopes, severely eroded","Rossmoyne",3,0.37,"PHEL"]
["Clinton","RoA0","Ross loam","Ross",5,0.32,"NHEL"]
["Clinton","RsA0","Ross silt loam","Ross",5,0.32,"NHEL"]
["Clinton","RuB1","Russell silt loam, 2 to 6 percent slopes","Russell",5,0.37,"PHEL"]
["Clinton","RuB2","Russell silt loam, 2 to 6 percent slopes, moderately eroded","Russell",5,0.37,"PHEL"]
["Clinton","RuC1","Russell silt loam, 6 to 12 percent slopes","Russell",5,0.37,"PHEL"]
["Clinton","RuC2","Russell silt loam, 6 to 12 percent slopes, moderately eroded","Russell",5,0.37,"PHEL"]
["Clinton","RuD1","Russell silt loam, 12 to 18 percent slopes","Russell",5,0.37,"HEL"]
["Clinton","RuD2","Russell silt loam, 12 to 18 percent slopes, moderately eroded","Russell",5,0.37,"HEL"]
["Clinton","RuE1","Russell silt loam, 18 to 25 percent slopes","Russell",5,0.37,"HEL"]
["Clinton","RuE2","Russell silt loam, 18 to 25 percent slopes, moderately eroded","Russell",5,0.37,"HEL"]
["Clinton","RvB3","Russell soils, 2 to 6 percent slopes, severely eroded","Russell",4,0.37,"PHEL"]
["Clinton","RvC3","Russell soils, 6 to 12 percent slopes, severely eroded","Russell",4,0.37,"PHEL"]
["Clinton","RvD3","Russell soils, 12 to 18 percent slopes, severely eroded","Russell",4,0.37,"HEL"]
["Clinton","RvE3","Russell soils, 18 to 25 percent slopes, severely eroded","Russell",4,0.37,"HEL"]
["Clinton","RxF3","Russell and Hennepin soils, 25 to 50 percent slopes, severely eroded","Russell",4,0.37,"HEL"]
["Clinton","SaA1","Sardinia silt loam, 0 to 2 percent slopes","Sardinia",5,0.37,"NHEL"]
["Clinton","SaB1","Sardinia silt loam, 2 to 6 percent slopes","Sardinia",5,0.37,"PHEL"]
["Clinton","SaB2","Sardinia silt loam, 2 to 6 percent slopes, moderately eroded","Sardinia",5,0.37,"PHEL"]
["Clinton","ShA0","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Clinton","SmA1","Sleeth silt loam, mixed substratum, 0 to 2 percent slopes","Sleeth",5,0.32,"NHEL"]
["Clinton","SmB1","Sleeth silt loam, mixed substratum, 2 to 6 percent slopes","Sleeth",5,0.32,"PHEL"]
["Clinton","SnA+","Sloan silt loam, overwashed","Sloan",5,0.37,"NHEL"]
["Clinton","SnA0","Sloan silt loam","Sloan",5,0.37,"NHEL"]
["Clinton","StA1","Sleeth silt loam","Sleeth",5,0.32,"NHEL"]
["Clinton","SyA0","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Clinton","ThA1","Thackery silt loam, 0 to 2 percent slopes","Thackery",4,0.37,"NHEL"]
["Clinton","ThB1","Thackery silt loam, 2 to 6 percent slopes","Thackery",4,0.37,"PHEL"]
["Clinton","TmA1","Thackery silt loam, mixed substratum, 0 to 2 percent slopes","Thackery",4,0.37,"NHEL"]
["Clinton","TmB1","Thackery silt loam, mixed substratum, 2 to 6 percent slopes","Thackery",4,0.37,"PHEL"]
["Clinton","UnA1","Uniontown silt loam, 0 to 2 percent slopes","Uniontown",4,0.37,"NHEL"]
["Clinton","UnB2","Uniontown silt loam, 2 to 6 percent slopes, moderately eroded","Uniontown",4,0.37,"PHEL"]
["Clinton","WbA1","Williamsburg silt loam, 0 to 2 percent slopes","Williamsburg",5,0.32,"NHEL"]
["Clinton","WbB1","Williamsburg silt loam, 2 to 6 percent slopes","Williamsburg",5,0.32,"PHEL"]
["Clinton","WbB2","Williamsburg silt loam, 2 to 6 percent slopes, moderately eroded","Williamsburg",5,0.32,"PHEL"]
["Clinton","WbC1","Williamsburg silt loam, 6 to 12 percent slopes","Williamsburg",5,0.32,"PHEL"]
["Clinton","WbC2","Williamsburg silt loam, 6 to 12 percent slopes, moderately eroded","Williamsburg",5,0.32,"PHEL"]
["Clinton","WbD2","Williamsburg silt loam, 12 to 18 percent slopes, moderately eroded","Williamsburg",5,0.32,"HEL"]
["Clinton","WbE2","Williamsburg silt loam, 18 to 25 percent slopes, moderately eroded","Williamsburg",5,0.32,"HEL"]
["Clinton","WeA+","Westland silt loam, overwashed","Westland",5,0.28000000000000003,"NHEL"]
["Clinton","WeA0","Westland silt loam","Westland",5,0.28000000000000003,"NHEL"]
["Clinton","WmA+","Westland silt loam, mixed substratum, overwashed","Westland",5,0.28000000000000003,"NHEL"]
["Clinton","WnA0","Westland silty clay loam, mixed substratum","Westland",5,0.28000000000000003,"NHEL"]
["Clinton","WtA0","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
["Clinton","XeA1","Xenia silt loam, 0 to 2 percent slopes","Xenia",5,0.37,"NHEL"]
["Clinton","XeB1","Xenia silt loam, 2 to 6 percent slopes","Xenia",5,0.37,"PHEL"]
["Clinton","XeB2","Xenia silt loam, 2 to 6 percent slopes, moderately eroded","Xenia",5,0.37,"PHEL"]
["Clinton","XeC1","Xenia silt loam, 6 to 12 percent slopes","Xenia",5,0.37,"PHEL"]
["Clinton","XeC2","Xenia silt loam, 6 to 12 percent slopes, moderately eroded","Xenia",5,0.37,"PHEL"]
["Clinton","XnB3","Xenia soils, 2 to 6 percent slopes, severely eroded","Xenia",5,0.37,"PHEL"]
["Clinton","XnC3","Xenia soils, 6 to 12 percent slopes, severely eroded","Xenia",5,0.37,"PHEL"]
[null,"Select","none","none"]
["Darke","Ag","Algiers silt loam, occasionally flooded","Algiers",5,0.37,"NHEL"]
["Darke","BnA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Darke","BnB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Darke","Br","Brookston silty clay loam","Brookston",5,0.28000000000000003,"NHEL"]
["Darke","Ca","Carlisle muck","Carlisle",2,null,"NHEL"]
["Darke","CeA","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Darke","CeB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Darke","CrA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Darke","CrB","Crosby silt loam, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Darke","DeA","Del Rey silt loam, 0 to 3 percent slopes","Del Rey",3,0.43,"PHEL"]
["Darke","Ed","Edwards muck","Edwards",2,null,"NHEL"]
["Darke","Ee","Eel silt loam, occasionally flooded","Eel",5,0.37,"NHEL"]
["Darke","EnA","Eldean loam, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Darke","EnB","Eldean loam, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Darke","ErC2","Eldean-Miamian complex, 6 to 12 percent slopes, eroded","Eldean",4,0.37,"PHEL"]
["Darke","ErD2","Eldean-Miamian complex, 12 to 18 percent slopes, eroded","Eldean",4,0.37,"HEL"]
["Darke","GnB","Glynwood silt loam, 2 to 6 percent slopes","Glynwood",3,0.43,"PHEL"]
["Darke","GnB2","Glynwood silt loam, 2 to 6 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Darke","GnC2","Glynwood silt loam, 6 to 12 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Darke","GyC3","Glynwood clay loam, 6 to 12 percent slopes, severely eroded","Glynwood",2,0.43,"HEL"]
["Darke","GyD3","Glynwood clay loam, 12 to 18 percent slopes, severely eroded","Glynwood",2,0.43,"HEL"]
["Darke","LeB","Lewisburg silt loam, 2 to 6 percent slopes","Lewisburg",3,0.43,"PHEL"]
["Darke","Ln","Linwood muck","Linwood",2,null,"NHEL"]
["Darke","Lp","Lippincott silty clay loam","Lippincott",5,0.28000000000000003,"NHEL"]
["Darke","Md","Medway silt loam, occasionally flooded","Medway",5,0.32,"NHEL"]
["Darke","MmA","Miamian silt loam, 0 to 2 percent slopes","Miamian",5,0.37,"NHEL"]
["Darke","MmB","Miamian silt loam, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Darke","MmC2","Miamian silt loam, 6 to 12 percent slopes, eroded","Miamian",5,0.37,"PHEL"]
["Darke","MmD2","Miamian silt loam, 12 to 18 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Darke","MmE","Miamian silt loam, 18 to 25 percent slopes","Miamian",5,0.37,"HEL"]
["Darke","MnC3","Miamian clay loam, 6 to 12 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Darke","MnD3","Miamian clay loam, 12 to 18 percent slopes, severely eroded","Miamian",4,0.37,"HEL"]
["Darke","Mt","Montgomery silty clay","Montgomery",5,0.37,"NHEL"]
["Darke","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Darke","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Darke","OdA","Odell silt loam, 0 to 3 percent slopes","Odell",5,0.28000000000000003,"NHEL"]
["Darke","Pa","Patton silty clay loam","Patton",5,0.28000000000000003,"NHEL"]
["Darke","Pe","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Darke","PyA","Pyrmont silt loam, 0 to 3 percent slopes","Pyrmont",3,0.43,"PHEL"]
["Darke","Sa","Saranac silty clay, frequently flooded","Saranac",5,0.24,"NHEL"]
["Darke","SeA","Savona silt loam, 0 to 2 percent slopes","Savona",4,0.37,"NHEL"]
["Darke","Sh","Shoals silt loam, occasionally flooded","Shoals",5,0.37,"NHEL"]
["Darke","Tr","Treaty silty clay loam","Treaty",5,0.32,"NHEL"]
["Darke","Ud","Udorthents, loamy","Udorthents"]
["Darke","W","Water","Water"]
["Darke","Wb","Wallkill silt loam","Wallkill",5,0.32,"NHEL"]
["Darke","WeA","Wea silt loam, 0 to 2 percent slopes","Wea",5,0.32,"NHEL"]
["Darke","Ws","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
[null,"Select","none","none"]
["Fayette","Ag","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Fayette","Bs","Brookston silty clay loam","Brookston",5,0.28000000000000003,"NHEL"]
["Fayette","CaB2","Cana silt loam, 2 to 6 percent slopes, moderately eroded","Cana",4,0.37,"PHEL"]
["Fayette","CaC2","Cana silt loam, 6 to 12 percent slopes, moderately eroded","Cana",4,0.37,"PHEL"]
["Fayette","CdC2","Casco and Rodman soils, 2 to 12 percent slopes, moderately eroded","Casco",3,0.24,"PHEL"]
["Fayette","CeA","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Fayette","CeB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Fayette","CeB2","Celina silt loam, 2 to 6 percent slopes, moderately eroded","Celina",5,0.37,"PHEL"]
["Fayette","CoB","Corwin silt loam, 2 to 6 percent slopes","Corwin",5,0.28000000000000003,"PHEL"]
["Fayette","CrA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Fayette","CrB","Crosby silt loam, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Fayette","Cw","Cut and fill land","Cut"]
["Fayette","FnA","Fox silt loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Fayette","FnB","Fox silt loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Fayette","FnB2","Fox silt loam, 2 to 6 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Fayette","FnC2","Fox silt loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Fayette","FoC3","Fox and Casco soils, 6 to 12 percent slopes, severely eroded","Fox",3,0.37,"PHEL"]
["Fayette","FrE2","Fox, Casco, and Rodman soils, 12 to 25 percent slopes, moderately eroded","Fox",4,0.37,"HEL"]
["Fayette","Gn","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Fayette","Gp","Gravel pits","Gravel"]
["Fayette","HeA","Henshaw silt loam, 0 to 2 percent slopes","Henshaw",4,0.43,"NHEL"]
["Fayette","HkA","Henshaw silt loam, dark variant, 0 to 2 percent slopes","Henshaw",5,0.28000000000000003,"NHEL"]
["Fayette","KeB","Kendallville silt loam, 2 to 6 percent slopes","Kendallville",3,0.37,"PHEL"]
["Fayette","KeB2","Kendallville silt loam, 2 to 6 percent slopes, moderately eroded","Kendallville",3,0.37,"PHEL"]
["Fayette","KeC2","Kendallville silt loam, 6 to 12 percent slopes, moderately eroded","Kendallville",3,0.37,"PHEL"]
["Fayette","KlC3","Kendallville clay loam, 6 to 12 percent slopes, severely eroded","Kendallville",2,0.37,"HEL"]
["Fayette","KlD3","Kendallville clay loam, 12 to 18 percent slopes, severely eroded","Kendallville",2,0.37,"HEL"]
["Fayette","Md","Medway silt loam","Medway",5,0.32,"NHEL"]
["Fayette","Me","Medway silt loam, moderately shallow variant","Medway",4,0.28000000000000003,"NHEL"]
["Fayette","MlB","Miamian silt loam, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Fayette","MlB2","Miamian silt loam, 2 to 6 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Fayette","MlC","Miamian silt loam, 6 to 12 percent slopes","Miamian",5,0.37,"PHEL"]
["Fayette","MlC2","Miamian silt loam, 6 to 12 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Fayette","MlD2","Miamian silt loam, 12 to 18 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Fayette","MmB3","Miamian clay loam, 2 to 6 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Fayette","MmC3","Miamian clay loam, 6 to 12 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Fayette","MmD3","Miamian clay loam, 12 to 18 percent slopes, severely eroded","Miamian",4,0.37,"HEL"]
["Fayette","MpE2","Miamian and Hennepin silt loams, 18 to 25 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Fayette","MpF2","Miamian and Hennepin silt loams, 25 to 35 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Fayette","MrF3","Miamian and Hennepin soils, 18 to 35 percent slopes, severely eroded","Miamian",4,0.37,"HEL"]
["Fayette","Ms","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Fayette","MtB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Fayette","MtB2","Milton silt loam, 2 to 6 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Fayette","MtC2","Milton silt loam, 6 to 12 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Fayette","OdA","Odell silt loam, 0 to 2 percent slopes","Odell",5,0.28000000000000003,"NHEL"]
["Fayette","Pa","Patton silty clay loam","Patton",5,0.28000000000000003,"NHEL"]
["Fayette","Pc","Patton silty clay loam, overwash","Patton",5,0.28000000000000003,"NHEL"]
["Fayette","Qu","Quarries","Quarries"]
["Fayette","RcB","Randolph silt loam, 2 to 6 percent slopes","Randolph",3,0.37,"PHEL"]
["Fayette","RmC","Ritchey and Romeo silt loams, 2 to 12 percent slopes","Ritchey",2,0.37,"PHEL"]
["Fayette","RmF2","Ritchey and Romeo silt loams, 12 to 35 percent slopes, moderately eroded","Ritchey",2,0.37,"HEL"]
["Fayette","Rs","Ross silt loam","Ross",5,0.32,"NHEL"]
["Fayette","SlA","Sleeth silt loam, 0 to 2 percent slopes","Sleeth",5,0.32,"NHEL"]
["Fayette","ThB","Thackery silt loam, 1 to 4 percent slopes","Thackery",4,0.37,"PHEL"]
["Fayette","W","Water","Water"]
["Fayette","We","Warners muck","Warners",5,null,"NHEL"]
["Fayette","WrB","Warsaw silt loam, 1 to 4 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
["Fayette","WsA","Wea silt loam, 0 to 2 percent slopes","Wea",5,0.32,"NHEL"]
["Fayette","Wu","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
["Fayette","Wv","Westland silty clay loam, overwash","Westland",5,0.28000000000000003,"NHEL"]
[null,"Select","none","none"]
["Greene","Ag","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Greene","BbB","Birkbeck silt loam, 1 to 4 percent slopes","Birbeck",5,0.37,"NHEL"]
["Greene","Bs","Brookston silty clay loam","Brookston",5,0.28000000000000003,"NHEL"]
["Greene","Bt","Brookston-Urban land complex","Brookston",5,0.28000000000000003,"NHEL"]
["Greene","CcD2","Casco-Eldean loams, 12 to 18 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Greene","CdE2","Casco-Rodman loams, 18 to 50 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Greene","CeA","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Greene","CeB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Greene","C.F.","Cut and fill land","Cut"]
["Greene","CrA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Greene","CrB","Crosby silt loam, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Greene","EdB","Edenton silt loam, 2 to 6 percent slopes","Edenton",3,0.43,"PHEL"]
["Greene","EdC2","Edenton silt loam, 6 to 12 percent slopes, moderately eroded","Edenton",3,0.43,"PHEL"]
["Greene","EdD2","Edenton silt loam, 12 to 18 percent slopes, moderately eroded","Edenton",3,0.43,"HEL"]
["Greene","Ee","Eel loam","Eel",5,0.37,"NHEL"]
["Greene","EmA","Eldean silt loam, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Greene","EmB","Eldean silt loam, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Greene","EmB2","Eldean silt loam, 2 to 6 percent slopes, moderately eroded","Eldean",4,0.37,"PHEL"]
["Greene","EmC2","Eldean silt loam, 6 to 12 percent slopes, moderately eroded","Eldean",4,0.37,"PHEL"]
["Greene","EnC3","Eldean clay loam, 6 to 12 percent slopes, severely eroded","Eldean",3,0.37,"PHEL"]
["Greene","EpC","Eldean-Urban land complex, rolling","Eldean",4,0.37,"PHEL"]
["Greene","FaF","Fairmount silty clay loam, moderately deep variant, 25 to 50 percent slopes","Fairmount",3,0.43,"HEL"]
["Greene","FnA","Fincastle silt loam, 0 to 2 percent slopes","Fincastle",5,0.37,"NHEL"]
["Greene","Gn","Genesee loam","Genesee",5,0.37,"NHEL"]
["Greene","G.P.","Gravel pits","Gravel"]
["Greene","IND WASTE","Industrial waste","Industrial"]
["Greene","Ln","Linwood muck","Linwood",2,null,"NHEL"]
["Greene","MhA","Miamian silt loam, 0 to 2 percent slopes","Miamian",5,0.37,"NHEL"]
["Greene","MhB","Miamian silt loam, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Greene","MhB2","Miamian silt loam, 2 to 6 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Greene","MhC2","Miamian silt loam, 6 to 12 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Greene","MhD2","Miamian silt loam, 12 to 18 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Greene","MlB3","Miamian clay loam, 2 to 6 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Greene","MlC3","Miamian clay loam, 6 to 12 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Greene","MlD3","Miamian clay loam, 12 to 18 percent slopes, severely eroded","Miamian",4,0.37,"HEL"]
["Greene","M.L.","Made land","Made"]
["Greene","MmD2","Miamian-Casco complex, 12 to 18 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Greene","MmE2","Miamian-Casco complex, 18 to 35 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Greene","MoB2","Miamian-Eldean silt loams, 2 to 6 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Greene","MoC2","Miamian-Eldean silt loams, 6 to 12 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Greene","MpE","Miamian and Hennepin soils, 18 to 25 percent slopes","Miamian",5,0.37,"HEL"]
["Greene","MpF","Miamian and Hennepin soils, 25 to 50 percent slopes","Miamian",5,0.37,"HEL"]
["Greene","MrB","Miamian-Urban land complex, undulating","Miamian",5,0.37,"PHEL"]
["Greene","MrC","Miamian-Urban land complex, rolling","Miamian",5,0.37,"PHEL"]
["Greene","Ms","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Greene","MtA","Milton silt loam, 0 to 2 percent slopes","Milton",4,0.37,"NHEL"]
["Greene","MtB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Greene","MtC2","Milton silt loam, 6 to 12 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Greene","MUF","Milton soils, channery variant, 25 to 50 percent slopes","Milton",4,0.28000000000000003,"HEL"]
["Greene","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Greene","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Greene","OcB2","Ockley silt loam, 2 to 6 percent slopes, moderately eroded","Ockley",5,0.37,"PHEL"]
["Greene","OdB","Ockley-Urban land complex, undulating","Ockley",5,0.37,"PHEL"]
["Greene","OeB","Odell silt loam, 2 to 6 percent slopes","Odell",5,0.28000000000000003,"PHEL"]
["Greene","Pa","Patton silty clay loam","Patton",5,0.28000000000000003,"NHEL"]
["Greene","QU.","Quarry","Quarry"]
["Greene","Ra","Ragsdale silty clay loam","Ragsdale",5,0.28000000000000003,"NHEL"]
["Greene","RbA","Randolph silt loam, 0 to 2 percent slopes","Randolph",3,0.37,"NHEL"]
["Greene","RdA","Raub silt loam, 0 to 2 percent slopes","Raub",5,0.28000000000000003,"NHEL"]
["Greene","RdB","Raub silt loam, 2 to 6 percent slopes","Raub",5,0.28000000000000003,"PHEL"]
["Greene","ReA","Reesville silt loam, 0 to 2 percent slopes","Reesville",5,0.37,"NHEL"]
["Greene","RhB","Ritchey silt loam, 2 to 6 percent slopes","Ritchey",2,0.37,"PHEL"]
["Greene","RhC","Ritchey silt loam, 6 to 12 percent slopes","Ritchey",2,0.37,"HEL"]
["Greene","RhD","Ritchey silt loam, 12 to 18 percent slopes","Ritchey",2,0.37,"HEL"]
["Greene","RhE2","Ritchey silt loam, 18 to 25 percent slopes, moderately eroded","Ritchey",2,0.37,"HEL"]
["Greene","Rs","Ross loam","Ross",5,0.32,"NHEL"]
["Greene","RtA","Rush silt loam, 0 to 2 percent slopes","Rush",5,0.37,"NHEL"]
["Greene","RtB","Rush silt loam, 2 to 6 percent slopes","Rush",5,0.37,"PHEL"]
["Greene","RuA","Russell silt loam, 0 to 2 percent slopes","Russell",5,0.37,"NHEL"]
["Greene","RvB","Russell-Miamian silt loams, 2 to 6 percent slopes","Russell",5,0.37,"PHEL"]
["Greene","RvB2","Russell-Miamian silt loams, 2 to 6 percent slopes, moderately eroded","Russell",5,0.37,"PHEL"]
["Greene","SlA","Sleeth silt loam, 0 to 2 percent slopes","Sleeth",5,0.32,"NHEL"]
["Greene","So","Sloan silty clay loam","sloan",5,0.37,"NHEL"]
["Greene","Sp","Sloan-Fill land complex","sloan",5,0.37,"NHEL"]
["Greene","Sr","Sloan-Urban land complex","sloan",5,0.37,"NHEL"]
["Greene","ThA","Thackery silt loam, 0 to 2 percent slopes","Thackery",4,0.37,"NHEL"]
["Greene","ThB","Thackery silt loam, 2 to 6 percent slopes","Thackery",4,0.37,"PHEL"]
["Greene","Ur","Urban land","Urban"]
["Greene","W","Water","Water"]
["Greene","WaA","Warsaw loam, 0 to 2 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
["Greene","WbA","Warsaw-Fill land complex, nearly level","Warsaw",4,0.28000000000000003,"NHEL"]
["Greene","WcA","Warsaw-Urban land complex, nearly level","Warsaw",4,0.28000000000000003,"NHEL"]
["Greene","WeB","Wea silt loam, 1 to 3 percent slopes","Wea",5,0.32,"NHEL"]
["Greene","Ws","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
["Greene","Wt","Westland-Urban land complex","Westland",5,0.28000000000000003,"NHEL"]
["Greene","XeA","Xenia silt loam, 0 to 2 percent slopes","Xenia",5,0.37,"NHEL"]
["Greene","XeB","Xenia silt loam, 2 to 6 percent slopes","Xenia",5,0.37,"PHEL"]
[null,"Select","none","none"]
["Hamilton","ArA","Ava silt loam, 0 to 3 percent slopes","Ava",4,0.43,"PHEL"]
["Hamilton","ArB2","Ava silt loam, 3 to 8 percent slopes, eroded","Ava",4,0.43,"PHEL"]
["Hamilton","ArC2","Ava silt loam, 8 to 15 percent slopes, eroded","Ava",4,0.43,"HEL"]
["Hamilton","AsB","Ava-Urban land complex, 3 to 8 percent slopes","Ava",4,0.43,"PHEL"]
["Hamilton","AsC","Ava-Urban land complex, 8 to 15 percent slopes","Ava",4,0.43,"HEL"]
["Hamilton","AvA","Avonburg silt loam, 0 to 2 percent slopes","Avonburg",4,0.43,"NHEL"]
["Hamilton","AwA","Avonburg-Urban land complex, 0 to 2 percent slopes","Avonburg",4,0.43,"NHEL"]
["Hamilton","BoD","Bonnell silt loam, 15 to 25 percent slopes","Bonnell",3,0.43,"HEL"]
["Hamilton","BoE","Bonnell silt loam, 25 to 35 percent slopes","Bonnell",3,0.43,"HEL"]
["Hamilton","BoF","Bonnell silt loam, 35 to 60 percent slopes","Bonnell",3,0.43,"HEL"]
["Hamilton","CcC2","Casco gravelly loam, 8 to 15 percent slopes, eroded","Casco",3,0.24,"PHEL"]
["Hamilton","CdD","Casco loam, 15 to 25 percent slopes","Casco",3,0.24,"HEL"]
["Hamilton","CdE","Casco loam, 25 to 35 percent slopes","Casco",3,0.24,"HEL"]
["Hamilton","CdF","Casco loam, 35 to 70 percent slopes","Casco",3,0.24,"HEL"]
["Hamilton","CnB2","Cincinnati silt loam, 3 to 8 percent slopes, eroded","Cincinnati",4,0.37,"PHEL"]
["Hamilton","CnC2","Cincinnati silt loam, 8 to 15 percent slopes, eroded","Cincinnati",4,0.37,"HEL"]
["Hamilton","DaB","Dana silt loam, 0 to 4 percent slopes","Dana",5,0.32,"NHEL"]
["Hamilton","EcB2","Eden silty clay loam, 3 to 8 percent slopes, eroded","Eden",3,0.43,"PHEL"]
["Hamilton","EcC2","Eden silty clay loam, 8 to 15 percent slopes, eroded","Eden",3,0.43,"HEL"]
["Hamilton","EcD","Eden silty clay loam, 15 to 25 percent slopes","Eden",3,0.43,"HEL"]
["Hamilton","EcE","Eden silty clay loam, 25 to 40 percent slopes","Eden",3,0.43,"HEL"]
["Hamilton","EdF","Eden flaggy silty clay loam, 40 to 60 percent slopes","Eden",3,0.43,"HEL"]
["Hamilton","EeB","Eden-Urban land complex, 3 to 8 percent slopes","Eden",3,0.43,"PHEL"]
["Hamilton","EeC","Eden-Urban land complex, 8 to 15 percent slopes","Eden",3,0.43,"HEL"]
["Hamilton","EeD","Eden-Urban land complex, 15 to 25 percent slopes","Eden",3,0.43,"HEL"]
["Hamilton","EpA","Eldean loam, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Hamilton","EpB2","Eldean loam, 2 to 6 percent slopes, eroded","Eldean",4,0.37,"PHEL"]
["Hamilton","EpC2","Eldean loam, 6 to 12 percent slopes, eroded","Eldean",4,0.37,"PHEL"]
["Hamilton","ErA","Eldean-Urban land complex, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Hamilton","ErB","Eldean-Urban land complex, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Hamilton","FdA","Fincastle silt loam, 0 to 2 percent slopes","Fincastle",5,0.37,"NHEL"]
["Hamilton","FeA","Fincastle-Urban land complex, 0 to 2 percent slopes","Fincastle",5,0.37,"NHEL"]
["Hamilton","FoA","Fox loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Hamilton","FoB2","Fox loam, 2 to 6 percent slopes, eroded","Fox",4,0.37,"PHEL"]
["Hamilton","FpA","Fox-Urban land complex, 0 to 3 percent slopes","Fox",4,0.37,"NHEL"]
["Hamilton","Gn","Genesee loam, occasionally flooded","Genesee",5,0.37,"NHEL"]
["Hamilton","Go","Genesee-Urban land complex, occasionally flooded","Genesee",5,0.37,"NHEL"]
["Hamilton","HeF","Hennepin silt loam, 35 to 60 percent slopes","Hennepin",4,0.32,"HEL"]
["Hamilton","HoA","Henshaw silt loam, 0 to 2 percent slopes","Henshaw",4,0.43,"NHEL"]
["Hamilton","Hu","Huntington silt loam, occasionally flooded","Huntington",5,0.28000000000000003,"NHEL"]
["Hamilton","Ju","Jules silt loam, occasionally flooded","Jules",5,0.37,"NHEL"]
["Hamilton","Lg","Lanier sandy loam, occasionally flooded","Lanier",5,0.2,"NHEL"]
["Hamilton","MaB","Markland silty clay loam, 2 to 6 percent slopes","Markland",3,0.43,"PHEL"]
["Hamilton","MaC2","Markland silty clay loam, 6 to 12 percent slopes, eroded","Markland",3,0.43,"HEL"]
["Hamilton","MaD2","Markland silty clay loam, 12 to 18 percent slopes, eroded","Markland",3,0.43,"HEL"]
["Hamilton","MaE2","Markland silty clay loam, 18 to 25 percent slopes, eroded","Markland",3,0.43,"HEL"]
["Hamilton","McA","Martinsville silt loam, 0 to 2 percent slopes","Martinsville",5,0.37,"NHEL"]
["Hamilton","McB","Martinsville silt loam, 2 to 6 percent slopes","Martinsville",5,0.37,"PHEL"]
["Hamilton","MnC2","Miamian silt loam, 8 to 15 percent slopes, eroded","Miamian",5,0.37,"PHEL"]
["Hamilton","MoD2","Miamian-Hennepin silt loams, 15 to 25 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Hamilton","MoE2","Miamian-Hennepin silt loams, 25 to 35 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Hamilton","MuC","Miamian-Urban land complex, 8 to 15 percent slopes","Miamian",5,0.37,"PHEL"]
["Hamilton","PbB2","Parke silt loam, 3 to 8 percent slopes, eroded","Parke",5,0.37,"PHEL"]
["Hamilton","PbC2","Parke silt loam, 8 to 15 percent slopes, eroded","Parke",5,0.37,"PHEL"]
["Hamilton","PbD","Parke silt loam, 15 to 25 percent slopes","Parke",5,0.37,"HEL"]
["Hamilton","PbE","Parke silt loam, 25 to 35 percent slopes","Parke",5,0.37,"HEL"]
["Hamilton","PcB","Parke-Urban land complex, 3 to 8 percent slopes","Parke",5,0.37,"PHEL"]
["Hamilton","PcC","Parke-Urban land complex, 8 to 15 percent slopes","Parke",5,0.37,"PHEL"]
["Hamilton","PfC","Pate silty clay loam, 8 to 15 percent slopes","Pate",3,0.37,"HEL"]
["Hamilton","PfD","Pate silty clay loam, 15 to 25 percent slopes","Pate",3,0.37,"HEL"]
["Hamilton","PfE","Pate silty clay loam, 25 to 35 percent slopes","Pate",3,0.37,"HEL"]
["Hamilton","PhD","Pate-Urban land complex, 15 to 25 percent slopes","Pate",3,0.37,"HEL"]
["Hamilton","Pn","Patton silty clay loam","Patton",5,0.28000000000000003,"NHEL"]
["Hamilton","Po","Pits, gravel","Pits"]
["Hamilton","PrA","Princeton sandy loam, 0 to 2 percent slopes","Princeton",5,0.24,"NHEL"]
["Hamilton","PrB","Princeton sandy loam, 2 to 6 percent slopes","Princeton",5,0.24,"PHEL"]
["Hamilton","PrC2","Princeton sandy loam, 6 to 12 percent slopes, eroded","Princeton",5,0.24,"PHEL"]
["Hamilton","RdA","Raub silt loam, 0 to 2 percent slopes","Raub",5,0.28000000000000003,"NHEL"]
["Hamilton","Rn","Ross loam, rarely flooded","Ross",5,0.32,"NHEL"]
["Hamilton","RpA","Rossmoyne silt loam, 0 to 3 percent slopes","Rossmoyne",4,0.37,"NHEL"]
["Hamilton","RpB2","Rossmoyne silt loam, 3 to 8 percent slopes, eroded","Rossmoyne",4,0.37,"PHEL"]
["Hamilton","RpC2","Rossmoyne silt loam, 8 to 15 percent slopes, eroded","Rossmoyne",4,0.37,"HEL"]
["Hamilton","RtA","Rossmoyne-Urban land complex, 0 to 3 percent slopes","Rossmoyne",4,0.37,"NHEL"]
["Hamilton","RtB","Rossmoyne-Urban land complex, 3 to 8 percent slopes","Rossmoyne",4,0.37,"PHEL"]
["Hamilton","RtC","Rossmoyne-Urban land complex, 8 to 15 percent slopes","Rossmoyne",4,0.37,"HEL"]
["Hamilton","RwB2","Russell silt loam, 3 to 8 percent slopes, eroded","Russell",5,0.37,"PHEL"]
["Hamilton","RxB","Russell-Urban land complex, 3 to 8 percent slopes","Russell",5,0.37,"PHEL"]
["Hamilton","St","Stonelick fine sandy loam, frequently flooded","Stonelick",5,0.24,"NHEL"]
["Hamilton","SwB2","Switzerland silt loam, 3 to 8 percent slopes, eroded","Switzerland",4,0.43,"PHEL"]
["Hamilton","SwC2","Switzerland silt loam, 8 to 15 percent slopes, eroded","Switzerland",4,0.43,"HEL"]
["Hamilton","SwD2","Switzerland silt loam, 15 to 25 percent slopes, eroded","Switzerland",4,0.43,"HEL"]
["Hamilton","SxB","Switzerland-Urban land complex, 3 to 8 percent slopes","Switzerland",4,0.43,"PHEL"]
["Hamilton","SxC","Switzerland-Urban land complex, 8 to 15 percent slopes","Switzerland",4,0.43,"HEL"]
["Hamilton","Ud","Udorthents, clayey","Udorthents"]
["Hamilton","Uf","Udorthents, loamy","Udorthents"]
["Hamilton","UgB","Urban land-Elkinsville complex, 3 to 8 percent slopes","Urban"]
["Hamilton","UgC","Urban land-Elkinsville complex, 8 to 15 percent slopes","Urban"]
["Hamilton","Uh","Urban land-Huntington complex, frequently flooded","Urban"]
["Hamilton","UmB","Urban land-Martinsville complex, 3 to 8 percent slopes","Urban"]
["Hamilton","UmC","Urban land-Martinsville complex, 8 to 15 percent slopes","Urban"]
["Hamilton","Uo","Urban land-Patton complex","Urban"]
["Hamilton","UrB","Urban land-Rossmoyne complex, 0 to 8 percent slopes","Urban"]
["Hamilton","Ux","Urban land-Stonelick complex, frequently flooded","Urban"]
["Hamilton","W","Water","Water"]
["Hamilton","Wa","Wakeland silt loam, occasionally flooded","Wakeland",5,0.37,"NHEL"]
["Hamilton","WbA","Warsaw variant sandy loam, 0 to 2 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
["Hamilton","WeA","Wea silt loam, 0 to 2 percent slopes","Wea",5,0.32,"NHEL"]
["Hamilton","WhA","Whitaker loam, 0 to 2 percent slopes","Whitaker",5,0.37,"NHEL"]
["Hamilton","XfA","Xenia silt loam, 0 to 2 percent slopes","Xenia",5,0.37,"NHEL"]
["Hamilton","XfB2","Xenia silt loam, 2 to 6 percent slopes, eroded","Xenia",5,0.37,"PHEL"]
[null,"Select","none","none"]
["Logan","Ag","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Logan","BeE","Berks silt loam, 18 to 25 percent slopes","Berks",3,0.24,"HEL"]
["Logan","BeF","Berks silt loam, 25 to 50 percent slopes","Berks",3,0.24,"HEL"]
["Logan","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Logan","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Logan","Bs","Brookston silty clay loam","Brookston",5,0.28000000000000003,"NHEL"]
["Logan","Ca","Carlisle muck","Carlisle",2,null,"NHEL"]
["Logan","Cc","Carlisle muck, ponded","Carlisle",2,null,"NHEL"]
["Logan","CdD2","Casco-Eldean complex, 12 to 18 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Logan","CeA","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Logan","CeB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Logan","CrA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Logan","CrB","Crosby silt loam, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Logan","CsA","Crosby-Urban land complex, nearly level","Crosby",3,0.43,"NHEL"]
["Logan","DeA","Del Rey silt loam, 0 to 2 percent slopes","Del Rey",3,0.43,"NHEL"]
["Logan","DeB","Del Rey silt loam, 2 to 6 percent slopes","Del Rey",3,0.43,"PHEL"]
["Logan","Ed","Edwards muck","Edwards",2,null,"NHEL"]
["Logan","Ee","Eel silt loam","Eel",5,0.37,"NHEL"]
["Logan","EmA","Eldean silt loam, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Logan","EmB","Eldean silt loam, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Logan","EmC2","Eldean silt loam, 6 to 12 percent slopes, moderately eroded","Eldean",4,0.37,"PHEL"]
["Logan","EpB","Eldean-Urban land complex, undulating","Eldean",4,0.37,"PHEL"]
["Logan","FlA","Fox loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Logan","FlB","Fox loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Logan","FuA","Fulton silt loam, 0 to 4 percent slopes","Fulton",3,0.43,"PHEL"]
["Logan","GaB","Gallman loam, 1 to 4 percent slopes","Gallman",5,0.32,"NHEL"]
["Logan","Gn","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Logan","GwB","Glynwood silt loam, 2 to 6 percent slopes","Glynwood",3,0.43,"PHEL"]
["Logan","HdA","Haskins loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Logan","HdB","Haskins loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Logan","HeA","Henshaw silt loam, 0 to 2 percent slopes","Henshaw",4,0.43,"NHEL"]
["Logan","HeB","Henshaw silt loam, 2 to 6 percent slopes","Henshaw",4,0.43,"PHEL"]
["Logan","HoA","Homer silt loam, 0 to 2 percent slopes","Homer",4,0.37,"NHEL"]
["Logan","HoB","Homer silt loam, 2 to 6 percent slopes","Homer",4,0.37,"PHEL"]
["Logan","La","Latty silty clay","Latty",5,0.28000000000000003,"NHEL"]
["Logan","Lb","Latty silty clay, occasionally flooded","Latty",5,0.28000000000000003,"NHEL"]
["Logan","Ln","Linwood muck","Linwood",2,null,"NHEL"]
["Logan","Lp","Lippincott silty clay loam","Lippincott",5,0.28000000000000003,"NHEL"]
["Logan","Ls","Lippincott-Urban land complex","Lippincott",5,0.28000000000000003,"NHEL"]
["Logan","Ma","Martisco mucky silt loam","Martisco",3,0.24,"NHEL"]
["Logan","Mc","Martisco Variant silt loam","Martisco",2,0.37,"NHEL"]
["Logan","MhB","Miamian silt loam, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Logan","MhC2","Miamian silt loam, 6 to 12 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Logan","MhD2","Miamian silt loam, 12 to 18 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Logan","MhE2","Miamian silt loam, 18 to 25 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Logan","MhF","Miamian silt loam, 25 to 50 percent slopes","Miamian",5,0.37,"HEL"]
["Logan","MlB","Miamian-Urban land complex, undulating","Miamian",5,0.37,"PHEL"]
["Logan","MlC","Miamian-Urban land complex, rolling","Miamian",5,0.37,"PHEL"]
["Logan","MmC2","Miamian Variant silt loam, 6 to 15 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Logan","MoB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Logan","MoC2","Milton silt loam, 6 to 12 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Logan","MoD2","Milton silt loam, 12 to 18 percent slopes, moderately eroded","Milton",4,0.37,"HEL"]
["Logan","Mt","Montgomery silty clay loam","Montgomery",5,0.37,"NHEL"]
["Logan","MyC2","Morley silt loam, 6 to 12 percent slopes, moderately eroded","Morley",3,0.43,"PHEL"]
["Logan","MyD2","Morley silt loam, 12 to 18 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Logan","Mz","Muskego muck","Muskego",2,null,"NHEL"]
["Logan","NaA","Nappanee silt loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Logan","NaB","Nappanee silt loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Logan","NnA","Nineveh silt loam, 0 to 2 percent slopes","Nineveh",4,0.28000000000000003,"NHEL"]
["Logan","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Logan","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Logan","PaB","Parr silt loam, 1 to 4 percent slopes","Parr",5,0.32,"NHEL"]
["Logan","Pb","Patton silt loam","Patton",5,0.28000000000000003,"NHEL"]
["Logan","Pc","Patton Variant silt loam","Patton",4,0.24,"NHEL"]
["Logan","Pd","Paulding clay","Paulding",5,0.28000000000000003,"NHEL"]
["Logan","Pe","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Logan","Pg","Pits, gravel","Pits"]
["Logan","Pk","Pits, quarries","Pits"]
["Logan","RoE","Rodman-Casco complex, 18 to 25 percent slopes","Rodman",3,0.2,"HEL"]
["Logan","RoF","Rodman-Casco complex, 25 to 50 percent slopes","Rodman",3,0.2,"HEL"]
["Logan","ScB","St. Clair silt loam, 2 to 6 percent slopes","St. Clair",3,0.37,"PHEL"]
["Logan","ScC2","St. Clair silt loam, 6 to 12 percent slopes, moderately eroded","St. Clair",3,0.37,"PHEL"]
["Logan","ScD2","St. Clair silt loam, 12 to 18 percent slopes, moderately eroded","St. Clair",3,0.37,"HEL"]
["Logan","ScE2","St. Clair silt loam, 18 to 35 percent slopes, moderately eroded","St. Clair",3,0.37,"HEL"]
["Logan","SgB","Shinrock silt loam, 2 to 6 percent slopes","Shinrock",3,0.37,"PHEL"]
["Logan","SgC","Shinrock silt loam, 6 to 12 percent slopes","Shinrock",3,0.37,"PHEL"]
["Logan","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Logan","SlA","Sleeth silt loam, 0 to 2 percent slopes","Sleeth",5,0.32,"NHEL"]
["Logan","So","Sloan silt loam","sloan",5,0.37,"NHEL"]
["Logan","Ud","Udorthents","Udorthents"]
["Logan","W","Water","Water"]
["Logan","Wa","Wallkill silt loam","Wallkill",5,0.32,"NHEL"]
["Logan","WeA","Wea Variant silt loam, 0 to 2 percent slopes","Wea",5,0.32,"NHEL"]
["Logan","WkF","Weikert shaly silt loam, 35 to 70 percent slopes","Weikert",2,0.28000000000000003,"HEL"]
["Logan","Wt","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
["Logan","Wu","Westland silty clay loam, clay substratum","Westland",5,0.28000000000000003,"NHEL"]
["Logan","Wv","Wetzel silty clay loam","Wetzel",5,0.37,"NHEL"]
["Logan","Wx","Willette muck","Willette",2,null,"NHEL"]
[null,"Select","none","none"]
["Madison","Ca","Carlisle muck","Carlisle",2,null,"NHEL"]
["Madison","CrA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Madison","CrB","Crosby silt loam, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Madison","CsA","Crosby-Lewisburg silt loams, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Madison","ElA","Eldean silt loam, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Madison","ElB","Eldean silt loam, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Madison","ElC2","Eldean silt loam, 6 to 12 percent slopes, eroded","Eldean",4,0.37,"PHEL"]
["Madison","KeB","Kendallville silt loam, 2 to 6 percent slopes","Kendallville",3,0.37,"PHEL"]
["Madison","KeC2","Kendallville silt loam, 6 to 12 percent slopes, eroded","Kendallville",3,0.37,"PHEL"]
["Madison","Ko","Kokomo silty clay loam","Kokomo",3,0.32,"NHEL"]
["Madison","LeB","Lewisburg-Celina silt loams, 2 to 6 percent slopes","Lewisburg",3,0.43,"PHEL"]
["Madison","Mk","Medway silt loam, occasionally flooded","Medway",5,0.32,"NHEL"]
["Madison","MlB","Miamian silt loam, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Madison","MlC2","Miamian silt loam, 6 to 12 percent slopes, eroded","Miamian",5,0.37,"PHEL"]
["Madison","MlD2","Miamian silt loam, 12 to 18 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Madison","MlE2","Miamian silt loam, 18 to 25 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Madison","MlF","Miamian silt loam, 25 to 50 percent slopes","Miamian",5,0.37,"HEL"]
["Madison","MnB","Miamian-Eldean silt loams, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Madison","MnC2","Miamian-Eldean silt loams, 6 to 12 percent slopes, eroded","Miamian",5,0.37,"PHEL"]
["Madison","OdA","Odell-Lewisburg complex, 0 to 2 percent slopes","Odell",5,0.28000000000000003,"NHEL"]
["Madison","OdB","Odell-Lewisburg complex, 2 to 6 percent slopes","Odell",5,0.28000000000000003,"PHEL"]
["Madison","Pa","Patton silty clay loam","Patton",5,0.28000000000000003,"NHEL"]
["Madison","Pg","Pits, gravel","Pits"]
["Madison","Rs","Ross silt loam, occasionally flooded","Ross",5,0.32,"NHEL"]
["Madison","So","Sloan silty clay loam, frequently flooded","sloan",5,0.37,"NHEL"]
["Madison","ThA","Thackery variant silt loam, 0 to 2 percent slopes","Thackery",5,0.37,"NHEL"]
["Madison","ThB","Thackery variant silt loam, 2 to 6 percent slopes","Thackery",5,0.37,"PHEL"]
["Madison","W","Water","Water"]
["Madison","WeA","Wea silt loam, 0 to 3 percent slopes","Wea",5,0.32,"NHEL"]
["Madison","Wt","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
["Madison","Wv","Westland silty clay loam, silty substratum","Westland",5,0.28000000000000003,"NHEL"]
[null,"Select","none","none"]
["Mercer","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Mercer","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Mercer","Ca","Carlisle muck","Carlisle",2,null,"NHEL"]
["Mercer","Df","Defiance silty clay","Defiance",5,0.37,"NHEL"]
["Mercer","DmA","Digby loam, 0 to 2 percent slopes","Digby",4,0.32,"NHEL"]
["Mercer","DmB","Digby loam, 2 to 6 percent slopes","Digby",4,0.32,"PHEL"]
["Mercer","Ed","Edwards muck","Edwards",2,null,"NHEL"]
["Mercer","Ee","Eel silt loam","Eel",5,0.37,"NHEL"]
["Mercer","ElB","Eldean loam, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Mercer","ElC2","Eldean loam, 6 to 12 percent slopes, moderately eroded","Eldean",4,0.37,"PHEL"]
["Mercer","EoB","Elliott silt loam, 1 to 4 percent slopes","Elliott",4,0.28000000000000003,"NHEL"]
["Mercer","GaB","Gallman sandy loam, 2 to 6 percent slopes","Gallman",5,0.32,"PHEL"]
["Mercer","GbB","Gallman loam, 2 to 6 percent slopes","Gallman",5,0.32,"NHEL"]
["Mercer","Gn","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Mercer","GwB","Glynwood silt loam, 2 to 6 percent slopes","Glynwood",3,0.43,"PHEL"]
["Mercer","GwB2","Glynwood silt loam, 2 to 6 percent slopes, moderately eroded","Glynwood",3,0.43,"PHEL"]
["Mercer","GwC2","Glynwood silt loam, 6 to 12 percent slopes, moderately eroded","Glynwood",3,0.43,"PHEL"]
["Mercer","HnA","Haskins loam, 0 to 2 percent slopes","Haskins",4,0.37,"NHEL"]
["Mercer","HnB","Haskins loam, 2 to 6 percent slopes","Haskins",4,0.37,"PHEL"]
["Mercer","McA","McGary silty clay loam, 0 to 2 percent slopes","McGary",3,0.43,"NHEL"]
["Mercer","McB","McGary silty clay loam, 2 to 6 percent slopes","McGary",3,0.43,"PHEL"]
["Mercer","Mg","Millgrove silty clay loam","Millgrove",5,0.28000000000000003,"NHEL"]
["Mercer","Mh","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Mercer","Mn","Montgomery silty clay","Montgomery",5,0.37,"NHEL"]
["Mercer","MrD2","Morley silt loam, 12 to 18 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Mercer","MrE2","Morley silt loam, 18 to 25 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Mercer","MsD3","Morley clay loam, 9 to 18 percent slopes, severely eroded","Morley",2,0.43,"HEL"]
["Mercer","OcA","Ockley loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Mercer","OcB","Ockley loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Mercer","On","Olentangy mucky silt loam","Olentangy",5,0.28000000000000003,"NHEL"]
["Mercer","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Mercer","Pn","Pewamo silty clay loam, ponded","Pewamo",5,0.24,"NHEL"]
["Mercer","Po","Pewamo silty clay","Pewamo",5,0.24,"NHEL"]
["Mercer","Ps","Pits, gravel","Pits"]
["Mercer","Qu","Quarries","Qaurries"]
["Mercer","RmB","Rawson loam, 2 to 6 percent slopes","Rawson",4,0.32,"PHEL"]
["Mercer","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Mercer","So","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Mercer","Ud","Udorthents, loamy","Udorthents"]
["Mercer","W","Water","Water"]
["Mercer","Wh","Wabasha silty clay","Wabasha",5,0.32,"NHEL"]
[null,"Select","none","none"]
["Miami","Ag","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Miami","BlA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Miami","BlB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Miami","BlB2","Blount silt loam, 2 to 6 percent slopes, moderately eroded","Blount",3,0.43,"PHEL"]
["Miami","Bs","Brookston silty clay loam","Brookston",5,0.28000000000000003,"NHEL"]
["Miami","CeA","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Miami","CeB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Miami","CeB2","Celina silt loam, 2 to 6 percent slopes, moderately eroded","Celina",5,0.37,"PHEL"]
["Miami","CoA","Corwin silt loam, 0 to 2 percent slopes","Corwin",5,0.28000000000000003,"NHEL"]
["Miami","CoB","Corwin silt loam, 2 to 6 percent slopes","Corwin",5,0.28000000000000003,"PHEL"]
["Miami","CrA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Miami","CrB","Crosby silt loam, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Miami","Ed","Edwards muck","Edwards",2,null,"NHEL"]
["Miami","Ee","Eel silt loam","Eel",5,0.37,"NHEL"]
["Miami","ElA","Eldean loam, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Miami","ElB","Eldean loam, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Miami","ElB2","Eldean loam, 2 to 6 percent slopes, moderately eroded","Eldean",4,0.37,"PHEL"]
["Miami","EmA","Eldean silt loam, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Miami","EmB","Eldean silt loam, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Miami","EoC2","Eldean-Casco gravelly loams, 6 to 12 percent slopes, moderately eroded","Eldean",4,0.37,"PHEL"]
["Miami","EoD2","Eldean-Casco gravelly loams, 12 to 18 percent slopes, moderately eroded","Eldean",4,0.37,"HEL"]
["Miami","EpD3","Eldean-Casco complex, 6 to 18 percent slopes, severely eroded","Eldean",3,0.37,"PHEL"]
["Miami","ErB","Eldean-Miamian complex, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Miami","ErC","Eldean-Miamian complex, 6 to 12 percent slopes","Eldean",4,0.37,"PHEL"]
["Miami","Gn","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Miami","GwB","Glynwood silt loam, 2 to 6 percent slopes","Glynwood",3,0.43,"PHEL"]
["Miami","GwB2","Glynwood silt loam, 2 to 6 percent slopes, moderately eroded","Glynwood",3,0.43,"PHEL"]
["Miami","GwC2","Glynwood silt loam, 6 to 12 percent slopes, moderately eroded","Glynwood",3,0.43,"PHEL"]
["Miami","GwD2","Glynwood silt loam, 12 to 18 percent slopes, moderately eroded","Glynwood",3,0.43,"HEL"]
["Miami","GyC3","Glynwood clay loam, 6 to 12 percent slopes, severely eroded","Glynwood",2,0.43,"HEL"]
["Miami","GyD3","Glynwood clay loam, 12 to 18 percent slopes, severely eroded","Glynwood",2,0.43,"HEL"]
["Miami","Ln","Linwood muck","Linwood",2,null,"NHEL"]
["Miami","LrE2","Lorenzo-Rodman gravelly loams, 18 to 50 percent slopes, moderately eroded","Lorenzo",3,0.28000000000000003,"HEL"]
["Miami","MaB","Martinsville and Ockley loams, till substratum, 2 to 6 percent slopes","Martinsville",5,0.37,"PHEL"]
["Miami","Md","Medway silt loam","Medway",5,0.32,"NHEL"]
["Miami","MhA","Miamian silt loam, 0 to 2 percent slopes","Miamian",5,0.37,"NHEL"]
["Miami","MhB","Miamian silt loam, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Miami","MhB2","Miamian silt loam, 2 to 6 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Miami","MhC2","Miamian silt loam, 6 to 12 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Miami","MhD2","Miamian silt loam, 12 to 18 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Miami","MkA","Miamian silt loam, limestone substratum, 0 to 2 percent slopes","Miamian",5,0.37,"NHEL"]
["Miami","MkB","Miamian silt loam, limestone substratum, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Miami","MkB2","Miamian silt loam, limestone substratum, 2 to 6 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Miami","MkC2","Miamian silt loam, limestone substratum, 6 to 12 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Miami","MlC3","Miamian clay loam, 6 to 12 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Miami","MlD3","Miamian clay loam, 12 to 18 percent slopes, severely eroded","Miamian",4,0.37,"HEL"]
["Miami","MmE","Miamian and Hennepin silt loams, 18 to 25 percent slopes","Miamian",5,0.37,"HEL"]
["Miami","MmF","Miamian and Hennepin silt loams, 25 to 50 percent slopes","Miamian",5,0.37,"HEL"]
["Miami","MnA","Millsdale silt loam, 0 to 2 percent slopes","Millsdale",4,0.32,"NHEL"]
["Miami","MnB","Millsdale silt loam, 2 to 6 percent slopes","Millsdale",4,0.32,"PHEL"]
["Miami","MoA","Millsdale silty clay loam, 0 to 2 percent slopes","Millsdale",4,0.32,"NHEL"]
["Miami","MoB","Millsdale silty clay loam, 2 to 6 percent slopes","Millsdale",4,0.32,"PHEL"]
["Miami","MpA","Milton silt loam, 0 to 2 percent slopes","Milton",4,0.37,"NHEL"]
["Miami","MpB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Miami","MpB2","Milton silt loam, 2 to 6 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Miami","MpC2","Milton silt loam, 6 to 12 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Miami","MpD2","Milton silt loam, 12 to 18 percent slopes, moderately eroded","Milton",4,0.37,"HEL"]
["Miami","Mt","Montgomery silty clay loam","Montgomery",5,0.37,"NHEL"]
["Miami","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Miami","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Miami","OdA","Odell silt loam, 0 to 2 percent slopes","Odell",5,0.28000000000000003,"NHEL"]
["Miami","OdB","Odell silt loam, 2 to 6 percent slopes","Odell",5,0.28000000000000003,"PHEL"]
["Miami","Pe","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Miami","RdA","Randolph silt loam, 0 to 2 percent slopes","Randolph",3,0.37,"NHEL"]
["Miami","RdB","Randolph silt loam, 2 to 6 percent slopes","Randolph",3,0.37,"PHEL"]
["Miami","RhB","Ritchey silt loam, 2 to 6 percent slopes","Ritchey",2,0.37,"PHEL"]
["Miami","RhC","Ritchey silt loam, 6 to 18 percent slopes","Ritchey",2,0.37,"HEL"]
["Miami","RhE","Ritchey silt loam, 18 to 50 percent slopes","Ritchey",2,0.37,"HEL"]
["Miami","Rs","Ross silt loam","Ross",5,0.32,"NHEL"]
["Miami","Rt","Ross silt loam, shallow variant","ross",2,0.28000000000000003,"NHEL"]
["Miami","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Miami","Sk","Shoals silt loam, moderately shallow variant","Shoals",4,0.37,"NHEL"]
["Miami","SlA","Sleeth silt loam, 0 to 2 percent slopes","Sleeth",5,0.32,"NHEL"]
["Miami","St","Stonelick loam","Stonelick",5,0.24,"NHEL"]
["Miami","W","Water","Water"]
["Miami","Wa","Wallkill silt loam","Wallkill",5,0.32,"NHEL"]
["Miami","WdA","Warsaw silt loam, 0 to 2 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
["Miami","WeA","Wea silt loam, 0 to 2 percent slopes","Wea",5,0.32,"NHEL"]
["Miami","Wt","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
[null,"Select","none","none"]
["Montgomery","Ag","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Montgomery","Bo","Borrow pits","Borrow"]
["Montgomery","Bp","Brookston silt loam","Brookston",5,0.28000000000000003,"NHEL"]
["Montgomery","Br","Brookston silt loam, overwash","Brookston",5,0.28000000000000003,"NHEL"]
["Montgomery","Bs","Brookston silty clay loam","Brookston",5,0.28000000000000003,"NHEL"]
["Montgomery","Bu","Brookston-Urban land complex","Brookston",5,0.28000000000000003,"NHEL"]
["Montgomery","Ca","Carlisle muck","Carlisle",2,null,"NHEL"]
["Montgomery","CeA","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Montgomery","CeB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Montgomery","CeB2","Celina silt loam, 2 to 6 percent slopes, moderately eroded","Celina",5,0.37,"PHEL"]
["Montgomery","ClB","Celina bouldery silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Montgomery","CoA","Corwin silt loam, 0 to 2 percent slopes","Corwin",5,0.28000000000000003,"NHEL"]
["Montgomery","CoB","Corwin silt loam, 2 to 6 percent slopes","Corwin",5,0.28000000000000003,"PHEL"]
["Montgomery","CsA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Montgomery","CtB","Crosby-Celina silt loams, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Montgomery","Cu","Crosby-Urban land complex","Crosby",3,0.43,"PHEL"]
["Montgomery","DaB","Dana silt loam, 2 to 6 percent slopes","Dana",5,0.32,"PHEL"]
["Montgomery","FaE2","Fairmount silty clay loam, 12 to 25 percent slopes, moderately eroded","Fairmount",2,0.37,"HEL"]
["Montgomery","FaF2","Fairmount silty clay loam, 25 to 50 percent slopes, moderately eroded","Fairmount",2,0.37,"HEL"]
["Montgomery","FcA","Fincastle silt loam, 0 to 4 percent slopes","Fincastle",5,0.37,"NHEL"]
["Montgomery","FkA","Fox sandy loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Montgomery","FkB","Fox sandy loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Montgomery","FlA","Fox loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Montgomery","FlB","Fox loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Montgomery","FlC2","Fox loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Montgomery","FmA","Fox silt loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Montgomery","FmB","Fox silt loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Montgomery","FmC2","Fox silt loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Montgomery","FmD2","Fox silt loam, 12 to 18 percent slopes, moderately eroded","Fox",4,0.37,"HEL"]
["Montgomery","FsC3","Fox soils, 6 to 12 percent slopes, severely eroded","Fox",3,0.37,"PHEL"]
["Montgomery","FuB","Fox-Urban land complex, gently sloping","Fox",4,0.37,"PHEL"]
["Montgomery","FuC","Fox-Urban land complex, rolling","Fox",4,0.37,"PHEL"]
["Montgomery","FuF","Fox-Urban land complex, steep","Fox",4,0.37,"HEL"]
["Montgomery","Gp","Gravel pits","Gravel"]
["Montgomery","HeE2","Hennepin and Miamian silt loams, 18 to 25 percent slopes, moderately eroded","Hennepin",4,0.32,"HEL"]
["Montgomery","HeF2","Hennepin and Miamian silt loams, 25 to 50 percent slopes, moderately eroded","Hennepin",4,0.32,"HEL"]
["Montgomery","HmF3","Hennepin and Miamian soils, 18 to 50 percent slopes, severely eroded","Hennepin",4,0.32,"HEL"]
["Montgomery","KeA","Kendallville silt loam, 0 to 2 percent slopes","Kendallville",3,0.37,"NHEL"]
["Montgomery","KeB","Kendallville silt loam, 2 to 6 percent slopes","Kendallville",3,0.37,"PHEL"]
["Montgomery","KeC2","Kendallville silt loam, 6 to 12 percent slopes, moderately eroded","Kendallville",3,0.37,"PHEL"]
["Montgomery","Ld","Landes sandy loam","Landes",5,0.2,"NHEL"]
["Montgomery","Lg","Lanier sandy loam","Lanier",5,0.2,"NHEL"]
["Montgomery","LsB","Lewisburg silt loam, 2 to 6 percent slopes","Lewisburg",3,0.43,"PHEL"]
["Montgomery","LxC2","Lorenzo-Rodman complex, 4 to 12 percent slopes, moderately eroded","Lorenzo",3,0.28000000000000003,"PHEL"]
["Montgomery","LxD2","Lorenzo-Rodman complex, 12 to 18 percent slopes, moderately eroded","Lorenzo",3,0.28000000000000003,"HEL"]
["Montgomery","Mb","Made land","Made"]
["Montgomery","Md","Medway silt loam","Medway",5,0.32,"NHEL"]
["Montgomery","MlA","Miamian silt loam, 0 to 2 percent slopes","Miamian",5,0.37,"NHEL"]
["Montgomery","MlB","Miamian silt loam, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Montgomery","MlB2","Miamian silt loam, 2 to 6 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Montgomery","MlC2","Miamian silt loam, 6 to 12 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Montgomery","MlD2","Miamian silt loam, 12 to 18 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Montgomery","MmB","Miamian bouldery silt loam, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Montgomery","MnB3","Miamian clay loam, 2 to 6 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Montgomery","MnC3","Miamian clay loam, 6 to 12 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Montgomery","MnD3","Miamian clay loam, 12 to 18 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Montgomery","MoB","Miamian-Urban land complex, undulating","Miamian",5,0.37,"PHEL"]
["Montgomery","MoC","Miamian-Urban land complex, rolling","Miamian",5,0.37,"PHEL"]
["Montgomery","MoE","Miamian-Urban land complex, steep","Miamian",5,0.37,"HEL"]
["Montgomery","MrA","Millsdale silty clay loam, 0 to 3 percent slopes","Millsdale",4,0.32,"NHEL"]
["Montgomery","MsA","Milton silt loam, 0 to 2 percent slopes","Milton",4,0.37,"NHEL"]
["Montgomery","MsB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Montgomery","MsB2","Milton silt loam, 2 to 6 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Montgomery","MsC2","Milton silt loam, 6 to 12 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Montgomery","MsD2","Milton silt loam, 12 to 18 percent slopes, moderately eroded","Milton",4,0.37,"HEL"]
["Montgomery","MtD3","Milton silty clay loam, 6 to 18 percent slopes, severely eroded","Milton",3,0.37,"PHEL"]
["Montgomery","MuB","Milton-Urban land complex, undulating","Milton",4,0.37,"PHEL"]
["Montgomery","MuC","Milton-Urban land complex, rolling","Milton",4,0.37,"PHEL"]
["Montgomery","MuD","Milton-Urban land complex, hilly","Milton",4,0.37,"HEL"]
["Montgomery","Mv","Montgomery silty clay loam","Montgomery",5,0.37,"NHEL"]
["Montgomery","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Montgomery","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Montgomery","PlB","Plattville silt loam, 2 to 6 percent slopes","Plattville",5,0.32,"PHEL"]
["Montgomery","PlC","Plattville silt loam, 6 to 12 percent slopes","Plattville",5,0.32,"PHEL"]
["Montgomery","PyA","Pyrmont silt loam, 0 to 2 percent slopes","Pyrmont",3,0.43,"NHEL"]
["Montgomery","Qu","Quarries","Quarries"]
["Montgomery","RcA","Randolph silt loam, 0 to 2 percent slopes","Randolph",3,0.37,"NHEL"]
["Montgomery","ReB","Ritchey silt loam, 2 to 6 percent slopes","Ritchey",2,0.37,"PHEL"]
["Montgomery","ReB2","Ritchey silt loam, 2 to 6 percent slopes, moderately eroded","Ritchey",2,0.37,"PHEL"]
["Montgomery","ReC2","Ritchey silt loam, 6 to 12 percent slopes, moderately eroded","Ritchey",2,0.37,"HEL"]
["Montgomery","ReE2","Ritchey silt loam, 12 to 25 percent slopes, moderately eroded","Ritchey",2,0.37,"HEL"]
["Montgomery","ReF2","Ritchey silt loam, 25 to 50 percent slopes, moderately eroded","Ritchey",2,0.37,"HEL"]
["Montgomery","RfD3","Ritchey silty clay loam, 6 to 18 percent slopes, severely eroded","Ritchey",2,0.37,"HEL"]
["Montgomery","Rh","Riverwash","Riverwash"]
["Montgomery","RlE2","Rodman and Fox soils, 18 to 25 percent slopes, moderately eroded","Rodman",3,0.2,"HEL"]
["Montgomery","RlF2","Rodman and Fox soils, 25 to 50 percent slopes, moderately eroded","Rodman",3,0.2,"HEL"]
["Montgomery","Rs","Ross silt loam","Ross",5,0.32,"NHEL"]
["Montgomery","Rt","Ross-Urban land complex","Ross",5,0.32,"NHEL"]
["Montgomery","RuB","Russell silt loam, 2 to 6 percent slopes","Russell",5,0.37,"PHEL"]
["Montgomery","RvC2","Russell-Miamian silt loams, 6 to 12 percent slopes, moderately eroded","Russell",5,0.37,"PHEL"]
["Montgomery","RvD2","Russell-Miamian silt loams, 12 to 18 percent slopes, moderately eroded","Russell",5,0.37,"HEL"]
["Montgomery","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Montgomery","So","Sloan silt loam","Sloan",5,0.37,"NHEL"]
["Montgomery","ThA","Thackery silt loam, till substratum, 0 to 2 percent slopes","Thackery",4,0.37,"NHEL"]
["Montgomery","TpA","Tippecanoe silt loam, 0 to 2 percent slopes","Tippecanoe",5,0.32,"NHEL"]
["Montgomery","Ua","Urban land, alluvial","Urban"]
["Montgomery","Ud","Udorthents","Udorthents"]
["Montgomery","Ug","Urban land, gravelly material","Urban"]
["Montgomery","Um","Urban land, loamy material","Urban"]
["Montgomery","W","Water","water"]
["Montgomery","WaA","Warsaw silt loam, 0 to 2 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
["Montgomery","WaB","Warsaw silt loam, 2 to 6 percent slopes","Warsaw",4,0.28000000000000003,"PHEL"]
["Montgomery","WeA","Wea silt loam, 0 to 2 percent slopes","Wea",5,0.32,"NHEL"]
["Montgomery","WeB","Wea silt loam, 2 to 6 percent slopes","Wea",5,0.32,"PHEL"]
["Montgomery","Ws","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
["Montgomery","WyB2","Wynn silt loam, 2 to 6 percent slopes, moderately eroded","Wynn",4,0.37,"PHEL"]
["Montgomery","XeA","Xenia silt loam, 0 to 2 percent slopes","Xenia",5,0.37,"NHEL"]
["Montgomery","XeB","Xenia silt loam, 2 to 6 percent slopes","Xenia",5,0.37,"PHEL"]
[null,"Select","none","none"]
["Preble","BbA","Birbeck silt loam, 0 to 2 percent slopes","Birbeck",5,0.37,"NHEL"]
["Preble","Bn","Bonpas silt loam","Bonpas",5,0.28000000000000003,"NHEL"]
["Preble","Bo","Bonpas silty clay loam","Bonpas",5,0.28000000000000003,"NHEL"]
["Preble","BrA ","Brookston silt loam, 0 to 2 percent slopes","Brookston",5,0.28000000000000003,"NHEL"]
["Preble","BsA","Brookston silty clay loam, 0 to 2 percent slopes","Brookston",5,0.28000000000000003,"NHEL"]
["Preble","CaE2","Casco, Rodman, and Fox soils, 18 to 25 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Preble","CaF2","Casco, Rodman, and Fox soils, 25 to 50 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Preble","CaF3","Casco, Rodman, and Fox soils, 25 to 50 percent slopes, severely eroded","Casco",3,0.24,"HEL"]
["Preble","CbB","Celina bouldery silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Preble","CeA","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Preble","CeB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Preble","CeB2","Celina silt loam, 2 to 6 percent slopes, eroded","Celina",5,0.37,"PHEL"]
["Preble","CmC2","Celina-Miami silt loams, 6 to 12 percent slopes, eroded","Celina",5,0.37,"PHEL"]
["Preble","CnE2","Channahon and Fairmount soils, 18 to 25 percent slopes, eroded","Channahon",2,0.37,"HEL"]
["Preble","CoA","Corwin silt loam, 0 to 2 percent slopes","Corwin",5,0.28000000000000003,"NHEL"]
["Preble","CoB","Corwin silt loam, 2 to 6 percent slopes","Corwin",5,0.28000000000000003,"PHEL"]
["Preble","Cr","Crane silt loam","Crane",5,0.28000000000000003,"NHEL"]
["Preble","CsA","Crosby bouldery silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Preble","CsB","Crosby bouldery silt loam, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Preble","CtA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Preble","CyB","Crosby-Celina silt loams, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Preble","DaA","Dana silt loam, 0 to 2 percent slopes","Dana",5,0.32,"NHEL"]
["Preble","DaB","Dana silt loam, 2 to 6 percent slopes","Dana",5,0.32,"PHEL"]
["Preble","FaF2","Fairmount soils, 25 to 50 percent slopes, moderately eroded","Fairmount",2,0.37,"HEL"]
["Preble","FcA","Fincastle silt loam, 0 to 2 percent slopes","Fincastle",5,0.37,"NHEL"]
["Preble","FcB","Fincastle silt loam, 2 to 6 percent slopes","Fincastle",5,0.37,"PHEL"]
["Preble","FgA","Fox gravelly loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Preble","FgB","Fox gravelly loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Preble","FgB2","Fox gravelly loam, 2 to 6 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Preble","FgC2","Fox gravelly loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Preble","FlA","Fox loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Preble","FlB","Fox loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Preble","FlB2","Fox loam, 2 to 6 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Preble","FlC2","Fox loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Preble","FmA","Fox silt loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Preble","FmB","Fox silt loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Preble","FmB2","Fox silt loam, 2 to 6 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Preble","FmC2","Fox silt loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Preble","FmD2","Fox silt loam, 12 to 18 percent slopes, moderately eroded","Fox",4,0.37,"HEL"]
["Preble","FsC3","Fox soils, 6 to 12 percent slopes, severely eroded","Fox",3,0.37,"PHEL"]
["Preble","FsD3","Fox soils, 12 to 18 percent slopes, severely eroded","Fox",3,0.37,"HEL"]
["Preble","Gp","Gravel Pits","Gravel"]
["Preble","GuC","Gullied land, rolling","Gullied"]
["Preble","GuD","Gullied land, hilly","Gullied"]
["Preble","GuF","Gullied land, steep","Gullied"]
["Preble","La","Landes gravelly sandy loam","Landes",5,0.2,"NHEL"]
["Preble","Ld","Landes sandy loam","Landes",5,0.2,"NHEL"]
["Preble","Lg","Landes sandy loam, gravelly subsoil variant","Landes",3,0.2,"NHEL"]
["Preble","LsB","Lewisburg silt loam, 2 to 6 percent slopes","Lewisburg",3,0.43,"PHEL"]
["Preble","LsB2","Lewisburg silt loam, 2 to 6 percent slopes, moderately eroded","Lewisburg",3,0.43,"PHEL"]
["Preble","LtC3","Lewisburg soils, 6 to 12 percent slopes, severely eroded","Lewisburg",2,0.43,"HEL"]
["Preble","Mb","Made land and borrow pits","Made"]
["Preble","Md","Medway silt loam","Medway",5,0.32,"NHEL"]
["Preble","MeC2","Miami bouldery silt loam, 6 to 12 percent slopes, eroded","Miami",5,0.37,"PHEL"]
["Preble","MlC","Miami silt loam, 6 to 12 percent slopes","Miami",5,0.37,"PHEL"]
["Preble","MlC2","Miami silt loam, 6 to 12 percent slopes, moderately eroded","Miami",5,0.37,"PHEL"]
["Preble","MlD","Miami silt loam, 12 to 18 percent slopes","Miami",5,0.37,"HEL"]
["Preble","MlD2 ","Miami silt loam, 12 to 18 percent slopes, moderately eroded","Miami",5,0.37,"HEL"]
["Preble","MmC3","Miami soils, 6 to 12 percent slopes, severely eroded","Miami",4,0.37,"PHEL"]
["Preble","MmD3","Miami soils, 12 to 18 percent slopes, severely eroded","Miami",4,0.37,"HEL"]
["Preble","MnB","Miami-Celina bouldery silt loams, 2 to 6 percent slopes","Miami",5,0.37,"PHEL"]
["Preble","MnB2","Miami-Celina bouldery silt loams, 2 to 6 percent slopes, moderately eroded","Miami",5,0.37,"PHEL"]
["Preble","MoB ","Miami-Celina silt loams, 2 to 6 percent slopes","Miami",5,0.37,"PHEL"]
["Preble","MoB2","Miami-Celina silt loams, 2 to 6 percent slopes, moderately eroded","Miami",5,0.37,"PHEL"]
["Preble","MpB3","Miami-Celina soils, 2 to 6 percent slopes, severely eroded","Miami",4,0.37,"PHEL"]
["Preble","MrE2","Miami, Fox, and Hennepin soils, 18 to 25 percent slopes, moderately eroded","Miami",5,0.37,"HEL"]
["Preble","MrE3","Miami, Fox, and Hennepin soils, 18 to 25 percent slopes, severely eroded","Miami",4,0.37,"HEL"]
["Preble","MrF2","Miami, Fox, and Hennepin soils, 25 to 50 percent slopes, moderately eroded","Miami",5,0.37,"HEL"]
["Preble","MrF3","Miami, Fox, and Hennepin soils, 25 to 50 percent slopes, severely eroded","Miami",4,0.37,"HEL"]
["Preble","MsA","Millsdale silt loam, 0 to 3 percent slopes","Millsdale",4,0.32,"NHEL"]
["Preble","MtA","Millsdale silty clay loam, 0 to 3 percent slopes","Millsdale",4,0.32,"NHEL"]
["Preble","MuA","Milton silt loam, 0 to 2 percent slopes","Milton",4,0.37,"NHEL"]
["Preble","MuB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Preble","MuB2","Milton silt loam, 2 to 6 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Preble","MuC2","Milton silt loam, 6 to 12 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Preble","MvC3","Milton soils, 6 to 12 percent slopes, severely eroded","Milton",3,0.37,"PHEL"]
["Preble","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Preble","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Preble","OkA","Ockley and Kendallville silt loams, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Preble","OkB","Ockley and Kendallville silt loams, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Preble","OkB2","Ockley and Kendallville silt loams, 2 to 6 percent slopes, moderately eroded","Ockley",5,0.37,"PHEL"]
["Preble","OkC2","Ockley and Kendallville silt loams, 6 to 12 percent slopes, moderately eroded","Ockley",5,0.37,"PHEL"]
["Preble","OkD2","Ockley and Kendallville silt loams, 12 to 18 percent slopes, moderately eroded","Ockley",5,0.37,"HEL"]
["Preble","OlC3","Ockley and Kendallville soils, 6 to 12 percent slopes, severely eroded","Ockley",4,0.37,"PHEL"]
["Preble","OlD3","Ockley and Kendallville soils, 12 to 18 percent slopes, severely eroded","Ockley",4,0.37,"HEL"]
["Preble","OsB","Odell silt loam, 2 to 6 percent slopes","Odell",5,0.28000000000000003,"PHEL"]
["Preble","PlB","Plattville silt loam, 2 to 6 percent slopes","Plattville",5,0.32,"PHEL"]
["Preble","PyA","Pyrmont silt loam, 0 to 2 percent slopes","Pyrmont",3,0.43,"NHEL"]
["Preble","PyB","Pyrmont silt loam, 2 to 6 percent slopes","Pyrmont",3,0.43,"PHEL"]
["Preble","Qu","Quarries","Quarries"]
["Preble","Ra","Ragsdale silt loam","Ragsdale",5,0.28000000000000003,"NHEL"]
["Preble","RcA","Randolph silt loam, 0 to 2 percent slopes","Randolph",3,0.37,"NHEL"]
["Preble","RcB","Randolph silt loam, 2 to 6 percent slopes","Randolph",3,0.37,"PHEL"]
["Preble","RdA","Raub and Dana silt loams, 0 to 2 percent slopes","Raub",5,0.28000000000000003,"NHEL"]
["Preble","ReA","Reesville silt loam, 0 to 2 percent slopes","Reesville",5,0.37,"NHEL"]
["Preble","RhB2","Ritchey and Channahon silt loams, 2 to 6 percent slopes, moderately eroded","Ritchey",2,0.37,"PHEL"]
["Preble","RhC2","Ritchey and Channahon silt loams, 6 to 12 percent slopes, moderately eroded","Ritchey",2,0.37,"HEL"]
["Preble","RhD2","Ritchey and Channahon silt loams, 12 to 18 percent slopes, moderately eroded","Ritchey",2,0.37,"HEL"]
["Preble","RnC3","Ritchey and Channahon soils, 6 to 12 percent slopes, severely eroded","Ritchey",2,0.37,"HEL"]
["Preble","RnD3","Ritchey and Channahon soils, 12 to 18 percent slopes, severely eroded","Ritchey",2,0.37,"HEL"]
["Preble","Ro","Riverwash","Riverwash"]
["Preble","Rs","Ross loam","Ross",5,0.32,"NHEL"]
["Preble","RuA","Russell silt loam, 0 to 2 percent slopes","Russell",5,0.37,"NHEL"]
["Preble","RuB","Russell silt loam, 2 to 6 percent slopes","Russell",5,0.37,"PHEL"]
["Preble","RuB2","Russell silt loam, 2 to 6 percent slopes, moderately eroded","Russell",5,0.37,"PHEL"]
["Preble","RuC2","Russell silt loam, 6 to 12 percent slopes, moderately eroded","Russell",5,0.37,"PHEL"]
["Preble","RuD2","Russell silt loam, 12 to 18 percent slopes, moderately eroded","Russell",5,0.37,"HEL"]
["Preble","RvC3","Russell soils, 6 to 12 percent slopes, severely eroded","Russell",4,0.37,"PHEL"]
["Preble","RvD3","Russell soils, 12 to 18 percent slopes, severely eroded","Russell",4,0.37,"HEL"]
["Preble","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Preble","SlA","Sleeth silt loam, 0 to 2 percent slopes","Sleeth",5,0.32,"NHEL"]
["Preble","So","Sloan silt loam","Sloan",5,0.37,"NHEL"]
["Preble","ThA","Thackery silt loam, 0 to 2 percent slopes","Thackery",4,0.37,"NHEL"]
["Preble","ThB","Thackery silt loam, 2 to 6 percent slopes","Thackery",4,0.37,"PHEL"]
["Preble","TpA","Tippecanoe silt loam, 0 to 2 percent slopes","Tippecanoe",5,0.32,"NHEL"]
["Preble","TpB","Tippecanoe silt loam, 2 to 6 percent slopes","Tippecanoe",5,0.32,"PHEL"]
["Preble","WaA","Warsaw silt loam, 0 to 2 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
["Preble","WeA","Wea silt loam, 0 to 2 percent slopes","Wea",5,0.32,"NHEL"]
["Preble","Wn","Westland silt loam","Westland",5,0.28000000000000003,"NHEL"]
["Preble","Ws","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
["Preble","WyB","Wynn silt loam, 2 to 6 percent slopes","Wynn",4,0.37,"PHEL"]
["Preble","WyB2","Wynn silt loam, 2 to 6 percent slopes, moderately eroded","Wynn",4,0.37,"PHEL"]
["Preble","WyC2","Wynn silt loam, 6 to 12 percent slopes, moderately eroded","Wynn",4,0.37,"PHEL"]
["Preble","XeA","Xenia silt loam, 0 to 2 percent slopes","Xenia",5,0.37,"NHEL"]
["Preble","XeB","Xenia silt loam, 2 to 6 percent slopes","Xenia",5,0.37,"PHEL"]
["Preble","XeB2","Xenia silt loam, 2 to 6 percent slopes, moderately eroded","Xenia",5,0.37,"PHEL"]
[null,"Select","none","none"]
["Shelby","Ag","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Shelby","BlA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Shelby","BlB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Shelby","Bs","Brookston silty clay loam","Brookston",5,0.28000000000000003,"NHEL"]
["Shelby","Ca","Carlisle muck","Carlisle",2,null,"NHEL"]
["Shelby","CeA","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Shelby","CeB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Shelby","CnA","Crane silt loam, 0 to 2 percent slopes","Crane",5,0.28000000000000003,"NHEL"]
["Shelby","CrA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Shelby","CrB","Crosby silt loam, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Shelby","Ee","Eel silt loam, occasionally flooded","Eel",5,0.37,"NHEL"]
["Shelby","Ef","Eel Variant silt loam, occasionally flooded","Eel",5,0.32,"NHEL"]
["Shelby","ElA","Eldean loam, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Shelby","ElB","Eldean loam, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Shelby","EoC2","Eldean-Casco complex, 6 to 15 percent slopes, eroded","Eldean",4,0.37,"PHEL"]
["Shelby","EsB2","Eldean-Morley complex, 2 to 6 percent slopes, eroded","Eldean",4,0.37,"PHEL"]
["Shelby","EsC2","Eldean-Morley complex, 6 to 15 percent slopes, eroded","Eldean",4,0.37,"PHEL"]
["Shelby","Ge","Genesee silt loam, occasionally flooded","Genesee",5,0.37,"NHEL"]
["Shelby","GlB","Glynwood silt loam, 2 to 6 percent slopes","Glynwood",3,0.43,"PHEL"]
["Shelby","GlB2","Glynwood silt loam, 2 to 6 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Shelby","GlC2","Glynwood silt loam, 6 to 12 percent slopes, eroded","Glynwood",3,0.43,"PHEL"]
["Shelby","GlD2","Glynwood silt loam, 12 to 18 percent slopes, eroded","Glynwood",3,0.43,"HEL"]
["Shelby","GmC3","Glynwood clay loam, 6 to 12 percent slopes, severely eroded","Glynwood",2,0.43,"HEL"]
["Shelby","GmD3","Glynwood clay loam, 12 to 18 percent slopes, severely eroded","Glynwood",2,0.43,"HEL"]
["Shelby","Md","Medway silt loam, occasionally flooded","Medway",5,0.32,"NHEL"]
["Shelby","MhB","Miamian silt loam, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Shelby","MhC2","Miamian silt loam, 6 to 12 percent slopes, eroded","Miamian",5,0.37,"PHEL"]
["Shelby","MhD2","Miamian silt loam, 12 to 18 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Shelby","MhE","Miamian silt loam, 18 to 25 percent slopes","Miamian",5,0.37,"HEL"]
["Shelby","MhF","Miamian silt loam, 25 to 50 percent slopes","Miamian",5,0.37,"HEL"]
["Shelby","MlC3","Miamian clay loam, 6 to 12 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Shelby","MoB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Shelby","Mt","Montgomery silty clay loam","Montgomery",5,0.37,"NHEL"]
["Shelby","Mw","Montgomery silty clay loam, gravelly substratum","Montgomery",5,0.37,"NHEL"]
["Shelby","MxE","Morley silt loam, 18 to 25 percent slopes","Morley",3,0.43,"HEL"]
["Shelby","MxF","Morley silt loam, 25 to 50 percent slopes","Morley",3,0.43,"HEL"]
["Shelby","OcA","Ockley silt loam, 0 to 3 percent slopes","Ockley",5,0.37,"NHEL"]
["Shelby","OdA","Odell silt loam, 0 to 2 percent slopes","Odell",5,0.28000000000000003,"NHEL"]
["Shelby","OdB","Odell silt loam, 2 to 6 percent slopes","Odell",5,0.28000000000000003,"PHEL"]
["Shelby","Pa","Patton silty clay loam","Patton",5,0.28000000000000003,"NHEL"]
["Shelby","Pd","Pewamo silt loam","Pewamo",5,0.24,"NHEL"]
["Shelby","Pe","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Shelby","Pg","Pits, gravel","Pits"]
["Shelby","Sh","Shoals silt loam, occasionally flooded","Shoals",5,0.37,"NHEL"]
["Shelby","St","Stonelick sandy loam, occasionally flooded","Stonelick",5,0.24,"NHEL"]
["Shelby","Ud","Udorthents","Udorthents"]
["Shelby","W","Water","water"]
["Shelby","Wb","Wallkill silty clay loam","Wallkill",5,0.32,"NHEL"]
["Shelby","WdA","Warsaw Variant silt loam, 0 to 2 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
[null,"Select","none","none"]
["Union","Ag","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Union","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Union","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Union","BoB2","Blount silt loam, 2 to 6 percent slopes, moderately eroded","Blount",3,0.43,"PHEL"]
["Union","Bs","Brookston silty clay loam","Brookston",5,0.28000000000000003,"NHEL"]
["Union","CeA","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Union","CeB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Union","CrA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Union","CrB","Crosby silt loam, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Union","Cu","Cut and Fill land","Cut"]
["Union","Ee","Eel silt loam","Eel",5,0.37,"NHEL"]
["Union","FoA","Fox silt loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Union","FoB","Fox silt loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Union","FoB2","Fox silt loam, 2 to 6 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Union","FoC2","Fox silt loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Union","Gn","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Union","Gp","Gravel pits","Gravel"]
["Union","HeA","Henshaw silt loam, 0 to 2 percent slopes","Henshaw",4,0.43,"NHEL"]
["Union","Ho","Homer silt loam","Homer",4,0.37,"NHEL"]
["Union","Ka","Kane silt loam","Kane",4,0.28000000000000003,"NHEL"]
["Union","KeA","Kendallville silt loam, 0 to 2 percent slopes","Kendallville",3,0.37,"NHEL"]
["Union","KeB","Kendallville silt loam, 2 to 6 percent slopes","Kendallville",3,0.37,"PHEL"]
["Union","Lc","Lippincott silty clay loam","Lippincott",5,0.28000000000000003,"NHEL"]
["Union","MlB","Miamian silt loam, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Union","MlC2","Miamian silt loam, 6 to 12 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Union","MlD2","Miamian silt loam, 12 to 18 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Union","MlF2","Miamian silt loam, 18 to 35 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Union","Mn","Montgomery silty clay loam","Montgomery",5,0.37,"NHEL"]
["Union","MrB","Morley silt loam, 2 to 6 percent slopes","Morley",3,0.43,"PHEL"]
["Union","MrB2","Morley silt loam, 2 to 6 percent slopes, moderately eroded","Morley",3,0.43,"PHEL"]
["Union","MrC","Morley silt loam, 6 to 12 percent slopes","Morley",3,0.43,"HEL"]
["Union","MrC2","Morley silt loam, 6 to 12 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Union","MrD2","Morley silt loam, 12 to 18 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Union","MrE2","Morley silt loam, 18 to 25 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Union","MrF2","Morley silt loam, 25 to 50 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Union","Mu","Muskego muck","Muskego",2,null,"NHEL"]
["Union","NpA","Nappanee silt loam, 0 to 2 percent slopes","Nappanee",3,0.43,"NHEL"]
["Union","NpB","Nappanee silt loam, 2 to 6 percent slopes","Nappanee",3,0.43,"PHEL"]
["Union","OdA","Odell silt loam, 0 to 2 percent slopes","Odell",5,0.28000000000000003,"NHEL"]
["Union","Pa","Paulding silty clay","Paulding",5,0.28000000000000003,"NHEL"]
["Union","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Union","Qu","Quarries","Quarries"]
["Union","Ro","Ross silt loam","Ross",5,0.32,"NHEL"]
["Union","ScB","St. Clair silt loam, 2 to 6 percent slopes","St. Clair",3,0.37,"PHEL"]
["Union","ScB2","St. Clair silt loam, 2 to 6 percent slopes, moderately eroded","St. Clair",3,0.37,"PHEL"]
["Union","ScC","St. Clair silt loam, 6 to 12 percent slopes","St. Clair",3,0.37,"PHEL"]
["Union","ScC2","St. Clair silt loam, 6 to 12 percent slopes, moderately eroded","St. Clair",3,0.37,"PHEL"]
["Union","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Union","SlA","Sleeth silt loam, 0 to 2 percent slopes","Sleeth",5,0.32,"NHEL"]
["Union","So","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Union","W","Water","water"]
["Union","WaB","Warsaw silt loam, 1 to 4 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
["Union","Wc","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
["Union","We","Wetzel silty clay loam","Wetzel",5,0.37,"NHEL"]
[null,"Select","none","none"]
["Warren","AbA","Abscota sand, calcareous variant","Abscota",5,0.15,"NHEL"]
["Warren","AfB","Alford silt loam, till substratum, 1 to 4 percent slopes","Alford",5,0.37,"PHEL"]
["Warren","Ag","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Warren","AvA","Avonburg silt loam, 0 to 2 percent slopes","Avonburg",4,0.43,"NHEL"]
["Warren","AvB","Avonburg silt loam, 2 to 6 percent slopes","Avonburg",4,0.43,"PHEL"]
["Warren","AvB2","Avonburg silt loam, 2 to 6 percent slopes, moderately eroded","Avonburg",4,0.43,"PHEL"]
["Warren","BbB","Birkbeck silt loam, 1 to 4 percent slopes","Birbeck",5,0.37,"NHEL"]
["Warren","Bc","Blanchester silt loam","Blanchester",5,0.37,"NHEL"]
["Warren","Br","Brookston silty clay loam","Brookston",5,0.28000000000000003,"NHEL"]
["Warren","CcB2","Casco loam, 2 to 6 percent slopes, moderately eroded","Casco",3,0.24,"PHEL"]
["Warren","CcC2","Casco loam, 6 to 12 percent slopes, moderately eroded","Casco",3,0.24,"PHEL"]
["Warren","CdD2","Casco-Rodman complex, 12 to 18 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Warren","CnB","Cincinnati silt loam, 2 to 6 percent slopes","Cincinnati",4,0.37,"PHEL"]
["Warren","CnB2","Cincinnati silt loam, 2 to 6 percent slopes, moderately eroded","Cincinnati",4,0.37,"PHEL"]
["Warren","CnC2","Cincinnati silt loam, 6 to 12 percent slopes, moderately eroded","Cincinnati",4,0.37,"PHEL"]
["Warren","Co","Clermont silt loam","Clermont",5,0.37,"NHEL"]
["Warren","CrB","Crider silt loam, 2 to 6 percent slopes","Crider",5,0.32,"PHEL"]
["Warren","Cu","Cut and fill land","Cut"]
["Warren","DaA","Dana silt loam, 0 to 2 percent slopes","Dana",5,0.32,"NHEL"]
["Warren","DaB","Dana silt loam, 2 to 6 percent slopes","Dana",5,0.32,"PHEL"]
["Warren","EdB2","Eden complex, 2 to 6 percent slopes, moderately eroded","Eden",3,0.43,"PHEL"]
["Warren","EdC2","Eden complex, 6 to 12 percent slopes, moderately eroded","Eden",3,0.43,"PHEL"]
["Warren","EdD2","Eden complex, 12 to 18 percent slopes, moderately eroded","Eden",3,0.43,"HEL"]
["Warren","EdE2","Eden complex, 18 to 25 percent slopes, moderately eroded","Eden",3,0.43,"HEL"]
["Warren","EdF2","Eden complex, 25 to 35 percent slopes, moderately eroded","Eden",3,0.43,"HEL"]
["Warren","Ee","Eel loam","Eel",5,0.37,"NHEL"]
["Warren","FaE2","Fairmount-Eden flaggy silty clay loams, 12 to 25 percent slopes, moderately eroded","Fairmount",2,0.37,"HEL"]
["Warren","FaF2","Fairmount-Eden flaggy silty clay loams, 25 to 50 percent slopes, moderately eroded","Fairmount",2,0.37,"HEL"]
["Warren","FhA","Fincastle silt loam, 0 to 2 percent slopes","Fincastle",5,0.37,"NHEL"]
["Warren","FhB","Fincastle silt loam, 2 to 6 percent slopes","Fincastle",5,0.37,"PHEL"]
["Warren","FlA","Fox loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Warren","FlB","Fox loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Warren","FlB2","Fox loam, 2 to 6 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Warren","FlC2","Fox loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Warren","FoD2","Fox-Casco complex, 12 to 18 percent slopes, moderately eroded","Fox",4,0.37,"HEL"]
["Warren","Gd","Genesee fine sandy loam","Genesee",5,0.37,"NHEL"]
["Warren","Gn","Genesee loam","Genesee",5,0.37,"NHEL"]
["Warren","Gp","Gravel pits","Gravel"]
["Warren","HeF","Hennepin silt loam, 25 to 35 percent slopes","Hennepin",4,0.32,"HEL"]
["Warren","HeF2","Hennepin silt loam, 25 to 35 percent slopes, moderately eroded","Hennepin",4,0.32,"HEL"]
["Warren","HmE","Hennepin-Miamian silt loams, 18 to 25 percent slopes","Hennepin",4,0.32,"HEL"]
["Warren","HmE2","Hennepin-Miamian silt loams, 18 to 25 percent slopes, moderately eroded","Hennepin",4,0.32,"HEL"]
["Warren","HnD3","Hennepin-Miamian complex, 12 to 18 percent slopes, severely eroded","Hennepin",4,0.32,"HEL"]
["Warren","HoB","Henshaw silt loam, 1 to 4 percent slopes","Henshaw",4,0.43,"PHEL"]
["Warren","HrB2","Hickory silt loam, 2 to 6 percent slopes, moderately eroded","Hickory",5,0.37,"PHEL"]
["Warren","HrC2","Hickory silt loam, 6 to 12 percent slopes, moderately eroded","Hickory",5,0.37,"PHEL"]
["Warren","HrD2","Hickory silt loam, 12 to 18 percent slopes, moderately eroded","Hickory",5,0.37,"HEL"]
["Warren","HsC3","Hickory clay loam, 6 to 12 percent slopes, severely eroded","Hickory",4,0.37,"PHEL"]
["Warren","HsD3","Hickory clay loam, 12 to 18 percent slopes, severely eroded","Hickory",4,0.37,"HEL"]
["Warren","HtE2","Hickory-Fairmount complex, 18 to 25 percent slopes, moderately eroded","Hickory",5,0.37,"HEL"]
["Warren","HtF2","Hickory-Fairmount complex, 25 to 50 percent slopes, moderately eroded","Hickory",5,0.37,"HEL"]
["Warren","IvA","Iva silt loam, till substratum, 0 to 2 percent slopes","Iva",4,0.43,"NHEL"]
["Warren","KeB","Kendallville loam, 2 to 6 percent slopes","Kendallville",3,0.37,"PHEL"]
["Warren","KeC2","Kendallville loam, 6 to 12 percent slopes, moderately eroded","Kendallville",3,0.37,"PHEL"]
["Warren","Kg","Kings silty clay loam, thick surface variant","Kings",4,0.37,"NHEL"]
["Warren","Lg","Lanier sandy loam","Lanier",5,0.2,"NHEL"]
["Warren","MmB3","Miamian clay loam, 2 to 6 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Warren","MmC3","Miamian clay loam, 6 to 12 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Warren","MnD2","Miamian-Hennepin silt loams, 12 to 18 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Warren","MrC2","Miamian-Russell silt loams, 6 to 12 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Warren","Mu","Muck","Muck",2,null,"NHEL"]
["Warren","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Warren","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Warren","OcB2","Ockley silt loam, 2 to 6 percent slopes, moderately eroded","Ockley",5,0.37,"PHEL"]
["Warren","PaB","Parke silt loam, 2 to 6 percent slopes","Parke",5,0.37,"PHEL"]
["Warren","PaD2","Parke silt loam, 6 to 18 percent slopes, moderately eroded","Parke",5,0.37,"PHEL"]
["Warren","Pb","Patton silt loam, silted","Patton",5,0.28000000000000003,"NHEL"]
["Warren","Pc","Patton silty clay loam","Patton",5,0.28000000000000003,"NHEL"]
["Warren","PlB","Plattville silt loam, 1 to 6 percent slopes","Plattville",5,0.32,"PHEL"]
["Warren","PrB","Princeton fine sandy loam, 2 to 6 percent slopes","Princeton",5,0.24,"PHEL"]
["Warren","PrC2","Princeton fine sandy loam, 6 to 12 percent slopes, moderately eroded","Princeton",5,0.24,"PHEL"]
["Warren","Ra","Ragsdale silty clay loam","Ragsdale",5,0.28000000000000003,"NHEL"]
["Warren","RbA","Rainsboro silt loam, 0 to 2 percent slopes","Rainsboro",4,0.43,"NHEL"]
["Warren","RbB","Rainsboro silt loam, 2 to 6 percent slopes","Rainsboro",4,0.43,"PHEL"]
["Warren","Re","Reesville silt loam","Reesville",5,0.37,"NHEL"]
["Warren","Rh","Riverwash","Riverwash"]
["Warren","RkE2","Rodman and Casco gravelly loams, 18 to 25 percent slopes, moderately eroded","Rodman",3,0.2,"HEL"]
["Warren","Rn","Ross loam","Ross",5,0.32,"NHEL"]
["Warren","RpA","Rossmoyne silt loam, 0 to 2 percent slopes","Rossmoyne",4,0.37,"NHEL"]
["Warren","RpB","Rossmoyne silt loam, 2 to 6 percent slopes","Rossmoyne",4,0.37,"PHEL"]
["Warren","RpB2","Rossmoyne silt loam, 2 to 6 percent slopes, moderately eroded","Rossmoyne",4,0.37,"PHEL"]
["Warren","RpC2","Rossmoyne silt loam, 6 to 12 percent slopes, moderately eroded","Rossmoyne",4,0.37,"PHEL"]
["Warren","RsB3","Rossmoyne silty clay loam, 2 to 6 percent slopes, severely eroded","Rossmoyne",3,0.37,"PHEL"]
["Warren","RsC3","Rossmoyne silty clay loam, 6 to 12 percent slopes, severely eroded","Rossmoyne",3,0.37,"PHEL"]
["Warren","RvA","Russell-Miamian silt loams, 0 to 2 percent slopes","Russell",5,0.37,"NHEL"]
["Warren","RvB","Russell-Miamian silt loams, 2 to 6 percent slopes","Russell",5,0.37,"PHEL"]
["Warren","RvB2","Russell-Miamian silt loams, 2 to 6 percent slopes, moderately eroded","Russell",5,0.37,"PHEL"]
["Warren","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Warren","So","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Warren","Ud","Udorthents","Udorthents"]
["Warren","UnB","Uniontown silt loam, 1 to 6 percent slopes","Uniontown",4,0.37,"PHEL"]
["Warren","W","Water","Water"]
["Warren","WaA","Warsaw loam, 0 to 2 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
["Warren","WaB","Warsaw loam, 2 to 6 percent slopes","Warsaw",4,0.28000000000000003,"PHEL"]
["Warren","WeA","Wea silt loam, 0 to 2 percent slopes","Wea",5,0.32,"NHEL"]
["Warren","WlA","Williamsburg silt loam, 0 to 2 percent slopes","Williamsburg",5,0.32,"NHEL"]
["Warren","WlB","Williamsburg silt loam, 2 to 6 percent slopes","Williamsburg",5,0.32,"PHEL"]
["Warren","WlC2","Williamsburg silt loam, 6 to 12 percent slopes, moderately eroded","Williamsburg",5,0.32,"PHEL"]
["Warren","WyB","Wynn silt loam, 2 to 6 percent slopes","Wynn",4,0.37,"PHEL"]
["Warren","WyB2","Wynn silt loam, 2 to 6 percent slopes, moderately eroded","Wynn",4,0.37,"PHEL"]
["Warren","WyC2","Wynn silt loam, 6 to 12 percent slopes, moderately eroded","Wynn",4,0.37,"PHEL"]
["Warren","WyC3","Wynn silt loam, 6 to 12 percent slopes, severely eroded","Wynn",3,0.37,"PHEL"]
["Warren","XeA","Xenia silt loam, 0 to 2 percent slopes","Xenia",5,0.37,"NHEL"]
["Warren","XeB","Xenia silt loam, 2 to 6 percent slopes","Xenia",5,0.37,"PHEL"]
["Warren","XeB2","Xenia silt loam, 2 to 6 percent slopes, moderately eroded","Xenia",5,0.37,"PHEL"]

{"sheet":"Area 5","index":6,"n_rows":1630,"n_cols":7,"rows_kept":1630,"cut":false,"hidden":false,"merged":[]}
["County","symbol","map unit name","Component","T","Kw","HEL"]
[null,"Select","none","none"]
["Adams","AaA","Aaron silt loam, 0 to 2 percent slopes","Aaron",3,0.37,"NHEL"]
["Adams","AaB","Aaron silt loam, 2 to 6 percent slopes","Aaron",3,0.37,"PHEL"]
["Adams","AvA","Avonburg silt loam, 0 to 2 percent slopes","Avonburg",4,0.43,"NHEL"]
["Adams","BkD","Berks silt loam, 15 to 25 percent slopes","Berks",3,0.24,"HEL"]
["Adams","BnB","Bratton silt loam, 2 to 8 percent slopes","Bratton",4,0.37,"PHEL"]
["Adams","BrC2","Bratton-Opequon complex, 8 to 15 percent slopes, eroded","Bratton",4,0.37,"HEL"]
["Adams","BsC2","Brushcreek silt loam, 6 to 12 percent slopes, eroded","Brushcreek",3,0.37,"HEL"]
["Adams","BtD2","Brushcreek-Lawshe complex, 12 to 25 percent slopes, eroded","Brushcreek",3,0.37,"HEL"]
["Adams","CkB","Cincinnati silt loam, 2 to 6 percent slopes","Cincinnati",4,0.37,"PHEL"]
["Adams","CkC2","Cincinnati silt loam, 6 to 12 percent slopes, eroded","Cincinnati",4,0.37,"PHEL"]
["Adams","CrB","Crider silt loam, 1 to 6 percent slopes","Crider",5,0.32,"PHEL"]
["Adams","EgE2","Eden flaggy silty clay loam, 25 to 40 percent slopes, eroded","Eden",3,0.43,"HEL"]
["Adams","EgF2","Eden flaggy silty clay loam, 40 to 70 percent slopes, eroded","Eden",3,0.43,"HEL"]
["Adams","EkB","Elkinsville silt loam, 1 to 6 percent slopes","Elkinsville",5,0.37,"PHEL"]
["Adams","FaC2","Faywood silt loam, 8 to 15 percent slopes, eroded","Faywood",3,0.37,"HEL"]
["Adams","FbD2","Faywood silty clay loam, 15 to 25 percent slopes, eroded","Faywood",3,0.37,"HEL"]
["Adams","Ge","Gessie loam, frequently flooded","Gessie",5,0.37,"NHEL"]
["Adams","JeB","Jessup silt loam, 1 to 8 percent slopes","Jessup",3,0.43,"PHEL"]
["Adams","JeC2","Jessup silt loam, 8 to 15 percent slopes, eroded","Jessup",3,0.43,"HEL"]
["Adams","JeD2","Jessup silt loam, 15 to 25 percent slopes, eroded","Jessup",3,0.43,"HEL"]
["Adams","JeE2","Jessup silt loam, 25 to 35 percent slopes, eroded","Jessup",3,0.43,"HEL"]
["Adams","LbC","Latham silt loam, 8 to 15 percent slopes","Latham",3,0.43,"HEL"]
["Adams","LbD2","Latham silt loam, 15 to 25 percent slopes, eroded","Latham",3,0.43,"HEL"]
["Adams","LkB","Licking silt loam, 1 to 6 percent slopes","Licking",3,0.43,"PHEL"]
["Adams","LkC2","Licking silt loam, 6 to 15 percent slopes, eroded","Licking",3,0.43,"HEL"]
["Adams","LkD2","Licking silt loam, 15 to 25 percent slopes, eroded","Licking",3,0.43,"HEL"]
["Adams","LoA","Loudon silt loam, 0 to 2 percent slopes","Loudon",3,0.43,"NHEL"]
["Adams","LoB","Loudon silt loam, 2 to 6 percent slopes","Loudon",3,0.43,"PHEL"]
["Adams","LoC2","Loudon silt loam, 6 to 15 percent slopes, eroded","Loudon",3,0.43,"HEL"]
["Adams","LwB","Lowell silt loam, 2 to 8 percent slopes","Lowell",3,0.37,"PHEL"]
["Adams","LwC2","Lowell silt loam, 8 to 15 percent slopes, eroded","Lowell",3,0.37,"HEL"]
["Adams","McA","McGary variant silty clay loam, 0 to 3 percent slopes, rarely flooded","McGary",3,0.43,"PHEL"]
["Adams","Ne","Newark silt loam, frequently flooded","Newark",5,0.32,"NHEL"]
["Adams","NkB","Nicholson silt loam, 1 to 6 percent slopes","Nicholson",3,0.43,"PHEL"]
["Adams","No","Nolin silt loam, occasionally flooded","Nolin",5,0.43,"NHEL"]
["Adams","OmB","Omulga silt loam, 1 to 6 percent slopes","Omulga",3,0.43,"PHEL"]
["Adams","OmC2","Omulga silt loam, 6 to 15 percent slopes, eroded","Omulga",3,0.43,"HEL"]
["Adams","OpD2","Opequon silty clay loam, 15 to 25 percent slopes, eroded","Opequon",1,0.43,"HEL"]
["Adams","OpE2","Opequon silty clay loam, 25 to 40 percent slopes, eroded","Opequon",1,0.43,"HEL"]
["Adams","OsF","Opequon silty clay loam, 40 to 60 percent slopes, very rocky","Opequon",1,0.43,"HEL"]
["Adams","OwB","Otwell silt loam, 1 to 6 percent slopes","Otwell",3,0.43,"PHEL"]
["Adams","OwC2","Otwell silt loam, 6 to 15 percent slopes, eroded","Otwell",3,0.43,"HEL"]
["Adams","Pe","Peoga silt loam","Peoga",4,0.43,"NHEL"]
["Adams","Pq","Pits, quarry","Pits"]
["Adams","PtB","Plainfield sand, 3 to 8 percent slopes","Plainsfield",5,0.17,"PHEL"]
["Adams","RoB","Rossmoyne silt loam, 1 to 6 percent slopes","Rossmoyne",4,0.37,"PHEL"]
["Adams","RoC2","Rossmoyne silt loam, 6 to 12 percent slopes, eroded","Rossmoyne",4,0.37,"PHEL"]
["Adams","SaB","Sardinia silt loam, 1 to 6 percent slopes","Sardinia",5,0.37,"PHEL"]
["Adams","ScB","Sciotoville silt loam, 1 to 6 percent slopes","Sciotoville",4,0.37,"PHEL"]
["Adams","ShE","Shelocta-Berks association, steep","Shelocta",4,0.32,"HEL"]
["Adams","ShF","Shelocta-Berks association, very steep","Shelocta",4,0.32,"HEL"]
["Adams","SmD","Shelocta-Muse association, hilly","Shelocta",4,0.32,"HEL"]
["Adams","SoE","Shelocta-Muse-Colyer association, steep","Shelocta",4,0.32,"HEL"]
["Adams","Sp","Skidmore gravelly loam, occasionally flooded","Skidmore",5,0.17,"NHEL"]
["Adams","TkA","Tilsit silt loam, 0 to 3 percent slopes","Tilsit",3,0.43,"PHEL"]
["Adams","TrB","Trappist silt loam, 3 to 8 percent slopes","Trappist",3,0.37,"PHEL"]
["Adams","TrC","Trappist silt loam, 8 to 15 percent slopes","Trappist",3,0.37,"HEL"]
["Adams","TrD2","Trappist silt loam, 15 to 25 percent slopes, eroded","Trappist",3,0.37,"HEL"]
["Adams","Ud","Udorthents, silty","Udorthents"]
["Adams","W","Water","Water"]
["Adams","WgC","Wernock silt loam, 8 to 15 percent slopes","Wernock",3,0.37,"HEL"]
["Adams","WmB","Williamsburg silt loam, 1 to 6 percent slopes","Williamsburg",5,0.32,"PHEL"]
["Adams","WmC2","Williamsburg silt loam, 6 to 15 percent slopes, eroded","Williamsburg",5,0.32,"PHEL"]
[null,"Select","none","none"]
["Athens","BaF","Barkcamp gravelly sandy loam, 40 to 70 percent slopes","Barkcamp",5,0.24,"HEL"]
["Athens","BkD","Berks-Westmoreland silt loams, 15 to 25 percent slopes","Berks",3,0.24,"HEL"]
["Athens","BkE","Berks-Westmoreland silt loams, 25 to 40 percent slopes","Berks",3,0.24,"HEL"]
["Athens","BkF","Berks-Westmoreland silt loams, 40 to 70 percent slopes","Berks",3,0.24,"HEL"]
["Athens","BoD","Bethesda shaly silty clay loam, 8 to 25 percent slopes","Bethesda",5,0.32,"PHEL"]
["Athens","BoE","Bethesda shaly silty clay loam, 25 to 40 percent slopes","Bethesda",5,0.32,"HEL"]
["Athens","BoF","Bethesda shaly silty clay loam, 40 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Athens","BrC","Brookside silt loam, 8 to 15 percent slopes","Brookside",5,0.37,"PHEL"]
["Athens","BrD","Brookside silt loam, 15 to 25 percent slopes","Brookside",5,0.37,"HEL"]
["Athens","BrE","Brookside silt loam, 25 to 40 percent slopes","Brookside",5,0.37,"HEL"]
["Athens","Cd","Chagrin loam, rarely flooded","Chagrin",5,0.32,"NHEL"]
["Athens","Cg","Chagrin silt loam, frequently flooded","Chagrin",5,0.32,"NHEL"]
["Athens","CmC","Clymer loam, 8 to 15 percent slopes","Clymer",3,0.24,"PHEL"]
["Athens","DtD","Dekalb-Westmoreland complex, 15 to 25 percent slopes","Dekalb",2,0.24,"HEL"]
["Athens","DtE","Dekalb-Westmoreland complex, 25 to 40 percent slopes","Dekalb",2,0.24,"HEL"]
["Athens","DtF","Dekalb-Westmoreland complex, 40 to 70 percent slopes","Dekalb",2,0.24,"HEL"]
["Athens","DuF","Dekalb-Westmoreland complex, benched, 40 to 70 percent slopes","Dekalb",2,0.24,"HEL"]
["Athens","DxA","Doles silt loam, 0 to 3 percent slopes","Doles",4,0.43,"NHEL"]
["Athens","Dy","Dumps, mine","Dumps"]
["Athens","EbF","Elba-Brookside-Berks complex, 40 to 70 percent slopes","Elba",3,0.43,"HEL"]
["Athens","FaD","Fairpoint silt loam, 8 to 25 percent slopes","Fairpoint",3,0.43,"HEL"]
["Athens","FbE","Fairpoint shaly clay loam, 25 to 40 percent slopes","Fairpoint",3,0.43,"HEL"]
["Athens","FbF","Fairpoint shaly clay loam, 40 to 70 percent slopes","Fairpoint",3,0.43,"HEL"]
["Athens","FcA","Fitchville silt loam, 0 to 3 percent slopes","Fitchville",5,0.37,"PHEL"]
["Athens","GaC","Gallia loam, 8 to 15 percent slopes","Gallia",5,0.37,"PHEL"]
["Athens","GmA","Glenford silt loam, 0 to 3 percent slopes","Glenford",5,0.37,"NHEL"]
["Athens","GmB","Glenford silt loam, 3 to 8 percent slopes","Glenford",5,0.37,"PHEL"]
["Athens","GmC","Glenford silt loam, 8 to 15 percent slopes","Glenford",5,0.37,"PHEL"]
["Athens","GsB","Guernsey silt loam, 3 to 8 percent slopes","Guernsey",3,0.43,"PHEL"]
["Athens","GsC","Guernsey silt loam, 8 to 15 percent slopes","Guernsey",3,0.43,"HEL"]
["Athens","GuC","Guernsey-Upshur complex, 8 to 15 percent slopes","Guernsey",3,0.43,"HEL"]
["Athens","GuD","Guernsey-Upshur complex, 15 to 25 percent slopes","Guernsey",3,0.43,"HEL"]
["Athens","HcA","Hackers silt loam, 0 to 3 percent slopes","Hackers",4,0.32,"NHEL"]
["Athens","LkB","Licking silt loam, 3 to 8 percent slopes","Licking",3,0.43,"PHEL"]
["Athens","LkC","Licking silt loam, 8 to 15 percent slopes","Licking",3,0.43,"HEL"]
["Athens","McA","McGary silt loam, 0 to 3 percent slopes","McGary",3,0.43,"PHEL"]
["Athens","Mh","Melvin silt loam, frequently flooded","Melvin",5,0.43,"NHEL"]
["Athens","Mp","Moshannon silt loam, frequently flooded","Moshannon",5,0.37,"NHEL"]
["Athens","NeC","Negley loam, 8 to 15 percent slopes","Negley",3,0.32,"HEL"]
["Athens","NgE","Negley gravelly loam, 25 to 40 percent slopes","Negley",3,0.32,"HEL"]
["Athens","Nn","Newark silt loam, frequently flooded","Newark",5,0.32,"NHEL"]
["Athens","No","Nolin silt loam, frequently flooded","Nolin",5,0.43,"NHEL"]
["Athens","Or","Orrville silt loam, frequently flooded","Orrville",5,0.37,"NHEL"]
["Athens","OtB","Omulga silt loam, 3 to 8 percent slopes","Omulga",3,0.43,"PHEL"]
["Athens","OtC","Omulga silt loam, 8 to 15 percent slopes","Omulga",3,0.43,"HEL"]
["Athens","PaB","Parke silt loam, 2 to 6 percent slopes","Parke",5,0.37,"PHEL"]
["Athens","Pg","Pits, gravel","Pits"]
["Athens","RcC","Richland loam, 8 to 15 percent slopes","Richland",5,0.37,"PHEL"]
["Athens","RcD","Richland loam, 15 to 25 percent slopes","Richland",5,0.37,"HEL"]
["Athens","RcE","Richland loam, 25 to 40 percent slopes","Richland",5,0.37,"HEL"]
["Athens","StD","Steinsburg sandy loam, 15 to 25 percent slopes","Steinsburg",2,0.28000000000000003,"HEL"]
["Athens","StE","Steinsburg sandy loam, 25 to 40 percent slopes","Steinsburg",2,0.28000000000000003,"HEL"]
["Athens","StF","Steinsburg sandy loam, 40 to 70 percent slopes","Steinsburg",2,0.28000000000000003,"HEL"]
["Athens","Ud","Udorthents, loamy","Udorthents"]
["Athens","UpC","Upshur silty clay loam, 8 to 15 percent slopes","Upshur",3,0.43,"HEL"]
["Athens","UpD","Upshur silty clay loam, 15 to 25 percent slopes","Upshur",3,0.43,"HEL"]
["Athens","UsC","Upshur-Elba silty clay loams, 8 to 15 percent slopes","Upshur",3,0.43,"HEL"]
["Athens","UsD","Upshur-Elba silty clay loams, 15 to 25 percent slopes","Upshur",3,0.43,"HEL"]
["Athens","VaC","Vandalia silty clay loam, 8 to 15 percent slopes","Vandalia",4,0.37,"PHEL"]
["Athens","VbD","Vandalia-Brookside complex, 15 to 25 percent slopes","Vandalia",4,0.37,"HEL"]
["Athens","VbE","Vandalia-Brookside complex, 25 to 40 percent slopes","Vandalia",4,0.37,"HEL"]
["Athens","VcD","Vandalia-Richland complex, 15 to 25 percent slopes","Vandalia",4,0.37,"HEL"]
["Athens","VcE","Vandalia-Richland complex, 25 to 40 percent slopes","Vandalia",4,0.37,"HEL"]
["Athens","VtC","Vincent silt loam, 6 to 12 percent slopes","Vincent",3,0.43,"HEL"]
["Athens","W","Water","Water"]
["Athens","WdB","Wellston silt loam, 3 to 8 percent slopes","Wellston",4,0.37,"PHEL"]
["Athens","WdC","Wellston silt loam, 8 to 15 percent slopes","Wellston",4,0.37,"PHEL"]
["Athens","WeB","Westmore silt loam, 3 to 8 percent slopes","Westmore",4,0.37,"PHEL"]
["Athens","WeC","Westmore silt loam, 8 to 15 percent slopes","Westmore",4,0.37,"PHEL"]
["Athens","WhC","Westmoreland-Guernsey silt loams, 8 to 15 percent slopes","Westmoreland",3,0.37,"HEL"]
["Athens","WhD","Westmoreland-Guernsey silt loams, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Athens","WhE","Westmoreland-Guernsey silt loams, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Athens","WhF","Westmoreland-Guernsey silt loams, 40 to 70 percent slopes","Westmoreland",3,0.37,"HEL"]
["Athens","WkF","Westmoreland-Guernsey silt loams, benched, 40 to 70 percent slopes","Westmoreland",3,0.37,"HEL"]
["Athens","WmC","Westmoreland-Upshur complex, 8 to 15 percent slopes","Westmoreland",3,0.37,"HEL"]
["Athens","WmD","Westmoreland-Upshur complex, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Athens","WmE","Westmoreland-Upshur complex, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Athens","WmF","Westmoreland-Upshur complex, 40 to 70 percent slopes","Westmoreland",3,0.37,"HEL"]
["Athens","WpB","Wheeling loam, 3 to 10 percent slopes","Wheeling",4,0.37,"PHEL"]
["Athens","WtB","Woodsfield silt loam, 3 to 8 percent slopes","Woodsfield",3,0.43,"PHEL"]
["Athens","WtC","Woodsfield silt loam, 8 to 15 percent slopes","Woodsfield",3,0.43,"HEL"]
["Athens","ZnB","Zanesville silt loam, 3 to 8 percent slopes","Zanesville",3,0.43,"PHEL"]
[null,"Select","None","none"]
["Brown","Ag","Algiers silt loam, frequently flooded","Algiers",5,0.37,"NHEL"]
["Brown","AtC2","Atlas silty clay loam, 6 to 12 percent slopes, eroded","Atlas",3,0.43,"HEL"]
["Brown","AvA","Avonburg silt loam, 0 to 2 percent slopes","Avonburg",4,0.43,"NHEL"]
["Brown","AwB2","Avonburg-Atlas complex, 2 to 6 percent slopes, eroded","Avonburg",4,0.43,"PHEL"]
["Brown","Bc","Blanchester silt loam","Blanchester",5,0.37,"NHEL"]
["Brown","BoD2","Bonnell silt loam, 15 to 25 percent slopes, eroded","Bonnell",3,0.43,"HEL"]
["Brown","BoE","Bonnell silt loam, 25 to 40 percent slopes","Bonnell",3,0.43,"HEL"]
["Brown","BoF","Bonnell silt loam, 40 to 60 percent slopes","Bonnell",3,0.43,"HEL"]
["Brown","BrD3","Bonnell silty clay loam, 15 to 25 percent slopes, severely eroded","Bonnell",3,0.43,"HEL"]
["Brown","ChF","Chili loam, 35 to 70 percent slopes","Chili",4,0.32,"HEL"]
["Brown","CnC2","Cincinnati silt loam, 6 to 12 percent slopes, eroded","Cincinnati",4,0.37,"PHEL"]
["Brown","Ct","Clermont silt loam","Clermont",5,0.37,"NHEL"]
["Brown","EaE","Eden flaggy silt loam, 25 to 40 percent slopes","Eden",3,0.43,"HEL"]
["Brown","EaF","Eden flaggy silt loam, 40 to 70 percent slopes","Eden",3,0.43,"HEL"]
["Brown","EkB","Elkinsville silt loam, 2 to 6 percent slopes","Elkinsville",5,0.37,"PHEL"]
["Brown","EkC2","Elkinsville silt loam, 6 to 12 percent slopes, eroded","Elkinsville",5,0.37,"PHEL"]
["Brown","FdD2","Faywood silt loam, 15 to 25 percent slopes, eroded","Faywood",3,0.37,"HEL"]
["Brown","FeC2","Faywood-Lowell silt loams, 8 to 15 percent slopes, eroded","Faywood",3,0.37,"HEL"]
["Brown","Ge","Genesee silt loam, occasionally flooded","Genesee",5,0.37,"NHEL"]
["Brown","JeC2","Jessup silt loam, 8 to 15 percent slopes, eroded","Jessup",3,0.43,"HEL"]
["Brown","JeD2","Jessup silt loam, 15 to 25 percent slopes, eroded","Jessup",3,0.43,"HEL"]
["Brown","Ju","Jules silt loam, frequently flooded","Jules",5,0.37,"NHEL"]
["Brown","LoB2","Loudon silt loam, 3 to 8 percent slopes, eroded","Loudon",3,0.43,"PHEL"]
["Brown","LwB2","Lowell silt loam, 3 to 8 percent slopes, eroded","Lowell",3,0.37,"PHEL"]
["Brown","No","Nolin silt loam, occasionally flooded","Nolin",5,0.43,"NHEL"]
["Brown","PaC2","Pate silty clay, 8 to 15 percent slopes, eroded","Pate",3,0.37,"HEL"]
["Brown","PaD2","Pate silty clay, 15 to 25 percent slopes, eroded","Pate",3,0.37,"HEL"]
["Brown","PaE2","Pate silty clay, 25 to 35 percent slopes, eroded","Pate",3,0.37,"HEL"]
["Brown","RpB","Rossmoyne silt loam, 1 to 6 percent slopes","Rossmoyne",4,0.37,"PHEL"]
["Brown","RpC2","Rossmoyne silt loam, 6 to 12 percent slopes, eroded","Rossmoyne",4,0.37,"PHEL"]
["Brown","RwC3","Rossmoyne-Bonnell complex, 6 to 12 percent slopes, severely eroded","Rossmoyne",3,0.37,"HEL"]
["Brown","SaB","Sardinia silt loam, 1 to 6 percent slopes","Sardinia",5,0.37,"PHEL"]
["Brown","ScA","Sciotoville silt loam, 0 to 2 percent slopes","Sciotoville",4,0.37,"NHEL"]
["Brown","Sh","Shoals silt loam, frequently flooded","Shoals",5,0.37,"NHEL"]
["Brown","W","Water","Water"]
["Brown","WvB","Williamsburg silt loam, 2 to 6 percent slopes","Williamsburg",5,0.32,"PHEL"]
[null,"Select","None","none"]
["Delaware","AdC","Alexandria silt loam, 6 to 12 percent slopes","Alexandria",4,0.37,"PHEL"]
["Delaware","AdC2","Alexandria silt loam, 6 to 12 percent slopes, moderately eroded","Alexandria",4,0.37,"PHEL"]
["Delaware","AdD","Alexandria silt loam, 12 to 18 percent slopes","Alexandria",4,0.37,"HEL"]
["Delaware","AdD2","Alexandria silt loam, 12 to 18 percent slopes, moderately eroded","Alexandria",4,0.37,"HEL"]
["Delaware","AdE","Alexandria silt loam, 18 to 25 percent slopes","Alexandria",4,0.37,"HEL"]
["Delaware","AdE2","Alexandria silt loam, 18 to 25 percent slopes, moderately eroded","Alexandria",4,0.37,"HEL"]
["Delaware","AeC3","Alexandria soils, 6 to 12 percent slopes, severely eroded","Alexandria",4,0.37,"PHEL"]
["Delaware","AeE3","Alexandria soils, 12 to 25 percent slopes, severely eroded","Alexandria",4,0.37,"HEL"]
["Delaware","AmF2","Alexandria and Morley silt loams, 25 to 40 percent slopes, moderately eroded","Alexandria",4,0.37,"HEL"]
["Delaware","As","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Delaware","BeA","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Delaware","BeB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Delaware","BeB2","Bennington silt loam, 2 to 6 percent slopes, moderately eroded","Bennington",3,0.43,"PHEL"]
["Delaware","BgA","Bennington silt loam, shale substratum, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Delaware","BgB","Bennington silt loam, shale substratum, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Delaware","BlA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Delaware","BlB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Delaware","Bo","Bonpas silty clay loam","Bonpass",5,0.28000000000000003,"NHEL"]
["Delaware","Bp","Borrow pit","Borrow"]
["Delaware","CaB","Cardington silt loam, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Delaware","CaB2","Cardington silt loam, 2 to 6 percent slopes, moderately eroded","Cardington",4,0.37,"PHEL"]
["Delaware","CaC","Cardington silt loam, 6 to 12 percent slopes","Cardington",4,0.37,"PHEL"]
["Delaware","CaC2","Cardington silt loam, 6 to 12 percent slopes, moderately eroded","Cardington",4,0.37,"PHEL"]
["Delaware","CfE2","Casco-Fox loams, 12 to 25 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Delaware","ClF","Colyer silt loam, 25 to 50 percent slopes","Colyer",2,0.37,"HEL"]
["Delaware","CnA","Condit silt loam, 0 to 2 percent slopes","Condit",5,0.37,"NHEL"]
["Delaware","Ee","Eel silt loam","Eel",5,0.37,"NHEL"]
["Delaware","FlA","Fox loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Delaware","FlB","Fox loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Delaware","FnA","Fox silt loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Delaware","FnB","Fox silt loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Delaware","FnB2","Fox silt loam, 2 to 6 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Delaware","FnC","Fox silt loam, 6 to 12 percent slopes","Fox",4,0.37,"PHEL"]
["Delaware","FnC2","Fox silt loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Delaware","FnD2","Fox silt loam, 12 to 18 percent slopes, moderately eroded","Fox",4,0.37,"HEL"]
["Delaware","Gn","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Delaware","Go","Genesee silt loam, shallow variant","Genesee",2,0.37,"NHEL"]
["Delaware","Gp","Gravel pit","Gravel"]
["Delaware","LoB","Loudonville silt loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Delaware","LoC2","Loudonville silt loam, 6 to 12 percent slopes, moderately eroded","Loudonville",4,0.32,"PHEL"]
["Delaware","LsF","Loudonville silt loam, shallow variant, 25 to 50 percent slopes","Loudonville",4,0.37,"HEL"]
["Delaware","Ma","Made land","Made"]
["Delaware","Mc","Marsh","Marsh"]
["Delaware","MgA","McGary silt loam, 0 to 2 percent slopes","McGary",3,0.43,"NHEL"]
["Delaware","Mn","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Delaware","MoA","Milton silt loam, 0 to 2 percent slopes","Milton",4,0.37,"NHEL"]
["Delaware","MoB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Delaware","MoB2","Milton silt loam, 2 to 6 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Delaware","MoC2","Milton silt loam, 6 to 12 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Delaware","MoD2","Milton silt loam, 12 to 18 percent slopes, moderately eroded","Milton",4,0.37,"HEL"]
["Delaware","MrB","Morley silt loam, 2 to 6 percent slopes","Morley",3,0.43,"PHEL"]
["Delaware","MrB2","Morley silt loam, 2 to 6 percent slopes, moderately eroded","Morley",3,0.43,"PHEL"]
["Delaware","MrC","Morley silt loam, 6 to 12 percent slopes","Morley",3,0.43,"HEL"]
["Delaware","MrC2","Morley silt loam, 6 to 12 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Delaware","MrD","Morley silt loam, 12 to 18 percent slopes","Morley",3,0.43,"HEL"]
["Delaware","MrD2","Morley silt loam, 12 to 18 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Delaware","MrE2","Morley silt loam, 18 to 25 percent slopes, moderately eroded","Morley",3,0.43,"HEL"]
["Delaware","MsC3","Morley soils, 6 to 12 percent slopes, severely eroded","Morley",2,0.43,"HEL"]
["Delaware","MsD3","Morley soils, 12 to 18 percent slopes, severely eroded","Morley",2,0.43,"HEL"]
["Delaware","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Delaware","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Delaware","OcB2","Ockley silt loam, 2 to 6 percent slopes, moderately eroded","Ockley",5,0.37,"PHEL"]
["Delaware","OcC","Ockley silt loam, 6 to 12 percent slopes","Ockley",5,0.37,"PHEL"]
["Delaware","OcC2","Ockley silt loam, 6 to 12 percent slopes, moderately eroded","Ockley",5,0.37,"PHEL"]
["Delaware","OcD2","Ockley silt loam, 12 to 18 percent slopes, moderately eroded","Ockley",5,0.37,"HEL"]
["Delaware","OsB","Ockley silt loam, till substratum, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Delaware","Pw","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Delaware","Qu","Quarry","Quarry"]
["Delaware","RaA","Randolph silt loam, 0 to 2 percent slopes","Randolph",3,0.37,"NHEL"]
["Delaware","RdB2","Rarden silt loam, 2 to 6 percent slopes, moderately eroded","Rarden",3,0.43,"PHEL"]
["Delaware","RdC2","Rarden silt loam, 6 to 12 percent slopes, moderately eroded","Rarden",3,0.43,"HEL"]
["Delaware","RdE","Rarden silt loam, 12 to 25 percent slopes","Rarden",3,0.43,"HEL"]
["Delaware","RdF","Rarden silt loam, 25 to 40 percent slopes","Rarden",3,0.43,"HEL"]
["Delaware","RhB","Ritchey silt loam, 2 to 6 percent slopes","Ritchey",2,0.37,"PHEL"]
["Delaware","RhC2","Ritchey silt loam, 6 to 12 percent slopes, moderately eroded","Ritchey",2,0.37,"HEL"]
["Delaware","RhE2","Ritchey silt loam, 12 to 25 percent slopes, moderately eroded","Ritchey",2,0.37,"HEL"]
["Delaware","Rk","Rock land, limestone, steep","Rock"]
["Delaware","Rn","Ross silt loam","Ross",5,0.32,"NHEL"]
["Delaware","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Delaware","SlA","Sleeth silt loam, 0 to 2 percent slopes","Sleeth",5,0.32,"NHEL"]
["Delaware","SlB","Sleeth silt loam, 2 to 6 percent slopes","Sleeth",5,0.32,"HEL"]
["Delaware","So","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Delaware","ThA","Thackery silt loam, 0 to 2 percent slopes","Thackery",4,0.37,"NHEL"]
["Delaware","ThB","Thackery silt loam, 2 to 6 percent slopes","Thackery",4,0.37,"PHEL"]
["Delaware","Wu","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
["Delaware","Wv","Willette muck","Willette",2,null,"NHEL"]
[null,"Select","None","none"]
["Fairfield","AaA1","Alexandria silt loam, 0 to 2 percent slopes","Alexandria",4,0.37,"NHEL"]
["Fairfield","AaB1","Alexandria silt loam, 2 to 6 percent slopes, slightly eroded","Alexandria",4,0.37,"PHEL"]
["Fairfield","AaB2","Alexandria silt loam, 2 to 6 percent slopes, moderately eroded","Alexandria",4,0.37,"PHEL"]
["Fairfield","AaC1","Alexandria silt loam, 6 to 12 percent slopes, slightly eroded","Alexandria",4,0.37,"PHEL"]
["Fairfield","AaC2","Alexandria silt loam, 6 to 12 percent slopes, moderately eroded","Alexandria",4,0.37,"PHEL"]
["Fairfield","AaD1","Alexandria silt loam, 12 to 18 percent slopes, slightly eroded","Alexandria",4,0.37,"HEL"]
["Fairfield","AaD2","Alexandria silt loam, 12 to 18 percent slopes, moderately eroded","Alexandria",4,0.37,"HEL"]
["Fairfield","AaE1","Alexandria silt loam, 18 to 25 percent slopes, slightly eroded","Alexandria",4,0.37,"HEL"]
["Fairfield","AaE2","Alexandria silt loam, 18 to 25 percent slopes, moderately eroded","Alexandria",4,0.37,"HEL"]
["Fairfield","AaF2","Alexandria silt loam, 25 to 50 percent slopes, moderately eroded","Alexandria",4,0.37,"HEL"]
["Fairfield","AbC3","Alexandria silty clay loam, 6 to 12 percent slopes, severely eroded","Alexandria",4,0.37,"PHEL"]
["Fairfield","AbD3","Alexandria silty clay loam, 12 to 18 percent slopes, severely eroded","Alexandria",4,0.37,"HEL"]
["Fairfield","AbE3","Alexandria silty clay loam, 18 to 25 percent slopes, severely eroded","Alexandria",4,0.37,"HEL"]
["Fairfield","AcA0","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Fairfield","AdA0","Algiers silty clay loam","Algiers",5,0.37,"NHEL"]
["Fairfield","BaA0","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Fairfield","BaB1","Bennington silt loam, 2 to 6 percent slopes, slightly eroded","Bennington",3,0.43,"PHEL"]
["Fairfield","BaB2","Bennington silt loam, 2 to 6 percent slopes, moderately eroded","Bennington",3,0.43,"PHEL"]
["Fairfield","BbA0","Brookston clay loam","Brookston",5,0.28000000000000003,"NHEL"]
["Fairfield","CaA1","Cardington silt loam , 0 to 2 percent slopes","Cardington",4,0.37,"NHEL"]
["Fairfield","CaB1","Cardington silt loam, 2 to 6 percent slopes, slightly eroded","Cardington",4,0.37,"PHEL"]
["Fairfield","CaB2","Cardington silt loam, 2 to 6 percent slopes, moderately eroded","Cardington",4,0.37,"PHEL"]
["Fairfield","CaC1","Cardington silt loam, 6 to 12 percent slopes, slightly eroded","Cardington",4,0.37,"PHEL"]
["Fairfield","CaC2","Cardington silt loam, 6 to 12 percent slopes, moderately eroded","Cardington",4,0.37,"PHEL"]
["Fairfield","CaD2","Cardington silt loam, 12 to 18 percent slopes, moderately eroded","Cardington",4,0.37,"HEL"]
["Fairfield","CbA0","Carlisle muck","Carlisle",2,null,"NHEL"]
["Fairfield","CcE3","Casco clay loam, 18 to 25 percent slopes, severely eroded","Casco",3,0.24,"HEL"]
["Fairfield","CdD2","Casco gravelly loam, 12 to 18 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Fairfield","CeE2","Casco loam, 18 to 25 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Fairfield","CgF2","Casco and Rodman loams, 25 to 40 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Fairfield","ChA1","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Fairfield","ChB1","Celina silt loam, 2 to 6 percent slopes, slightly eroded","Celina",5,0.37,"PHEL"]
["Fairfield","ChB2","Celina silt loam, 2 to 6 percent slopes, moderately eroded","Celina",5,0.37,"PHEL"]
["Fairfield","CkA0","Chagrin fine sandy loam","Chagrin",5,0.32,"NHEL"]
["Fairfield","CmA0","Chagrin silt loam","Chagrin",5,0.32,"NHEL"]
["Fairfield","CnA0","Condit silt loam","Condit",5,0.37,"NHEL"]
["Fairfield","CoA0","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Fairfield","CoB1","Crosby silt loam, 2 to 6 percent slopes, slightly eroded","Crosby",3,0.43,"PHEL"]
["Fairfield","EaA0","Eel loam","Eel",5,0.37,"NHEL"]
["Fairfield","EbA0","Eel silt loam","Eel",5,0.37,"NHEL"]
["Fairfield","FaD3","Fox clay loam, 12 to 18 percent slopes, severely eroded","Fox",3,0.37,"HEL"]
["Fairfield","FbC3","Fox gravelly clay loam, 6 to 12 percent slopes, severely eroded","Fox",3,0.37,"PHEL"]
["Fairfield","FcA1","Fox gravelly loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Fairfield","FcB1","Fox gravelly loam, 2 to 6 percent slopes, slightly eroded","Fox",4,0.37,"PHEL"]
["Fairfield","FcB2","Fox gravelly loam, 2 to 6 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Fairfield","FcC2","Fox gravelly loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Fairfield","FdA1","Fox loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Fairfield","FdB1","Fox loam, 2 to 6 percent slopes, slightly eroded","Fox",4,0.37,"PHEL"]
["Fairfield","FdB2","Fox loam, 2 to 6 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Fairfield","FdC2","Fox loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Fairfield","FdD2","Fox loam, 12 to 18 percent slopes, moderately eroded","Fox",4,0.37,"HEL"]
["Fairfield","FeA1","Fox silt loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Fairfield","FeB1","Fox silt loam, 2 to 6 percent slopes, slightly eroded","Fox",4,0.37,"PHEL"]
["Fairfield","FeB2","Fox silt loam, 2 to 6 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Fairfield","FeC1","Fox silt loam, 6 to 12 percent slopes, slightly eroded","Fox",4,0.37,"PHEL"]
["Fairfield","FeC2","Fox silt loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Fairfield","FgC3","Fox silty clay loam, 6 to 12 percent slopes, severely eroded","Fox",3,0.37,"PHEL"]
["Fairfield","GaA0","Genesee loam","Genesee",5,0.37,"NHEL"]
["Fairfield","GbA0","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Fairfield","Gc","Gravel and sand pits","Gravel"]
["Fairfield","HaB1","Hanover silt loam, 2 to 6 percent slopes, slightly eroded","Hanover",5,0.37,"PHEL"]
["Fairfield","HaB2","Hanover silt loam, 2 to 6 percent slopes, moderately eroded","Hanover",5,0.37,"PHEL"]
["Fairfield","HaC1","Hanover silt loam, 6 to 12 percent slopes, slightly eroded","Hanover",5,0.37,"PHEL"]
["Fairfield","HaC2","Hanover silt loam, 6 to 12 percent slopes, moderately eroded","Hanover",5,0.37,"PHEL"]
["Fairfield","HaD1","Hanover silt loam, 12 to 18 percent slopes, slightly eroded","Hanover",5,0.37,"HEL"]
["Fairfield","HaD2","Hanover silt loam, 12 to 18 percent slopes, moderately eroded","Hanover",5,0.37,"HEL"]
["Fairfield","HaD3","Hanover silt loam, 12 to 18 percent slopes, severely eroded","Hanover",4,0.37,"HEL"]
["Fairfield","KaC2","Keene silt loam, shallow, 2 to 12 percent slopes, slightly to moderately eroded","Keene",4,0.37,"PHEL"]
["Fairfield","KbD3","Keene silty clay loam, shallow, 12 to 18 percent slopes, severely eroded","Keene",4,0.37,"HEL"]
["Fairfield","KcA1","Kendallville silt loam, 0 to 2 percent slopes","Kendallville",3,0.37,"NHEL"]
["Fairfield","KcB1","Kendallville silt loam, 2 to 6 percent slopes, slightly eroded","Kendallville",3,0.37,"PHEL"]
["Fairfield","KcB2","Kendallville silt loam, 2 to 6 percent slopes, moderately eroded","Kendallville",3,0.37,"PHEL"]
["Fairfield","KcC2","Kendallville silt loam, 6 to 12 percent slopes, moderately eroded","Kendallville",3,0.37,"PHEL"]
["Fairfield","KcD2","Kendallville silt loam, 12 to 18 percent slopes, moderately to severely eroded","Kendallville",3,0.37,"HEL"]
["Fairfield","LaA0","Lobdell fine sandy loam","Lobdell",5,0.37,"NHEL"]
["Fairfield","LbA0","Lobdell silt loam","Lobdell",5,0.37,"NHEL"]
["Fairfield","LcB1","Loudonville silt loam, 2 to 6 percent slopes, slightly eroded","Loudonville",4,0.32,"PHEL"]
["Fairfield","LcB2","Loudonville silt loam, 2 to 6 percent slopes, moderately eroded","Loudonville",4,0.32,"PHEL"]
["Fairfield","LcC1","Loudonville silt loam, 6 to 12 percent slopes, slightly eroded","Loudonville",4,0.32,"PHEL"]
["Fairfield","LcC2","Loudonville silt loam, 6 to 12 percent slopes, moderately eroded","Loudonville",4,0.32,"PHEL"]
["Fairfield","LcC3","Loudonville silt loam, 6 to 12 percent slopes, severely eroded","Loudonville",4,0.32,"PHEL"]
["Fairfield","LcD1","Loudonville silt loam, 12 to 18 percent slopes, slightly eroded","Loudonville",4,0.32,"HEL"]
["Fairfield","LcD2","Loudonville silt loam, 12 to 18 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Fairfield","LcD3","Loudonville silt loam, 12 to 18 percent slopes, severely eroded","Loudonville",4,0.32,"HEL"]
["Fairfield","LcE1","Loudonville silt loam, 18 to 25 percent slopes, slightly eroded","Loudonville",4,0.32,"HEL"]
["Fairfield","LcE2","Loudonville silt loam, 18 to 25 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Fairfield","LcE3","Loudonville silt loam, 18 to 25 percent slopes, severely eroded","Loudonville",4,0.32,"HEL"]
["Fairfield","LcF2","Loudonville silt loam, 25 to 50 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Fairfield","Ma","Made land","Made"]
["Fairfield","MbA0","Marengo silt loam","Marengo",5,0.28000000000000003,"NHEL"]
["Fairfield","McA0","Marengo silty clay loam","Marengo",5,0.28000000000000003,"NHEL"]
["Fairfield","MdA1","Markland and Glenford silt loams, 0 to 2 percent slopes","Markland",3,0.43,"NHEL"]
["Fairfield","MdB1","Markland and Glenford silt loams, 2 to 6 percent slopes, slightly eroded","Markland",3,0.43,"PHEL"]
["Fairfield","MdB2","Markland and Glenford silt loams, 2 to 6 percent slopes, moderately eroded","Markland",3,0.43,"PHEL"]
["Fairfield","MeA0","McGary and Fitchville loams, 0 to 2 percent slopes","McGary",3,0.43,"NHEL"]
["Fairfield","MgA1","McGary and Fitchville silt loams, 0 to 2 percent slopes","McGary",3,0.43,"NHEL"]
["Fairfield","MgB1","McGary and Fitchville silt loams, 2 to 6 percent slopes, slightly eroded","McGary",3,0.43,"PHEL"]
["Fairfield","MhA0","McGary and Sebring silt loams, 0 to 2 percent slopes","McGary",3,0.43,"NHEL"]
["Fairfield","MkA0","Mentor silt loam, 0 to 2 percent slopes","Mentor",5,0.37,"NHEL"]
["Fairfield","MkB1","Mentor silt loam, 2 to 6 percent slopes, slightly eroded","Mentor",5,0.37,"PHEL"]
["Fairfield","MkB2","Mentor silt loam, 2 to 6 percent slopes, moderately eroded","Mentor",5,0.37,"PHEL"]
["Fairfield","MkC1","Mentor silt loam, 6 to 12 percent slopes, slightly eroded","Mentor",5,0.37,"PHEL"]
["Fairfield","MkC2","Mentor silt loam, 6 to 12 percent slopes, moderately eroded","Mentor",5,0.37,"PHEL"]
["Fairfield","MkD2","Mentor silt loam, 12 to 18 percent slopes, moderately eroded","Mentor",5,0.37,"HEL"]
["Fairfield","MmB1","Miami silt loam, 2 to 6 percent slopes, slightly eroded","Miami",5,0.37,"PHEL"]
["Fairfield","MmB2","Miami silt loam, 2 to 6 percent slopes, moderately eroded","Miami",5,0.37,"PHEL"]
["Fairfield","MmC2","Miami silt loam, 6 to 12 percent slopes, moderately eroded","Miami",5,0.37,"PHEL"]
["Fairfield","MmD2","Miami silt loam, 12 to 18 percent slopes, moderately eroded","Miami",5,0.37,"HEL"]
["Fairfield","MnC3","Miami silty clay loam, 6 to 12 percent slopes, severely eroded","Miami",4,0.37,"PHEL"]
["Fairfield","MnD3","Miami silty clay loam, 12 to 18 percent slopes, severely eroded","Miami",4,0.37,"HEL"]
["Fairfield","MoA0","Montgomery silt loam","Montgomery",5,0.37,"NHEL"]
["Fairfield","MpA0","Montgomery silty clay loam","Montgomery",5,0.37,"NHEL"]
["Fairfield","MrC1","Muskingum fine and very fine sandy loams, 6 to 12 percent slopes, slightly to moderately eroded","Muskingum",3,0.37,"PHEL"]
["Fairfield","MrD2","Muskingum fine and very fine sandy loams, 12 to 18 percent slopes, slightly to moderately eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MrE2","Muskingum fine and very fine sandy loams, 18 to 25 percent slopes, slightly to moderately eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MsD2","Muskingum rocky sandy loam, 6 to 18 percent slopes, slightly to moderately eroded","Muskingum",3,0.37,"PHEL"]
["Fairfield","MsE1","Muskingum rocky sandy loam, 18 to 25 percent slopes, slightly to moderately eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MsG1","Muskingum rocky sandy loam, 25 to 50 percent slopes, slightly to moderately eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MtB1","Muskingum sandy loam, 2 to 6 percent slopes, slightly to moderately eroded","Muskingum",3,0.37,"PHEL"]
["Fairfield","MtC1","Muskingum sandy loam, 6 to 12 percent slopes, slightly eroded","Muskingum",3,0.37,"PHEL"]
["Fairfield","MtC2","Muskingum sandy loam, 6 to 12 percent slopes, moderately eroded","Muskingum",3,0.37,"PHEL"]
["Fairfield","MtD1","Muskingum sandy loam, 12 to 18 percent slopes","Muskingum",3,0.37,"HEL"]
["Fairfield","MtD2","Muskingum sandy loam, 12 to 18 percent slopes, moderately eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MtD3","Muskingum sandy loam, 12 to 18 percent slopes, severely eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MtE1","Muskingum sandy loam, 18 to 25 percent slopes, slightly eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MtE2","Muskingum sandy loam, 18 to 25 percent slopes, moderately eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MtE3","Muskingum sandy loam, 18 to 25 percent slopes, severely eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MtF1","Muskingum sandy loam, 25 to 50 percent slopes, slightly eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MtF2","Muskingum sandy loam, 25 to 50 percent slopes, moderately eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MuB1","Muskingum silt loam, 2 to 6 percent slopes, slightly to moderately eroded","Muskingum",3,0.37,"PHEL"]
["Fairfield","MuC1","Muskingum silt loam, 6 to 12 percent slopes, slightly eroded","Muskingum",3,0.37,"PHEL"]
["Fairfield","MuC2","Muskingum silt loam, 6 to 12 percent slopes, moderately eroded","Muskingum",3,0.37,"PHEL"]
["Fairfield","MuC3","Muskingum silt loam, 6 to 12 percent slopes, severely eroded","Muskingum",3,0.37,"PHEL"]
["Fairfield","MuD1","Muskingum silt loam, 12 to 18 percent slopes, slightly eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MuD2","Muskingum silt loam, 12 to 18 percent slopes, moderately eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MuD3","Muskingum silt loam, 12 to 18 percent slopes, severely eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MuE1","Muskingum silt loam, 18 to 25 percent slopes, slightly eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MuE2","Muskingum silt loam, 18 to 25 percent slopes, moderately eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MuE3","Muskingum silt loam, 18 to 25 percent slopes, severely eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MuF1","Muskingum silt loam, 25 to 50 percent slopes, slightly eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","MuF2","Muskingum silt loam, 25 to 50 percent slopes, moderately to severely eroded","Muskingum",3,0.37,"HEL"]
["Fairfield","NaC2","Negley gravelly and sandy loams, 6 to 12 percent slopes, moderately eroded","Negley",3,0.32,"PHEL"]
["Fairfield","NaD2","Negley gravelly and sandy loams, 12 to 18 percent slopes, moderately eroded","Negley",3,0.32,"HEL"]
["Fairfield","NaD3","Negley gravelly and sandy loams, 12 to 18 percent slopes, severely eroded","Negley",2,0.32,"HEL"]
["Fairfield","NaE1","Negley gravelly and sandy loams, 18 to 25 percent slopes, slightly eroded","Negley",3,0.32,"HEL"]
["Fairfield","NaE2","Negley gravelly and sandy loams, 18 to 25 percent slopes, moderately eroded","Negley",3,0.32,"HEL"]
["Fairfield","NaE3","Negley gravelly and sandy loams, 18 to 25 percent slopes, severely eroded","Negley",2,0.32,"HEL"]
["Fairfield","NaF1","Negley gravelly and sandy loams, 25 to 50 percent slopes, slightly eroded","Negley",3,0.32,"HEL"]
["Fairfield","NaF2","Negley gravelly and sandy loams, 25 to 50 percent slopes, moderately eroded","Negley",3,0.32,"HEL"]
["Fairfield","NaF3","Negley gravelly and sandy loams, 25 to 50 percent slopes, severely eroded","Negley",2,0.32,"HEL"]
["Fairfield","OaA1","Ockley loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Fairfield","OaB1","Ockley loam, 2 to 6 percent slopes, slightly eroded","Ockley",5,0.37,"PHEL"]
["Fairfield","OaB2","Ockley loam, 2 to 6 percent slopes, moderately eroded","Ockley",5,0.37,"PHEL"]
["Fairfield","ObA1","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Fairfield","ObB1","Ockley silt loam, 2 to 6 percent slopes, slightly eroded","Ockley",5,0.37,"PHEL"]
["Fairfield","ObB2","Ockley silt loam, 2 to 6 percent slopes, moderately eroded","Ockley",5,0.37,"PHEL"]
["Fairfield","ObC1","Ockley silt loam, 6 to 12 percent slopes, slightly eroded","Ockley",5,0.37,"PHEL"]
["Fairfield","ObC2","Ockley silt loam, 6 to 12 percent slopes, moderately eroded","Ockley",5,0.37,"PHEL"]
["Fairfield","OcA0","Orrville fine sandy loam","Orrville",5,0.37,"NHEL"]
["Fairfield","OdA0","Orrville silt loam","Orrville",5,0.37,"NHEL"]
["Fairfield","OeB2","Otwell silt loam, 2 to 6 percent slopes, slightly to moderately eroded","Otwell",3,0.43,"PHEL"]
["Fairfield","OeC1","Otwell silt loam, 6 to 12 percent slopes, slightly eroded","Otwell",3,0.43,"HEL"]
["Fairfield","OeC2","Otwell silt loam, 6 to 12 percent slopes, moderately eroded","Otwell",3,0.43,"HEL"]
["Fairfield","OeD2","Otwell silt loam, 12 to 18 percent slopes, moderately eroded","Otwell",3,0.43,"HEL"]
["Fairfield","OeE2","Otwell silt loam, 18 to 25 percent slopes, moderately eroded","Otwell",3,0.43,"HEL"]
["Fairfield","PaB1","Parke silt loam, 2 to 6 percent slopes, slightly eroded","Parke",5,0.37,"PHEL"]
["Fairfield","PaB2","Parke silt loam, 2 to 6 percent slopes, moderately eroded","Parke",5,0.37,"PHEL"]
["Fairfield","PaC1","Parke silt loam, 6 to 12 percent slopes, slightly eroded","Parke",5,0.37,"PHEL"]
["Fairfield","PaC2","Parke silt loam, 6 to 12 percent slopes, moderately eroded","Parke",5,0.37,"PHEL"]
["Fairfield","PaD1","Parke silt loam, 12 to 18 percent slopes, slightly eroded","Parke",5,0.37,"HEL"]
["Fairfield","PaD2","Parke silt loam, 12 to 18 percent slopes, moderately eroded","Parke",5,0.37,"HEL"]
["Fairfield","PaE1","Parke silt loam, 18 to 25 percent slopes, slightly eroded","Parke",5,0.37,"HEL"]
["Fairfield","PaE2","Parke silt loam, 18 to 25 percent slopes, moderately eroded","Parke",5,0.37,"HEL"]
["Fairfield","PbD3","Parke silty clay loam, 12 to 18 percent slopes, severely eroded","Parke",4,0.37,"HEL"]
["Fairfield","PbE3","Parke silty clay loam, 18 to 25 percent slopes, severely eroded","Parke",4,0.37,"HEL"]
["Fairfield","PcA1","Pike silt loam, 0 to 2 percent slopes","Pike",5,0.37,"NHEL"]
["Fairfield","PcB1","Pike silt loam, 2 to 6 percent slopes","Pike",5,0.37,"PHEL"]
["Fairfield","PcB2","Pike silt loam, 2 to 6 percent slopes, moderately eroded","Pike",5,0.37,"PHEL"]
["Fairfield","PcC2","Pike silt loam, 6 to 12 percent slopes, moderately eroded","Pike",5,0.37,"PHEL"]
["Fairfield","Ra","Riverwash","Riverwash"]
["Fairfield","RbA0","Ross silt loam","Ross",5,0.32,"NHEL"]
["Fairfield","SaA0","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Fairfield","SbA1","Sleeth silt loam, 0 to 2 percent slopes","Sleeth",5,0.32,"NHEL"]
["Fairfield","SbB1","Sleeth silt loam, 2 to 6 percent slopes, slightly eroded","Sleeth",5,0.32,"PHEL"]
["Fairfield","ScA0","Sloan silt loam","Sloan",5,0.37,"NHEL"]
["Fairfield","SdA0","Sloan silty clay loam","Sloan",5,0.37,"NHEL"]
["Fairfield","TaA1","Thackery silt loam, 0 to 2 percent slopes","Thackery",4,0.37,"NHEL"]
["Fairfield","TaB1","Thackery silt loam, 2 to 6 percent slopes, slightly eroded","Thackery",4,0.37,"PHEL"]
["Fairfield","TbA1","Tippecanoe silt loam","Tippecanoe",5,0.32,"NHEL"]
["Fairfield","WaA0","Wallkill silt loam","Wallkill",5,0.32,"NHEL"]
["Fairfield","WbA0","Wallkill silty clay loam","Wallkill",5,0.32,"NHEL"]
["Fairfield","WcA0","Warsaw silt loam, 0 to 2 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
["Fairfield","WcB1","Warsaw silt loam, 2 to 6 percent slopes, slightly eroded","Warsaw",4,0.28000000000000003,"PHEL"]
["Fairfield","WdA1","Wea silt loam, 0 to 2 percent slopes","Wea",5,0.32,"NHEL"]
["Fairfield","WdB1","Wea silt loam, 2 to 6 percent slopes, slightly eroded","Wea",5,0.32,"PHEL"]
["Fairfield","WeB1","Wellston silt loam, 2 to 6 percent slopes, slightly eroded","Wellston",4,0.37,"PHEL"]
["Fairfield","WeC1","Wellston silt loam, 6 to 12 percent slopes, slightly eroded","Wellston",4,0.37,"PHEL"]
["Fairfield","WeC2","Wellston silt loam, 6 to 12 percent slopes, moderately eroded","Wellston",4,0.37,"PHEL"]
["Fairfield","WeD2","Wellston silt loam, 12 to 18 percent slopes, slightly to moderately eroded","Wellston",4,0.37,"HEL"]
["Fairfield","WgA0","Westland silt loam","Westland",5,0.28000000000000003,"NHEL"]
["Fairfield","WhA0","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
["Fairfield","WkA0","Willette muck","Willette",2,null,"NHEL"]
[null,"Select","None","none"]
["Franklin","AdB","Alexandria silt loam, 2 to 6 percent slopes","Alexandria",4,0.37,"PHEL"]
["Franklin","AdC2","Alexandria silt loam, 6 to 12 percent slopes, eroded","Alexandria",4,0.37,"PHEL"]
["Franklin","AdD2","Alexandria silt loam, 12 to 18 percent slopes, eroded","Alexandria",4,0.37,"HEL"]
["Franklin","AdE2","Alexandria silt loam, 18 to 25 percent slopes, eroded","Alexandria",4,0.37,"HEL"]
["Franklin","Ag","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Franklin","BeA","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Franklin","BeB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Franklin","BfA","Bennington-Urban land complex, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Franklin","BfB","Bennington-Urban land complex, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Franklin","BoA","Blount silt loam, 0 to 2 percent slopes","Blount",3,0.43,"NHEL"]
["Franklin","BoB","Blount silt loam, 2 to 6 percent slopes","Blount",3,0.43,"PHEL"]
["Franklin","CaB","Cardington silt loam, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Franklin","CaB2","Cardington silt loam, 2 to 6 percent slopes, eroded","Cardington",4,0.37,"PHEL"]
["Franklin","CaC2","Cardington silt loam, 6 to 12 percent slopes, eroded","Cardington",4,0.37,"PHEL"]
["Franklin","CbB","Cardington-Urban land complex, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Franklin","CbC","Cardington-Urban land complex, 6 to 12 percent slopes","Cardington",4,0.37,"PHEL"]
["Franklin","Cc","Carlisle muck","Carlisle",2,null,"NHEL"]
["Franklin","CeA","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Franklin","CeB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Franklin","CeB2","Celina silt loam, 2 to 6 percent slopes, eroded","Celina",5,0.37,"PHEL"]
["Franklin","CeC2","Celina silt loam, 6 to 12 percent slopes, eroded","Celina",5,0.37,"PHEL"]
["Franklin","CfB","Celina-Urban land complex, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Franklin","Cn","Condit silt loam","Condit",5,0.37,"NHEL"]
["Franklin","CpA","Crane silt loam, 0 to 2 percent slopes","Crane",5,0.28000000000000003,"NHEL"]
["Franklin","CrA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Franklin","CrB","Crosby silt loam, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Franklin","CsA","Crosby-Urban land complex, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Franklin","CsB","Crosby-Urban land complex, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Franklin","DAM","Dam","Dam"]
["Franklin","Ee","Eel silt loam, occasionally flooded","Eel",5,0.37,"NHEL"]
["Franklin","ElA","Eldean silt loam, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Franklin","ElB","Eldean silt loam, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Franklin","ElC2","Eldean silt loam, 6 to 12 percent slopes, eroded","Eldean",4,0.37,"PHEL"]
["Franklin","ElD2","Eldean silt loam, 12 to 18 percent slopes, eroded","Eldean",4,0.37,"HEL"]
["Franklin","EmA","Eldean-Urban land complex, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Franklin","EmB","Eldean-Urban land complex, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Franklin","Gn","Genesee silt loam, occasionally flooded","Genesee",5,0.37,"NHEL"]
["Franklin","GwB","Glynwood silt loam, 2 to 6 percent slopes","glynwood",3,0.43,"PHEL"]
["Franklin","GwC2","Glynwood silt loam, 6 to 12 percent slopes, eroded","glynwood",3,0.43,"HEL"]
["Franklin","HeE2","Hennepin and Miamian loams, 18 to 25 percent slopes, eroded","Hennepin",4,0.32,"HEL"]
["Franklin","HeF2","Hennepin and Miamian loams, 25 to 50 percent slopes, eroded","Hennepin",4,0.32,"HEL"]
["Franklin","KeA","Kendallville silt loam, 0 to 2 percent slopes","Kendallville",3,0.37,"NHEL"]
["Franklin","KeB","Kendallville silt loam, 2 to 6 percent slopes","Kendallville",3,0.37,"PHEL"]
["Franklin","KeC2","Kendallville silt loam, 6 to 12 percent slopes, eroded","Kendallville",3,0.37,"PHEL"]
["Franklin","Ko","Kokomo silty clay loam","Kokomo",3,0.32,"NHEL"]
["Franklin","Ku","Kokomo-Urban land complex","Kokomo",3,0.32,"NHEL"]
["Franklin","LeB","Lewisburg-Crosby complex, 2 to 6 percent slopes","Lewisburg",3,0.43,"PHEL"]
["Franklin","Mh","Medway silt loam, occasionally flooded","Medway",5,0.32,"NHEL"]
["Franklin","MkB","Miamian silt loam, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Franklin","MlB2","Miamian silty clay loam, 2 to 6 percent slopes, eroded","Miamian",5,0.37,"PHEL"]
["Franklin","MlC2","Miamian silty clay loam, 6 to 12 percent slopes, eroded","Miamian",5,0.37,"PHEL"]
["Franklin","MlD2","Miamian silty clay loam, 12 to 18 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Franklin","MmC3","Miamian clay loam, 6 to 12 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Franklin","MnC","Miamian-Urban land complex, 6 to 12 percent slopes","Miamian",5,0.37,"PHEL"]
["Franklin","MoB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Franklin","MoC2","Milton silt loam, 6 to 12 percent slopes, eroded","Milton",4,0.37,"PHEL"]
["Franklin","MpB","Milton-Urban land complex, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Franklin","MpC","Milton-Urban land complex, 6 to 12 percent slopes","Milton",4,0.37,"PHEL"]
["Franklin","MrB","Mitiwanga silt loam, 2 to 6 percent slopes","Mitiwanga",4,0.32,"PHEL"]
["Franklin","Ms","Montgomery silty clay loam","Montgomery",5,0.37,"NHEL"]
["Franklin","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Franklin","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Franklin","OcC2","Ockley silt loam, 6 to 12 percent slopes, eroded","Ockley",5,0.37,"PHEL"]
["Franklin","Pm","Pewamo silty clay loam","Pewamo",5,0.24,"NHEL"]
["Franklin","Pn","Pewamo-Urban land complex","Pewamo",5,0.24,"NHEL"]
["Franklin","Pt","Pits, quarry","Pits"]
["Franklin","RhB","Ritchey silt loam, 2 to 6 percent slopes","Ritchey",2,0.37,"PHEL"]
["Franklin","RhD2","Ritchey silt loam, 12 to 18 percent slopes, eroded","Ritchey",2,0.37,"HEL"]
["Franklin","Rs","Ross silt loam, occasionally flooded","Ross",5,0.32,"NHEL"]
["Franklin","Sh","Shoals silt loam, occasionally flooded","Shoals",5,0.37,"NHEL"]
["Franklin","SlA","Sleeth silt loam, 0 to 2 percent slopes","Sleeth",5,0.32,"NHEL"]
["Franklin","SmA","Sleeth-Urban land complex, 0 to 2 percent slopes","Sleeth",5,0.32,"NHEL"]
["Franklin","So","Sloan silt loam, frequently flooded","Sloan",5,0.37,"NHEL"]
["Franklin","ThA","Thackery silt loam, 0 to 2 percent slopes","Thackery",4,0.37,"NHEL"]
["Franklin","ThB","Thackery silt loam, 2 to 6 percent slopes","Thackery",4,0.37,"PHEL"]
["Franklin","Up","Udorthents, loamy, rolling","Udorthents"]
["Franklin","Ur","Udorthents, loamy, sloping","Udorthents"]
["Franklin","Us","Udorthents, loamy, steep","Udorthents"]
["Franklin","Ut","Udorthents-Urban land complex, gently rolling","Udorthents"]
["Franklin","Uu","Urban land-Bennington complex, 2 to 6 percent slopes","Urban"]
["Franklin","Uv","Urban land-Celina complex, 2 to 12 percent slopes","Urban"]
["Franklin","Uw","Urban land-Genesee complex, occasionally flooded","Urban"]
["Franklin","Ux","Urban land-Ockley complex, 0 to 6 percent slopes","Urban"]
["Franklin","W","Water","Water"]
["Franklin","WdA","Warsaw silt loam, 0 to 2 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
["Franklin","WdB","Warsaw silt loam, 2 to 6 percent slopes","Warsaw",4,0.28000000000000003,"PHEL"]
["Franklin","WeA","Wea silt loam, 0 to 2 percent slopes","Wea",5,0.32,"NHEL"]
["Franklin","WeB","Wea silt loam, 2 to 6 percent slopes","Wea",5,0.32,"PHEL"]
["Franklin","Wt","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
[null,"Select","None","none"]
["Gallia","AaC","Aaron silt loam, 8 to 15 percent slopes","Aaron",3,0.37,"HEL"]
["Gallia","AkB","Allegheny loam, 3 to 8 percent slopes","Allegheny",4,0.32,"PHEL"]
["Gallia","AkC","Allegheny loam, 8 to 15 percent slopes","Allegheny",4,0.32,"PHEL"]
["Gallia","AkD","Allegheny loam, 15 to 25 percent slopes","Allegheny",4,0.32,"HEL"]
["Gallia","BcF","Berks-Upshur association, very steep","Berks",3,0.24,"HEL"]
["Gallia","BhD","Bethesda channery clay loam, 8 to 25 percent slopes","Bethesda",5,0.32,"PHEL"]
["Gallia","BhF","Bethesda channery clay loam, 40 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Gallia","Cg","Chagrin silt loam, frequently flooded","Chagrin",5,0.32,"NHEL"]
["Gallia","ChD","Clymer loam, 15 to 25 percent slopes","Clymer",3,0.24,"HEL"]
["Gallia","CkB","Clymer silt loam, 3 to 8 percent slopes","Clymer",3,0.24,"PHEL"]
["Gallia","CkC","Clymer silt loam, 8 to 15 percent slopes","Clymer",3,0.24,"HEL"]
["Gallia","CoB","Coolville silt loam, 1 to 6 percent slopes","Clymer",4,0.43,"PHEL"]
["Gallia","Cu","Cuba silt loam, occasionally flooded","Cuba",5,0.37,"NHEL"]
["Gallia","DbA","Doles silt loam, 0 to 3 percent slopes","Doles",4,0.43,"NHEL"]
["Gallia","Dm","Dumps, mine","Dumps"]
["Gallia","EkB","Elkinsville silt loam, 1 to 6 percent slopes","Elkinsville",5,0.37,"PHEL"]
["Gallia","FaB","Fairpoint channery silty clay loam, 1 to 8 percent slopes","Fairpoint",3,0.43,"HEL"]
["Gallia","FaD","Fairpoint channery silty clay loam, 8 to 25 percent slopes","Fairpoint",3,0.43,"PHEL"]
["Gallia","FaE","Fairpoint channery silty clay loam, 25 to 40 percent slopes","Fairpoint",3,0.43,"HEL"]
["Gallia","GaC2","Gallia loam, 8 to 15 percent slopes, eroded","Gallia",5,0.37,"HEL"]
["Gallia","GbB","Gallipolis silt loam, 1 to 6 percent slopes","Gallipolis",5,0.37,"NHEL"]
["Gallia","GbC","Gallipolis silt loam, 6 to 15 percent slopes","Gallipolis",5,0.37,"PHEL"]
["Gallia","GdE","Gilpin-Rarden association, steep","Gilpin",3,0.32,"HEL"]
["Gallia","GeE","Gilpin-Steinsburg-Upshur association, steep","Gilpin",3,0.32,"HEL"]
["Gallia","GsC","Guernsey-Gilpin silt loams, 8 to 15 percent slopes","Guernsey",3,0.43,"HEL"]
["Gallia","GwE","Guernsey-Gilpin association, steep","Guernsey",3,0.43,"HEL"]
["Gallia","KaB","Kanawha silt loam, 1 to 8 percent slopes","Kanawha",4,0.32,"PHEL"]
["Gallia","Kg","Kyger loamy sand, frequently flooded","Kyger",5,0.17,"NHEL"]
["Gallia","LcB","Licking silt loam, 1 to 6 percent slopes","Licking",3,0.43,"PHEL"]
["Gallia","LcC2","Licking silt loam, 6 to 15 percent slopes, eroded","Licking",3,0.43,"HEL"]
["Gallia","LcD2","Licking silt loam, 15 to 25 percent slopes, eroded","Licking",3,0.43,"HEL"]
["Gallia","LgD","Lily loam, 15 to 25 percent slopes","Lily",2,0.28000000000000003,"HEL"]
["Gallia","LhC","Lily silt loam, 8 to 15 percent slopes","Lily",2,0.28000000000000003,"PHEL"]
["Gallia","LmD","Lily-Rarden complex, 15 to 25 percent slopes","Lily",2,0.28000000000000003,"HEL"]
["Gallia","LpD","Lily-Upshur complex, 15 to 25 percent slopes","Lily",2,0.28000000000000003,"HEL"]
["Gallia","Ls","Lindside silt loam, occasionally flooded","Lindside",5,0.28000000000000003,"NHEL"]
["Gallia","McB","McGary silt loam, 1 to 6 percent slopes","McGary",3,0.43,"PHEL"]
["Gallia","MoC","Monongahela loam, 8 to 15 percent slopes","Monongahela",4,0.43,"HEL"]
["Gallia","Ne","Newark silt loam, frequently flooded","Newark",5,0.32,"NHEL"]
["Gallia","No","Nolin silt loam, occasionally flooded","Nolin",5,0.43,"NHEL"]
["Gallia","OmB","Omulga silt loam, 1 to 6 percent slopes","Omulga",3,0.43,"PHEL"]
["Gallia","OmC","Omulga silt loam, 6 to 15 percent slopes","Omulga",3,0.43,"HEL"]
["Gallia","Or","Orrville silt loam, frequently flooded","Orrville",5,0.37,"NHEL"]
["Gallia","Pe","Peoga silt loam","Peoga",4,0.43,"NHEL"]
["Gallia","PgB","Pinegrove sandy loam, 1 to 8 percent slopes","Pinegrove",5,0.24,"NHEL"]
["Gallia","PnD","Pinegrove sand, 8 to 25 percent slopes","Pinegrove",5,0.15,"PHEL"]
["Gallia","PnF","Pinegrove sand, 25 to 70 percent slopes","Pinegrove",5,0.15,"HEL"]
["Gallia","Pp","Piopolis silt loam, frequently flooded","Piopolis",4,0.43,"NHEL"]
["Gallia","Ps","Pits, sand and gravel","Pits"]
["Gallia","Pv","Pope fine sandy loam, frequently flooded","Pope",5,0.37,"NHEL"]
["Gallia","Px","Pope silt loam, occasionally flooded","Pope",5,0.37,"NHEL"]
["Gallia","RbC2","Rarden-Gilpin silt loams, 8 to 15 percent slopes, eroded","Rarden",3,0.43,"HEL"]
["Gallia","RbD2","Rarden-Gilpin silt loams, 15 to 25 percent slopes, eroded","Rarden",3,0.43,"HEL"]
["Gallia","RtE","Rarden-Steinsburg association, steep","Rarden",3,0.43,"HEL"]
["Gallia","ScE","Steinsburg-Clymer association, steep","Steinsburg",2,0.28000000000000003,"HEL"]
["Gallia","SrF","Steinsburg-Rock outcrop association, very steep","Steinsburg",2,0.28000000000000003,"HEL"]
["Gallia","St","Stendal silt loam, occasionally flooded","Stendal",5,0.37,"NHEL"]
["Gallia","TgA","Taggart silt loam, 0 to 3 percent slopes","Taggart",5,0.37,"NHEL"]
["Gallia","UgC2","Upshur-Gilpin complex, 8 to 15 percent slopes, eroded","Upshur",3,0.43,"HEL"]
["Gallia","UgD2","Upshur-Gilpin complex, 15 to 25 percent slopes, eroded","Upshur",3,0.43,"HEL"]
["Gallia","UgE","Upshur-Gilpin complex, 25 to 50 percent slopes","Upshur",3,0.43,"HEL"]
["Gallia","VaC2","Vandalia silty clay loam, 6 to 15 percent slopes, eroded","Vandalia",4,0.37,"HEL"]
["Gallia","VaD3","Vandalia silty clay loam, 15 to 25 percent slopes, severely eroded","Vandalia",4,0.37,"HEL"]
["Gallia","VnD3","Vandalia-Gilpin complex, 15 to 25 percent slopes, severely eroded","Vandalia",4,0.37,"HEL"]
["Gallia","W","Water","Water"]
["Gallia","WeB","Wellston silt loam, 1 to 6 percent slopes","Wellston",4,0.37,"PHEL"]
["Gallia","WhA","Wheeling silt loam, 0 to 3 percent slopes","Wheeling",4,0.37,"NHEL"]
["Gallia","WhB","Wheeling silt loam, 3 to 6 percent slopes","Wheeling",4,0.37,"PHEL"]
["Gallia","WhC","Wheeling silt loam, 6 to 15 percent slopes","Wheeling",4,0.37,"HEL"]
["Gallia","WhE","Wheeling silt loam, 25 to 40 percent slopes","Wheeling",4,0.37,"HEL"]
["Gallia","WoB","Woodsfield silt loam, 1 to 6 percent slopes","Woodsfield",3,0.43,"PHEL"]
["Gallia","ZaB","Zanesville silt loam, 1 to 6 percent slopes","Zanesville",3,0.43,"PHEL"]
[null,"Select","None","none"]
["Highland","Ag","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Highland","AtB","Atlas silt loam, 2 to 6 percent slopes","Atlas",3,0.43,"PHEL"]
["Highland","AtB2","Atlas silt loam, 2 to 6 percent slopes, moderately eroded","Atlas",3,0.43,"PHEL"]
["Highland","AtC2","Atlas silt loam, 6 to 12 percent slopes, moderately eroded","Atlas",3,0.43,"HEL"]
["Highland","AtC3","Atlas silt loam, 6 to 12 percent slopes, severely eroded","Atlas",2,0.43,"HEL"]
["Highland","AvA","Avonburg silt loam, 0 to 2 percent slopes","Avonburg",4,0.43,"NHEL"]
["Highland","AvB","Avonburg silt loam, 2 to 6 percent slopes","Avonburg",4,0.43,"PHEL"]
["Highland","AxA","Avonburg-Urban land complex, nearly level","Avonburg",4,0.43,"NHEL"]
["Highland","BeC2","Beasley silt loam, 6 to 12 percent slopes, moderately eroded","Beasley",3,0.43,"HEL"]
["Highland","BeD2","Beasley silt loam, 12 to 18 percent slopes, moderately eroded","Beasley",3,0.43,"HEL"]
["Highland","BgF","Berks-Muskingum channery silt loams, 18 to 35 percent slopes","Berks",3,0.24,"HEL"]
["Highland","BgG","Berks-Muskingum channery silt loams, 35 to 50 percent slopes","Berks",3,0.24,"HEL"]
["Highland","BhD","Berks-Muskingum-Neotoma channery silt loams, 6 to 18 percent slopes","Berks",3,0.24,"PHEL"]
["Highland","BhF","Berks-Muskingum-Neotoma channery silt loams, 18 to 35 percent slopes","Berks",3,0.24,"HEL"]
["Highland","BhG","Berks-Muskingum-Neotoma channery silt loams, 35 to 50 percent slopes","Berks",3,0.24,"HEL"]
["Highland","Bk","Blanchester silt loam","Blanchester",5,0.37,"NHEL"]
["Highland","BmC2","Boston-Bratton complex, 6 to 12 percent slopes, moderately eroded","Boston",3,0.37,"PHEL"]
["Highland","BmC3","Boston-Bratton complex, 6 to 12 percent slopes, severely eroded","Boston",3,0.37,"PHEL"]
["Highland","BmD2","Boston-Bratton complex, 12 to 18 percent slopes, moderately eroded","Boston",3,0.37,"HEL"]
["Highland","BmD3","Boston-Bratton complex, 12 to 18 percent slopes, severely eroded","Boston",3,0.37,"HEL"]
["Highland","BmE2","Boston-Bratton complex, 18 to 25 percent slopes, moderately eroded","Boston",3,0.37,"HEL"]
["Highland","BnB","Boston-Grayford silt loams, 2 to 6 percent slopes","Boston",3,0.37,"PHEL"]
["Highland","BnB2","Boston-Grayford silt loams, 2 to 6 percent slopes, moderately eroded","Boston",3,0.37,"PHEL"]
["Highland","BoB","Boston-Urban land complex, gently sloping","Boston",3,0.37,"PHEL"]
["Highland","BoC","Boston-Urban land complex, sloping","Boston",3,0.37,"PHEL"]
["Highland","BpB","Bratton silt loam, 2 to 6 percent slopes","Bratton",4,0.37,"PHEL"]
["Highland","BpB2","Bratton silt loam, 2 to 6 percent slopes, moderately eroded","Bratton",4,0.37,"PHEL"]
["Highland","BpC2","Bratton silt loam, 6 to 12 percent slopes, moderately eroded","Bratton",4,0.37,"PHEL"]
["Highland","BpD2","Bratton silt loam, 12 to 18 percent slopes, moderately eroded","Bratton",4,0.37,"HEL"]
["Highland","BrD3","Bratton silty clay loam, 12 to 18 percent slopes, severely eroded","Bratton",3,0.37,"HEL"]
["Highland","Bs","Brookston silt loam","Brookston",5,0.28000000000000003,"NHEL"]
["Highland","Bt","Brookston silty clay loam","Brookston",5,0.28000000000000003,"NHEL"]
["Highland","CaB","Cana silt loam, 2 to 6 percent slopes","Cana",4,0.37,"PHEL"]
["Highland","CaC2","Cana silt loam, 6 to 12 percent slopes, moderately eroded","Cana",4,0.37,"PHEL"]
["Highland","CaD2","Cana silt loam, 12 to 18 percent slopes, moderately eroded","Cana",4,0.37,"HEL"]
["Highland","CaF","Cana silt loam, 18 to 35 percent slopes","Cana",4,0.37,"HEL"]
["Highland","CcD3","Casco loam, 12 to 18 percent slopes, severely eroded","Casco",3,0.24,"HEL"]
["Highland","CcF2","Casco loam, 18 to 35 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Highland","CeB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Highland","CfB","Celina-Urban land complex, gently sloping","Celina",5,0.37,"PHEL"]
["Highland","C.F.L.","Cut and Fill Land","Cut"]
["Highland","CgA","Celina-Xenia silt loams, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Highland","CgB","Celina-Xenia silt loams, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Highland","ChB","Cincinnati silt loam, 2 to 6 percent slopes","Cincinnati",4,0.37,"PHEL"]
["Highland","ChC2","Cincinnati silt loam, 6 to 12 percent slopes, moderately eroded","Cincinnati",4,0.37,"PHEL"]
["Highland","ChD2","Cincinnati silt loam, 12 to 18 percent slopes, moderately eroded","Cincinnati",4,0.37,"HEL"]
["Highland","City Dump","City Dump","City dump"]
["Highland","Cm","Clermont silt loam","Clermont",5,0.37,"NHEL"]
["Highland","CoD2","Colyer-Trappist complex, 12 to 18 percent slopes, moderately eroded","Colyer",2,0.37,"HEL"]
["Highland","CoF","Colyer-Trappist complex, 18 to 35 percent slopes","Colyer",2,0.37,"HEL"]
["Highland","CoG","Colyer-Trappist complex, 35 to 50 percent slopes","Colyer",2,0.37,"HEL"]
["Highland","CrA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Highland","CsA","Crosby-Fincastle silt loams, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Highland","CsB","Crosby-Fincastle silt loams, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Highland","CuA","Crosby-Urban land complex, nearly level","Crosby",3,0.43,"PHEL"]
["Highland","DaA","Dana silt loam, 0 to 2 percent slopes","Dana",5,0.32,"NHEL"]
["Highland","DaB","Dana silt loam, 2 to 6 percent slopes","Dana",5,0.32,"PHEL"]
["Highland","DAM","Dam","Dam"]
["Highland","DuA","Dubois silt loam, 0 to 2 percent slopes","Dubois",4,0.43,"NHEL"]
["Highland","DuB","Dubois silt loam, 2 to 6 percent slopes","Dubois",4,0.43,"PHEL"]
["Highland","EbC2","Edenton silt loam, 6 to 12 percent slopes, moderately eroded","Edenton",3,0.43,"HEL"]
["Highland","EbD2","Edenton silt loam, 12 to 18 percent slopes, moderately eroded","Edenton",3,0.43,"HEL"]
["Highland","EbF2","Edenton silt loam, 18 to 35 percent slopes, moderately eroded","Edenton",3,0.43,"HEL"]
["Highland","Ee","Eel silt loam","Eel",5,0.37,"NHEL"]
["Highland","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Highland","FcB","Fitchville silt loam, 2 to 6 percent slopes","Fitchville",5,0.37,"PHEL"]
["Highland","FlC2","Fox loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Highland","FlD2","Fox loam, 12 to 18 percent slopes, moderately eroded","Fox",4,0.37,"HEL"]
["Highland","FnA","Fox silt loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Highland","FnB","Fox silt loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Highland","FoC3","Fox clay loam, 6 to 12 percent slopes, severely eroded","Fox",3,0.37,"PHEL"]
["Highland","GaC","Gasconade silty clay loam, 6 to 12 percent slopes","Gasconade",2,0.32,"HEL"]
["Highland","GaD2","Gasconade silty clay loam, 12 to 18 percent slopes, moderately eroded","Gasconade",2,0.32,"HEL"]
["Highland","GbF2","Gasconade flaggy silty clay loam, 18 to 35 percent slopes, moderately eroded","Gasconade",2,0.32,"HEL"]
["Highland","GbG","Gasconade flaggy silty clay loam, 35 to 50 percent slopes","Gasconade",2,0.32,"HEL"]
["Highland","Gn","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Highland","G.P.","Gravel pits","Gravel"]
["Highland","GuB","Guernsey silt loam, 2 to 6 percent slopes","Guernsey",3,0.43,"PHEL"]
["Highland","GuC","Guernsey silt loam, 6 to 12 percent slopes","Guernsey",3,0.43,"HEL"]
["Highland","GvC3","Guernsey silty clay loam, 6 to 12 percent slopes, severely eroded","Guernsey",3,0.43,"HEL"]
["Highland","GxD3","Guernsey soils, 12 to 18 percent slopes, severely eroded","Guernsey",3,0.43,"HEL"]
["Highland","HbA","Haubstadt silt loam, 0 to 2 percent slopes","Haubstadt",3,0.43,"NHEL"]
["Highland","HbB","Haubstadt silt loam, 2 to 6 percent slopes","Haubstadt",3,0.43,"PHEL"]
["Highland","HbC2","Haubstadt silt loam, 6 to 12 percent slopes, moderately eroded","Haubstadt",3,0.43,"HEL"]
["Highland","HbC3","Haubstadt silt loam, 6 to 12 percent slopes, severely eroded","Haubstadt",3,0.43,"HEL"]
["Highland","HbD2","Haubstadt silt loam, 12 to 18 percent slopes, moderately eroded","Haubstadt",3,0.43,"HEL"]
["Highland","HbD3","Haubstadt silt loam, 12 to 18 percent slopes, severely eroded","Haubstadt",3,0.43,"HEL"]
["Highland","HcB","Haubstadt-Urban land complex, gently sloping","Haubstadt",3,0.43,"PHEL"]
["Highland","HcC","Haubstadt-Urban land complex, sloping","Haubstadt",3,0.43,"HEL"]
["Highland","HeF2","Hennepin-Miamian silt loams, 18 to 35 percent slopes, moderately eroded","Hennepin",4,0.32,"HEL"]
["Highland","HeG2","Hennepin-Miamian silt loams, 35 to 50 percent slopes, moderately eroded","Hennepin",4,0.32,"HEL"]
["Highland","HfE3","Hennepin-Miamian complex, 12 to 25 percent slopes, severely eroded","Hennepin",4,0.32,"HEL"]
["Highland","HkC2","Hickory silt loam, 6 to 12 percent slopes, moderately eroded","Hickory",5,0.37,"PHEL"]
["Highland","HkD2","Hickory silt loam, 12 to 18 percent slopes, moderately eroded","Hickory",5,0.37,"HEL"]
["Highland","HkE2","Hickory silt loam, 18 to 25 percent slopes, moderately eroded","Hickory",5,0.37,"HEL"]
["Highland","HkF2","Hickory silt loam, 25 to 35 percent slopes, moderately eroded","Hickory",5,0.37,"HEL"]
["Highland","HyC3","Hickory clay loam, 6 to 12 percent slopes, severely eroded","Hickory",4,0.37,"PHEL"]
["Highland","HyD3","Hickory clay loam, 12 to 18 percent slopes, severely eroded","Hickory",4,0.37,"HEL"]
["Highland","HyE3","Hickory clay loam, 18 to 25 percent slopes, severely eroded","Hickory",4,0.37,"HEL"]
["Highland","JeD","Jessup silt loam, 12 to 18 percent slopes","Jessup",3,0.43,"HEL"]
["Highland","JoC","Johnsburg silt loam, 2 to 8 percent slopes","Johnsburg",3,0.43,"PHEL"]
["Highland","KeB","Kendallville silt loam, 2 to 6 percent slopes","Kendallville",3,0.37,"PHEL"]
["Highland","KeC2","Kendallville silt loam, 6 to 12 percent slopes, moderately eroded","Kendallville",3,0.37,"PHEL"]
["Highland","KeD2","Kendallville silt loam, 12 to 18 percent slopes, moderately eroded","Kendallville",3,0.37,"HEL"]
["Highland","KfD3","Kendallville clay loam, 12 to 18 percent slopes, severely eroded","Kendallville",2,0.37,"HEL"]
["Highland","LhB","Lawshe silty clay loam, 2 to 6 percent slopes","Lawshe",3,0.32,"PHEL"]
["Highland","LhC2","Lawshe silty clay loam, 6 to 12 percent slopes, moderately eroded","Lawshe",3,0.32,"PHEL"]
["Highland","LhD2","Lawshe silty clay loam, 12 to 18 percent slopes, moderately eroded","Lawshe",3,0.32,"HEL"]
["Highland","LlD3","Lawshe silty clay, 12 to 18 percent slopes, severely eroded","Lawshe",2,0.32,"HEL"]
["Highland","LoB","Loudon silt loam, 2 to 6 percent slopes","Loudon",3,0.43,"PHEL"]
["Highland","LoB2","Loudon silt loam, 2 to 6 percent slopes, moderately eroded","Loudon",3,0.43,"PHEL"]
["Highland","LoC2","Loudon silt loam, 6 to 12 percent slopes, moderately eroded","Loudon",3,0.43,"HEL"]
["Highland","LoD2","Loudon silt loam, 12 to 18 percent slopes, moderately eroded","Loudon",3,0.43,"HEL"]
["Highland","LpE2","Loudon-Edenton silt loams, 18 to 25 percent slopes, moderately eroded","Loudon",3,0.43,"HEL"]
["Highland","MdB","Markland silt loam, 2 to 6 percent slopes","Markland",3,0.43,"PHEL"]
["Highland","MdC2","Markland silt loam, 6 to 12 percent slopes, moderately eroded","Markland",3,0.43,"HEL"]
["Highland","MdD2","Markland silt loam, 12 to 18 percent slopes, moderately eroded","Markland",3,0.43,"HEL"]
["Highland","MgB","McGary silt loam, 0 to 4 percent slopes","McGary",3,0.43,"PHEL"]
["Highland","MlB","Miamian silt loam, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Highland","MlB2","Miamian silt loam, 2 to 6 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Highland","MlC2","Miamian silt loam, 6 to 12 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Highland","MlD2","Miamian silt loam, 12 to 18 percent slopes, moderately eroded","Miamian",5,0.37,"HEL"]
["Highland","MlE","Miamian silt loam, 18 to 25 percent slopes","Miamian",5,0.37,"HEL"]
["Highland","MmC3","Miamian clay loam, 6 to 12 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Highland","MrB","Miamian-Russell silt loams, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Highland","MrB2","Miamian-Russell silt loams, 2 to 6 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Highland","MrC2","Miamian-Russell silt loams, 6 to 12 percent slopes, moderately eroded","Miamian",5,0.37,"PHEL"]
["Highland","MsB","Miamian-Urban land complex, gently sloping","Miamian",5,0.37,"PHEL"]
["Highland","Mt","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Highland","MuB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Highland","MuB2","Milton silt loam, 2 to 6 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Highland","MuC2","Milton silt loam, 6 to 12 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Highland","MuD2","Milton silt loam, 12 to 18 percent slopes, moderately eroded","Milton",4,0.37,"HEL"]
["Highland","MwC3","Milton clay loam, 6 to 12 percent slopes, severely eroded","Milton",3,0.37,"PHEL"]
["Highland","My","Montgomery silty clay loam","Montgomery",5,0.37,"NHEL"]
["Highland","NdC","Negley loam, 6 to 12 percent slopes","Negley",3,0.32,"PHEL"]
["Highland","NdD","Negley loam, 12 to 18 percent slopes","Negley",3,0.32,"HEL"]
["Highland","NdE","Negley loam, 18 to 25 percent slopes","Negley",3,0.32,"HEL"]
["Highland","NdF","Negley loam, 25 to 35 percent slopes","Negley",3,0.32,"HEL"]
["Highland","NeB","Negley silt loam, 2 to 6 percent slopes","Negley",3,0.32,"PHEL"]
["Highland","NfC3","Negley clay loam, 6 to 12 percent slopes, severely eroded","Negley",2,0.32,"PHEL"]
["Highland","NfD3","Negley clay loam, 12 to 18 percent slopes, severely eroded","Negley",2,0.32,"HEL"]
["Highland","NgF","Negley-Fox complex, 18 to 35 percent slopes","Negley",3,0.32,"HEL"]
["Highland","NnB","Nicholson silt loam, 2 to 6 percent slopes","Nicholson",3,0.43,"PHEL"]
["Highland","NnB2","Nicholson silt loam, 2 to 6 percent slopes, moderately eroded","Nicholson",3,0.43,"PHEL"]
["Highland","NnC2","Nicholson silt loam, 6 to 12 percent slopes, moderately eroded","Nicholson",3,0.43,"HEL"]
["Highland","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Highland","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Highland","OcC2","Ockley silt loam, 6 to 12 percent slopes, moderately eroded","Ockley",5,0.37,"PHEL"]
["Highland","OdB","Ockley-Urban land complex, gently sloping","Ockley",5,0.37,"PHEL"]
["Highland","OpD2","Opequon silt loam, 6 to 18 percent slopes, moderately eroded","Opequon",1,0.43,"HEL"]
["Highland","OpE2","Opequon silt loam, 18 to 25 percent slopes, moderately eroded","Opequon",1,0.43,"HEL"]
["Highland","OsF2","Opequon stony silt loam, 18 to 35 percent slopes, moderately eroded","Opequon",1,0.43,"HEL"]
["Highland","OsG","Opequon stony silt loam, 35 to 50 percent slopes","Opequon",1,0.43,"HEL"]
["Highland","OtD3","Opequon clay, 6 to 18 percent slopes, severely eroded","Opequon",1,0.43,"HEL"]
["Highland","OwB","Otwell silt loam, 2 to 6 percent slopes","Otwell",3,0.43,"PHEL"]
["Highland","OwC2","Otwell silt loam, 6 to 12 percent slopes, moderately eroded","Otwell",3,0.43,"HEL"]
["Highland","OwD2","Otwell silt loam, 12 to 18 percent slopes, moderately eroded","Otwell",3,0.43,"HEL"]
["Highland","OwE2","Otwell silt loam, 18 to 25 percent slopes, moderately eroded","Otwell",3,0.43,"HEL"]
["Highland","OwF","Otwell silt loam, 25 to 35 percent slopes","Otwell",3,0.43,"HEL"]
["Highland","Pa","Patton silt loam","Patton",5,0.28000000000000003,"NHEL"]
["Highland","Pb","Patton silt loam, till substratum","Patton",5,0.28000000000000003,"NHEL"]
["Highland","Pe","Peoga silt loam","Peoga",4,0.43,"NHEL"]
["Highland","Pn","Philo silt loam","Philo",5,0.37,"NHEL"]
["Highland","QU.","Quarries","Quarries"]
["Highland","Rn","Ross silt loam","Ross",5,0.32,"NHEL"]
["Highland","RpA","Rossmoyne silt loam, 0 to 2 percent slopes","Rossmoyne",4,0.37,"NHEL"]
["Highland","RpB","Rossmoyne silt loam, 2 to 6 percent slopes","Rossmoyne",4,0.37,"PHEL"]
["Highland","RpB2","Rossmoyne silt loam, 2 to 6 percent slopes, moderately eroded","Rossmoyne",4,0.37,"PHEL"]
["Highland","RpC2","Rossmoyne silt loam, 6 to 12 percent slopes, moderately eroded","Rossmoyne",4,0.37,"PHEL"]
["Highland","RpD2","Rossmoyne silt loam, 12 to 18 percent slopes, moderately eroded","Rossmoyne",4,0.37,"HEL"]
["Highland","RsC3","Rossmoyne silty clay loam, 6 to 12 percent slopes, severely eroded","Rossmoyne",3,0.37,"PHEL"]
["Highland","RtB","Rossmoyne-Urban land complex, gently sloping","Rossmoyne",4,0.37,"PHEL"]
["Highland","RuB","Russell silt loam, 2 to 6 percent slopes","Russell",5,0.37,"PHEL"]
["Highland","SaA","Sardinia silt loam, 0 to 2 percent slopes","Sardinia",5,0.37,"NHEL"]
["Highland","SaB","Sardinia silt loam, 2 to 6 percent slopes","Sardinia",5,0.37,"PHEL"]
["Highland","SaC2","Sardinia silt loam, 6 to 12 percent slopes, moderately eroded","Sardinia",5,0.37,"PHEL"]
["Highland","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Highland","SlA","Sleeth silt loam, 0 to 2 percent slopes","Sleeth",5,0.32,"NHEL"]
["Highland","Sn","Sloan silt loam","Sloan",5,0.37,"NHEL"]
["Highland","St","Stonelick loam","Stonelick",5,0.24,"NHEL"]
["Highland","ThA","Thackery silt loam, 0 to 2 percent slopes","Thackery",4,0.37,"NHEL"]
["Highland","ThB","Thackery silt loam, 2 to 6 percent slopes","Thackery",4,0.37,"PHEL"]
["Highland","TrE","Trappist silt loam, 18 to 25 percent slopes","Trappist",3,0.37,"HEL"]
["Highland","TsB","Trappist-Muse silt loams, 2 to 6 percent slopes","Trappist",3,0.37,"PHEL"]
["Highland","TsC2","Trappist-Muse silt loams, 6 to 12 percent slopes, moderately eroded","Trappist",3,0.37,"PHEL"]
["Highland","TsD2","Trappist-Muse silt loams, 12 to 18 percent slopes, moderately eroded","Trappist",3,0.37,"HEL"]
["Highland","TuD","Tuscarawas channery silt loam, 6 to 18 percent slopes","Tuscarawas",4,0.28000000000000003,"PHEL"]
["Highland","TuF","Tuscarawas channery silt loam, 18 to 35 percent slopes","Tuscarawas",4,0.28000000000000003,"HEL"]
["Highland","W","Water","Water"]
["Highland","WaA","Warsaw silt loam, 0 to 2 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
["Highland","WeA","Wea silt loam, 0 to 2 percent slopes","Wea",5,0.32,"NHEL"]
["Highland","WeB","Wea silt loam, 2 to 6 percent slopes","Wea",5,0.32,"PHEL"]
["Highland","WlC","Wellston silt loam, 6 to 12 percent slopes","Wellston",4,0.37,"PHEL"]
["Highland","WlD","Wellston silt loam, 12 to 18 percent slopes","Wellston",4,0.37,"HEL"]
["Highland","Ws","Westland silt loam, overwash","Westland",5,0.28000000000000003,"NHEL"]
["Highland","Wt","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
["Highland","WvA","Williamsburg silt loam, 0 to 2 percent slopes","Williamsburg",5,0.32,"NHEL"]
["Highland","WvB","Williamsburg silt loam, 2 to 6 percent slopes","Williamsburg",5,0.32,"PHEL"]
["Highland","WvC","Williamsburg silt loam, 6 to 12 percent slopes","Williamsburg",5,0.32,"PHEL"]
["Highland","XeB","Xenia silt loam, 2 to 6 percent slopes","Xenia",5,0.37,"PHEL"]
[null,"Select","None","none"]
["Hocking","AdD2","Alexandria silt loam, 12 to 18 percent slopes, eroded","Alexandria",4,0.37,"HEL"]
["Hocking","AdE","Alexandria silt loam, 18 to 25 percent slopes","Alexandria",4,0.37,"HEL"]
["Hocking","AdF","Alexandria silt loam, 25 to 40 percent slopes","Alexandria",4,0.37,"HEL"]
["Hocking","AfB","Alford silt loam, 2 to 6 percent slopes","Alford",5,0.37,"PHEL"]
["Hocking","AfC","Alford silt loam, 6 to 12 percent slopes","Alford",5,0.37,"PHEL"]
["Hocking","AgB","Allegheny loam, 2 to 6 percent slopes","Allegheny",4,0.32,"PHEL"]
["Hocking","AgC","Allegheny loam, 6 to 12 percent slopes","Allegheny",4,0.32,"PHEL"]
["Hocking","BeA","Bennington silt loam, 0 to 3 percent slopes","Bennington",3,0.43,"NHEL"]
["Hocking","BtB","Bethesda channery loam, 0 to 8 percent slopes","Bethesda",5,0.32,"PHEL"]
["Hocking","BtC","Bethesda channery loam, 8 to 20 percent slopes","Bethesda",5,0.32,"PHEL"]
["Hocking","BtE","Bethesda channery loam, 20 to 40 percent slopes","Bethesda",5,0.32,"HEL"]
["Hocking","BtF","Bethesda channery loam, 40 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Hocking","BuB","Bethesda silty clay loam, 0 to 8 percent slopes","Bethesda",3,0.43,"PHEL"]
["Hocking","BuC","Bethesda silty clay loam, 8 to 20 percent slopes","Bethesda",3,0.43,"HEL"]
["Hocking","BuE","Bethesda silty clay loam, 20 to 40 percent slopes","Bethesda",3,0.43,"HEL"]
["Hocking","CaC2","Cana Variant silt loam, 8 to 15 percent slopes, eroded","Cana",5,0.37,"PHEL"]
["Hocking","CaD2","Cana Variant silt loam, 15 to 25 percent slopes, eroded","Cana",5,0.37,"HEL"]
["Hocking","CdB","Cardington silt loam, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Hocking","CdC2","Cardington silt loam, 6 to 12 percent slopes, eroded","Cardington",4,0.37,"PHEL"]
["Hocking","CeF","Cedarfalls-Rock outcrop complex, 40 to 70 percent slopes","Cedarfalls",4,0.24,"HEL"]
["Hocking","Cg","Chagrin silt loam, frequently flooded","Chagrin",5,0.32,"NHEL"]
["Hocking","ChA","Chili loam, 0 to 3 percent slopes","Chili",4,0.32,"NHEL"]
["Hocking","ChC2","Chili loam, 8 to 15 percent slopes, eroded","Chili",4,0.32,"PHEL"]
["Hocking","CkB","Cincinnati silt loam, 2 to 6 percent slopes","Cincinnati",4,0.37,"PHEL"]
["Hocking","CkC2","Cincinnati silt loam, 6 to 12 percent slopes, eroded","Cincinnati",4,0.37,"PHEL"]
["Hocking","CtC","Cruze silt loam, 8 to 15 percent slopes","Cruze",3,0.37,"HEL"]
["Hocking","DkF","Dekalb-Shelocta-Rock outcrop complex, 40 to 70 percent slopes","Dekalb",2,0.24,"HEL"]
["Hocking","EcA","Euclid silt loam, rarely flooded","Euclid",5,0.37,"NHEL"]
["Hocking","GfA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Hocking","GfB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Hocking","GuC","Guernsey silt loam, 8 to 15 percent slopes","Guernsey",3,0.43,"HEL"]
["Hocking","HmD2","Hickory silt loam, 12 to 18 percent slopes, eroded","Hickory",5,0.37,"HEL"]
["Hocking","HmE","Hickory silt loam, 18 to 25 percent slopes","Hickory",5,0.37,"HEL"]
["Hocking","HmF","Hickory silt loam, 25 to 40 percent slopes","Hickory",5,0.37,"HEL"]
["Hocking","LkB","Licking silt loam, 2 to 6 percent slopes","Licking",3,0.43,"PHEL"]
["Hocking","LkC2","Licking silt loam, 6 to 12 percent slopes, eroded","Licking",3,0.43,"HEL"]
["Hocking","LkD2","Licking silt loam, 12 to 18 percent slopes, eroded","Licking",3,0.43,"HEL"]
["Hocking","LnC","Lily silt loam, 8 to 15 percent slopes","Lily",3,0.28000000000000003,"PHEL"]
["Hocking","LnD","Lily silt loam, 15 to 25 percent slopes","Lily",3,0.28000000000000003,"HEL"]
["Hocking","McA","McGary silt loam, 0 to 3 percent slopes","McGary",3,0.43,"PHEL"]
["Hocking","Me","Melvin silt loam, frequently flooded","Melvin",5,0.43,"NHEL"]
["Hocking","NeC","Negley silt loam, 8 to 15 percent slopes","Negley",3,0.32,"HEL"]
["Hocking","NeD","Negley silt loam, 15 to 25 percent slopes","Negley",3,0.32,"HEL"]
["Hocking","NeE","Negley silt loam, 25 to 40 percent slopes","Negley",3,0.32,"HEL"]
["Hocking","NeF","Negley silt loam, 40 to 70 percent slopes","Negley",3,0.32,"HEL"]
["Hocking","Or","Orrville silt loam, frequently flooded","Orrville",5,0.37,"NHEL"]
["Hocking","OtB","Otwell silt loam, 2 to 6 percent slopes","Otwell",3,0.43,"PHEL"]
["Hocking","OtC","Otwell silt loam, 6 to 12 percent slopes","Otwell",3,0.43,"HEL"]
["Hocking","OtD2","Otwell silt loam, 12 to 18 percent slopes, eroded","Otwell",3,0.43,"HEL"]
["Hocking","Po","Pope loam, occasionally flooded","Pope",5,0.37,"NHEL"]
["Hocking","SaC","Shelocta silt loam, 8 to 15 percent slopes","Shelocta",4,0.32,"PHEL"]
["Hocking","SaD","Shelocta silt loam, 15 to 25 percent slopes","Shelocta",4,0.32,"HEL"]
["Hocking","SbE","Shelocta-Berks complex, 25 to 40 percent slopes","Shelocta",4,0.32,"HEL"]
["Hocking","ScD","Shelocta-Cruze silt loams, 15 to 25 percent slopes","Shelocta",4,0.32,"HEL"]
["Hocking","ScE","Shelocta-Cruze silt loams, 25 to 40 percent slopes","Shelocta",4,0.32,"HEL"]
["Hocking","ScF","Shelocta-Cruze silt loams, 40 to 70 percent slopes","Shelocta",4,0.32,"HEL"]
["Hocking","St","Stonelick loam, occasionally flooded","Stonelick",5,0.24,"NHEL"]
["Hocking","Ud","Udorthents","Udorthents"]
["Hocking","W","Water","Water"]
["Hocking","WeB","Wellston silt loam, 2 to 6 percent slopes","Wellston",4,0.37,"PHEL"]
["Hocking","WeC","Wellston silt loam, 6 to 15 percent slopes","Wellston",4,0.37,"PHEL"]
["Hocking","WfC","Wellston-Cruze silt loams, 8 to 15 percent slopes","Wellston",4,0.37,"PHEL"]
["Hocking","WgC","Wellston-Guernsey silt loams, 8 to 15 percent slopes","Wellston",4,0.37,"PHEL"]
["Hocking","WmB","Westmore silt loam, 2 to 6 percent slopes","Westmore",4,0.37,"PHEL"]
["Hocking","WmC","Westmore silt loam, 6 to 15 percent slopes","Westmore",4,0.37,"PHEL"]
["Hocking","WoD","Westmoreland silt loam, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Hocking","WpE","Westmoreland-Berks complex, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Hocking","WpF","Westmoreland-Berks complex, 40 to 70 percent slopes","Westmoreland",3,0.37,"HEL"]
["Hocking","WrD","Westmoreland-Guernsey silt loams, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Hocking","WrE","Westmoreland-Guernsey silt loams, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Hocking","WrF","Westmoreland-Guernsey silt loams, 40 to 70 percent slopes","Westmoreland",3,0.37,"HEL"]
["Hocking","WtA","Wheeling silt loam, 0 to 3 percent slopes","Wheeling",4,0.37,"NHEL"]
["Hocking","ZnB","Zanesville silt loam, 2 to 6 percent slopes","Zanesville",3,0.43,"PHEL"]
["Hocking","ZnC","Zanesville silt loam, 6 to 15 percent slopes","Zanesville",3,0.43,"HEL"]
[null,"Select","None","none"]
["Jackson","AkB","Allegheny loam, 3 to 8 percent slopes","Allegheny",4,0.32,"PHEL"]
["Jackson","AkC","Allegheny loam, 8 to 15 percent slopes","Allegheny",4,0.32,"PHEL"]
["Jackson","AkD","Allegheny loam, 15 to 25 percent slopes","Allegheny",4,0.32,"HEL"]
["Jackson","BaD","Barkcamp gravelly loamy sand, 8 to 25 percent slopes","Barkcamp",5,0.24,"PHEL"]
["Jackson","BhB","Bethesda shaly clay loam, 0 to 8 percent slopes","Bethesda",5,0.32,"PHEL"]
["Jackson","BhD","Bethesda shaly clay loam, 8 to 25 percent slopes","Bethesda",5,0.32,"PHEL"]
["Jackson","BhE","Bethesda shaly clay loam, 25 to 40 percent slopes","Bethesda",5,0.32,"HEL"]
["Jackson","BrD","Brownsville channery silt loam, 15 to 25 percent slopes","Brownsville",5,0.2,"PHEL"]
["Jackson","BsF","Brownsville-Shelocta association, steep","Brownsville",5,0.2,"HEL"]
["Jackson","ChD","Clymer loam, 15 to 25 percent slopes","Clymer",3,0.24,"HEL"]
["Jackson","CkB","Clymer silt loam, 3 to 8 percent slopes","Clymer",3,0.24,"PHEL"]
["Jackson","CkC","Clymer silt loam, 8 to 15 percent slopes","Clymer",3,0.24,"PHEL"]
["Jackson","CoB","Coolville silt loam, 3 to 8 percent slopes","Coolville",4,0.43,"PHEL"]
["Jackson","Cu","Cuba silt loam, occasionally flooded","Cuba",5,0.37,"NHEL"]
["Jackson","DbA","Doles silt loam, 0 to 3 percent slopes","Doles",4,0.43,"NHEL"]
["Jackson","Dd","Dumps","Dumps"]
["Jackson","Dm","Dumps, mine","Dumps "]
["Jackson","ErC","Ernest silt loam, 8 to 15 percent slopes","Ernest",3,0.43,"HEL"]
["Jackson","ErD","Ernest silt loam, 15 to 25 percent slopes","Ernest",3,0.43,"HEL"]
["Jackson","FaB","Fairpoint silty clay loam, 0 to 8 percent slopes","Fairpoint",3,0.43,"PHEL"]
["Jackson","FaD","Fairpoint silty clay loam, 8 to 25 percent slopes","Fairpoint",3,0.43,"HEL"]
["Jackson","OmA","Omulga silt loam, 0 to 3 percent slopes","Omulga",3,0.43,"PHEL"]
["Jackson","OmB","Omulga silt loam, 3 to 8 percent slopes","Omulga",3,0.43,"PHEL"]
["Jackson","OmC","Omulga silt loam, 8 to 15 percent slopes","Omulga",3,0.43,"HEL"]
["Jackson","Or","Orrville silt loam, frequently flooded","Orrville",5,0.37,"NHEL"]
["Jackson","Pb","Piopolis silt loam, frequently flooded","Piopolis",4,0.43,"NHEL"]
["Jackson","Pc","Piopolis silt loam, ponded","Piopolis",4,0.43,"NHEL"]
["Jackson","Pt","Pits, quarry","Pits"]
["Jackson","Pv","Pope sandy loam, frequently flooded","Pope",5,0.37,"NHEL"]
["Jackson","Pw","Pope fine sandy loam, rarely flooded","Pope",5,0.37,"NHEL"]
["Jackson","Px","Pope silt loam, frequently flooded","Pope",5,0.37,"NHEL"]
["Jackson","RaB","Rarden silt loam, 3 to 8 percent slopes","Rarden",3,0.43,"PHEL"]
["Jackson","RaC2","Rarden silt loam, 8 to 15 percent slopes, eroded","Rarden",3,0.43,"HEL"]
["Jackson","RbC2","Rarden-Wharton silt loams, 8 to 15 percent slopes, eroded","Rarden",3,0.43,"HEL"]
["Jackson","RbD2","Rarden-Wharton silt loams, 15 to 25 percent slopes, eroded","Rarden",3,0.43,"HEL"]
["Jackson","RcC","Richland silt loam, clayey substratum, 8 to 15 percent slopes","Richland",5,0.37,"PHEL"]
["Jackson","RgC","Rigley sandy loam, 8 to 15 percent slopes","Rigley",4,0.24,"PHEL"]
["Jackson","RgD","Rigley sandy loam, 15 to 25 percent slopes","Rigley",4,0.24,"HEL"]
["Jackson","RkD","Rigley-Rarden complex, 15 to 25 percent slopes","Rigley",4,0.24,"HEL"]
["Jackson","RmE","Rigley-Clymer association, steep","Rigley",4,0.24,"HEL"]
["Jackson","RnE","Rigley-Rarden association, steep","Rigley",4,0.24,"HEL"]
["Jackson","RrG","Rigley-Rock outcrop association, very steep","Rigley",4,0.24,"HEL"]
["Jackson","ShE","Shelocta-Rarden association, steep","Shelocta",4,0.32,"HEL"]
["Jackson","Sk","Skidmore gravelly loam, frequently flooded","Skidmore",5,0.17,"NHEL"]
["Jackson","St","Stendal silt loam, occasionally flooded","Stendal",5,0.37,"NHEL"]
["Jackson","TeB","Tilsit silt loam, 3 to 8 percent slopes","Tilsit",3,0.43,"PHEL"]
["Jackson","TrA","Tygart silt loam, 0 to 3 percent slopes","Tygart",3,0.43,"PHEL"]
["Jackson","Ud","Udorthents","Udorthents"]
["Jackson","W","Water","Water"]
["Jackson","WeB","Wellston silt loam, 3 to 8 percent slopes","Wellston",4,0.37,"PHEL"]
["Jackson","WeC","Wellston silt loam, 8 to 15 percent slopes","Wellston",4,0.37,"PHEL"]
["Jackson","WhC","Wharton silt loam, 8 to 15 percent slopes","Wharton",3,0.37,"HEL"]
["Jackson","WhD","Wharton silt loam, 15 to 25 percent slopes","Wharton",3,0.37,"HEL"]
["Jackson","WtB","Wyatt silt loam, 3 to 8 percent slopes","Wyatt",3,0.43,"PHEL"]
["Jackson","WyC2","Wyatt silty clay loam, 8 to 15 percent slopes, eroded","Wyatt",2,0.43,"HEL"]
["Jackson","WyD2","Wyatt silty clay loam, 15 to 25 percent slopes, eroded","Wyatt",2,0.43,"HEL"]
[null,"Select","None","none"]
["Lawrence","BdD","Bethesda channery silty clay loam, 8 to 25 percent slopes","Bethesda",5,0.32,"HEL"]
["Lawrence","BdF","Bethesda channery silty clay loam, 25 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Lawrence","Cg","Chagrin loam, frequently flooded","Chagrin",5,0.32,"NHEL"]
["Lawrence","CtB","Coolville-Tilsit silt loams, 2 to 6 percent slopes","Coolville",4,0.43,"PHEL"]
["Lawrence","Cu","Cuba silt loam, occasionally flooded","Cuba",5,0.37,"NHEL"]
["Lawrence","Dp","Dumps","Dumps"]
["Lawrence","EkB","Elkinsville silt loam, 1 to 6 percent slopes","Elkinsville",5,0.37,"NHEL"]
["Lawrence","EkE","Elkinsville silt loam, 15 to 40 percent slopes","Elkinsville",5,0.37,"HEL"]
["Lawrence","EmB","Elkinsville-Urban land complex, 1 to 8 percent slopes","Elkinsville",5,0.37,"PHEL"]
["Lawrence","FaD","Fairpoint channery silty clay loam, 8 to 25 percent slopes","Fairpoint",3,0.43,"HEL"]
["Lawrence","GmD","Gilpin-Latham silt loams, 15 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Lawrence","KaB","Kanawha silt loam, 2 to 6 percent slopes","Kanawha",4,0.32,"PHEL"]
["Lawrence","KaC","Kanawha silt loam, 6 to 12 percent slopes","Kanawha",4,0.32,"HEL"]
["Lawrence","Kg","Kyger loamy sand, frequently flooded","Kyger",5,0.17,"NHEL"]
["Lawrence","LaD","Lakin loamy fine sand, 8 to 25 percent slopes","Lakin",5,0.17,"PHEL"]
["Lawrence","LhD","Latham-Steinsburg complex, 15 to 25 percent slopes","Latham",3,0.43,"HEL"]
["Lawrence","LkB","Licking silt loam, 1 to 6 percent slopes","Licking",3,0.43,"PHEL"]
["Lawrence","LnC2","Licking silty clay loam, 6 to 12 percent slopes, eroded","Licking",3,0.43,"HEL"]
["Lawrence","LtC","Lily loam, 8 to 15 percent slopes","Lily",2,0.28000000000000003,"HEL"]
["Lawrence","LtD","Lily loam, 15 to 25 percent slopes","Lily",2,0.28000000000000003,"HEL"]
["Lawrence","McA","McGary silt loam, 0 to 2 percent slopes","McGary",3,0.43,"NHEL"]
["Lawrence","Me","Melvin silt loam, ponded","Melvin",5,0.43,"NHEL"]
["Lawrence","MrB","Morristown channery silty clay loam, 0 to 8 percent slopes","Morristown",5,0.32,"PHEL"]
["Lawrence","MrD","Morristown channery silty clay loam, 8 to 25 percent slopes","Morristown",5,0.32,"HEL"]
["Lawrence","MrF","Morristown channery silty clay loam, 25 to 70 percent slopes","Morristown",5,0.32,"HEL"]
["Lawrence","No","Nolin silt loam, occasionally flooded","Nolin",5,0.43,"NHEL"]
["Lawrence","OmC2","Omulga silt loam, 6 to 15 percent slopes, eroded","Omulga",3,0.43,"HEL"]
["Lawrence","Or","Orrville silt loam, frequently flooded","Orrville",5,0.37,"NHEL"]
["Lawrence","Pe","Peoga silt loam, rarely flooded","Peoga",4,0.43,"NHEL"]
["Lawrence","PgD","Pinegrove loamy coarse sand, 8 to 25 percent slopes","Pinegrove",5,0.17,"PHEL"]
["Lawrence","PgF","Pinegrove loamy coarse sand, 25 to 70 percent slopes","Pinegrove",5,0.17,"HEL"]
["Lawrence","PkD","Pinegrove silty clay loam, 8 to 25 percent slopes","Pinegrove",5,0.43,"HEL"]
["Lawrence","Pn","Piopolis silty clay loam, frequently flooded","Piopolis",4,0.43,"NHEL"]
["Lawrence","Ps","Pits, sand and gravel","Pits"]
["Lawrence","RbC","Rarden-Gilpin silt loams, 8 to 15 percent slopes","Rarden",3,0.43,"HEL"]
["Lawrence","RbD","Rarden-Gilpin silt loams, 15 to 25 percent slopes","Rarden",3,0.43,"HEL"]
["Lawrence","RnD","Rarden-Lily complex, 15 to 25 percent slopes","Rarden",3,0.43,"HEL"]
["Lawrence","SaB","Sciotoville silt loam, 1 to 6 percent slopes","Sciotoville",4,0.37,"PHEL"]
["Lawrence","SbB","Shelocta silt loam, 2 to 6 percent slopes","Shelocta",4,0.32,"PHEL"]
["Lawrence","SbC","Shelocta silt loam, 6 to 15 percent slopes","Shelocta",4,0.32,"HEL"]
["Lawrence","SbD","Shelocta silt loam, 15 to 25 percent slopes","Shelocta",4,0.32,"HEL"]
["Lawrence","SdE","Shelocta-Latham association, steep","Shelocta",4,0.32,"HEL"]
["Lawrence","SfE","Steinsburg-Clymer association, steep","Steinsburg",2,0.28000000000000003,"HEL"]
["Lawrence","SsF","Steinsburg-Shelocta association, very steep","Steinsburg",2,0.28000000000000003,"HEL"]
["Lawrence","St","Stendal silt loam, occasionally flooded","Stendal",5,0.37,"NHEL"]
["Lawrence","Tg","Tioga loam, occasionally flooded","Tioga",5,0.37,"NHEL"]
["Lawrence","To","Tioga loam, frequently flooded","Tioga",5,0.37,"NHEL"]
["Lawrence","UgC","Upshur-Gilpin complex, 8 to 15 percent slopes","Upshur",3,0.43,"HEL"]
["Lawrence","UgD","Upshur-Gilpin complex, 15 to 25 percent slopes","Upshur",3,0.43,"HEL"]
["Lawrence","UgE","Upshur-Gilpin complex, 25 to 40 percent slopes","Upshur",3,0.43,"HEL"]
["Lawrence","UgF","Upshur-Gilpin complex, 40 to 70 percent slopes","Upshur",3,0.43,"HEL"]
["Lawrence","UsE","Upshur-Gilpin-Steinsburg association, steep","Upshur",3,0.43,"HEL"]
["Lawrence","UtF","Upshur-Rock outcrop association, very steep","Upshur",3,0.43,"HEL"]
["Lawrence","VaD3","Vandalia silty clay loam, 15 to 25 percent slopes, severely eroded","Vandalia",4,0.37,"HEL"]
["Lawrence","W","Water","Water"]
["Lawrence","WaB","Watertown sandy loam, 1 to 8 percent slopes","Watertown",4,0.17,"NHEL"]
["Lawrence","WeA","Weinbach silt loam, 0 to 2 percent slopes","Weinbach",4,0.43,"NHEL"]
["Lawrence","WmB","Wheeling silt loam, 1 to 6 percent slopes","Wheeling",4,0.37,"PHEL"]
["Lawrence","WmC2","Wheeling silt loam, 6 to 15 percent slopes, eroded","Wheeling",4,0.37,"HEL"]
["Lawrence","WoB","Woodsfield silt loam, 3 to 8 percent slopes","Woodsfield",3,0.43,"PHEL"]
[null,"Select","None","none"]
["Meigs","AgC","Aaron-Gilpin complex, 8 to 15 percent slopes","Aaron",3,0.37,"HEL"]
["Meigs","AuC2","Aaron-Upshur complex, 8 to 15 percent slopes, eroded","Aaron",3,0.37,"HEL"]
["Meigs","Cg","Chagrin silt loam, frequently flooded","Chagrin",5,0.32,"NHEL"]
["Meigs","CkA","Cidermill silt loam, 0 to 2 percent slopes","Cidermill",4,0.37,"NHEL"]
["Meigs","CkB","Cidermill silt loam, 2 to 6 percent slopes","Cidermill",4,0.37,"PHEL"]
["Meigs","CnA","Conotton gravelly loam, 0 to 2 percent slopes","Conotton",3,0.24,"NHEL"]
["Meigs","CnC","Conotton gravelly loam, 6 to 12 percent slopes","Conotton",3,0.24,"HEL"]
["Meigs","CnE","Conotton gravelly loam, 18 to 40 percent slopes","Conotton",3,0.24,"HEL"]
["Meigs","DoA","Doles silt loam, 0 to 2 percent slopes","Doles",4,0.43,"NHEL"]
["Meigs","Dp","Dumps, mine","Dumps"]
["Meigs","DuC","Duncannon silt loam, 6 to 12 percent slopes","Duncannon",4,0.37,"HEL"]
["Meigs","EkA","Elkinsville silt loam, 0 to 2 percent slopes","Elkinsville",5,0.37,"NHEL"]
["Meigs","GaC","Gallia loam, 6 to 12 percent slopes","Gallia",5,0.37,"PHEL"]
["Meigs","GaD","Gallia loam, 12 to 18 percent slopes","Gallia",5,0.37,"HEL"]
["Meigs","GbA","Gallipolis silt loam, 0 to 2 percent slopes","Gallipolis",5,0.37,"NHEL"]
["Meigs","GbB","Gallipolis silt loam, 2 to 6 percent slopes","Gallipolis",5,0.37,"PHEL"]
["Meigs","GhB","Gilpin silt loam, 3 to 8 percent slopes","Gilpin",3,0.32,"PHEL"]
["Meigs","GhC2","Gilpin silt loam, 8 to 15 percent slopes, eroded","Gilpin",3,0.32,"HEL"]
["Meigs","GkD2","Gilpin-Rarden complex, 15 to 25 percent slopes, eroded","Gilpin",3,0.32,"HEL"]
["Meigs","GkE","Gilpin-Rarden complex, 25 to 40 percent slopes","Gilpin",3,0.32,"HEL"]
["Meigs","GuC","Gilpin-Upshur complex, 8 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Meigs","GuD","Gilpin-Upshur complex, 15 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Meigs","GuE","Gilpin-Upshur complex, 25 to 50 percent slopes","Gilpin",3,0.32,"HEL"]
["Meigs","GwD","Guernsey-Gilpin complex, 15 to 25 percent slopes","Guernsey",3,0.43,"HEL"]
["Meigs","GwE","Guernsey-Gilpin complex, 25 to 40 percent slopes","Guernsey",3,0.43,"HEL"]
["Meigs","KeB","Keene silt loam, 2 to 6 percent slopes","Keene",4,0.37,"PHEL"]
["Meigs","KeC","Keene silt loam, 6 to 12 percent slopes","Keene",4,0.37,"HEL"]
["Meigs","Ky","Kyger loamy sand, frequently flooded","Kyger",5,0.17,"NHEL"]
["Meigs","LaB","Lakin loamy fine sand, 1 to 6 percent slopes","Lakin",5,0.17,"NHEL"]
["Meigs","LaC","Lakin loamy fine sand, 6 to 12 percent slopes","Lakin",5,0.17,"PHEL"]
["Meigs","LaD","Lakin loamy fine sand, 12 to 18 percent slopes","Lakin",5,0.17,"HEL"]
["Meigs","LaE","Lakin loamy fine sand, 18 to 40 percent slopes","Lakin",5,0.17,"HEL"]
["Meigs","LkB","Licking silt loam, 1 to 6 percent slopes","Licking",3,0.43,"PHEL"]
["Meigs","LkC2","Licking silt loam, 6 to 12 percent slopes, eroded","Licking",3,0.43,"HEL"]
["Meigs","LkD2","Licking silt loam, 12 to 18 percent slopes, eroded","Licking",3,0.43,"HEL"]
["Meigs","Mo","Moshannon silt loam, frequently flooded","Moshannon",5,0.37,"NHEL"]
["Meigs","Nk","Newark silt loam, frequently flooded","Newark",5,0.32,"NHEL"]
["Meigs","No","Nolin silt loam, frequently flooded","Nolin",5,0.43,"NHEL"]
["Meigs","OmB","Omulga silt loam, 2 to 6 percent slopes","Omulga",3,0.43,"PHEL"]
["Meigs","OmC","Omulga silt loam, 6 to 12 percent slopes","Omulga",3,0.43,"HEL"]
["Meigs","Or","Orrville silt loam, frequently flooded","Orrville",5,0.37,"NHEL"]
["Meigs","PnB","Pinegrove coarse sandy loam, 0 to 8 percent slopes","Pinegrove",5,0.24,"PHEL"]
["Meigs","PnD","Pinegrove coarse sandy loam, 8 to 25 percent slopes","Pinegrove",5,0.24,"PHEL"]
["Meigs","PnF","Pinegrove coarse sandy loam, 25 to 70 percent slopes","Pinegrove",5,0.24,"HEL"]
["Meigs","PuB","Pinegrove silty clay loam, 0 to 8 percent slopes","Pinegrove",5,0.43,"PHEL"]
["Meigs","PuD","Pinegrove silty clay loam, 8 to 25 percent slopes","Pinegrove",5,0.43,"HEL"]
["Meigs","PuF","Pinegrove silty clay loam, 25 to 70 percent slopes","Pinegrove",5,0.43,"HEL"]
["Meigs","Px","Pits, gravel","Pits"]
["Meigs","RaC2","Rarden silt loam, 8 to 15 percent slopes, eroded","Rarden",3,0.43,"HEL"]
["Meigs","RcB","Richland silt loam, 2 to 6 percent slopes","Richland",5,0.37,"PHEL"]
["Meigs","StF","Steinsburg fine sandy loam, 40 to 70 percent slopes","Steinsburg",2,0.28000000000000003,"HEL"]
["Meigs","TaA","Taggart silt loam, 0 to 2 percent slopes","Taggart",5,0.37,"NHEL"]
["Meigs","UbC","Upshur silt loam, 8 to 15 percent slopes","Upshur",3,0.43,"HEL"]
["Meigs","UgC2","Upshur-Gilpin complex, 8 to 15 percent slopes, eroded","Upshur",3,0.43,"HEL"]
["Meigs","UgD","Upshur-Gilpin complex, 15 to 25 percent slopes","Upshur",3,0.43,"HEL"]
["Meigs","UgE","Upshur-Gilpin complex, 25 to 50 percent slopes","Upshur",3,0.43,"HEL"]
["Meigs","UsD","Upshur-Steinsburg complex, 15 to 25 percent slopes","Upshur",3,0.43,"HEL"]
["Meigs","UsE","Upshur-Steinsburg complex, 25 to 50 percent slopes","Upshur",3,0.43,"HEL"]
["Meigs","VaC2","Vandalia silt loam, 8 to 15 percent slopes, eroded","Vandalia",4,0.37,"HEL"]
["Meigs","VaD2","Vandalia silt loam, 15 to 25 percent slopes, eroded","Vandalia",4,0.37,"HEL"]
["Meigs","VnB2","Vincent silty clay loam, 2 to 6 percent slopes, eroded","Vincent",3,0.43,"PHEL"]
["Meigs","VnC2","Vincent silty clay loam, 6 to 12 percent slopes, eroded","Vincent",3,0.43,"HEL"]
["Meigs","W","Water","Water"]
["Meigs","WgD","Westmoreland-Gilpin complex, 15 to 25 percent slopes","Westmoreland",3,0.37,"HEL"]
["Meigs","WgE","Westmoreland-Gilpin complex, 25 to 40 percent slopes","Westmoreland",3,0.37,"HEL"]
["Meigs","WgF","Westmoreland-Gilpin complex, 40 to 70 percent slopes","Westmoreland",3,0.37,"HEL"]
["Meigs","WoB","Woodsfield silt loam, 2 to 6 percent slopes","Woodsfield",3,0.43,"PHEL"]
[null,"Select","None","none"]
["Pickaway","AdB2","Alexandria silt loam, 2 to 6 percent slopes, eroded","Alexandria",4,0.37,"PHEL"]
["Pickaway","AdC2","Alexandria silt loam, 6 to 12 percent slopes, eroded","Alexandria",4,0.37,"PHEL"]
["Pickaway","AdD2","Alexandria silt loam, 12 to 18 percent slopes, eroded","Alexandria",4,0.37,"HEL"]
["Pickaway","AdE","Alexandria silt loam, 18 to 35 percent slopes","Alexandria",4,0.37,"HEL"]
["Pickaway","Ag","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Pickaway","BnA","Bennington silt loam, 0 to 2 percent slopes","Bennington",3,0.43,"NHEL"]
["Pickaway","BnB","Bennington silt loam, 2 to 6 percent slopes","Bennington",3,0.43,"PHEL"]
["Pickaway","CaB","Cana Variant silt loam, 2 to 6 percent slopes","Cana",4,0.37,"PHEL"]
["Pickaway","CaD","Cana Variant silt loam, 6 to 18 percent slopes","Cana",4,0.37,"PHEL"]
["Pickaway","CaF","Cana Variant silt loam, 18 to 50 percent slopes","Cana",4,0.37,"HEL"]
["Pickaway","CdB","Cardington silt loam, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Pickaway","CdC2","Cardington silt loam, 6 to 12 percent slopes, eroded","Cardington",4,0.37,"PHEL"]
["Pickaway","Cf","Carlisle muck","Carlisle",2,null,"NHEL"]
["Pickaway","CgC","Casco gravelly loam, 6 to 12 percent slopes","Casco",3,0.24,"PHEL"]
["Pickaway","ChD","Casco-Kendallville complex, 12 to 18 percent slopes","Casco",3,0.24,"HEL"]
["Pickaway","ChE","Casco-Kendallville complex, 18 to 35 percent slopes","Casco",3,0.24,"HEL"]
["Pickaway","CkD","Casco-Rodman gravelly loams, 12 to 18 percent slopes","Casco",3,0.24,"HEL"]
["Pickaway","CkE","Casco-Rodman gravelly loams, 18 to 35 percent slopes","Casco",3,0.24,"HEL"]
["Pickaway","ClA","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Pickaway","ClB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Pickaway","CnC","Celina Variant silt loam, 6 to 15 percent slopes","Celina",4,0.37,"PHEL"]
["Pickaway","CoA","Corwin silt loam, 0 to 2 percent slopes","Corwin",5,0.28000000000000003,"NHEL"]
["Pickaway","CoB","Corwin silt loam, 2 to 6 percent slopes","Corwin",5,0.28000000000000003,"PHEL"]
["Pickaway","CrA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Pickaway","CrB","Crosby silt loam, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Pickaway","CuA","Crosby-Urban land complex, nearly level","Crosby",3,0.43,"NHEL"]
["Pickaway","Ee","Eel silt loam, occasionally flooded","Eel",5,0.37,"NHEL"]
["Pickaway","ElA","Eldean loam, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Pickaway","ElB","Eldean loam, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Pickaway","ElC2","Eldean loam, 6 to 12 percent slopes, eroded","Eldean",4,0.37,"PHEL"]
["Pickaway","EnA","Eldean gravelly loam, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Pickaway","EnB2","Eldean gravelly loam, 2 to 6 percent slopes, eroded","Eldean",4,0.37,"PHEL"]
["Pickaway","EpA","Eldean-Kendallville loams, 0 to 2 percent slopes","Eldean",4,0.37,"NHEL"]
["Pickaway","EpB","Eldean-Kendallville loams, 2 to 6 percent slopes","Eldean",4,0.37,"PHEL"]
["Pickaway","EpC2","Eldean-Kendallville loams, 6 to 12 percent slopes, eroded","Eldean",4,0.37,"PHEL"]
["Pickaway","EuA","Eldean-Urban land complex, nearly level","Eldean",4,0.37,"NHEL"]
["Pickaway","EuB","Eldean-Urban land complex, gently sloping","Eldean",4,0.37,"PHEL"]
["Pickaway","Gn","Genesee silt loam, occasionally flooded","Genesee",5,0.37,"NHEL"]
["Pickaway","HeE","Hennepin-Miamian silt loams, 18 to 25 percent slopes","Hennepin",4,0.32,"HEL"]
["Pickaway","HeF","Hennepin-Miamian silt loams, 25 to 50 percent slopes","Hennepin",4,0.32,"HEL"]
["Pickaway","HnA","Henshaw silt loam, 0 to 4 percent slopes","Henshaw",4,0.43,"PHEL"]
["Pickaway","Ko","Kokomo silty clay loam","Kokomo",3,0.32,"NHEL"]
["Pickaway","Ln","Linwood muck","Linwood",2,null,"NHEL"]
["Pickaway","LoB","Loudonville silt loam, 2 to 6 percent slopes","Loudonville",4,0.32,"PHEL"]
["Pickaway","LoC","Loudonville silt loam, 6 to 18 percent slopes","Loudonville",4,0.32,"PHEL"]
["Pickaway","LoF","Loudonville silt loam, 18 to 50 percent slopes","Loudonville",4,0.32,"HEL"]
["Pickaway","Md","Medway silt loam, occasionally flooded","Medway",5,0.32,"NHEL"]
["Pickaway","MfB2","Miamian silt loam, 2 to 6 percent slopes, eroded","Miamian",5,0.37,"PHEL"]
["Pickaway","MfC2","Miamian silt loam, 6 to 12 percent slopes, eroded","Miamian",5,0.37,"PHEL"]
["Pickaway","MfD2","Miamian silt loam, 12 to 18 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Pickaway","MhC3","Miamian clay loam, 6 to 12 percent slopes, severely eroded","Miamian",4,0.37,"PHEL"]
["Pickaway","MhD3","Miamian clay loam, 12 to 18 percent slopes, severely eroded","Miamian",4,0.37,"HEL"]
["Pickaway","MkA","Miamian-Kendallville silt loams, 0 to 2 percent slopes","Miamian",5,0.37,"NHEL"]
["Pickaway","MkB","Miamian-Kendallville silt loams, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Pickaway","MkC2","Miamian-Kendallville silt loams, 6 to 12 percent slopes, eroded","Miamian",5,0.37,"PHEL"]
["Pickaway","MkD2","Miamian-Kendallville silt loams, 12 to 18 percent slopes, eroded","Miamian",5,0.37,"HEL"]
["Pickaway","MlA","Miamian-Lewisburg silt loams, 0 to 2 percent slopes","Miamian",5,0.37,"NHEL"]
["Pickaway","MlB","Miamian-Lewisburg silt loams, 2 to 6 percent slopes","Miamian",5,0.37,"PHEL"]
["Pickaway","MmB","Miamian-Urban land complex, gently undulating","Miamian",5,0.37,"PHEL"]
["Pickaway","Mt","Montgomery silty clay loam","Montgomery",5,0.37,"NHEL"]
["Pickaway","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Pickaway","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Pickaway","Pa","Patton silty clay loam","Patton",5,0.28000000000000003,"NHEL"]
["Pickaway","Pg","Pits, gravel","Pits"]
["Pickaway","PrB","Princeton sandy loam, 2 to 6 percent slopes","Princeton",5,0.24,"PHEL"]
["Pickaway","PrC","Princeton sandy loam, 6 to 12 percent slopes","Princeton",5,0.24,"PHEL"]
["Pickaway","Rh","Riverwash","Riverwash"]
["Pickaway","RoC","Rodman gravelly sandy loam, 4 to 12 percent slopes","Rodman",3,0.15,"PHEL"]
["Pickaway","Rs","Ross loam, occasionally flooded","Ross",5,0.32,"NHEL"]
["Pickaway","Rt","Ross silt loam, overwash, frequently flooded","Ross",5,0.32,"NHEL"]
["Pickaway","Sh","Shoals silt loam, occasionally flooded","Shoals",5,0.37,"NHEL"]
["Pickaway","SlA","Sleeth silt loam, 0 to 2 percent slopes","Sleeth",5,0.32,"NHEL"]
["Pickaway","Sn","Sloan silt loam, occasionally flooded","Sloan",5,0.37,"NHEL"]
["Pickaway","St","Stonelick sandy loam","Stonelick",5,0.24,"NHEL"]
["Pickaway","ThA","Thackery silt loam, 0 to 2 percent slopes","Thackery",4,0.37,"NHEL"]
["Pickaway","ThB","Thackery silt loam, 2 to 6 percent slopes","Thackery",4,0.37,"PHEL"]
["Pickaway","TpA","Tippecanoe silt loam, 0 to 2 percent slopes","Tippecanoe",5,0.32,"NHEL"]
["Pickaway","Ud","Udorthents","Udorthents"]
["Pickaway","Ur","Urban land","Urban"]
["Pickaway","W","Water","Water"]
["Pickaway","WbA","Warsaw loam, 0 to 2 percent slopes","Warsaw",4,0.28000000000000003,"NHEL"]
["Pickaway","WbB","Warsaw loam, 2 to 6 percent slopes","Warsaw",4,0.28000000000000003,"PHEL"]
["Pickaway","WeA","Wea silt loam, 0 to 2 percent slopes","Wea",5,0.32,"NHEL"]
["Pickaway","WeB","Wea silt loam, 2 to 6 percent slopes","Wea",5,0.32,"PHEL"]
["Pickaway","Ws","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
[null,"Select","None","none"]
["Pike","AgD","Allegheny Variant loam, 15 to 25 percent slopes","Allegheny",5,0.32,"HEL"]
["Pike","BdC","Blairton-Rarden-Gilpin association, rolling","Blairton",3,0.43,"HEL"]
["Pike","BrB2","Bratton silt loam, 3 to 8 percent slopes, eroded","Bratton",4,0.37,"PHEL"]
["Pike","Cf","Clifty silt loam, occasionally flooded","Clifty",5,0.32,"NHEL"]
["Pike","CoB","Coolville silt loam, 1 to 8 percent slopes","Coolville",4,0.43,"PHEL"]
["Pike","CoC","Coolville silt loam, 8 to 15 percent slopes","Coolville",4,0.43,"HEL"]
["Pike","CpC","Coolville-Blairton association, rolling","Coolville",4,0.43,"HEL"]
["Pike","DoA","Doles silt loam, 0 to 3 percent slopes","Doles",4,0.43,"NHEL"]
["Pike","En","Elkinsville silt loam, rarely flooded","Elkinsville",5,0.37,"NHEL"]
["Pike","ErC","Ernest silt loam, 8 to 15 percent slopes","Ernest",3,0.43,"HEL"]
["Pike","FoA","Fox loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Pike","FoB","Fox loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Pike","FoC","Fox loam, 6 to 12 percent slopes","Fox",4,0.37,"PHEL"]
["Pike","Ge","Genesee silt loam, occasionally flooded","Genesee",5,0.37,"NHEL"]
["Pike","GpB","Gilpin silt loam, 3 to 8 percent slopes","Gilpin",3,0.32,"PHEL"]
["Pike","GpC","Gilpin silt loam, 8 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Pike","GpD","Gilpin silt loam, 15 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Pike","Ha","Haymond silt loam, occasionally flooded","Haymond",5,0.37,"NHEL"]
["Pike","Hu","Huntington silt loam, occasionally flooded","Huntington",5,0.28000000000000003,"NHEL"]
["Pike","LaC","Latham silt loam, 8 to 15 percent slopes","Latham",3,0.43,"HEL"]
["Pike","LdD","Latham-Wharton silt loams, 15 to 25 percent slopes","Latham",3,0.43,"HEL"]
["Pike","MaB2","Markland silty clay loam, 3 to 8 percent slopes, eroded","Markland",3,0.43,"PHEL"]
["Pike","MaC2","Markland silty clay loam, 8 to 15 percent slopes, eroded","Markland",3,0.43,"HEL"]
["Pike","MaD2","Markland silty clay loam, 15 to 25 percent slopes, eroded","Markland",3,0.43,"HEL"]
["Pike","Mh","Martinsville loam, rarely flooded","Martinsville",5,0.37,"NHEL"]
["Pike","MkA","McGary silt loam, 0 to 4 percent slopes","McGary",3,0.43,"PHEL"]
["Pike","Mn","Melvin silt loam, occasionally flooded","Melvin",5,0.43,"NHEL"]
["Pike","MoD","Miami Variant silt loam, 15 to 30 percent slopes","Miami",5,0.37,"HEL"]
["Pike","MpD3","Miamian clay loam, 15 to 25 percent slopes, severely eroded","Miamian",4,0.37,"HEL"]
["Pike","Mr","Montgomery Variant silt loam, frequently floooded","Montgomery",5,0.37,"NHEL"]
["Pike","NgC","Negley loam, 8 to 15 percent slopes","Negley",3,0.32,"HEL"]
["Pike","NgD","Negley loam, 15 to 25 percent slopes","Negley",3,0.32,"HEL"]
["Pike","NgE","Negley loam, 25 to 35 percent slopes","Negley",3,0.32,"HEL"]
["Pike","OmA","Omulga silt loam, 0 to 3 percent slopes","Omulga",3,0.43,"PHEL"]
["Pike","OmB","Omulga silt loam, 3 to 8 percent slopes","Omulga",3,0.43,"PHEL"]
["Pike","OmC","Omulga silt loam, 8 to 15 percent slopes","Omulga",3,0.43,"HEL"]
["Pike","OoC2","Opequon-Bratton silt loams, 8 to 15 percent slopes, eroded","Opequon",1,0.43,"HEL"]
["Pike","OpD2","Opequon silt loam, 15 to 30 percent slopes, eroded","Opequon",1,0.43,"HEL"]
["Pike","Or","Orrville silt loam, frequently flooded","Orrville",5,0.37,"NHEL"]
["Pike","OwA","Otwell silt loam, 0 to 3 percent slopes","Otwell",3,0.43,"PHEL"]
["Pike","OwB","Otwell silt loam, 3 to 8 percent slopes","Otwell",3,0.43,"PHEL"]
["Pike","PaA","Parke silt loam, 0 to 3 percent slopes","Parke",5,0.37,"NHEL"]
["Pike","PaB","Parke silt loam, 3 to 8 percent slopes","Parke",5,0.37,"PHEL"]
["Pike","Pe","Peoga silt loam","Peoga",4,0.43,"NHEL"]
["Pike","Pg","Pits, gravel","Pits"]
["Pike","Pn","Pits, quarry","Pits"]
["Pike","PrB","Princeton fine sandy loam, 3 to 8 percent slopes","Princeton",5,0.24,"PHEL"]
["Pike","PrC","Princeton fine sandy loam, 8 to 15 percent slopes","Princeton",5,0.24,"PHEL"]
["Pike","PrD","Princeton fine sandy loam, 15 to 30 percent slopes","Princeton",5,0.24,"HEL"]
["Pike","Pu","Purdy Variant silt loam","Purdy",3,0.43,"NHEL"]
["Pike","RdC","Rarden silt loam, 8 to 15 percent slopes","Rarden",3,0.43,"HEL"]
["Pike","RdD","Rarden silt loam, 15 to 25 percent slopes","Rarden",3,0.43,"HEL"]
["Pike","RhC","Richland silt loam, clayey substratum, 8 to 15 percent slopes","Richland",5,0.37,"PHEL"]
["Pike","ShD","Shelocta silt loam, 15 to 25 percent slopes","Shelocta",4,0.32,"HEL"]
["Pike","SnF","Shelocta-Brownsville association, steep","Shelocta",4,0.28000000000000003,"HEL"]
["Pike","SoF","Shelocta-Rigley association, steep","Shelocta",4,0.32,"HEL"]
["Pike","SpF","Shelocta-Latham association, steep","Shelocta",4,0.32,"HEL"]
["Pike","SrA","Skidmore Variant gravelly loam, 0 to 3 percent slopes","Skidmore",2,0.28000000000000003,"NHEL"]
["Pike","SrB","Skidmore Variant gravelly loam, 3 to 8 percent slopes","Skidmore",2,0.28000000000000003,"PHEL"]
["Pike","Ss","Stendal silt loam, occasionally flooded","Stendal",5,0.37,"NHEL"]
["Pike","St","Stonelick loam, occasionally flooded","Stonelick",5,0.24,"NHEL"]
["Pike","TgA","Taggart silt loam, 0 to 4 percent slopes","Taggart",5,0.37,"NHEL"]
["Pike","Th","Taggart silt loam, rarely flooded","Taggart",5,0.37,"NHEL"]
["Pike","TkA","Tilsit silt loam, 0 to 4 percent slopes","Tilsit",3,0.43,"PHEL"]
["Pike","TrD","Trappist silt loam, 15 to 25 percent slopes","Trappist",3,0.37,"HEL"]
["Pike","TsF","Trappist-Shelocta association, steep","Trappist",3,0.37,"HEL"]
["Pike","UoA","Urbanland-Omulga complex, 0 to 6 percent slopes","Urbanland"]
["Pike","W","Water","Water"]
["Pike","WeB","Wernock Variant silt loam, 3 to 8 percent slopes","Wernock",4,0.37,"PHEL"]
["Pike","WhD","Wharton silt loam, 15 to 25 percent slopes","Wharton",3,0.37,"HEL"]
["Pike","Wm","Wilbur silt loam, occasionally flooded","Wilbur",5,0.37,"NHEL"]
["Pike","WyB2","Wyatt silty clay loam, 3 to 8 percent slopes, eroded","Wyatt",2,0.43,"PHEL"]
["Pike","WyC2","Wyatt silty clay loam, 8 to 15 percent slopes, eroded","Wyatt",2,0.43,"HEL"]
[null,"Select","None","none"]
["Ross","Ab ","Abscota sandy loam, calcareous variant","Abscota",5,0.17,"NHEL"]
["Ross","AdC2","Alexandria silt loam, 6 to 12 percent slopes, moderately eroded","Alexandria",4,0.37,"PHEL"]
["Ross","AdD2","Alexandria silt loam, 12 to 18 percent slopes, moderately eroded","Alexandria",4,0.37,"HEL"]
["Ross","AdE2","Alexandria silt loam, 18 to 25 percent slopes, moderately eroded","Alexandria",4,0.37,"HEL"]
["Ross","AdF2"," Alexandria silt loam, 25 to 40 percent slopes, moderately eroded","Alexandria",4,0.37,"HEL"]
["Ross","AeD3","Alexandria soils, 12 to 18 percent slopes, severely eroded","Alexandria",4,0.37,"HEL"]
["Ross","AeE3","Alexandria soils, 18 to 25 percent slopes, severely eroded","Alexandria",4,0.37,"HEL"]
["Ross","AfC2","Alford silt loam, 6 to 12 percent slopes, moderately eroded","Alford",5,0.37,"PHEL"]
["Ross","AfD2","Alford silt loam, 12 to 18 percent slopes, moderately eroded","Alford",5,0.37,"HEL"]
["Ross","AfE2","Alford silt loam, 18 to 25 percent slopes, moderately eroded","Alford",5,0.37,"HEL"]
["Ross","Ag ","Algiers silt loam","Algiers",5,0.37,"NHEL"]
["Ross","AlA","Alvin fine sandy loam, 0 to 2 percent slopes","Alvin",5,0.24,"NHEL"]
["Ross","AlB","Alvin fine sandy loam, 2 to 6 percent slopes","Alvin",5,0.24,"PHEL"]
["Ross","AlC2","Alvin fine sandy loam, 6 to 12 percent slopes, moderately eroded","Alvin",5,0.24,"PHEL"]
["Ross","AvA","Avonburg silt loam, 0 to 2 percent slopes","Avonburg",4,0.43,"NHEL"]
["Ross","AvB","Avonburg silt loam, 2 to 6 percent slopes","Avonburg",4,0.43,"PHEL"]
["Ross","BaA","Bartle silt loam, 0 to 2 percent slopes","Bartle",4,0.43,"NHEL"]
["Ross","BaB","Bartle silt loam, 2 to 6 percent slopes","Bartle",4,0.43,"PHEL"]
["Ross","Bo ","Bonpas silty clay loam","Bonpas",5,0.28000000000000003,"NHEL"]
["Ross","Br ","Brookston silt loam","Brookston",5,0.28000000000000003,"NHEL"]
["Ross","Bs","Brookston silty clay loam","Brookston",5,0.28000000000000003,"NHEL"]
["Ross","CaB","Cana silt loam, 2 to 6 percent slopes","Cana",4,0.37,"PHEL"]
["Ross","CaB2","Cana silt loam, 2 to 6 percent slopes, moderately eroded","Cana",4,0.37,"PHEL"]
["Ross","CaC","Cana silt loam, 6 to 12 percent slopes","Cana",4,0.37,"PHEL"]
["Ross","CaC2","Cana silt loam, 6 to 12 percent slopes, moderately eroded","Cana",4,0.37,"PHEL"]
["Ross","CaD","Cana silt loam, 12 to 18 percent slopes","Cana",4,0.37,"HEL"]
["Ross","CaD2","Cana silt loam, 12 to 18 percent slopes, moderately eroded","Cana",4,0.37,"HEL"]
["Ross","CaE","Cana silt loam, 18 to 25 percent slopes","Cana",4,0.37,"HEL"]
["Ross","CaF","Cana silt loam, 25 to 45 percent slopes","Cana",4,0.37,"HEL"]
["Ross","CeC3","Cana soils, 6 to 12 percent slopes, severely eroded","Cana",3,0.37,"PHEL"]
["Ross","CeD3","Cana soils, 12 to 18 percent slopes, severely eroded","Cana",3,0.37,"HEL"]
["Ross","CeF3","Cana soils, 18 to 35 percent slopes, severely eroded","Cana",3,0.37,"HEL"]
["Ross","CfE","Cana very flaggy silt loam, 18 to 25 percent slopes","Cana",4,0.37,"HEL"]
["Ross","CfF","Cana very flaggy silt loam, 25 to 35 percent slopes","Cana",4,0.37,"HEL"]
["Ross","CgF","Cana-Colyer very flaggy silt loams, 25 to 35 percent slopes","Cana",4,0.37,"HEL"]
["Ross","ChB","Cardington silt loam, 2 to 6 percent slopes","Cardington",4,0.37,"PHEL"]
["Ross","ChC2","Cardington silt loam, 6 to 12 percent slopes, moderately eroded","Cardington",4,0.37,"PHEL"]
["Ross","ChD2","Cardington silt loam, 12 to 18 percent slopes, moderately eroded","Cardington",4,0.37,"HEL"]
["Ross","CkC3","Cardington soils, 6 to 12 percent slopes, severely eroded","Cardington",4,0.37,"PHEL"]
["Ross","CkD3","Cardington soils, 12 to 18 percent slopes, severely eroded","Cardington",4,0.37,"HEL"]
["Ross","Cm","Carlisle muck","Carlisle",2,null,"NHEL"]
["Ross","CnE2","Casco and Lorenzo soils, 18 to 25 percent slopes, moderately eroded","Casco",3,0.24,"HEL"]
["Ross","CnE3","Casco and Lorenzo soils, 18 to 25 percent slopes, severely eroded","Casco",3,0.24,"HEL"]
["Ross","CoA","Celina silt loam, 0 to 2 percent slopes","Celina",5,0.37,"NHEL"]
["Ross","CoB","Celina silt loam, 2 to 6 percent slopes","Celina",5,0.37,"PHEL"]
["Ross","CoB2","Celina silt loam, 2 to 6 percent slopes, moderately eroded","Celina",5,0.37,"PHEL"]
["Ross","Cp","Clermont silt loam","Clermont",5,0.37,"NHEL"]
["Ross","CrE","Colyer shaly silt loam, 12 to 25 percent slopes","Colyer",2,0.28000000000000003,"HEL"]
["Ross","CrG","Colyer shaly silt loam, 25 to 75 percent slopes","Colyer",2,0.28000000000000003,"HEL"]
["Ross","CsE","Colyer-Cana complex, 18 to 25 percent slopes","Colyer",2,0.28000000000000003,"HEL"]
["Ross","CsG","Colyer-Cana complex, 25 to 75 percent slopes","Colyer",2,0.28000000000000003,"HEL"]
["Ross","CtB","Coolville silt loam, 2 to 6 percent slopes","Coolville",4,0.43,"PHEL"]
["Ross","CtB2","Coolville silt loam, 2 to 6 percent slopes, moderately eroded","Coolville",4,0.43,"PHEL"]
["Ross","CtC2","Coolville silt loam, 6 to 12 percent slopes, moderately eroded","Coolville",4,0.43,"PHEL"]
["Ross","CvA","Crosby silt loam, 0 to 2 percent slopes","Crosby",3,0.43,"NHEL"]
["Ross","CvB","Crosby silt loam, 2 to 6 percent slopes","Crosby",3,0.43,"PHEL"]
["Ross","CwB","Cruze silt loam, 2 to 6 percent slopes","Cruze",3,0.37,"PHEL"]
["Ross","CwC2","Cruze silt loam, 6 to 12 percent slopes, moderately eroded","Cruze",3,0.37,"PHEL"]
["Ross","CwD2","Cruze silt loam, 12 to 18 percent slopes, moderately eroded","Cruze",3,0.37,"HEL"]
["Ross","CwE","Cruze silt loam, 18 to 25 percent slopes","Cruze",3,0.37,"HEL"]
["Ross","CzC3","Cruze soils, 6 to 12 percent slopes, severely eroded","Cruze",2,0.37,"PHEL"]
["Ross","CzD3","Cruze soils, 12 to 18 percent slopes, severely eroded","Cruze",2,0.37,"HEL"]
["Ross","DnG","Dekalb and Neotoma extremely rocky fine sandy loams, 25 to 70 percent slopes","Dekalb",2,0.24,"HEL"]
["Ross","DoG","Dekalb and Neotoma fine sandy loams, 35 to 70 percent slopes","Dekalb",2,0.24,"HEL"]
["Ross","Ee","Eel silt loam","Eel",5,0.37,"NHEL"]
["Ross","Fa","Fawcett silt loam","Fawcett",3,0.43,"NHEL"]
["Ross","FgA","Fox gravelly loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Ross","FgB","Fox gravelly loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Ross","FgC2","Fox gravelly loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Ross","FlA","Fox loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Ross","FlB","Fox loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Ross","FlC2","Fox loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Ross","FmA","Fox sandy loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Ross","FmB","Fox sandy loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Ross","FnA","Fox silt loam, 0 to 2 percent slopes","Fox",4,0.37,"NHEL"]
["Ross","FnB","Fox silt loam, 2 to 6 percent slopes","Fox",4,0.37,"PHEL"]
["Ross","FnB2","Fox silt loam, 2 to 6 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Ross","FnC2","Fox silt loam, 6 to 12 percent slopes, moderately eroded","Fox",4,0.37,"PHEL"]
["Ross","FoC3","Fox soils, 6 to 12 percent slopes, severely eroded","Fox",3,0.37,"PHEL"]
["Ross","FwD2","Fox and Warsaw soils, 12 to 18 percent slopes, moderately eroded","Fox",4,0.37,"HEL"]
["Ross","FwD3","Fox and Warsaw soils, 12 to 18 percent slopes, severely eroded","Fox",3,0.37,"HEL"]
["Ross","Ge","Genesee fine sandy loam","Genesee",5,0.37,"NHEL"]
["Ross","Gn","Genesee silt loam","Genesee",5,0.37,"NHEL"]
["Ross","Go","Genesee silty clay loam","Genesee",5,0.37,"NHEL"]
["Ross","He","Henshaw silt loam","Henshaw",4,0.43,"NHEL"]
["Ross","HkC2","Hickory silt loam, 6 to 12 percent slopes, moderately eroded","Hickory",5,0.37,"PHEL"]
["Ross","HkD2","Hickory silt loam, 12 to 18 percent slopes, moderately eroded","Hickory",5,0.37,"HEL"]
["Ross","HkE","Hickory silt loam, 18 to 25 percent slopes","Hickory",5,0.37,"HEL"]
["Ross","HoD3","Hickory soils, 12 to 18 percent slopes, severely eroded","Hickory",4,0.37,"HEL"]
["Ross","HoE3","Hickory soils, 18 to 25 percent slopes, severely eroded","Hickory",4,0.37,"HEL"]
["Ross","HoF","Hickory soils, 25 to 45 percent slopes","Hickory",5,0.37,"HEL"]
["Ross","KeA","Kendallville silt loam, 0 to 2 percent slopes","Kendallville",3,0.37,"NHEL"]
["Ross","KeB","Kendallville silt loam, 2 to 6 percent slopes","Kendallville",3,0.37,"PHEL"]
["Ross","KeC2","Kendallville silt loam, 6 to 12 percent slopes, moderately eroded","Kendallville",3,0.37,"PHEL"]
["Ross","KeD2","Kendallville silt loam, 12 to 18 percent slopes, moderately eroded","Kendallville",3,0.37,"HEL"]
["Ross","KeE2","Kendallville silt loam, 18 to 25 percent slopes, moderately eroded ","Kendallville",3,0.37,"HEL"]
["Ross","KnC3","Kendallville soils, 6 to 12 percent slopes, severely eroded","Kendallville",2,0.37,"HEL"]
["Ross","KnD3","Kendallville soils, 12 to 18 percent slopes, severely eroded","Kendallville",2,0.37,"HEL"]
["Ross","KnE3","Kendallville soils, 18 to 25 percent slopes, severely eroded","Kendallville",2,0.37,"HEL"]
["Ross","KnF2","Kendallville soils, 25 to 45 percent slopes, moderately eroded","Kendallville",3,0.37,"HEL"]
["Ross","LaC2","Latham silt loam, 6 to 12 percent slopes, moderately eroded","Latham",3,0.43,"PHEL"]
["Ross","LaD2","Latham silt loam, 12 to 18 percent slopes, moderately eroded","Latham",3,0.43,"HEL"]
["Ross","LaE","Latham silt loam, 18 to 25 percent slopes","Latham",3,0.43,"HEL"]
["Ross","LaE2","Latham silt loam, 18 to 25 percent slopes, moderately eroded","Latham",3,0.43,"HEL"]
["Ross","LhD3","Latham soils, 12 to 18 percent slopes, severely eroded","Latham",2,0.43,"HEL"]
["Ross","LhE3","Latham soils, 18 to 25 percent slopes, severely eroded","Latham",2,0.43,"HEL"]
["Ross","LhF","Latham soils, 25 to 40 percent slopes","Latham",3,0.43,"HEL"]
["Ross","LoC","Loudonville silt loam, 6 to 12 percent slopes","Loudonville",4,0.32,"PHEL"]
["Ross","LoD2","Loudonville silt loam, 12 to 18 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Ross","LoE2","Loudonville silt loam, 18 to 25 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Ross","LoF2","Loudonville silt loam, 25 to 45 percent slopes, moderately eroded","Loudonville",4,0.32,"HEL"]
["Ross","MaA","Markland silt loam, 0 to 2 percent slopes","Markland",3,0.43,"NHEL"]
["Ross","MaB","Markland silt loam, 2 to 6 percent slopes","Markland",3,0.43,"PHEL"]
["Ross","MaC2","Markland silt loam, 6 to 12 percent slopes, moderately eroded","Markland",3,0.43,"PHEL"]
["Ross","MaD2","Markland silt loam, 12 to 18 percent slopes, moderately eroded","Markland",3,0.43,"HEL"]
["Ross","MaE2","Markland silt loam, 18 to 25 percent slopes, moderately eroded","Markland",3,0.43,"HEL"]
["Ross","MaF2","Markland silt loam, 25 to 35 percent slopes, moderately eroded","Markland",3,0.43,"HEL"]
["Ross","MeC3","Markland soils, 6 to 12 percent slopes, severely eroded","Markland",2,0.43,"HEL"]
["Ross","MeD3","Markland soils, 12 to 18 percent slopes, severely eroded","Markland",2,0.43,"HEL"]
["Ross","MgA","McGary silt loam, 0 to 2 percent slopes","McGary",3,0.43,"NHEL"]
["Ross","MgB","McGary silt loam, 2 to 6 percent slopes","McGary",3,0.43,"PHEL"]
["Ross","MhD3","Mentor soils, 12 to 18 percent slopes, severely eroded","Mentor",5,0.37,"HEL"]
["Ross","MkA","Mentor very fine sandy loam, 0 to 2 percent slopes","Mentor",5,0.37,"NHEL"]
["Ross","MkB","Mentor very fine sandy loam, 2 to 6 percent slopes","Mentor",5,0.37,"PHEL"]
["Ross","MkC2","Mentor very fine sandy loam, 6 to 12 percent slopes, moderately eroded","Mentor",5,0.37,"PHEL"]
["Ross","MkD2","Mentor very fine sandy loam, 12 to 18 percent slopes, moderately eroded","Mentor",5,0.37,"HEL"]
["Ross","MkE2","Mentor very fine sandy loam, 18 to 25 percent slopes, moderately eroded","Mentor",5,0.37,"HEL"]
["Ross","MlB","Miami silt loam, 2 to 6 percent slopes","Miami",5,0.37,"PHEL"]
["Ross","MlB2","Miami silt loam, 2 to 6 percent slopes, moderately eroded","Miami",5,0.37,"PHEL"]
["Ross","MlC","Miami silt loam, 6 to 12 percent slopes","Miami",5,0.37,"PHEL"]
["Ross","MlC2","Miami silt loam, 6 to 12 percent slopes, moderately eroded","Miami",5,0.37,"PHEL"]
["Ross","MlD","Miami silt loam, 12 to 18 percent slopes","Miami",5,0.37,"HEL"]
["Ross","MlD2","Miami silt loam, 12 to 18 percent slopes, moderately eroded","Miami",5,0.37,"HEL"]
["Ross","MlE","Miami silt loam, 18 to 25 percent slopes","Miami",5,0.37,"HEL"]
["Ross","MmB3","Miami soils, 2 to 6 percent slopes, severely eroded","Miami",4,0.37,"PHEL"]
["Ross","MmC3","Miami soils, 6 to 12 percent slopes, severely eroded","Miami",4,0.37,"PHEL"]
["Ross","MmD3","Miami soils, 12 to 18 percent slopes, severely eroded","Miami",4,0.37,"HEL"]
["Ross","MmE3","Miami soils, 18 to 25 percent slopes, severely eroded","Miami",4,0.37,"HEL"]
["Ross","MmF","Miami soils, 25 to 40 percent slopes","Miami",5,0.37,"HEL"]
["Ross","Mn","Millsdale silty clay loam","Millsdale",4,0.32,"NHEL"]
["Ross","MoB","Milton silt loam, 2 to 6 percent slopes","Milton",4,0.37,"PHEL"]
["Ross","MoC2","Milton silt loam, 6 to 12 percent slopes, moderately eroded","Milton",4,0.37,"PHEL"]
["Ross","MoE2","Milton silt loam, 18 to 25 percent slopes, moderately eroded","Milton",4,0.37,"HEL"]
["Ross","MpA","Monongahela silt loam, 0 to 2 percent slopes","Monongahela",3,0.43,"NHEL"]
["Ross","MpB","Monongahela silt loam, 2 to 6 percent slopes","Monongahela",3,0.43,"PHEL"]
["Ross","MpC2","Monongahela silt loam, 6 to 12 percent slopes, moderately eroded","Monongahela",3,0.43,"PHEL"]
["Ross","MrD","Muskingum very stony silt loam, 6 to 18 percent slopes","Muskingum",3,0.37,"PHEL"]
["Ross","MsE","Muskingum and Latham stony silt loams, 12 to 25 percent slopes","Muskingum",3,0.37,"HEL"]
["Ross","MtG","Muskingum and Latham very stony silt loams, 25 to 70 percent slopes","Muskingum",3,0.37,"HEL"]
["Ross","MuE","Muskingum, Berks, and Neotoma very stony silt loams, 18 to 25 percent slopes","Muskingum",3,0.37,"HEL"]
["Ross","MuG","Muskingum, Berks, and Neotoma very stony silt loams, 25 to 70 percent slopes","Muskingum",3,0.37,"HEL"]
["Ross","NeC2","Negley soils, 6 to 12 percent slopes, moderately eroded","Negley",3,0.32,"PHEL"]
["Ross","NfD2","Negley and Fox soils, 12 to 18 percent slopes, moderately eroded","Negley",3,0.32,"HEL"]
["Ross","NfD3","Negley and Fox soils, 12 to 18 percent slopes, severely eroded","Negley",2,0.32,"HEL"]
["Ross","NfE2","Negley and Fox soils, 18 to 25 percent slopes, moderately eroded","Negley",3,0.32,"HEL"]
["Ross","NfE3","Negley and Fox soils, 18 to 25 percent slopes, severely eroded","Negley",2,0.32,"HEL"]
["Ross","NlF","Negley, Fox, and Lorenzo soils, 25 to 40 percent slopes","Negley",3,0.32,"HEL"]
["Ross","OcA","Ockley silt loam, 0 to 2 percent slopes","Ockley",5,0.37,"NHEL"]
["Ross","OcB","Ockley silt loam, 2 to 6 percent slopes","Ockley",5,0.37,"PHEL"]
["Ross","PaB","Parke silt loam, 2 to 6 percent slopes","Parke",5,0.37,"PHEL"]
["Ross","PaC2","Parke silt loam, 6 to 12 percent slopes, moderately eroded","Parke",5,0.37,"PHEL"]
["Ross","PaD2","Parke silt loam, 12 to 18 percent slopes, moderately eroded","Parke",5,0.37,"HEL"]
["Ross","PaE","Parke silt loam, 18 to 25 percent slopes","Parke",5,0.37,"HEL"]
["Ross","PeC3","Parke soils, 6 to 12 percent slopes, severely eroded","Parke",4,0.37,"PHEL"]
["Ross","PeD3","Parke soils, 12 to 18 percent slopes, severely eroded","Parke",4,0.37,"HEL"]
["Ross","PeE3","Parke soils, 18 to 25 percent slopes, severely eroded","Parke",4,0.37,"HEL"]
["Ross","PgC2","Parke-Negley Complex, 6 to 12 percent slopes, moderately eroded","Parke",5,0.37,"PHEL"]
["Ross","PhB","Pekin fine sandy loam, 2 to 6 percent slopes","Pekin",4,0.43,"PHEL"]
["Ross","PkA","Pekin silt loam, 0 to 2 percent slopes","Pekin",4,0.43,"NHEL"]
["Ross","PkB","Pekin silt loam, 2 to 6 percent slopes","Pekin",4,0.43,"PHEL"]
["Ross","PkC2","Pekin silt loam, 6 to 12 percent slopes, moderately eroded","Pekin",4,0.43,"PHEL"]
["Ross","PkD2","Pekin silt loam, 12 to 18 percent slopes, moderately eroded","Pekin",4,0.43,"HEL"]
["Ross","PlB","Pekin silt loam, over clay, 2 to 6 percent slopes","Pekin",4,0.43,"PHEL"]
["Ross","PlC2","Pekin silt loam, over clay, 6 to 12 percent slopes, moderately eroded","Pekin",4,0.43,"PHEL"]
["Ross","PlD2","Pekin silt loam, over clay, 12 to 18 percent slopes, moderately eroded","Pekin",4,0.43,"HEL"]
["Ross","PlE2","Pekin silt loam, over clay, 18 to 25 percent slopes, moderately eroded","Pekin",4,0.43,"HEL"]
["Ross","PmC3","Pekin soils, 6 to 12 percent slopes, severely eroded","Pekin",4,0.43,"PHEL"]
["Ross","Pn","Philo silt loam","Philo",5,0.37,"NHEL"]
["Ross","Po","Philo soils, channery variant","Philo",5,0.37,"NHEL"]
["Ross","PpA","Pike silt loam, 0 to 2 percent slopes","Pike",5,0.37,"NHEL"]
["Ross","PpB","Pike silt loam, 2 to 6 percent slopes","Pike",5,0.37,"PHEL"]
["Ross","Pr","Pope silt loam","Pope",5,0.37,"NHEL"]
["Ross","Ps","Pope soils, channery variant","Pope",5,0.37,"NHEL"]
["Ross","RaA","Rainsboro silt loam, 0 to 2 percent slopes","Rainsboro",4,0.43,"NHEL"]
["Ross","RaB","Rainsboro silt loam, 2 to 6 percent slopes","Rainsboro",4,0.43,"PHEL"]
["Ross","RaC2","Rainsboro silt loam, 6 to 12 percent slopes, moderately eroded","Rainsboro",4,0.43,"PHEL"]
["Ross","RaD2","Rainsboro silt loam, 12 to 18 percent slopes, moderately eroded","Rainsboro",4,0.43,"HEL"]
["Ross","RbC3","Rainsboro soils, 6 to 12 percent slopes, severely eroded","Rainsboro",3,0.43,"PHEL"]
["Ross","RbD3","Rainsboro soils, 12 to 18 percent slopes, severely eroded","Rainsboro",3,0.43,"HEL"]
["Ross","RdD","Rarden silt loam, 12 to 18 percent slopes","Rarden",3,0.43,"HEL"]
["Ross","RdD2","Rarden silt loam, 12 to 18 percent slopes, moderately eroded","Rarden",3,0.43,"HEL"]
["Ross","RdE2","Rarden silt loam, 18 to 25 percent slopes, moderately eroded","Rarden",3,0.43,"HEL"]
["Ross","ReD3","Rarden soils, 12 to 18 percent slopes, severely eroded","Rarden",2,0.43,"HEL"]
["Ross","RfC","Rarden and Coolville silt loams, 6 to 12 percent slopes","Rarden",3,0.43,"PHEL"]
["Ross","RfC2","Rarden and Coolville silt loams, 6 to 12 percent slopes, moderately eroded","Rarden",3,0.43,"PHEL"]
["Ross","RgC3","Rarden and Coolville soils, 6 to 12 percent slopes, severely eroded","Rarden",2,0.43,"HEL"]
["Ross","RhF2","Ritchey silt loam, 25 to 35 percent slopes, moderately eroded","Ritchey",2,0.37,"HEL"]
["Ross","Rk","Riverwash","Riverwash"]
["Ross","RIG","Rodman-Lorenzo complex, 25 to 50 percent slopes","Rodman",3,0.15,"HEL"]
["Ross","Rm","Ross fine sandy loam","Ross",5,0.32,"NHEL"]
["Ross","Rn","Ross silt loam","Ross",5,0.32,"NHEL"]
["Ross","Ro","Ross silty clay loam","Ross",5,0.32,"NHEL"]
["Ross","RpA","Rossmoyne silt loam, 0 to 2 percent slopes","Rossmoyne",4,0.37,"NHEL"]
["Ross","RpB","Rossmoyne silt loam, 2 to 6 percent slopes","Rossmoyne",4,0.37,"PHEL"]
["Ross","RpB2","Rossmoyne silt loam, 2 to 6 percent slopes, moderately eroded","Rossmoyne",4,0.37,"PHEL"]
["Ross","RpC2","Rossmoyne silt loam, 6 to 12 percent slopes, moderately eroded","Rossmoyne",4,0.37,"PHEL"]
["Ross","RpD2","Rossmoyne silt loam, 12 to 18 percent slopes, moderately eroded","Rossmoyne",4,0.37,"HEL"]
["Ross","RpE2","Rossmoyne silt loam, 18 to 25 percent slopes, moderately eroded","Rossmoyne",4,0.37,"HEL"]
["Ross","RsC3","Rossmoyne soils, 6 to 12 percent slopes, severely eroded","Rossmoyne",3,0.37,"PHEL"]
["Ross","RsD3","Rossmoyne soils, 12 to 18 percent slopes, severely eroded","Rossmoyne",3,0.37,"HEL"]
["Ross","Sh","Shoals silt loam","Shoals",5,0.37,"NHEL"]
["Ross","Sl","Sleeth silt loam","Sleeth",5,0.32,"NHEL"]
["Ross","Sn","Stendal silt loam","Stendal",5,0.37,"NHEL"]
["Ross","Sr","Stone quarries","Stone"]
["Ross","TaA","Taggart silt loam, 0 to 2 percent slopes","Taggart",5,0.37,"NHEL"]
["Ross","TaB","Taggart silt loam, 2 to 6 percent slopes","Taggart",5,0.37,"PHEL"]
["Ross","Te","Taggart silt loam, wet","Taggart",5,0.37,"NHEL"]
["Ross","ThA","Thackery silt loam, 0 to 2 percent slopes","Thackery",4,0.37,"NHEL"]
["Ross","ThB","Thackery silt loam, 2 to 6 percent slopes","Thackery",4,0.37,"PHEL"]
["Ross","Ty","Tyler silt loam","Tyler",3,0.43,"NHEL"]
["Ross","UnA","Uniontown silt loam, 0 to 2 percent slopes","Uniontown",4,0.37,"NHEL"]
["Ross","UnB","Uniontown silt loam, 2 to 6 percent slopes","Uniontown",4,0.37,"PHEL"]
["Ross","UnC2","Uniontown silt loam, 6 to 12 percent slopes, moderately eroded","Uniontown",4,0.37,"PHEL"]
["Ross","Wa","Wallkill silt loam","Wallkill",5,0.32,"NHEL"]
["Ross","We","Warners mucky silt loam","Warners",5,0.43,"NHEL"]
["Ross","Wl","Warsaw loam","Warsaw",4,0.28000000000000003,"NHEL"]
["Ross","WsA","Wea silt loam, 0 to 2 percent slopes","Wea",5,0.32,"NHEL"]
["Ross","WsB","Wea silt loam, 2 to 6 percent slopes","Wea",5,0.32,"PHEL"]
["Ross","WtC","Wellston silt loam, 6 to 12 percent slopes","Wellston",4,0.37,"PHEL"]
["Ross","Wu","Westland silty clay loam","Westland",5,0.28000000000000003,"NHEL"]
["Ross","Wv","Willette muck","Willette",2,null,"NHEL"]
[null,"Select","None","none"]
["Scioto","AfD","Alford silt loam, 10 to 25 percent slopes","Alford",5,0.37,"HEL"]
["Scioto","BeC","Berks channery silt loam, 8 to 15 percent slopes","Berks",3,0.24,"PHEL"]
["Scioto","BhD","Bethesda very shaly clay loam, 8 to 25 percent slopes","Bethesda",5,0.32,"PHEL"]
["Scioto","BrF","Brownsville-Rock outcrop association, very steep","Brownsville",5,0.2,"HEL"]
["Scioto","CaF","Casco loam, 40 to 70 percent slopes","Casco",3,0.24,"HEL"]
["Scioto","CoB","Coolville silt loam, 1 to 8 percent slopes","Coolville",4,0.43,"PHEL"]
["Scioto","CpC","Coolville-Rarden silt loams, 8 to 15 percent slopes","Coolville",4,0.43,"HEL"]
["Scioto","Cu","Cuba silt loam, occasionally flooded","Cuba",5,0.37,"NHEL"]
["Scioto","DoA ","Doles silt loam, 0 to 3 percent slopes","Doles",4,0.43,"NHEL"]
["Scioto","Dp","Dumps","Dumps"]
["Scioto","EkB","Elkinsville silt loam, 1 to 8 percent slopes","Elkinsville",5,0.37,"PHEL"]
["Scioto","EkE","Elkinsville silt loam, 25 to 40 percent slopes","Elkinsville",5,0.37,"HEL"]
["Scioto","EmB","Elkinsville-Urban land complex, 1 to 8 percent slopes","Elkinsville",5,0.37,"PHEL"]
["Scioto","ErD","Ernest silt loam, 15 to 25 percent slopes","Ernest",3,0.43,"HEL"]
["Scioto","FcA","Fitchville silt loam, 0 to 3 percent slopes","Fitchville",5,0.37,"NHEL"]
["Scioto","Ge","Genesee silt loam, occasionally flooded","Genesee",5,0.37,"NHEL"]
["Scioto","Ha","Haymond silt loam, occasionally flooded","Haymond",5,0.37,"NHEL"]
["Scioto","Hu","Huntington silt loam, occasionally flooded","Huntington",5,0.28000000000000003,"NHEL"]
["Scioto","La","Landes fine sandy loam, occasionally flooded","Landes",5,0.2,"NHEL"]
["Scioto","LbC","Latham silt loam, 8 to 15 percent slopes","Latham",3,0.43,"HEL"]
["Scioto","LbD","Latham silt loam, 15 to 25 percent slopes","Latham",3,0.43,"HEL"]
["Scioto","LcE","Latham-Brownsville-Shelocta association, steep","Latham",3,0.43,"HEL"]
["Scioto","LgD","Latham-Gilpin association, hilly","Latham",3,0.43,"HEL"]
["Scioto","LsD","Latham-Steinsburg association, hilly","Latham",3,0.43,"HEL"]
["Scioto","MoB","Monongahela silt loam, 1 to 8 percent slopes","Monongahela",3,0.43,"PHEL"]
["Scioto","MoC2","Monongahela silt loam, 8 to 15 percent slopes, eroded","Monongahela",3,0.43,"HEL"]
["Scioto","No","Nolin silt loam, occasionally flooded","Nolin",5,0.43,"NHEL"]
["Scioto","OcB","Ockley loam, 1 to 8 percent slopes","Ockley",5,0.37,"PHEL"]
["Scioto","OmB","Omulga silt loam, 1 to 8 percent slopes","Omulga",3,0.43,"PHEL"]
["Scioto","OmC","Omulga silt loam, 8 to 15 percent slopes","Omulga",3,0.43,"HEL"]
["Scioto","OpB","Omulga-Urban land complex, 1 to 8 percent slopes","Omulga",3,0.43,"PHEL"]
["Scioto","OpC","Omulga-Urban land complex, 8 to 15 percent slopes","Omulga",3,0.43,"HEL"]
["Scioto","Pe","Peoga silt loam, rarely flooded","Peoga",4,0.43,"NHEL"]
["Scioto","Po","Piopolis silt loam, ponded","Piopolis",4,0.43,"NHEL"]
["Scioto","Ps","Pits, gravel","Pits"]
["Scioto","Pt","Pits, quarry","Pits"]
["Scioto","RbC","Rarden silt loam, 8 to 15 percent slopes","Rarden",3,0.43,"HEL"]
["Scioto","Ro","Rossburg silty clay loam, occasionally flooded","Rossburg",5,0.37,"NHEL"]
["Scioto","SaB","Sardinia silt loam, 1 to 8 percent slopes","Sardinia",5,0.37,"PHEL"]
["Scioto","SacB","Sciotoville silt loam, 1 to 8 percent slopes","Sciotoville",4,0.37,"PHEL"]
["Scioto","SbB","Shelocta silt loam, 3 to 8 percent slopes","Shelocta",4,0.32,"PHEL"]
["Scioto","SbC","Shelocta silt loam, 8 to 15 percent slopes","Shelocta",4,0.32,"PHEL"]
["Scioto","SbD","Shelocta silt loam, 15 to 25 percent slopes","Shelocta",4,0.32,"HEL"]
["Scioto","ScE","Shelocta-Brownsville association, steep","Shelocta",4,0.32,"HEL"]
["Scioto","ScF","Shelocta-Brownsville association, very steep","Shelocta",4,0.32,"HEL"]
["Scioto","SeF","Shelocta-Steinsburg association, very steep","Shelocta",4,0.32,"HEL"]
["Scioto","SfE","Shelocta-Wharton-Latham association, steep","Shelocta",4,0.32,"HEL"]
["Scioto","Sk","Skidmore silt loam, occasionally flooded","Skidmore",5,0.17,"NHEL"]
["Scioto","St","Stendal silt loam, occasionally flooded","Stendal",5,0.37,"NHEL"]
["Scioto","TcB","Tilsit-Coolville association, undulating","Tilsit",3,0.43,"HEL"]
["Scioto","To","Tioga loam, occasionally flooded","Tioga",5,0.37,"NHEL"]
["Scioto","Ud","Udorthents","Udorthents"]
["Scioto","W","Water","Water"]
["Scioto","WeA","Weinbach silt loam, 0 to 3 percent slopes","Weinbach",4,0.43,"NHEL"]
["Scioto","WfD","Wharton silt loam, 15 to 25 percent slopes","Wharton",3,0.37,"HEL"]
["Scioto","WkD","Wharton-Urban land complex, 8 to 20 percent slopes","Wharton",3,0.37,"HEL"]
["Scioto","WmB","Wheeling silt loam, 1 to 8 percent slopes","Wheeling",4,0.37,"PHEL"]
["Scioto","WpB","Wheeling-Urban land complex, 1 to 8 percent slopes","Wheeling",4,0.37,"PHEL"]
["Scioto","WyB","Wyatt silt loam, 1 to 8 percent slopes","Wyatt",3,0.43,"PHEL"]
["Scioto","WyC2","Wyatt silt loam, 8 to 15 percent slopes, eroded","Wyatt",3,0.43,"HEL"]
[null,"Select","None","none"]
["Vinton","AbC","Aaron silt loam, 6 to 15 percent slopes","Aaron",3,0.37,"HEL"]
["Vinton","BgC","Berks-Tarhollow complex, 6 to 15 percent slopes","Berks",3,0.24,"HEL"]
["Vinton","BhB","Bethesda silty clay loam, 0 to 8 percent slopes","Bethesda",3,0.43,"PHEL"]
["Vinton","BhC","Bethesda silty clay loam, 8 to 20 percent slopes","Bethesda",3,0.43,"HEL"]
["Vinton","BhE","Bethesda silty clay loam, 20 to 40 percent slopes","Bethesda",3,0.43,"HEL"]
["Vinton","BmC","Bethesda channery clay loam, 8 to 20 percent slopes","Bethesda",5,0.32,"HEL"]
["Vinton","BmE","Bethesda channery clay loam, 20 to 40 percent slopes","Bethesda",5,0.32,"HEL"]
["Vinton","BmF","Bethesda channery clay loam, 40 to 70 percent slopes","Bethesda",5,0.32,"HEL"]
["Vinton","Bo","Bonnie silt loam, frequently flooded","Bonnie",5,0.43,"NHEL"]
["Vinton","Bp","Bonnie silt loam, ponded","Bonnie",5,0.43,"NHEL"]
["Vinton","Cg","Chagrin silt loam, frequently flooded","Chagrin",5,0.32,"NHEL"]
["Vinton","ChA","Chavies silt loam, 0 to 2 percent slopes, rarely flooded","Chavies",4,0.24,"NHEL"]
["Vinton","ChB","Chavies silt loam, 2 to 6 percent slopes, rarely flooded","Chavies",4,0.24,"NHEL"]
["Vinton","CmC","Chavies silt loam, 6 to 15 percent slopes","Chavies",4,0.24,"PHEL"]
["Vinton","Cp","Clifty silt loam, occasionally flooded","Clifty",5,0.32,"NHEL"]
["Vinton","CwD","Cruze silt loam, 12 to 20 percent slopes","Cruze",3,0.37,"HEL"]
["Vinton","CwE","Cruze silt loam, 20 to 35 percent slopes","Cruze",3,0.37,"HEL"]
["Vinton","Cy","Cuba silt loam, frequently flooded","Cuba",5,0.37,"NHEL"]
["Vinton","DoA","Doles silt loam, 0 to 2 percent slopes","Doles",4,0.43,"NHEL"]
["Vinton","Dy","Dumps, mine","Dumps"]
["Vinton","ErC","Ernest silt loam, 6 to 15 percent slopes","Ernest",3,0.43,"HEL"]
["Vinton","ErD","Ernest silt loam, 15 to 25 percent slopes","Ernest",3,0.43,"HEL"]
["Vinton","FaB","Fairpoint clay loam, 0 to 8 percent slopes","Fairpoint",3,0.43,"PHEL"]
["Vinton","FaC","Fairpoint clay loam, 8 to 20 percent slopes","Fairpoint",3,0.43,"HEL"]
["Vinton","FcA","Fitchville silt loam, 0 to 2 percent slopes","Fitchville",5,0.37,"NHEL"]
["Vinton","GaC","Germano-Gilpin complex, 6 to 15 percent slopes","Germano",4,0.24,"PHEL"]
["Vinton","GaD","Germano-Gilpin complex, 15 to 25 percent slopes","Germano",4,0.24,"HEL"]
["Vinton","GaE","Germano-Gilpin complex, 25 to 40 percent slopes","Germano",4,0.24,"HEL"]
["Vinton","GbC2","Gilpin silt loam, 6 to 15 percent slopes, eroded","Gilpin",3,0.32,"HEL"]
["Vinton","GcC","Gilpin-Aaron complex, 6 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Vinton","GgD","Gilpin-Guernsey complex, 15 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Vinton","GgE","Gilpin-Guernsey complex, 25 to 40 percent slopes","Gilpin",3,0.32,"HEL"]
["Vinton","GgF","Gilpin-Guernsey complex, 40 to 70 percent slopes","Gilpin",3,0.32,"HEL"]
["Vinton","GhC","Gilpin-Rarden complex, 6 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Vinton","GhD","Gilpin-Rarden complex, 15 to 25 percent slopes","Gilpin",3,0.32,"HEL"]
["Vinton","GhE","Gilpin-Rarden complex, 25 to 40 percent slopes","Gilpin",3,0.32,"HEL"]
["Vinton","GmC","Gilpin-Tarhollow complex, 6 to 15 percent slopes","Gilpin",3,0.32,"HEL"]
["Vinton","GnA","Glenford silt loam, 0 to 2 percent slopes","Glenford",5,0.37,"NHEL"]
["Vinton","GnB","Glenford silt loam, 2 to 6 percent slopes","Glenford",5,0.37,"PHEL"]
["Vinton","LcB","Licking silt loam, 2 to 6 percent slopes","Licking",3,0.43,"PHEL"]
["Vinton","LcC2","Licking silt loam, 6 to 15 percent slopes","Licking",3,0.43,"HEL"]
["Vinton","LcD2","Licking silt loam, 15 to 25 percent slopes","Licking",3,0.43,"HEL"]
["Vinton","McA","McGary silty clay loam, 0 to 2 percent slopes","McGary",3,0.43,"NHEL"]
["Vinton","Nw","Newark silt loam, frequently flooded","Newark",5,0.32,"NHEL"]
["Vinton","OmA","Omulga silt loam, 0 to 2 percent slopes","Omulga",3,0.43,"NHEL"]
["Vinton","OmB","Omulga silt loam, 2 to 6 percent slopes","Omulga",3,0.43,"PHEL"]
["Vinton","OmC","Omulga silt loam, 6 to 15 percent slopes","Omulga",3,0.43,"HEL"]
["Vinton","Or","Orrville silt loam, frequently flooded","Orrville",5,0.37,"NHEL"]
["Vinton","Ph","Philo silt loam, frequently flooded","Philo",5,0.37,"NHEL"]
["Vinton","Pm","Piopolis silt loam, frequently flooded","Piopolis",4,0.43,"NHEL"]
["Vinton","Pn","Pope loam, occasionally flooded","Pope",5,0.37,"NHEL"]
["Vinton","Po","Pope loam, frequently flooded","Pope",5,0.37,"NHEL"]
["Vinton","RaC2","Rarden silt loam, 6 to 15 percent slopes","Rarden",3,0.43,"HEL"]
["Vinton","RbC2","Rarden-Wharton complex, 6 to 15 percent slopes","Rarden",3,0.43,"HEL"]
["Vinton","RbD2","Rarden-Wharton complex, 15 to 25 percent slopes","Rarden",3,0.43,"HEL"]
["Vinton","RcD","Richland loam, 15 to 25 percent slopes","Richland",5,0.37,"HEL"]
["Vinton","RcE","Richland loam, 25 to 40 percent slopes","Richland",5,0.37,"HEL"]
["Vinton","SbE","Sewell channery fine sandy loam, 20 to 40 percent slopes","Sewell",5,0.32,"HEL"]
["Vinton","SdE","Shelocta-Brownsville association, steep","Shelocta",4,0.32,"HEL"]
["Vinton","SdF","Shelocta-Brownsville association, very steep","Shelocta",4,0.32,"HEL"]
["Vinton","Sk","Skidmore gravelly loam, frequently flooded","Skidmore",5,0.17,"NHEL"]
["Vinton","StE","Steinsburg-Gilpin association, steep","Steinsburg",2,0.28000000000000003,"HEL"]
["Vinton","StF","Steinsburg-Gilpin association, very steep","Steinsburg",2,0.28000000000000003,"HEL"]
["Vinton","TaB","Tarhollow silt loam, 2 to 6 percent slopes","Tarhollow",5,0.43,"PHEL"]
["Vinton","TeB","Tilsit silt loam, 3 to 8 percent slopes","Tilsit",3,0.43,"PHEL"]
["Vinton","Tg","Tioga fine sandy loam, frequently flooded","Tioga",5,0.37,"NHEL"]
["Vinton","Ud","Udorthents","Udorthents"]
["Vinton","W","Water","Water"]
["Vinton","WbC","Wellston silt loam, 6 to 15 percent slopes","Wellston",4,0.37,"HEL"]
["Vinton","WkC","Wharton-Latham complex, 6 to 15 percent slopes","Wellston",3,0.37,"HEL"]
["Vinton","WkD","Wharton-Latham complex, 15 to 25 percent slopes","Wharton",3,0.37,"HEL"]
["Vinton","WkE","Wharton-Latham complex, 25 to 40 percent slopes","Wharton",3,0.37,"HEL"]
["Vinton","WtB","Wyatt silt loam, 2 to 6 percent slopes","Wyatt",3,0.43,"PHEL"]
["Vinton","WyC2","Wyatt silty clay loam, 6 to 15 percent slopes","Wyatt",2,0.43,"HEL"]
["Vinton","ZnB","Zanesville silt loam, 2 to 6 percent slopes","Zanesville",3,0.43,"PHEL"]

{"sheet":"R_Values","index":7,"n_rows":91,"n_cols":2,"rows_kept":91,"cut":false,"hidden":false,"merged":[]}
["Table 1. Ohio, R-Values"]
["County ","R-Values"]
["Select",0]
["Adams",175]
["Allen",125]
["Ashland",150]
["Ashtabula",125]
["Athens",150]
["Auglaize",150]
["Belmont",150]
["Brown",175]
["Butler",150]
["Carroll",150]
["Champaign",150]
["Clark",150]
["Clermont",175]
["Clinton",150]
["Columbiana",150]
["Coshocton",150]
["Crawford",125]
["Cuyahoga",125]
["Darke",150]
["Defiance",125]
["Delaware",150]
["Erie",125]
["Fairfield",150]
["Fayette",150]
["Franklin",150]
["Fulton",125]
["Gallia",150]
["Geauga",125]
["Greene",150]
["Guernsey",150]
["Hamilton",175]
["Hancock",125]
["Hardin",125]
["Harrison",150]
["Henry",125]
["Highland",150]
["Hocking",150]
["Holmes",150]
["Huron",125]
["Jackson",150]
["Jefferson",150]
["Knox",150]
["Lake",125]
["Lawrence",150]
["Licking",150]
["Logan",150]
["Lorain",125]
["Lucas",125]
["Madison",150]
["Mahoning",125]
["Marion",125]
["Medina",125]
["Meigs",150]
["Mercer",150]
["Miami",150]
["Monroe",150]
["Montgomery",150]
["Morgan",150]
["Morrow",150]
["Muskingum",150]
["Noble",150]
["Ottawa",125]
["Paulding",125]
["Perry",150]
["Pickaway",150]
["Pike",150]
["Portage",125]
["Preble",150]
["Putnam",125]
["Richland",150]
["Ross",150]
["Sandusky",125]
["Scioto",150]
["Seneca",125]
["Shelby",150]
["Stark",150]
["Summit",125]
["Trumbull",125]
["Tuscarawas",150]
["Union",150]
["Van_Wert",150]
["Vinton",150]
["Warren",150]
["Washington",150]
["Wayne",150]
["Williams",125]
["Wood",125]
["Wyandot",125]